D/RIL     ( 1891): Created IPC FMT client

D/RIL     ( 1891): Created IPC RFS client

D/RIL     ( 1891): Created SRS client

D/RIL-IPC ( 1891): Starting i9300 modem boot

D/RIL-IPC ( 1891): Opened modem image device

D/RIL-IPC ( 1891): Mapped modem image data to memory

D/RIL-IPC ( 1891): Opened modem boot device

D/RIL-IPC ( 1891): Opened modem link device

D/RIL-IPC ( 1891): Turned the modem off

D/RIL-IPC ( 1891): Turned the modem on

D/RIL-IPC ( 1891): Waited for link connected

D/RIL-IPC ( 1891): Wrote ATAT in ASCII

D/RIL-IPC ( 1891): Read chip id (0x16)

D/RIL-IPC ( 1891): Wrote PSI header

D/RIL-IPC ( 1891): Wrote PSI, CRC is 0xc8

D/RIL-IPC ( 1891): Wrote PSI CRC (0xc8)

D/RIL-IPC ( 1891): Read PSI CRC ACK

D/RIL-IPC ( 1891): Read PSI ACK

D/RIL-IPC ( 1891): Sent XMM626 HSIC PSI

D/RIL-IPC ( 1891): Wrote EBL size

D/RIL-IPC ( 1891): Wrote EBL, CRC is 0xb5

D/RIL-IPC ( 1891): Wrote EBL CRC (0xb5)

D/RIL-IPC ( 1891): Sent XMM626 HSIC EBL

D/RIL-IPC ( 1891): Read port config

D/RIL-IPC ( 1891): Sent XMM626 HSIC port config

D/RIL-IPC ( 1891): Sent XMM626 HSIC SEC start

D/RIL-IPC ( 1891): Sent XMM626 HSIC firmware

D/RIL-IPC ( 1891): Checked nv_data path

D/RIL-IPC ( 1891): Checked nv_data md5 path

D/RIL-IPC ( 1891): Calculated nv_data md5: 1455f7aaa8936eda837ebc27acf1c818

D/RIL-IPC ( 1891): Read nv_data md5: 1455f7aaa8936eda837ebc27acf1c818

D/RIL-IPC ( 1891): Checked nv_data backup path

D/RIL-IPC ( 1891): Loaded nv_data

D/RIL-IPC ( 1891): Sent XMM626 HSIC nv_data

D/RIL-IPC ( 1891): Sent XMM626 HSIC SEC end

D/RIL-IPC ( 1891): Sent XMM626 HSIC HW reset

D/RIL-IPC ( 1891): Waiting for host wake failed

D/RIL-IPC ( 1891): Waited for host wake

D/RIL-IPC ( 1891): Waited for link connected

D/RIL     ( 1891): Opened IPC FMT client

D/RIL     ( 1891): Started IPC FMT client loop

D/RIL     ( 1891): Opened IPC RFS client

D/RIL     ( 1891): Started IPC RFS client loop

D/RIL-SRS ( 1891): Started SRS server loop

D/RIL     ( 1891): Opened SRS client

D/RIL     ( 1891): Started SRS client loop

E/RILC    ( 1891): RIL_register: RIL version 7

D/RIL-IPC ( 1891): 

D/RIL-IPC ( 1891): xmm626_sec_modem_fmt_recv: Received FMT message

D/RIL-IPC ( 1891): xmm626_sec_modem_fmt_recv: Message: aseq=0xff, command=IPC_PWR_PHONE_PWR_UP, type=IPC_TYPE_NOTI, size=0

D/RIL     ( 1891): Updating RIL radio state to 0

D/RIL-IPC ( 1891): 

D/RIL-IPC ( 1891): xmm626_sec_modem_fmt_recv: Received FMT message

D/RIL-IPC ( 1891): xmm626_sec_modem_fmt_recv: Message: aseq=0x00, command=IPC_MISC_ME_IMSI, type=IPC_TYPE_NOTI, size=16

D/RIL-IPC ( 1891): ================================= IPC FMT data =================================

D/RIL-IPC ( 1891): [0000]   0F 30 30 30 30 30 30 30  30 30 30 30 30 30 30 30   .0000000 00000000

D/RIL-IPC ( 1891): ================================================================================

D/RIL-IPC ( 1891): 

D/RIL-IPC ( 1891): xmm626_sec_modem_fmt_recv: Received FMT message

D/RIL-IPC ( 1891): xmm626_sec_modem_fmt_recv: Message: aseq=0xff, command=IPC_NET_REGIST, type=IPC_TYPE_NOTI, size=11

D/RIL-IPC ( 1891): ================================= IPC FMT data =================================

D/RIL-IPC ( 1891): [0000]   FF 02 01 00 00 00 00 00  00 00 00                  ........ ...

D/RIL-IPC ( 1891): ================================================================================

D/RIL-IPC ( 1891): 

D/RIL-IPC ( 1891): xmm626_sec_modem_fmt_recv: Received FMT message

D/RIL-IPC ( 1891): xmm626_sec_modem_fmt_recv: Message: aseq=0xff, command=IPC_NET_REGIST, type=IPC_TYPE_NOTI, size=11

D/RIL-IPC ( 1891): ================================= IPC FMT data =================================

D/RIL-IPC ( 1891): [0000]   FF 03 01 00 00 00 00 00  00 00 00                  ........ ...

D/RIL-IPC ( 1891): ================================================================================

D/RIL-IPC ( 1891): 

D/RIL-IPC ( 1891): xmm626_sec_modem_fmt_recv: Received FMT message

D/RIL-IPC ( 1891): xmm626_sec_modem_fmt_recv: Message: aseq=0x00, command=IPC_DISP_ICON_INFO, type=IPC_TYPE_NOTI, size=4

D/RIL-IPC ( 1891): ================================= IPC FMT data =================================

D/RIL-IPC ( 1891): [0000]   FF 00 00 00                                        ....

D/RIL-IPC ( 1891): ================================================================================

I/PHONE   ( 2434): Network Mode set to 0

I/PHONE   ( 2434): Cdma Subscription set to 1

I/PHONE   ( 2434): RILClassname is RIL

D/RILJ    ( 2434): RIL(context, preferredNetworkType=0 cdmaSubscription=1)

D/RILJ    ( 2434): Starting RILReceiver

D/RIL_UiccController( 2434): Creating UiccController

I/PHONE   ( 2434): Creating GSMPhone

I/RILC    ( 1891): libril: new connection

I/RILC    ( 1891): RIL Daemon version: Samsung-RIL

I/RILJ    ( 2434): Connected to 'rild' socket

D/RILJ    ( 2434): [UNSL]< UNSOL_RIL_CONNECTED {7}

D/RILJ    ( 2434): [0000]> RADIO_POWER off

D/RIL     ( 1891): 1 RIL request in the queue (1 pending, 0 handled, 0 unhandled)

D/RIL     ( 1891): Requesting low power mode power state

D/RIL-IPC ( 1891): 

D/RIL-IPC ( 1891): xmm626_sec_modem_fmt_send: Sent FMT message

D/RIL-IPC ( 1891): xmm626_sec_modem_fmt_send: Message: mseq=0x01, command=IPC_PWR_PHONE_STATE, type=IPC_TYPE_EXEC, size=2

D/RIL-IPC ( 1891): ================================= IPC FMT data =================================

D/RIL-IPC ( 1891): [0000]   01 00                                              ..

D/RIL-IPC ( 1891): ================================================================================

D/RILJ    ( 2434): [0001]> REQUEST_SET_PREFERRED_NETWORK_TYPE : 0

D/RIL     ( 1891): 2 RIL requests in the queue (1 pending, 1 handled, 0 unhandled)

D/RIL-IPC ( 1891): 

D/RIL-IPC ( 1891): xmm626_sec_modem_fmt_send: Sent FMT message

D/RIL-IPC ( 1891): xmm626_sec_modem_fmt_send: Message: mseq=0x02, command=IPC_NET_MODE_SEL, type=IPC_TYPE_SET, size=1

D/RIL-IPC ( 1891): ================================= IPC FMT data =================================

D/RIL-IPC ( 1891): [0000]   01                                                 .

D/RIL-IPC ( 1891): ================================================================================

D/RILJ    ( 2434): [0002]> RIL_REQUEST_CDMA_SET_SUBSCRIPTION_SOURCE : 1

D/RIL     ( 1891): 3 RIL requests in the queue (1 pending, 2 handled, 0 unhandled)

D/RIL     ( 1891): Unhandled RIL request: 77

D/RIL     ( 1891): 2 RIL requests in the queue (0 pending, 2 handled, 0 unhandled)

D/RILJ    ( 2434): [UNSL]< UNSOL_RESPONSE_RADIO_STATE_CHANGED RADIO_OFF

D/RILB    ( 2434): Notifying: radio available

D/RILJ    ( 2434): [0003]> SCREEN_STATE: true

D/RIL     ( 1891): 3 RIL requests in the queue (1 pending, 2 handled, 0 unhandled)

D/RILJ    ( 2434): [0002]< RIL_REQUEST_CDMA_SET_SUBSCRIPTION_SOURCE error: com.android.internal.telephony.CommandException: REQUEST_NOT_SUPPORTED

D/PHONE   ( 2434): mDoesRilSendMultipleCallRing=false

D/PHONE   ( 2434): mCallRingDelay=3000

D/RILJ    ( 2434): setPhoneType=1 old value=0

D/RIL-IPC ( 1891): 

D/RIL-IPC ( 1891): xmm626_sec_modem_fmt_recv: Received FMT message

D/RIL-IPC ( 1891): xmm626_sec_modem_fmt_recv: Message: aseq=0x01, command=IPC_GEN_PHONE_RES, type=IPC_TYPE_RESP, size=5

D/RIL-IPC ( 1891): ================================= IPC FMT data =================================

D/RIL-IPC ( 1891): [0000]   01 07 01 00 80                                     .....

D/RIL-IPC ( 1891): ================================================================================

D/RIL     ( 1891): Generic response was expected

D/RIL-IPC ( 1891): 

D/RIL-IPC ( 1891): xmm626_sec_modem_fmt_recv: Received FMT message

D/RIL-IPC ( 1891): xmm626_sec_modem_fmt_recv: Message: aseq=0x01, command=IPC_PWR_PHONE_STATE, type=IPC_TYPE_NOTI, size=1

D/RIL-IPC ( 1891): ================================= IPC FMT data =================================

D/RIL-IPC ( 1891): [0000]   01                                                 .

D/RIL-IPC ( 1891): ================================================================================

D/RIL     ( 1891): Power state is low power mode

D/RIL     ( 1891): 2 RIL requests in the queue (0 pending, 1 handled, 1 unhandled)

D/RILJ    ( 2434): [0000]< RADIO_POWER 

D/RIL-IPC ( 1891): 

D/RIL-IPC ( 1891): xmm626_sec_modem_fmt_recv: Received FMT message

D/RIL-IPC ( 1891): xmm626_sec_modem_fmt_recv: Message: aseq=0x02, command=IPC_GEN_PHONE_RES, type=IPC_TYPE_RESP, size=5

D/RIL-IPC ( 1891): ================================= IPC FMT data =================================

D/RIL-IPC ( 1891): [0000]   08 0A 03 00 80                                     .....

D/RIL-IPC ( 1891): ================================================================================

D/RIL     ( 1891): Generic response was expected

D/RIL     ( 1891): 1 RIL request in the queue (0 pending, 0 handled, 1 unhandled)

D/RILJ    ( 2434): [0001]< REQUEST_SET_PREFERRED_NETWORK_TYPE 

D/SMS     ( 2434): SMSDispatcher: ctor mSmsCapable=true format=3gpp mSmsReceiveDisabled=false mSmsSendDisabled=false

D/GSM     ( 2434): [GsmDCT] DCT.constructor

D/GSM     ( 2434): [GsmDCT] GsmDCT.constructor

D/GSM     ( 2434): [ApnContext:default] set mDependencyMet as false current state is true

D/GSM     ( 2434): [ApnContext:default] set enabled as true, current state is false

D/GSM     ( 2434): [GsmDCT] applyNewState(default, true(true), true(false))

D/GSM     ( 2434): [ApnContext:default] set reason as dependencyMet,current state IDLE

D/GSM     ( 2434): [ApnContext:default] set enabled as true, current state is true

D/GSM     ( 2434): [ApnContext:default] set mDependencyMet as true current state is false

D/GSM     ( 2434): [GsmDCT] trySetupData for type:default due to dependencyMet

D/GSM     ( 2434): [GsmDCT] trySetupData with mIsPsRestricted=false

D/GSM     ( 2434): [GsmDCT] isDataAllowed: not allowed due to - gprs= 1 - SIM not loaded

D/GSM     ( 2434): [GsmDCT] notifyOffApnsOfAvailability skipped apn due to isReady==false: {mApnType=default mState=IDLE mWaitingApns=null mWaitingApnsPermanentFailureCountDown=0 mApnSetting=null mDataConnectionAc=null mReason=dependencyMet mRetryCount=0 mDataEnabled=true mDependencyMet=true}

D/GSM     ( 2434): [ApnContext:mms] set mDependencyMet as false current state is true

D/GSM     ( 2434): [GsmDCT] applyNewState(mms, false(false), true(false))

D/GSM     ( 2434): [ApnContext:mms] set enabled as false, current state is false

D/GSM     ( 2434): [ApnContext:mms] set mDependencyMet as true current state is false

D/GSM     ( 2434): [ApnContext:supl] set mDependencyMet as false current state is true

D/GSM     ( 2434): [GsmDCT] applyNewState(supl, false(false), true(false))

D/GSM     ( 2434): [ApnContext:supl] set enabled as false, current state is false

D/GSM     ( 2434): [ApnContext:supl] set mDependencyMet as true current state is false

D/GSM     ( 2434): [ApnContext:dun] set mDependencyMet as false current state is true

D/GSM     ( 2434): [GsmDCT] applyNewState(dun, false(false), true(false))

D/GSM     ( 2434): [ApnContext:dun] set enabled as false, current state is false

D/GSM     ( 2434): [ApnContext:dun] set mDependencyMet as true current state is false

D/GSM     ( 2434): [ApnContext:hipri] set mDependencyMet as false current state is true

D/GSM     ( 2434): [GsmDCT] applyNewState(hipri, false(false), true(false))

D/GSM     ( 2434): [ApnContext:hipri] set enabled as false, current state is false

D/GSM     ( 2434): [ApnContext:hipri] set mDependencyMet as true current state is false

D/RILB    ( 2434): registerForRilConnected h=Handler (com.android.internal.telephony.PhoneProxy) {415bb620} w=4

D/RILB    ( 2434): Notifying: ril connected mRilVersion=7

D/RIL_IccCardProxy( 2434): Creating

D/RIL_IccCardProxy( 2434): Broadcasting intent ACTION_SIM_STATE_CHANGED NOT_READY reason null

D/RIL_IccCardProxy( 2434): Setting radio tech UMTS

D/RIL_IccCardProxy( 2434): updateQuietMode: 3GPP subscription -> newQuietMode=false

D/RIL_IccCardProxy( 2434): updateQuietMode: QuietMode is false (app_type=1 isLteOnCdmaMode=false cdmaSource=-1)

D/RILJ    ( 2434): [0004]> SET_SUPP_SVC_NOTIFICATION

D/RIL     ( 1891): 2 RIL requests in the queue (1 pending, 0 handled, 1 unhandled)

D/RIL     ( 1891): Unhandled RIL request: 62

D/RIL     ( 1891): 1 RIL request in the queue (0 pending, 0 handled, 1 unhandled)

D/RILJ    ( 2434): [0004]< SET_SUPP_SVC_NOTIFICATION error: com.android.internal.telephony.CommandException: REQUEST_NOT_SUPPORTED

D/RILJ    ( 2434): [0005]> RADIO_POWER on

D/RIL     ( 1891): 2 RIL requests in the queue (1 pending, 0 handled, 1 unhandled)

D/RIL     ( 1891): Requesting normal power state

D/RIL-IPC ( 1891): 

D/RIL-IPC ( 1891): xmm626_sec_modem_fmt_send: Sent FMT message

D/RIL-IPC ( 1891): xmm626_sec_modem_fmt_send: Message: mseq=0x03, command=IPC_PWR_PHONE_STATE, type=IPC_TYPE_EXEC, size=2

D/RIL-IPC ( 1891): ================================= IPC FMT data =================================

D/GSM     ( 2434): [GsmSST] Poll ServiceState done:  oldSS=[1 home null null null  Unknown CSS not supported 0 0 RoamInd=0 DefRoamInd=0 EmergOnly=false] newSS=[3 home null null null  Unknown CSS not supported -1 -1 RoamInd=-1 DefRoamInd=-1 EmergOnly=false] oldGprs=1 newData=1 oldMaxDataCalls=1 mNewMaxDataCalls=1 oldReasonDataDenied=-1 mNewReasonDataDenied=-1 oldType=Unknown newType=Unknown

D/RIL-IPC ( 1891): [0000]   02 02                                              ..

D/RIL-IPC ( 1891): ================================================================================

D/GSM     ( 2434): [GsmSST] updateSpnDisplay: radio is off w/ showPlmn=false plmn=null

D/GSM     ( 2434): [GsmSST] updateSpnDisplay: changed sending intent rule=0 showPlmn='false' plmn='null' showSpn='false' spn=''

D/GSM     ( 2434): [GsmSST] operatorNumeric is null

D/GSM     ( 2434): [GsmDCT] handleMessage msg={ what=270369 when=-111ms obj=android.os.AsyncResult@415ccfe8 }

D/GSM     ( 2434): [GsmDCT] handleMessage msg={ what=270337 when=-97ms obj=android.os.AsyncResult@415cdbb0 }

D/GSM     ( 2434): [GsmDCT] onRadioAvailable

D/GSM     ( 2434): [GsmDCT] overall state is IDLE

D/GSM     ( 2434): [GsmDCT] handleMessage msg={ what=270342 when=-98ms obj=android.os.AsyncResult@415cdca0 }

D/GSM     ( 2434): [ApnContext:dun] setRetryCount: 0

D/GSM     ( 2434): [ApnContext:supl] setRetryCount: 0

D/GSM     ( 2434): [ApnContext:hipri] setRetryCount: 0

D/GSM     ( 2434): [ApnContext:default] setRetryCount: 0

D/GSM     ( 2434): [ApnContext:mms] setRetryCount: 0

D/GSM     ( 2434): [GsmDCT] onRadioOffOrNotAvailable: is off and clean up all connections

D/GSM     ( 2434): [GsmDCT] cleanUpAllConnections: tearDown=false reason=radioTurnedOff

D/GSM     ( 2434): [ApnContext:dun] set reason as radioTurnedOff,current state IDLE

D/GSM     ( 2434): [GsmDCT] cleanUpConnection: E tearDown=false reason=radioTurnedOff apnContext={mApnType=dun mState=IDLE mWaitingApns=null mWaitingApnsPermanentFailureCountDown=0 mApnSetting=null mDataConnectionAc=null mReason=radioTurnedOff mRetryCount=0 mDataEnabled=false mDependencyMet=true}

D/GSM     ( 2434): [ApnContext:dun] setState: IDLE, previous state:IDLE

D/GSM     ( 2434): [GsmDCT] isDataAllowed: not allowed due to - gprs= 1 - SIM not loaded

D/GSM     ( 2434): [GsmDCT] isDataPossible(dun): possible=false isDataAllowed=false apnTypePossible=true apnContextisEnabled=false apnContextState()=IDLE

D/RIL-IPC ( 1891): 

D/RIL-IPC ( 1891): xmm626_sec_modem_fmt_recv: Received FMT message

D/RIL-IPC ( 1891): xmm626_sec_modem_fmt_recv: Message: aseq=0x03, command=IPC_GEN_PHONE_RES, type=IPC_TYPE_RESP, size=5

D/GSM     ( 2434): [GsmDCT] get active apn string for type:dun

D/RIL-IPC ( 1891): ================================= IPC FMT data =================================

D/RIL-IPC ( 1891): [0000]   01 07 01 00 80                                     .....

D/RIL-IPC ( 1891): ================================================================================

D/RIL     ( 1891): Generic response was expected

D/RIL-IPC ( 1891): 

D/RIL-IPC ( 1891): xmm626_sec_modem_fmt_recv: Received FMT message

D/RIL-IPC ( 1891): xmm626_sec_modem_fmt_recv: Message: aseq=0x03, command=IPC_PWR_PHONE_STATE, type=IPC_TYPE_NOTI, size=1

D/RIL-IPC ( 1891): ================================= IPC FMT data =================================

D/RIL-IPC ( 1891): [0000]   02                                                 .

D/RIL-IPC ( 1891): ================================================================================

D/RIL     ( 1891): Power state is normal

D/RIL     ( 1891): 1 RIL request in the queue (0 pending, 0 handled, 1 unhandled)

D/RIL     ( 1891): Updating RIL radio state to 2

D/RIL-IPC ( 1891): 

D/RIL-IPC ( 1891): xmm626_sec_modem_fmt_recv: Received FMT message

D/RIL-IPC ( 1891): xmm626_sec_modem_fmt_recv: Message: aseq=0xff, command=IPC_NET_REGIST, type=IPC_TYPE_NOTI, size=11

D/RIL-IPC ( 1891): ================================= IPC FMT data =================================

D/RIL-IPC ( 1891): [0000]   FF 02 01 00 00 00 00 00  00 00 00                  ........ ...

D/RIL-IPC ( 1891): ================================================================================

D/RIL-IPC ( 1891): 

D/RIL-IPC ( 1891): xmm626_sec_modem_fmt_recv: Received FMT message

D/RIL-IPC ( 1891): xmm626_sec_modem_fmt_recv: Message: aseq=0xff, command=IPC_NET_REGIST, type=IPC_TYPE_NOTI, size=11

D/RIL-IPC ( 1891): ================================= IPC FMT data =================================

D/RIL-IPC ( 1891): [0000]   FF 03 01 00 00 00 00 00  00 00 00                  ........ ...

D/RIL-IPC ( 1891): ================================================================================

D/RIL     ( 1891): 0 RIL request in the queue (0 pending, 0 handled, 0 unhandled)

D/RIL     ( 1891): 2 RIL requests data in the queue

D/RIL-IPC ( 1891): 

D/RIL-IPC ( 1891): xmm626_sec_modem_rfs_recv: Received RFS message

D/RIL-IPC ( 1891): xmm626_sec_modem_rfs_recv: Message: aseq=0x01, command=IPC_RFS_NV_WRITE_ITEM, size=12

D/RIL-IPC ( 1891): ================================= IPC RFS data =================================

D/RIL-IPC ( 1891): [0000]   09 00 1A 00 04 00 00 00  0F 00 93 40               ........ ...@

D/RIL-IPC ( 1891): ================================================================================

D/RIL-IPC ( 1891): Checked nv_data path

D/RILJ    ( 2434): [0005]< RADIO_POWER 

D/RILJ    ( 2434): [UNSL]< UNSOL_VOICE_RADIO_TECH_CHANGED {3}

D/RILJ    ( 2434): [UNSL]< UNSOL_RESPONSE_RADIO_STATE_CHANGED RADIO_ON

D/RILB    ( 2434): Notifying: Radio On

D/RILJ    ( 2434): [UNSL]< UNSOL_RESPONSE_VOICE_NETWORK_STATE_CHANGED

D/RILJ    ( 2434): [UNSL]< UNSOL_RESPONSE_VOICE_NETWORK_STATE_CHANGED

D/RILJ    ( 2434): [UNSL]< UNSOL_RESPONSE_VOICE_NETWORK_STATE_CHANGED

D/RILJ    ( 2434): [0003]< SCREEN_STATE 

D/GSM     ( 2434): [ApnContext:dun] setDataConnection: old dc=null new dc=null this={mApnType=dun mState=IDLE mWaitingApns=null mWaitingApnsPermanentFailureCountDown=0 mApnSetting=null mDataConnectionAc=null mReason=radioTurnedOff mRetryCount=0 mDataEnabled=false mDependencyMet=true}

D/GSM     ( 2434): [ApnContext:dun] setDataConnectionAc: old dcac=null new dcac=null

D/GSM     ( 2434): [GsmDCT] cleanUpConnection: X tearDown=false reason=radioTurnedOff apnContext={mApnType=dun mState=IDLE mWaitingApns=null mWaitingApnsPermanentFailureCountDown=0 mApnSetting=null mDataConnectionAc=null mReason=radioTurnedOff mRetryCount=0 mDataEnabled=false mDependencyMet=true} dc=null

D/GSM     ( 2434): [ApnContext:supl] set reason as radioTurnedOff,current state IDLE

D/GSM     ( 2434): [GsmDCT] cleanUpConnection: E tearDown=false reason=radioTurnedOff apnContext={mApnType=supl mState=IDLE mWaitingApns=null mWaitingApnsPermanentFailureCountDown=0 mApnSetting=null mDataConnectionAc=null mReason=radioTurnedOff mRetryCount=0 mDataEnabled=false mDependencyMet=true}

D/GSM     ( 2434): [ApnContext:supl] setState: IDLE, previous state:IDLE

D/GSM     ( 2434): [GsmDCT] isDataAllowed: not allowed due to - gprs= 1 - SIM not loaded

D/GSM     ( 2434): [GsmDCT] isDataPossible(supl): possible=false isDataAllowed=false apnTypePossible=true apnContextisEnabled=false apnContextState()=IDLE

D/GSM     ( 2434): [GsmDCT] get active apn string for type:supl

D/GSM     ( 2434): [ApnContext:supl] setDataConnection: old dc=null new dc=null this={mApnType=supl mState=IDLE mWaitingApns=null mWaitingApnsPermanentFailureCountDown=0 mApnSetting=null mDataConnectionAc=null mReason=radioTurnedOff mRetryCount=0 mDataEnabled=false mDependencyMet=true}

D/GSM     ( 2434): [ApnContext:supl] setDataConnectionAc: old dcac=null new dcac=null

D/GSM     ( 2434): [GsmDCT] cleanUpConnection: X tearDown=false reason=radioTurnedOff apnContext={mApnType=supl mState=IDLE mWaitingApns=null mWaitingApnsPermanentFailureCountDown=0 mApnSetting=null mDataConnectionAc=null mReason=radioTurnedOff mRetryCount=0 mDataEnabled=false mDependencyMet=true} dc=null

D/GSM     ( 2434): [ApnContext:hipri] set reason as radioTurnedOff,current state IDLE

D/GSM     ( 2434): [GsmDCT] cleanUpConnection: E tearDown=false reason=radioTurnedOff apnContext={mApnType=hipri mState=IDLE mWaitingApns=null mWaitingApnsPermanentFailureCountDown=0 mApnSetting=null mDataConnectionAc=null mReason=radioTurnedOff mRetryCount=0 mDataEnabled=false mDependencyMet=true}

D/GSM     ( 2434): [ApnContext:hipri] setState: IDLE, previous state:IDLE

D/GSM     ( 2434): [GsmDCT] isDataAllowed: not allowed due to - gprs= 1 - SIM not loaded

D/GSM     ( 2434): [GsmDCT] isDataPossible(hipri): possible=false isDataAllowed=false apnTypePossible=true apnContextisEnabled=false apnContextState()=IDLE

D/GSM     ( 2434): [GsmDCT] get active apn string for type:hipri

D/GSM     ( 2434): [ApnContext:hipri] setDataConnection: old dc=null new dc=null this={mApnType=hipri mState=IDLE mWaitingApns=null mWaitingApnsPermanentFailureCountDown=0 mApnSetting=null mDataConnectionAc=null mReason=radioTurnedOff mRetryCount=0 mDataEnabled=false mDependencyMet=true}

D/GSM     ( 2434): [ApnContext:hipri] setDataConnectionAc: old dcac=null new dcac=null

D/GSM     ( 2434): [GsmDCT] cleanUpConnection: X tearDown=false reason=radioTurnedOff apnContext={mApnType=hipri mState=IDLE mWaitingApns=null mWaitingApnsPermanentFailureCountDown=0 mApnSetting=null mDataConnectionAc=null mReason=radioTurnedOff mRetryCount=0 mDataEnabled=false mDependencyMet=true} dc=null

D/GSM     ( 2434): [ApnContext:default] set reason as radioTurnedOff,current state IDLE

D/GSM     ( 2434): [GsmDCT] cleanUpConnection: E tearDown=false reason=radioTurnedOff apnContext={mApnType=default mState=IDLE mWaitingApns=null mWaitingApnsPermanentFailureCountDown=0 mApnSetting=null mDataConnectionAc=null mReason=radioTurnedOff mRetryCount=0 mDataEnabled=true mDependencyMet=true}

D/GSM     ( 2434): [ApnContext:default] setState: IDLE, previous state:IDLE

D/GSM     ( 2434): [GsmDCT] isDataAllowed: not allowed due to - gprs= 1 - SIM not loaded

D/GSM     ( 2434): [GsmDCT] isDataPossible(default): possible=false isDataAllowed=false apnTypePossible=true apnContextisEnabled=true apnContextState()=IDLE

D/GSM     ( 2434): [GsmDCT] get active apn string for type:default

D/GSM     ( 2434): [ApnContext:default] setDataConnection: old dc=null new dc=null this={mApnType=default mState=IDLE mWaitingApns=null mWaitingApnsPermanentFailureCountDown=0 mApnSetting=null mDataConnectionAc=null mReason=radioTurnedOff mRetryCount=0 mDataEnabled=true mDependencyMet=true}

D/GSM     ( 2434): [ApnContext:default] setDataConnectionAc: old dcac=null new dcac=null

D/GSM     ( 2434): [GsmDCT] cleanUpConnection: X tearDown=false reason=radioTurnedOff apnContext={mApnType=default mState=IDLE mWaitingApns=null mWaitingApnsPermanentFailureCountDown=0 mApnSetting=null mDataConnectionAc=null mReason=radioTurnedOff mRetryCount=0 mDataEnabled=true mDependencyMet=true} dc=null

D/GSM     ( 2434): [ApnContext:mms] set reason as radioTurnedOff,current state IDLE

D/GSM     ( 2434): [GsmDCT] cleanUpConnection: E tearDown=false reason=radioTurnedOff apnContext={mApnType=mms mState=IDLE mWaitingApns=null mWaitingApnsPermanentFailureCountDown=0 mApnSetting=null mDataConnectionAc=null mReason=radioTurnedOff mRetryCount=0 mDataEnabled=false mDependencyMet=true}

D/GSM     ( 2434): [ApnContext:mms] setState: IDLE, previous state:IDLE

D/GSM     ( 2434): [GsmDCT] isDataAllowed: not allowed due to - gprs= 1 - SIM not loaded

D/GSM     ( 2434): [GsmDCT] isDataPossible(mms): possible=false isDataAllowed=false apnTypePossible=true apnContextisEnabled=false apnContextState()=IDLE

D/GSM     ( 2434): [GsmDCT] get active apn string for type:mms

D/GSM     ( 2434): [ApnContext:mms] setDataConnection: old dc=null new dc=null this={mApnType=mms mState=IDLE mWaitingApns=null mWaitingApnsPermanentFailureCountDown=0 mApnSetting=null mDataConnectionAc=null mReason=radioTurnedOff mRetryCount=0 mDataEnabled=false mDependencyMet=true}

D/GSM     ( 2434): [ApnContext:mms] setDataConnectionAc: old dcac=null new dcac=null

D/GSM     ( 2434): [GsmDCT] cleanUpConnection: X tearDown=false reason=radioTurnedOff apnContext={mApnType=mms mState=IDLE mWaitingApns=null mWaitingApnsPermanentFailureCountDown=0 mApnSetting=null mDataConnectionAc=null mReason=radioTurnedOff mRetryCount=0 mDataEnabled=false mDependencyMet=true} dc=null

D/GSM     ( 2434): [GsmDCT] stopNetStatPoll

D/GSM     ( 2434): [GsmDCT] notifyOffApnOfAvailability type:dun

D/GSM     ( 2434): [GsmDCT] isDataAllowed: not allowed due to - gprs= 1 - SIM not loaded

D/GSM     ( 2434): [GsmDCT] isDataPossible(dun): possible=false isDataAllowed=false apnTypePossible=true apnContextisEnabled=false apnContextState()=IDLE

D/GSM     ( 2434): [GsmDCT] get active apn string for type:dun

D/RIL-RFS ( 1891): Wrote 4 nv_data byte(s) at offset 0x1a0009

D/RIL-IPC ( 1891): 

D/RIL-IPC ( 1891): xmm626_sec_modem_rfs_send: Sent RFS message

D/RIL-IPC ( 1891): xmm626_sec_modem_rfs_send: Message: mseq=0x01, command=IPC_RFS_NV_WRITE_ITEM, size=9

D/RIL-IPC ( 1891): ================================= IPC RFS data =================================

D/RIL-IPC ( 1891): [0000]   01 09 00 1A 00 04 00 00  00                        ........ .

D/RIL-IPC ( 1891): ================================================================================

D/RIL-IPC ( 1891): 

D/RIL-IPC ( 1891): xmm626_sec_modem_fmt_recv: Received FMT message

D/RIL-IPC ( 1891): xmm626_sec_modem_fmt_recv: Message: aseq=0x00, command=IPC_DISP_ICON_INFO, type=IPC_TYPE_NOTI, size=4

D/RIL-IPC ( 1891): ================================= IPC FMT data =================================

D/RIL-IPC ( 1891): [0000]   FF 00 00 05                                        ....

D/RIL-IPC ( 1891): ================================================================================

D/RIL     ( 1891): Signal strength is 1

D/GSM     ( 2434): [GsmDCT] notifyOffApnOfAvailability type:supl

D/GSM     ( 2434): [GsmDCT] isDataAllowed: not allowed due to - gprs= 1 - SIM not loaded

D/GSM     ( 2434): [GsmDCT] isDataPossible(supl): possible=false isDataAllowed=false apnTypePossible=true apnContextisEnabled=false apnContextState()=IDLE

D/GSM     ( 2434): [GsmDCT] get active apn string for type:supl

D/RIL-IPC ( 1891): 

D/RIL-IPC ( 1891): xmm626_sec_modem_rfs_recv: Received RFS message

D/RIL-IPC ( 1891): xmm626_sec_modem_rfs_recv: Message: aseq=0x01, command=IPC_RFS_NV_WRITE_ITEM, size=9

D/RIL-IPC ( 1891): ================================= IPC RFS data =================================

D/RIL-IPC ( 1891): [0000]   10 00 1A 00 01 00 00 00  02                        ........ .

D/RIL-IPC ( 1891): ================================================================================

D/RIL-IPC ( 1891): Checked nv_data path

D/GSM     ( 2434): [GsmDCT] notifyOffApnOfAvailability type:hipri

D/GSM     ( 2434): [GsmDCT] isDataAllowed: not allowed due to - gprs= 1 - SIM not loaded

D/GSM     ( 2434): [GsmDCT] isDataPossible(hipri): possible=false isDataAllowed=false apnTypePossible=true apnContextisEnabled=false apnContextState()=IDLE

D/GSM     ( 2434): [GsmDCT] get active apn string for type:hipri

D/GSM     ( 2434): [GsmDCT] notifyOffApnsOfAvailability skipped apn due to isReady==false: {mApnType=default mState=IDLE mWaitingApns=null mWaitingApnsPermanentFailureCountDown=0 mApnSetting=null mDataConnectionAc=null mReason=radioTurnedOff mRetryCount=0 mDataEnabled=true mDependencyMet=true}

D/GSM     ( 2434): [GsmDCT] notifyOffApnOfAvailability type:mms

D/GSM     ( 2434): [GsmDCT] isDataAllowed: not allowed due to - gprs= 1 - SIM not loaded

D/GSM     ( 2434): [GsmDCT] isDataPossible(mms): possible=false isDataAllowed=false apnTypePossible=true apnContextisEnabled=false apnContextState()=IDLE

D/GSM     ( 2434): [GsmDCT] get active apn string for type:mms

D/GSM     ( 2434): [GsmDCT] handleMessage msg={ what=270345 when=-140ms obj=android.os.AsyncResult@415cdf78 }

D/GSM     ( 2434): [GsmDCT] onDataConnectionDetached: stop polling and notify detached

D/GSM     ( 2434): [GsmDCT] stopNetStatPoll

D/GSM     ( 2434): [GsmDCT] notifyDataConnection: reason=dataDetached

D/GSM     ( 2434): [GsmDCT] notifyDataConnection: type:default

D/GSM     ( 2434): [GsmDCT] isDataAllowed: not allowed due to - gprs= 1 - SIM not loaded

D/GSM     ( 2434): [GsmDCT] isDataPossible(default): possible=false isDataAllowed=false apnTypePossible=true apnContextisEnabled=true apnContextState()=IDLE

D/GSM     ( 2434): [GsmDCT] get active apn string for type:default

D/GSM     ( 2434): [GsmDCT] notifyOffApnOfAvailability type:dun

D/GSM     ( 2434): [GsmDCT] isDataAllowed: not allowed due to - gprs= 1 - SIM not loaded

D/GSM     ( 2434): [GsmDCT] isDataPossible(dun): possible=false isDataAllowed=false apnTypePossible=true apnContextisEnabled=false apnContextState()=IDLE

D/GSM     ( 2434): [GsmDCT] get active apn string for type:dun

D/GSM     ( 2434): [GsmDCT] notifyOffApnOfAvailability type:supl

D/GSM     ( 2434): [GsmDCT] isDataAllowed: not allowed due to - gprs= 1 - SIM not loaded

D/GSM     ( 2434): [GsmDCT] isDataPossible(supl): possible=false isDataAllowed=false apnTypePossible=true apnContextisEnabled=false apnContextState()=IDLE

D/GSM     ( 2434): [GsmDCT] get active apn string for type:supl

D/GSM     ( 2434): [GsmDCT] notifyOffApnOfAvailability type:hipri

D/GSM     ( 2434): [GsmDCT] isDataAllowed: not allowed due to - gprs= 1 - SIM not loaded

D/GSM     ( 2434): [GsmDCT] isDataPossible(hipri): possible=false isDataAllowed=false apnTypePossible=true apnContextisEnabled=false apnContextState()=IDLE

D/GSM     ( 2434): [GsmDCT] get active apn string for type:hipri

D/GSM     ( 2434): [GsmDCT] notifyOffApnsOfAvailability skipped apn due to isReady==false: {mApnType=default mState=IDLE mWaitingApns=null mWaitingApnsPermanentFailureCountDown=0 mApnSetting=null mDataConnectionAc=null mReason=radioTurnedOff mRetryCount=0 mDataEnabled=true mDependencyMet=true}

D/GSM     ( 2434): [GsmDCT] notifyOffApnOfAvailability type:mms

D/GSM     ( 2434): [GsmDCT] isDataAllowed: not allowed due to - gprs= 1 - SIM not loaded

D/GSM     ( 2434): [GsmDCT] isDataPossible(mms): possible=false isDataAllowed=false apnTypePossible=true apnContextisEnabled=false apnContextState()=IDLE

D/GSM     ( 2434): [GsmDCT] get active apn string for type:mms

D/RIL-RFS ( 1891): Wrote 1 nv_data byte(s) at offset 0x1a0010

D/RIL-IPC ( 1891): 

D/RIL-IPC ( 1891): xmm626_sec_modem_rfs_send: Sent RFS message

D/RIL-IPC ( 1891): xmm626_sec_modem_rfs_send: Message: mseq=0x01, command=IPC_RFS_NV_WRITE_ITEM, size=9

D/RIL-IPC ( 1891): ================================= IPC RFS data =================================

D/RIL-IPC ( 1891): [0000]   01 10 00 1A 00 01 00 00  00                        ........ .

D/RIL-IPC ( 1891): ================================================================================

D/GSM     ( 2434): [GsmDCT] handleMessage msg={ what=270348 when=-148ms obj=android.os.AsyncResult@415ce0d0 }

D/GSM     ( 2434): [ApnContext:dun] setRetryCount: 0

D/GSM     ( 2434): [ApnContext:supl] setRetryCount: 0

D/GSM     ( 2434): [ApnContext:hipri] setRetryCount: 0

D/GSM     ( 2434): [ApnContext:default] setRetryCount: 0

D/GSM     ( 2434): [ApnContext:mms] setRetryCount: 0

D/GSM     ( 2434): [GsmDCT] onRoamingOff

D/GSM     ( 2434): [GsmDCT] notifyOffApnOfAvailability type:dun

D/GSM     ( 2434): [GsmDCT] isDataAllowed: not allowed due to - gprs= 1 - SIM not loaded

D/GSM     ( 2434): [GsmDCT] isDataPossible(dun): possible=false isDataAllowed=false apnTypePossible=true apnContextisEnabled=false apnContextState()=IDLE

D/GSM     ( 2434): [GsmDCT] get active apn string for type:dun

D/GSM     ( 2434): [GsmDCT] notifyOffApnOfAvailability type:supl

D/GSM     ( 2434): [GsmDCT] isDataAllowed: not allowed due to - gprs= 1 - SIM not loaded

D/GSM     ( 2434): [GsmDCT] isDataPossible(supl): possible=false isDataAllowed=false apnTypePossible=true apnContextisEnabled=false apnContextState()=IDLE

D/GSM     ( 2434): [GsmDCT] get active apn string for type:supl

D/GSM     ( 2434): [GsmDCT] notifyOffApnOfAvailability type:hipri

D/GSM     ( 2434): [GsmDCT] isDataAllowed: not allowed due to - gprs= 1 - SIM not loaded

D/GSM     ( 2434): [GsmDCT] isDataPossible(hipri): possible=false isDataAllowed=false apnTypePossible=true apnContextisEnabled=false apnContextState()=IDLE

D/GSM     ( 2434): [GsmDCT] get active apn string for type:hipri

D/GSM     ( 2434): [GsmDCT] notifyOffApnsOfAvailability skipped apn due to isReady==false: {mApnType=default mState=IDLE mWaitingApns=null mWaitingApnsPermanentFailureCountDown=0 mApnSetting=null mDataConnectionAc=null mReason=radioTurnedOff mRetryCount=0 mDataEnabled=true mDependencyMet=true}

D/GSM     ( 2434): [GsmDCT] notifyOffApnOfAvailability type:mms

D/GSM     ( 2434): [GsmDCT] isDataAllowed: not allowed due to - gprs= 1 - SIM not loaded

D/GSM     ( 2434): [GsmDCT] isDataPossible(mms): possible=false isDataAllowed=false apnTypePossible=true apnContextisEnabled=false apnContextState()=IDLE

D/GSM     ( 2434): [GsmDCT] get active apn string for type:mms

D/GSM     ( 2434): [ApnContext:dun] setRetryCount: 0

D/GSM     ( 2434): [ApnContext:supl] setRetryCount: 0

D/GSM     ( 2434): [ApnContext:hipri] setRetryCount: 0

D/GSM     ( 2434): [ApnContext:default] setRetryCount: 0

D/GSM     ( 2434): [ApnContext:mms] setRetryCount: 0

D/GSM     ( 2434): [ApnContext:default] set reason as roamingOff,current state IDLE

D/GSM     ( 2434): [GsmDCT] trySetupData for type:default due to roamingOff

D/GSM     ( 2434): [GsmDCT] trySetupData with mIsPsRestricted=false

D/GSM     ( 2434): [GsmDCT] isDataAllowed: not allowed due to - gprs= 1 - SIM not loaded

D/GSM     ( 2434): [GsmDCT] notifyOffApnOfAvailability type:dun

D/GSM     ( 2434): [GsmDCT] isDataAllowed: not allowed due to - gprs= 1 - SIM not loaded

D/GSM     ( 2434): [GsmDCT] isDataPossible(dun): possible=false isDataAllowed=false apnTypePossible=true apnContextisEnabled=false apnContextState()=IDLE

D/GSM     ( 2434): [GsmDCT] get active apn string for type:dun

D/GSM     ( 2434): [GsmDCT] notifyOffApnOfAvailability type:supl

D/GSM     ( 2434): [GsmDCT] isDataAllowed: not allowed due to - gprs= 1 - SIM not loaded

D/GSM     ( 2434): [GsmDCT] isDataPossible(supl): possible=false isDataAllowed=false apnTypePossible=true apnContextisEnabled=false apnContextState()=IDLE

D/GSM     ( 2434): [GsmDCT] get active apn string for type:supl

D/GSM     ( 2434): [GsmDCT] notifyOffApnOfAvailability type:hipri

D/GSM     ( 2434): [GsmDCT] isDataAllowed: not allowed due to - gprs= 1 - SIM not loaded

D/GSM     ( 2434): [GsmDCT] isDataPossible(hipri): possible=false isDataAllowed=false apnTypePossible=true apnContextisEnabled=false apnContextState()=IDLE

D/GSM     ( 2434): [GsmDCT] get active apn string for type:hipri

D/GSM     ( 2434): [GsmDCT] notifyOffApnsOfAvailability skipped apn due to isReady==false: {mApnType=default mState=IDLE mWaitingApns=null mWaitingApnsPermanentFailureCountDown=0 mApnSetting=null mDataConnectionAc=null mReason=roamingOff mRetryCount=0 mDataEnabled=true mDependencyMet=true}

D/GSM     ( 2434): [GsmDCT] notifyOffApnOfAvailability type:mms

D/GSM     ( 2434): [GsmDCT] isDataAllowed: not allowed due to - gprs= 1 - SIM not loaded

D/GSM     ( 2434): [GsmDCT] isDataPossible(mms): possible=false isDataAllowed=false apnTypePossible=true apnContextisEnabled=false apnContextState()=IDLE

D/GSM     ( 2434): [GsmDCT] get active apn string for type:mms

D/RILJ    ( 2434): [0006]> BASEBAND_VERSION

D/RILJ    ( 2434): [0007]> GET_IMEI

D/RIL     ( 1891): 1 RIL request in the queue (1 pending, 0 handled, 0 unhandled)

D/RIL     ( 1891): 2 RIL requests data in the queue

D/RIL-IPC ( 1891): 

D/RIL-IPC ( 1891): xmm626_sec_modem_fmt_send: Sent FMT message

D/RIL-IPC ( 1891): xmm626_sec_modem_fmt_send: Message: mseq=0x04, command=IPC_MISC_ME_VERSION, type=IPC_TYPE_GET, size=1

D/RIL-IPC ( 1891): ================================= IPC FMT data =================================

D/RIL-IPC ( 1891): [0000]   FF                                                 .

D/RIL-IPC ( 1891): ================================================================================

D/RILJ    ( 2434): [0008]> GET_IMEISV

D/RIL-IPC ( 1891): 

D/RIL-IPC ( 1891): xmm626_sec_modem_fmt_recv: Received FMT message

D/RIL-IPC ( 1891): xmm626_sec_modem_fmt_recv: Message: aseq=0x04, command=IPC_MISC_ME_VERSION, type=IPC_TYPE_RESP, size=148

D/RIL-IPC ( 1891): ================================= IPC FMT data =================================

D/RIL-IPC ( 1891): [0000]   1F 49 39 33 30 30 58 58  55 47 4E 41 38 00 00 00   .I9300XX UGNA8...

D/RIL-IPC ( 1891): [0010]   00 00 00 00 00 00 00 00  00 00 00 00 00 00 00 00   ........ ........

D/RIL-IPC ( 1891): [0020]   00 4D 50 20 31 2E 31 30  30 00 00 00 00 00 00 00   .MP 1.10 0.......

D/RIL-IPC ( 1891): [0030]   00 00 00 00 00 00 00 00  00 00 00 00 00 00 00 00   ........ ........

D/RIL-IPC ( 1891): [0040]   00 32 30 31 32 2E 37 2E  34 00 00 00 00 00 00 00   .2012.7. 4.......

D/RIL-IPC ( 1891): [0050]   00 00 00 00 00 00 00 00  00 00 00 00 00 00 00 00   ........ ........

D/RIL-IPC ( 1891): [0060]   00 47 54 2D 49 39 33 30  30 4D 42 44 43 59 4F 00   .GT-I930 0MBDCYO.

D/RIL-IPC ( 1891): [0070]   00 00 00 00 00 00 00 00  00 00 00 00 00 00 00 00   ........ ........

D/RIL-IPC ( 1891): [0080]   00 49 39 33 30 30 00 00  00 00 00 00 00 00 00 00   .I9300.. ........

D/RIL-IPC ( 1891): [0090]   00 00 00 00                                        ....

D/RIL-IPC ( 1891): ================================================================================

D/RIL     ( 1891): 0 RIL request in the queue (0 pending, 0 handled, 0 unhandled)

D/RIL     ( 1891): 2 RIL requests data in the queue

D/RILJ    ( 2434): [0006]< BASEBAND_VERSION I9300XXUGNA8

D/RIL     ( 1891): 1 RIL request in the queue (1 pending, 0 handled, 0 unhandled)

D/RIL     ( 1891): 2 RIL requests data in the queue

D/RIL     ( 1891): 2 RIL requests in the queue (2 pending, 0 handled, 0 unhandled)

D/RIL     ( 1891): 2 RIL requests data in the queue

D/RIL-IPC ( 1891): 

D/RIL-IPC ( 1891): xmm626_sec_modem_fmt_send: Sent FMT message

D/RIL-IPC ( 1891): xmm626_sec_modem_fmt_send: Message: mseq=0x05, command=IPC_MISC_ME_SN, type=IPC_TYPE_GET, size=1

D/RIL-IPC ( 1891): ================================= IPC FMT data =================================

D/RIL-IPC ( 1891): [0000]   01                                                 .

D/RIL-IPC ( 1891): ================================================================================

D/RIL-IPC ( 1891): 

D/RIL-IPC ( 1891): xmm626_sec_modem_fmt_recv: Received FMT message

D/RIL-IPC ( 1891): xmm626_sec_modem_fmt_recv: Message: aseq=0x05, command=IPC_MISC_ME_SN, type=IPC_TYPE_RESP, size=34

D/RIL-IPC ( 1891): ================================= IPC FMT data =================================

D/RIL-IPC ( 1891): [0000]   01 11 33 35 33 38 31 37  30 35 31 38 32 38 37 31   ..353817 05182871

D/RIL-IPC ( 1891): [0010]   33 30 31 00 00 00 00 00  00 00 00 00 00 00 00 00   301..... ........

D/RIL-IPC ( 1891): [0020]   00 4D                                              .M

D/RIL-IPC ( 1891): ================================================================================

D/RIL     ( 1891): 1 RIL request in the queue (0 pending, 1 handled, 0 unhandled)

D/RIL     ( 1891): 2 RIL requests data in the queue

D/RIL     ( 1891): 0 RIL request in the queue (0 pending, 0 handled, 0 unhandled)

D/RIL     ( 1891): 2 RIL requests data in the queue

D/RILJ    ( 2434): [0007]< GET_IMEI 

D/RILJ    ( 2434): [0008]< GET_IMEISV 

D/PHONE   ( 2434): [PhoneProxy] Ignoring voice radio technology changed message. newVoiceRadioTech = 3 Active Phone = GSM

D/RILJ    ( 2434): [0009]> OPERATOR

D/RIL     ( 1891): 1 RIL request in the queue (1 pending, 0 handled, 0 unhandled)

D/RIL     ( 1891): 2 RIL requests data in the queue

D/RILJ    ( 2434): [0010]> DATA_REGISTRATION_STATE

D/RIL-IPC ( 1891): 

D/RIL-IPC ( 1891): xmm626_sec_modem_fmt_send: Sent FMT message

D/RIL-IPC ( 1891): xmm626_sec_modem_fmt_send: Message: mseq=0x06, command=IPC_NET_SERVING_NETWORK, type=IPC_TYPE_GET, size=0

D/RIL-IPC ( 1891): 

D/RIL-IPC ( 1891): xmm626_sec_modem_fmt_recv: Received FMT message

D/RIL-IPC ( 1891): xmm626_sec_modem_fmt_recv: Message: aseq=0x06, command=IPC_NET_SERVING_NETWORK, type=IPC_TYPE_RESP, size=11

D/RIL-IPC ( 1891): ================================= IPC FMT data =================================

D/RIL-IPC ( 1891): [0000]   02 05 FF 30 30 30 30 30  23 00 00                  ...00000 #..

D/RIL-IPC ( 1891): ================================================================================

E/RIL     ( 1891): ipc2ril_net_operator: Finding operator with PLMN 00 failed

D/RIL     ( 1891): 0 RIL request in the queue (0 pending, 0 handled, 0 unhandled)

D/RIL     ( 1891): 2 RIL requests data in the queue

D/RILJ    ( 2434): [0009]< OPERATOR error: com.android.internal.telephony.CommandException: GENERIC_FAILURE

D/RIL     ( 1891): 1 RIL request in the queue (1 pending, 0 handled, 0 unhandled)

D/RIL     ( 1891): 2 RIL requests data in the queue

D/RIL     ( 1891): 0 RIL request in the queue (0 pending, 0 handled, 0 unhandled)

D/RIL     ( 1891): 1 RIL request data in the queue

D/RILJ    ( 2434): [0010]< DATA_REGISTRATION_STATE {0, 0, 0, 0, 3}

D/RILJ    ( 2434): [0011]> VOICE_REGISTRATION_STATE

D/RIL     ( 1891): 1 RIL request in the queue (1 pending, 0 handled, 0 unhandled)

D/RIL     ( 1891): 1 RIL request data in the queue

D/RIL     ( 1891): 0 RIL request in the queue (0 pending, 0 handled, 0 unhandled)

D/RILJ    ( 2434): [0011]< VOICE_REGISTRATION_STATE {0, 0, 0, 0, null, null, null, null, null, null, null, null, null, null, null}

D/RILJ    ( 2434): [0012]> QUERY_NETWORK_SELECTION_MODE

D/RIL     ( 1891): 1 RIL request in the queue (1 pending, 0 handled, 0 unhandled)

D/RIL-IPC ( 1891): 

D/RIL-IPC ( 1891): xmm626_sec_modem_fmt_send: Sent FMT message

D/RIL-IPC ( 1891): xmm626_sec_modem_fmt_send: Message: mseq=0x07, command=IPC_NET_PLMN_SEL, type=IPC_TYPE_GET, size=0

D/RIL_UiccController( 2434): Received EVENT_ICC_STATUS_CHANGED, calling getIccCardStatus

D/RILJ    ( 2434): [0013]> GET_SIM_STATUS

D/RIL-IPC ( 1891): 

D/RIL-IPC ( 1891): xmm626_sec_modem_fmt_recv: Received FMT message

D/RIL-IPC ( 1891): xmm626_sec_modem_fmt_recv: Message: aseq=0x07, command=IPC_NET_PLMN_SEL, type=IPC_TYPE_RESP, size=1

D/RIL-IPC ( 1891): ================================= IPC FMT data =================================

D/RIL-IPC ( 1891): [0000]   02                                                 .

D/RIL-IPC ( 1891): ================================================================================

D/RIL     ( 1891): 0 RIL request in the queue (0 pending, 0 handled, 0 unhandled)

D/RILJ    ( 2434): [0012]< QUERY_NETWORK_SELECTION_MODE {0}

D/RIL     ( 1891): 1 RIL request in the queue (1 pending, 0 handled, 0 unhandled)

D/RIL-IPC ( 1891): 

D/RIL-IPC ( 1891): xmm626_sec_modem_fmt_send: Sent FMT message

D/RIL-IPC ( 1891): xmm626_sec_modem_fmt_send: Message: mseq=0x08, command=IPC_SEC_PIN_STATUS, type=IPC_TYPE_GET, size=0

D/RILJ    ( 2434): [0014]> GET_CURRENT_CALLS

D/RIL-IPC ( 1891): 

D/RIL-IPC ( 1891): xmm626_sec_modem_fmt_recv: Received FMT message

D/RIL-IPC ( 1891): xmm626_sec_modem_fmt_recv: Message: aseq=0x08, command=IPC_GEN_PHONE_RES, type=IPC_TYPE_RESP, size=5

D/RIL-IPC ( 1891): ================================= IPC FMT data =================================

D/RIL-IPC ( 1891): [0000]   05 01 02 0E 00                                     .....

D/RIL-IPC ( 1891): ================================================================================

D/RIL     ( 1891): Ignoring generic response for command IPC_SEC_PIN_STATUS

D/RIL     ( 1891): 2 RIL requests in the queue (1 pending, 1 handled, 0 unhandled)

D/RIL-IPC ( 1891): 

D/RIL-IPC ( 1891): xmm626_sec_modem_fmt_send: Sent FMT message

D/RIL-IPC ( 1891): xmm626_sec_modem_fmt_send: Message: mseq=0x09, command=IPC_CALL_LIST, type=IPC_TYPE_GET, size=0

D/RILJ    ( 2434): [0015]> RIL_REQUEST_VOICE_RADIO_TECH

D/RIL-IPC ( 1891): 

D/RIL-IPC ( 1891): xmm626_sec_modem_fmt_recv: Received FMT message

D/RIL-IPC ( 1891): xmm626_sec_modem_fmt_recv: Message: aseq=0x09, command=IPC_CALL_LIST, type=IPC_TYPE_RESP, size=1

D/RIL-IPC ( 1891): ================================= IPC FMT data =================================

D/RIL-IPC ( 1891): [0000]   00                                                 .

D/RIL-IPC ( 1891): ================================================================================

D/RIL     ( 1891): 1 RIL request in the queue (0 pending, 1 handled, 0 unhandled)

D/RILJ    ( 2434): [0014]< GET_CURRENT_CALLS  

D/RILJ    ( 2434): [0015]< RIL_REQUEST_VOICE_RADIO_TECH {3}

D/RILJ    ( 2434): [0016]> RIL_REQUEST_CDMA_GET_SUBSCRIPTION_SOURCE

D/RILJ    ( 2434): [0017]> OPERATOR

D/RILJ    ( 2434): [0016]< RIL_REQUEST_CDMA_GET_SUBSCRIPTION_SOURCE {0}

D/RIL     ( 1891): 2 RIL requests in the queue (1 pending, 1 handled, 0 unhandled)

D/RILJ    ( 2434): [0018]> DATA_REGISTRATION_STATE

D/RIL-IPC ( 1891): 

D/RIL-IPC ( 1891): xmm626_sec_modem_fmt_send: Sent FMT message

D/RIL-IPC ( 1891): xmm626_sec_modem_fmt_send: Message: mseq=0x0a, command=IPC_NET_SERVING_NETWORK, type=IPC_TYPE_GET, size=0

D/RIL-IPC ( 1891): 

D/RIL-IPC ( 1891): xmm626_sec_modem_fmt_recv: Received FMT message

D/RIL-IPC ( 1891): xmm626_sec_modem_fmt_recv: Message: aseq=0x0a, command=IPC_NET_SERVING_NETWORK, type=IPC_TYPE_RESP, size=11

D/RIL-IPC ( 1891): ================================= IPC FMT data =================================

D/RIL-IPC ( 1891): [0000]   02 05 FF 30 30 30 30 30  23 00 00                  ...00000 #..

D/RIL-IPC ( 1891): ================================================================================

E/RIL     ( 1891): ipc2ril_net_operator: Finding operator with PLMN 00 failed

D/RIL     ( 1891): 1 RIL request in the queue (0 pending, 1 handled, 0 unhandled)

D/RILJ    ( 2434): [0017]< OPERATOR error: com.android.internal.telephony.CommandException: GENERIC_FAILURE

D/RIL     ( 1891): 2 RIL requests in the queue (1 pending, 1 handled, 0 unhandled)

D/RIL-IPC ( 1891): 

D/RIL-IPC ( 1891): xmm626_sec_modem_fmt_send: Sent FMT message

D/RIL-IPC ( 1891): xmm626_sec_modem_fmt_send: Message: mseq=0x0b, command=IPC_NET_REGIST, type=IPC_TYPE_GET, size=2

D/RIL-IPC ( 1891): ================================= IPC FMT data =================================

D/RILJ    ( 2434): [0019]> VOICE_REGISTRATION_STATE

D/RIL-IPC ( 1891): [0000]   FF 03                                              ..

D/RIL-IPC ( 1891): ================================================================================

D/RIL     ( 1891): 3 RIL requests in the queue (1 pending, 2 handled, 0 unhandled)

D/RIL-IPC ( 1891): 

D/RIL-IPC ( 1891): xmm626_sec_modem_fmt_send: Sent FMT message

D/RIL-IPC ( 1891): xmm626_sec_modem_fmt_send: Message: mseq=0x0c, command=IPC_NET_REGIST, type=IPC_TYPE_GET, size=2

D/RIL-IPC ( 1891): ================================= IPC FMT data =================================

D/RIL-IPC ( 1891): [0000]   FF 02                                              ..

D/RIL-IPC ( 1891): ================================================================================

D/RIL-IPC ( 1891): 

D/RIL-IPC ( 1891): xmm626_sec_modem_fmt_recv: Received FMT message

D/RIL-IPC ( 1891): xmm626_sec_modem_fmt_recv: Message: aseq=0x0b, command=IPC_NET_REGIST, type=IPC_TYPE_RESP, size=11

D/RIL-IPC ( 1891): ================================= IPC FMT data =================================

D/RIL-IPC ( 1891): [0000]   FF 03 01 00 00 00 00 00  00 00 00                  ........ ...

D/RIL-IPC ( 1891): ================================================================================

D/RILJ    ( 2434): [0020]> QUERY_NETWORK_SELECTION_MODE

D/RIL     ( 1891): 2 RIL requests in the queue (0 pending, 2 handled, 0 unhandled)

D/RILJ    ( 2434): [0018]< DATA_REGISTRATION_STATE {0, 0, 0, 0, 3}

D/RIL-IPC ( 1891): 

D/RIL-IPC ( 1891): xmm626_sec_modem_fmt_recv: Received FMT message

D/RIL-IPC ( 1891): xmm626_sec_modem_fmt_recv: Message: aseq=0x0c, command=IPC_NET_REGIST, type=IPC_TYPE_RESP, size=11

D/RIL-IPC ( 1891): ================================= IPC FMT data =================================

D/RIL-IPC ( 1891): [0000]   FF 02 01 00 00 00 00 00  00 00 00                  ........ ...

D/RIL-IPC ( 1891): ================================================================================

D/RIL     ( 1891): 1 RIL request in the queue (0 pending, 1 handled, 0 unhandled)

D/RIL     ( 1891): 2 RIL requests in the queue (1 pending, 1 handled, 0 unhandled)

D/RIL-IPC ( 1891): 

D/RIL-IPC ( 1891): xmm626_sec_modem_fmt_send: Sent FMT message

D/RIL-IPC ( 1891): xmm626_sec_modem_fmt_send: Message: mseq=0x0d, command=IPC_NET_PLMN_SEL, type=IPC_TYPE_GET, size=0

D/RILJ    ( 2434): [0021]> OPERATOR

D/RILJ    ( 2434): [0019]< VOICE_REGISTRATION_STATE {0, 0, 0, 0, null, null, null, null, null, null, null, null, null, null, null}

D/RIL-IPC ( 1891): 

D/RIL-IPC ( 1891): xmm626_sec_modem_fmt_recv: Received FMT message

D/RIL-IPC ( 1891): xmm626_sec_modem_fmt_recv: Message: aseq=0x0d, command=IPC_NET_PLMN_SEL, type=IPC_TYPE_RESP, size=1

D/RIL-IPC ( 1891): ================================= IPC FMT data =================================

D/RIL-IPC ( 1891): [0000]   02                                                 .

D/RIL-IPC ( 1891): ================================================================================

D/RIL     ( 1891): 1 RIL request in the queue (0 pending, 1 handled, 0 unhandled)

D/RILJ    ( 2434): [0020]< QUERY_NETWORK_SELECTION_MODE {0}

D/RILJ    ( 2434): [0022]> DATA_REGISTRATION_STATE

D/RIL     ( 1891): 2 RIL requests in the queue (1 pending, 1 handled, 0 unhandled)

D/RIL-IPC ( 1891): 

D/RIL-IPC ( 1891): xmm626_sec_modem_fmt_send: Sent FMT message

D/RIL-IPC ( 1891): xmm626_sec_modem_fmt_send: Message: mseq=0x0e, command=IPC_NET_SERVING_NETWORK, type=IPC_TYPE_GET, size=0

D/RIL-IPC ( 1891): 

D/RIL-IPC ( 1891): xmm626_sec_modem_fmt_recv: Received FMT message

D/RIL-IPC ( 1891): xmm626_sec_modem_fmt_recv: Message: aseq=0x0e, command=IPC_NET_SERVING_NETWORK, type=IPC_TYPE_RESP, size=11

D/RIL-IPC ( 1891): ================================= IPC FMT data =================================

D/RIL-IPC ( 1891): [0000]   02 05 FF 30 30 30 30 30  23 00 00                  ...00000 #..

D/RIL-IPC ( 1891): ================================================================================

E/RIL     ( 1891): ipc2ril_net_operator: Finding operator with PLMN 00 failed

D/RIL     ( 1891): 1 RIL request in the queue (0 pending, 1 handled, 0 unhandled)

D/RILJ    ( 2434): [0021]< OPERATOR error: com.android.internal.telephony.CommandException: GENERIC_FAILURE

D/RIL     ( 1891): 2 RIL requests in the queue (1 pending, 1 handled, 0 unhandled)

D/RILJ    ( 2434): [0023]> VOICE_REGISTRATION_STATE

D/RIL-IPC ( 1891): 

D/RIL-IPC ( 1891): xmm626_sec_modem_fmt_send: Sent FMT message

D/RIL-IPC ( 1891): xmm626_sec_modem_fmt_send: Message: mseq=0x0f, command=IPC_NET_REGIST, type=IPC_TYPE_GET, size=2

D/RIL-IPC ( 1891): ================================= IPC FMT data =================================

D/RIL-IPC ( 1891): [0000]   FF 03                                              ..

D/RIL-IPC ( 1891): ================================================================================

D/RIL-IPC ( 1891): 

D/RIL-IPC ( 1891): xmm626_sec_modem_fmt_recv: Received FMT message

D/RIL-IPC ( 1891): xmm626_sec_modem_fmt_recv: Message: aseq=0x0f, command=IPC_NET_REGIST, type=IPC_TYPE_RESP, size=11

D/RIL-IPC ( 1891): ================================= IPC FMT data =================================

D/RIL-IPC ( 1891): [0000]   FF 03 01 00 00 00 00 00  00 00 00                  ........ ...

D/RIL-IPC ( 1891): ================================================================================

D/RIL     ( 1891): 1 RIL request in the queue (0 pending, 1 handled, 0 unhandled)

D/RILJ    ( 2434): [0022]< DATA_REGISTRATION_STATE {0, 0, 0, 0, 3}

D/RIL     ( 1891): 2 RIL requests in the queue (1 pending, 1 handled, 0 unhandled)

D/RIL-IPC ( 1891): 

D/RIL-IPC ( 1891): xmm626_sec_modem_fmt_send: Sent FMT message

D/RIL-IPC ( 1891): xmm626_sec_modem_fmt_send: Message: mseq=0x10, command=IPC_NET_REGIST, type=IPC_TYPE_GET, size=2

D/RIL-IPC ( 1891): ================================= IPC FMT data =================================

D/RIL-IPC ( 1891): [0000]   FF 02                                              ..

D/RIL-IPC ( 1891): ================================================================================

D/RILJ    ( 2434): [0024]> QUERY_NETWORK_SELECTION_MODE

D/RIL-IPC ( 1891): 

D/RIL-IPC ( 1891): xmm626_sec_modem_fmt_recv: Received FMT message

D/RIL-IPC ( 1891): xmm626_sec_modem_fmt_recv: Message: aseq=0x10, command=IPC_NET_REGIST, type=IPC_TYPE_RESP, size=11

D/RIL-IPC ( 1891): ================================= IPC FMT data =================================

D/RIL-IPC ( 1891): [0000]   FF 02 01 00 00 00 00 00  00 00 00                  ........ ...

D/RIL-IPC ( 1891): ================================================================================

D/RIL     ( 1891): 1 RIL request in the queue (0 pending, 1 handled, 0 unhandled)

D/RILJ    ( 2434): [0023]< VOICE_REGISTRATION_STATE {0, 0, 0, 0, null, null, null, null, null, null, null, null, null, null, null}

D/RILJ    ( 2434): [0025]> OPERATOR

D/RIL     ( 1891): 2 RIL requests in the queue (1 pending, 1 handled, 0 unhandled)

D/RIL-IPC ( 1891): 

D/RIL-IPC ( 1891): xmm626_sec_modem_fmt_send: Sent FMT message

D/RIL-IPC ( 1891): xmm626_sec_modem_fmt_send: Message: mseq=0x11, command=IPC_NET_PLMN_SEL, type=IPC_TYPE_GET, size=0

D/RILJ    ( 2434): [0026]> DATA_REGISTRATION_STATE

D/RIL-IPC ( 1891): 

D/RIL-IPC ( 1891): xmm626_sec_modem_fmt_recv: Received FMT message

D/RIL-IPC ( 1891): xmm626_sec_modem_fmt_recv: Message: aseq=0x11, command=IPC_NET_PLMN_SEL, type=IPC_TYPE_RESP, size=1

D/RIL-IPC ( 1891): ================================= IPC FMT data =================================

D/RIL-IPC ( 1891): [0000]   02                                                 .

D/RIL-IPC ( 1891): ================================================================================

D/RIL     ( 1891): 1 RIL request in the queue (0 pending, 1 handled, 0 unhandled)

D/RIL     ( 1891): 2 RIL requests in the queue (1 pending, 1 handled, 0 unhandled)

D/RIL-IPC ( 1891): 

D/RIL-IPC ( 1891): xmm626_sec_modem_fmt_send: Sent FMT message

D/RIL-IPC ( 1891): xmm626_sec_modem_fmt_send: Message: mseq=0x12, command=IPC_NET_SERVING_NETWORK, type=IPC_TYPE_GET, size=0

D/RILJ    ( 2434): [0024]< QUERY_NETWORK_SELECTION_MODE {0}

D/RIL-IPC ( 1891): 

D/RIL-IPC ( 1891): xmm626_sec_modem_fmt_recv: Received FMT message

D/RIL-IPC ( 1891): xmm626_sec_modem_fmt_recv: Message: aseq=0x12, command=IPC_NET_SERVING_NETWORK, type=IPC_TYPE_RESP, size=11

D/RIL-IPC ( 1891): ================================= IPC FMT data =================================

D/RIL-IPC ( 1891): [0000]   02 05 FF 30 30 30 30 30  23 00 00                  ...00000 #..

D/RIL-IPC ( 1891): ================================================================================

E/RIL     ( 1891): ipc2ril_net_operator: Finding operator with PLMN 00 failed

D/RIL     ( 1891): 1 RIL request in the queue (0 pending, 1 handled, 0 unhandled)

D/RILJ    ( 2434): [0027]> VOICE_REGISTRATION_STATE

D/RILJ    ( 2434): [0028]> QUERY_NETWORK_SELECTION_MODE

D/RIL     ( 1891): 2 RIL requests in the queue (1 pending, 1 handled, 0 unhandled)

D/RIL     ( 1891): 3 RIL requests in the queue (2 pending, 1 handled, 0 unhandled)

D/RIL-IPC ( 1891): 

D/RIL-IPC ( 1891): xmm626_sec_modem_fmt_send: Sent FMT message

D/RIL-IPC ( 1891): xmm626_sec_modem_fmt_send: Message: mseq=0x13, command=IPC_NET_REGIST, type=IPC_TYPE_GET, size=2

D/RIL-IPC ( 1891): ================================= IPC FMT data =================================

D/RIL-IPC ( 1891): [0000]   FF 03                                              ..

D/RIL-IPC ( 1891): ================================================================================

D/RIL-IPC ( 1891): 

D/RIL-IPC ( 1891): xmm626_sec_modem_fmt_send: Sent FMT message

D/RIL-IPC ( 1891): xmm626_sec_modem_fmt_send: Message: mseq=0x14, command=IPC_NET_REGIST, type=IPC_TYPE_GET, size=2

D/RIL-IPC ( 1891): ================================= IPC FMT data =================================

D/RIL-IPC ( 1891): [0000]   FF 02                                              ..

D/RIL-IPC ( 1891): ================================================================================

D/RIL     ( 1891): 4 RIL requests in the queue (1 pending, 3 handled, 0 unhandled)

D/RIL-IPC ( 1891): 

D/RIL-IPC ( 1891): xmm626_sec_modem_fmt_send: Sent FMT message

D/RIL-IPC ( 1891): xmm626_sec_modem_fmt_send: Message: mseq=0x15, command=IPC_NET_PLMN_SEL, type=IPC_TYPE_GET, size=0

D/RIL-IPC ( 1891): 

D/RIL-IPC ( 1891): xmm626_sec_modem_fmt_recv: Received FMT message

D/RIL-IPC ( 1891): xmm626_sec_modem_fmt_recv: Message: aseq=0x13, command=IPC_NET_REGIST, type=IPC_TYPE_RESP, size=11

D/RIL-IPC ( 1891): ================================= IPC FMT data =================================

D/RILJ    ( 2434): [0025]< OPERATOR error: com.android.internal.telephony.CommandException: GENERIC_FAILURE

D/RIL-IPC ( 1891): [0000]   FF 03 01 00 00 00 00 00  00 00 00                  ........ ...

D/RIL-IPC ( 1891): ================================================================================

D/RIL     ( 1891): 3 RIL requests in the queue (0 pending, 3 handled, 0 unhandled)

D/RILJ    ( 2434): [0026]< DATA_REGISTRATION_STATE {0, 0, 0, 0, 3}

D/RIL-IPC ( 1891): 

D/RIL-IPC ( 1891): xmm626_sec_modem_fmt_recv: Received FMT message

D/RIL-IPC ( 1891): xmm626_sec_modem_fmt_recv: Message: aseq=0x14, command=IPC_NET_REGIST, type=IPC_TYPE_RESP, size=11

D/RIL-IPC ( 1891): ================================= IPC FMT data =================================

D/RIL-IPC ( 1891): [0000]   FF 02 01 00 00 00 00 00  00 00 00                  ........ ...

D/RIL-IPC ( 1891): ================================================================================

D/RIL     ( 1891): 2 RIL requests in the queue (0 pending, 2 handled, 0 unhandled)

D/RILJ    ( 2434): [0027]< VOICE_REGISTRATION_STATE {0, 0, 0, 0, null, null, null, null, null, null, null, null, null, null, null}

D/RIL-IPC ( 1891): 

D/RIL-IPC ( 1891): xmm626_sec_modem_fmt_recv: Received FMT message

D/RIL-IPC ( 1891): xmm626_sec_modem_fmt_recv: Message: aseq=0x15, command=IPC_NET_PLMN_SEL, type=IPC_TYPE_RESP, size=1

D/RIL-IPC ( 1891): ================================= IPC FMT data =================================

D/RIL-IPC ( 1891): [0000]   02                                                 .

D/RIL-IPC ( 1891): ================================================================================

D/RIL     ( 1891): 1 RIL request in the queue (0 pending, 1 handled, 0 unhandled)

D/RILJ    ( 2434): [0028]< QUERY_NETWORK_SELECTION_MODE {0}

D/GSM     ( 2434): Baseband version: I9300XXUGNA8

D/PHONE   ( 2434): [PhoneProxy] Ignoring voice radio technology changed message. newVoiceRadioTech = 3 Active Phone = GSM

D/CDMA    ( 2434): [CdmaSSM] CDMA_SUBSCRIPTION_SOURCE event = 2

D/CDMA    ( 2434): [CdmaSSM] Subscription Source Changed : 1 >> 0

E/GSM     ( 2434): [GsmSST] RIL implementation has returned an error where it must succeedcom.android.internal.telephony.CommandException: GENERIC_FAILURE

D/GSM     ( 2434): [GsmSST] Poll ServiceState done:  oldSS=[3 home null null null  Unknown CSS not supported -1 -1 RoamInd=-1 DefRoamInd=-1 EmergOnly=false] newSS=[1 home null null null  Unknown CSS not supported -1 -1 RoamInd=-1 DefRoamInd=-1 EmergOnly=false] oldGprs=1 newData=1 oldMaxDataCalls=1 mNewMaxDataCalls=1 oldReasonDataDenied=-1 mNewReasonDataDenied=-1 oldType=Unknown newType=Unknown

D/GSM     ( 2434): [GsmSST] updateSpnDisplay: radio is on but out of service, set plmn='No service.'

D/GSM     ( 2434): [GsmSST] updateSpnDisplay: changed sending intent rule=0 showPlmn='true' plmn='No service.' showSpn='false' spn=''

D/GSM     ( 2434): [GsmSST] operatorNumeric is null

D/RIL_IccCardProxy( 2434): updateQuietMode: 3GPP subscription -> newQuietMode=false

D/RIL_IccCardProxy( 2434): updateQuietMode: QuietMode is false (app_type=1 isLteOnCdmaMode=false cdmaSource=-1)

D/RIL_IccCardProxy( 2434): Broadcasting intent ACTION_SIM_STATE_CHANGED ABSENT reason null

D/RIL-IPC ( 1891): 

D/RIL-IPC ( 1891): xmm626_sec_modem_fmt_recv: Received FMT message

D/RIL-IPC ( 1891): xmm626_sec_modem_fmt_recv: Message: aseq=0xff, command=IPC_NET_REGIST, type=IPC_TYPE_NOTI, size=11

D/RIL-IPC ( 1891): ================================= IPC FMT data =================================

D/RIL-IPC ( 1891): [0000]   FF 02 04 00 00 00 00 00  00 00 00                  ........ ...

D/RIL-IPC ( 1891): ================================================================================

D/RIL-IPC ( 1891): 

D/RIL-IPC ( 1891): xmm626_sec_modem_fmt_recv: Received FMT message

D/RIL-IPC ( 1891): xmm626_sec_modem_fmt_recv: Message: aseq=0xff, command=IPC_NET_REGIST, type=IPC_TYPE_NOTI, size=11

D/RIL-IPC ( 1891): ================================= IPC FMT data =================================

D/RIL-IPC ( 1891): [0000]   FF 03 01 00 00 00 00 00  00 00 00                  ........ ...

D/RIL-IPC ( 1891): ================================================================================

D/RIL-IPC ( 1891): 

D/RIL-IPC ( 1891): xmm626_sec_modem_fmt_recv: Received FMT message

D/RIL-IPC ( 1891): xmm626_sec_modem_fmt_recv: Message: aseq=0x00, command=IPC_NET_SERVING_NETWORK, type=IPC_TYPE_NOTI, size=11

D/RIL-IPC ( 1891): ================================= IPC FMT data =================================

D/RIL-IPC ( 1891): [0000]   02 04 FF 32 30 36 31 30  23 00 00                  ...20610 #..

D/RIL-IPC ( 1891): ================================================================================

D/RIL-IPC ( 1891): 

D/RIL-IPC ( 1891): xmm626_sec_modem_fmt_recv: Received FMT message

D/RIL-IPC ( 1891): xmm626_sec_modem_fmt_recv: Message: aseq=0x00, command=IPC_SEC_SIM_ICC_TYPE, type=IPC_TYPE_NOTI, size=1

D/RIL-IPC ( 1891): ================================= IPC FMT data =================================

D/RIL-IPC ( 1891): [0000]   02                                                 .

D/RIL-IPC ( 1891): ================================================================================

D/RIL-IPC ( 1891): 

D/RIL-IPC ( 1891): xmm626_sec_modem_fmt_recv: Received FMT message

D/RIL-IPC ( 1891): xmm626_sec_modem_fmt_recv: Message: aseq=0x00, command=IPC_SEC_PIN_STATUS, type=IPC_TYPE_NOTI, size=2

D/RIL-IPC ( 1891): ================================= IPC FMT data =================================

D/RIL-IPC ( 1891): [0000]   03 01                                              ..

D/RIL-IPC ( 1891): ================================================================================

D/RIL     ( 1891): ipc2ril_sec_pin_status_response: Selecting status application 3 on 10

D/RIL     ( 1891): Updating RIL radio state to 3

D/RIL-IPC ( 1891): 

D/RIL-IPC ( 1891): xmm626_sec_modem_fmt_recv: Received FMT message

D/RIL-IPC ( 1891): xmm626_sec_modem_fmt_recv: Message: aseq=0x00, command=IPC_SAT_PROACTIVE_CMD, type=IPC_TYPE_INDI, size=13

D/RIL-IPC ( 1891): ================================= IPC FMT data =================================

D/RIL-IPC ( 1891): [0000]   0B 00 D0 09 81 03 01 02  00 82 02 81 82            ........ .....

D/RIL-IPC ( 1891): ================================================================================

D/RIL-IPC ( 1891): Unhandled IPC FMT message: IPC_SAT_PROACTIVE_CMD

D/RILJ    ( 2434): [UNSL]< UNSOL_RESPONSE_VOICE_NETWORK_STATE_CHANGED

D/RILJ    ( 2434): [UNSL]< UNSOL_RESPONSE_VOICE_NETWORK_STATE_CHANGED

D/RILJ    ( 2434): [UNSL]< UNSOL_RESPONSE_VOICE_NETWORK_STATE_CHANGED

D/RILJ    ( 2434): [UNSL]< UNSOL_RESPONSE_SIM_STATUS_CHANGED

D/RILJ    ( 2434): [UNSL]< UNSOL_RESPONSE_RADIO_STATE_CHANGED RADIO_ON

D/RILJ    ( 2434): [UNSL]< UNSOL_RESPONSE_SIM_STATUS_CHANGED

D/RILJ    ( 2434): [0029]> OPERATOR

D/RILJ    ( 2434): [0030]> DATA_REGISTRATION_STATE

D/RIL     ( 1891): 2 RIL requests in the queue (1 pending, 1 handled, 0 unhandled)

D/RIL     ( 1891): 4 RIL requests data in the queue

D/RIL     ( 1891): 1 RIL request in the queue (0 pending, 1 handled, 0 unhandled)

D/RIL     ( 1891): 3 RIL requests data in the queue

D/RILJ    ( 2434): [0031]> VOICE_REGISTRATION_STATE

D/RIL     ( 1891): 2 RIL requests in the queue (1 pending, 1 handled, 0 unhandled)

D/RIL     ( 1891): 3 RIL requests data in the queue

D/RIL     ( 1891): 1 RIL request in the queue (0 pending, 1 handled, 0 unhandled)

D/RIL     ( 1891): 2 RIL requests data in the queue

D/RILJ    ( 2434): [0029]< OPERATOR {Mobistar, Mobistar, 20610}

D/RILJ    ( 2434): [0032]> QUERY_NETWORK_SELECTION_MODE

D/RILJ    ( 2434): [0033]> OPERATOR

D/RILJ    ( 2434): [0030]< DATA_REGISTRATION_STATE {0, 0, 0, 0, 3}

D/RILJ    ( 2434): [0034]> DATA_REGISTRATION_STATE

D/RIL     ( 1891): 2 RIL requests in the queue (1 pending, 1 handled, 0 unhandled)

D/RIL     ( 1891): 2 RIL requests data in the queue

D/RIL     ( 1891): 1 RIL request in the queue (0 pending, 1 handled, 0 unhandled)

D/RIL     ( 1891): 1 RIL request data in the queue

D/RILJ    ( 2434): [0035]> VOICE_REGISTRATION_STATE

D/RILJ    ( 2434): [0031]< VOICE_REGISTRATION_STATE {10, 0, 0, 0, null, null, null, null, null, null, null, null, null, null, null}

D/RILJ    ( 2434): [0036]> QUERY_NETWORK_SELECTION_MODE

D/RILJ    ( 2434): [0037]> OPERATOR

D/RILJ    ( 2434): [0038]> DATA_REGISTRATION_STATE

D/RILJ    ( 2434): [0039]> VOICE_REGISTRATION_STATE

D/RILJ    ( 2434): [0040]> QUERY_NETWORK_SELECTION_MODE

D/RIL_UiccController( 2434): Received EVENT_ICC_STATUS_CHANGED, calling getIccCardStatus

D/RILJ    ( 2434): [0041]> GET_SIM_STATUS

D/RIL_UiccController( 2434): Received EVENT_ICC_STATUS_CHANGED, calling getIccCardStatus

D/RILJ    ( 2434): [0042]> GET_SIM_STATUS

D/RIL     ( 1891): 2 RIL requests in the queue (1 pending, 1 handled, 0 unhandled)

D/RIL     ( 1891): 1 RIL request data in the queue

D/RIL     ( 1891): 3 RIL requests in the queue (2 pending, 1 handled, 0 unhandled)

D/RIL     ( 1891): 1 RIL request data in the queue

D/RIL-IPC ( 1891): 

D/RIL-IPC ( 1891): xmm626_sec_modem_fmt_send: Sent FMT message

D/RIL-IPC ( 1891): xmm626_sec_modem_fmt_send: Message: mseq=0x16, command=IPC_NET_PLMN_SEL, type=IPC_TYPE_GET, size=0

D/RIL-IPC ( 1891): 

D/RIL-IPC ( 1891): xmm626_sec_modem_fmt_send: Sent FMT message

D/RIL-IPC ( 1891): xmm626_sec_modem_fmt_send: Message: mseq=0x17, command=IPC_NET_SERVING_NETWORK, type=IPC_TYPE_GET, size=0

D/RIL     ( 1891): 4 RIL requests in the queue (1 pending, 3 handled, 0 unhandled)

D/RIL     ( 1891): 1 RIL request data in the queue

D/RIL-IPC ( 1891): 

D/RIL-IPC ( 1891): xmm626_sec_modem_fmt_send: Sent FMT message

D/RIL-IPC ( 1891): xmm626_sec_modem_fmt_send: Message: mseq=0x18, command=IPC_NET_REGIST, type=IPC_TYPE_GET, size=2

D/RIL-IPC ( 1891): ================================= IPC FMT data =================================

D/RIL-IPC ( 1891): [0000]   FF 03                                              ..

D/RIL-IPC ( 1891): ================================================================================

D/RIL     ( 1891): 5 RIL requests in the queue (1 pending, 4 handled, 0 unhandled)

D/RIL     ( 1891): 1 RIL request data in the queue

D/RIL-IPC ( 1891): 

D/RIL-IPC ( 1891): xmm626_sec_modem_fmt_send: Sent FMT message

D/RIL-IPC ( 1891): xmm626_sec_modem_fmt_send: Message: mseq=0x19, command=IPC_NET_REGIST, type=IPC_TYPE_GET, size=2

D/RIL-IPC ( 1891): ================================= IPC FMT data =================================

D/RIL-IPC ( 1891): [0000]   FF 02                                              ..

D/RIL-IPC ( 1891): ================================================================================

D/RIL     ( 1891): 6 RIL requests in the queue (1 pending, 5 handled, 0 unhandled)

D/RIL     ( 1891): 1 RIL request data in the queue

D/RIL-IPC ( 1891): 

D/RIL-IPC ( 1891): xmm626_sec_modem_fmt_send: Sent FMT message

D/RIL-IPC ( 1891): xmm626_sec_modem_fmt_send: Message: mseq=0x1a, command=IPC_NET_PLMN_SEL, type=IPC_TYPE_GET, size=0

D/RIL     ( 1891): 7 RIL requests in the queue (1 pending, 6 handled, 0 unhandled)

D/RIL     ( 1891): 1 RIL request data in the queue

D/RIL     ( 1891): 8 RIL requests in the queue (1 pending, 6 handled, 1 unhandled)

D/RIL     ( 1891): 1 RIL request data in the queue

D/RIL     ( 1891): 9 RIL requests in the queue (1 pending, 6 handled, 2 unhandled)

D/RIL     ( 1891): 1 RIL request data in the queue

D/RIL     ( 1891): 10 RIL requests in the queue (1 pending, 6 handled, 3 unhandled)

D/RIL     ( 1891): 1 RIL request data in the queue

D/RIL-IPC ( 1891): 

D/RIL-IPC ( 1891): xmm626_sec_modem_fmt_send: Sent FMT message

D/RIL-IPC ( 1891): xmm626_sec_modem_fmt_send: Message: mseq=0x1b, command=IPC_NET_PLMN_SEL, type=IPC_TYPE_GET, size=0

D/RIL     ( 1891): 11 RIL requests in the queue (1 pending, 7 handled, 3 unhandled)

D/RIL     ( 1891): 1 RIL request data in the queue

D/RIL     ( 1891): 12 RIL requests in the queue (1 pending, 7 handled, 4 unhandled)

D/RIL     ( 1891): 1 RIL request data in the queue

D/RIL-IPC ( 1891): 

D/RIL-IPC ( 1891): xmm626_sec_modem_fmt_recv: Received FMT message

D/RIL-IPC ( 1891): xmm626_sec_modem_fmt_recv: Message: aseq=0x16, command=IPC_NET_PLMN_SEL, type=IPC_TYPE_RESP, size=1

D/RIL-IPC ( 1891): ================================= IPC FMT data =================================

D/RIL-IPC ( 1891): [0000]   02                                                 .

D/RIL-IPC ( 1891): ================================================================================

D/RIL     ( 1891): 11 RIL requests in the queue (0 pending, 6 handled, 5 unhandled)

D/RIL     ( 1891): 1 RIL request data in the queue

D/RILJ    ( 2434): [0032]< QUERY_NETWORK_SELECTION_MODE {0}

D/RIL-IPC ( 1891): 

D/RIL-IPC ( 1891): xmm626_sec_modem_fmt_recv: Received FMT message

D/RIL-IPC ( 1891): xmm626_sec_modem_fmt_recv: Message: aseq=0x17, command=IPC_NET_SERVING_NETWORK, type=IPC_TYPE_RESP, size=11

D/RIL-IPC ( 1891): ================================= IPC FMT data =================================

D/RIL-IPC ( 1891): [0000]   02 04 FF 32 30 36 31 30  23 00 00                  ...20610 #..

D/RIL-IPC ( 1891): ================================================================================

D/RIL     ( 1891): 10 RIL requests in the queue (0 pending, 5 handled, 5 unhandled)

D/RIL     ( 1891): 1 RIL request data in the queue

D/RIL-IPC ( 1891): 

D/RIL-IPC ( 1891): xmm626_sec_modem_fmt_send: Sent FMT message

D/RIL-IPC ( 1891): xmm626_sec_modem_fmt_send: Message: mseq=0x1c, command=IPC_NET_SERVING_NETWORK, type=IPC_TYPE_GET, size=0

D/RIL-IPC ( 1891): 

D/RIL-IPC ( 1891): xmm626_sec_modem_fmt_recv: Received FMT message

D/RIL-IPC ( 1891): xmm626_sec_modem_fmt_recv: Message: aseq=0x18, command=IPC_NET_REGIST, type=IPC_TYPE_RESP, size=11

D/RIL-IPC ( 1891): ================================= IPC FMT data =================================

D/RIL-IPC ( 1891): [0000]   FF 03 01 00 00 00 00 00  00 00 00                  ........ ...

D/RIL-IPC ( 1891): ================================================================================

D/RIL     ( 1891): 9 RIL requests in the queue (0 pending, 5 handled, 4 unhandled)

D/RIL     ( 1891): 1 RIL request data in the queue

D/RIL-IPC ( 1891): 

D/RIL-IPC ( 1891): xmm626_sec_modem_fmt_send: Sent FMT message

D/RIL-IPC ( 1891): xmm626_sec_modem_fmt_send: Message: mseq=0x1d, command=IPC_NET_REGIST, type=IPC_TYPE_GET, size=2

D/RIL-IPC ( 1891): ================================= IPC FMT data =================================

D/RIL-IPC ( 1891): [0000]   FF 03                                              ..

D/RIL-IPC ( 1891): ================================================================================

D/RIL-IPC ( 1891): 

D/RIL-IPC ( 1891): xmm626_sec_modem_fmt_recv: Received FMT message

D/RIL-IPC ( 1891): xmm626_sec_modem_fmt_recv: Message: aseq=0x19, command=IPC_NET_REGIST, type=IPC_TYPE_RESP, size=11

D/RIL-IPC ( 1891): ================================= IPC FMT data =================================

D/RIL-IPC ( 1891): [0000]   FF 02 04 00 00 00 00 00  00 00 00                  ........ ...

D/RIL-IPC ( 1891): ================================================================================

D/RIL     ( 1891): 8 RIL requests in the queue (0 pending, 5 handled, 3 unhandled)

D/RIL     ( 1891): 1 RIL request data in the queue

D/RIL-IPC ( 1891): 

D/RIL-IPC ( 1891): xmm626_sec_modem_fmt_send: Sent FMT message

D/RIL-IPC ( 1891): xmm626_sec_modem_fmt_send: Message: mseq=0x1e, command=IPC_NET_REGIST, type=IPC_TYPE_GET, size=2

D/RIL-IPC ( 1891): ================================= IPC FMT data =================================

D/RIL-IPC ( 1891): [0000]   FF 02                                              ..

D/RIL-IPC ( 1891): ================================================================================

D/RILJ    ( 2434): [0033]< OPERATOR {Mobistar, Mobistar, 20610}

D/RILJ    ( 2434): [0034]< DATA_REGISTRATION_STATE {0, 0, 0, 0, 3}

D/RILJ    ( 2434): [0035]< VOICE_REGISTRATION_STATE {10, 0, 0, 0, null, null, null, null, null, null, null, null, null, null, null}

D/RIL-IPC ( 1891): 

D/RIL-IPC ( 1891): xmm626_sec_modem_fmt_recv: Received FMT message

D/RIL-IPC ( 1891): xmm626_sec_modem_fmt_recv: Message: aseq=0x1a, command=IPC_NET_PLMN_SEL, type=IPC_TYPE_RESP, size=1

D/RIL-IPC ( 1891): ================================= IPC FMT data =================================

D/RIL-IPC ( 1891): [0000]   02                                                 .

D/RIL-IPC ( 1891): ================================================================================

D/RIL     ( 1891): 7 RIL requests in the queue (0 pending, 5 handled, 2 unhandled)

D/RIL     ( 1891): 1 RIL request data in the queue

D/RIL-IPC ( 1891): 

D/RIL-IPC ( 1891): xmm626_sec_modem_fmt_recv: Received FMT message

D/RIL-IPC ( 1891): xmm626_sec_modem_fmt_recv: Message: aseq=0x1b, command=IPC_NET_PLMN_SEL, type=IPC_TYPE_RESP, size=1

D/RIL-IPC ( 1891): ================================= IPC FMT data =================================

D/RIL-IPC ( 1891): [0000]   02                                                 .

D/RIL-IPC ( 1891): ================================================================================

D/RIL     ( 1891): 6 RIL requests in the queue (0 pending, 4 handled, 2 unhandled)

D/RIL     ( 1891): 1 RIL request data in the queue

D/RILJ    ( 2434): [0036]< QUERY_NETWORK_SELECTION_MODE {0}

D/RIL-IPC ( 1891): 

D/RIL-IPC ( 1891): xmm626_sec_modem_fmt_recv: Received FMT message

D/RIL-IPC ( 1891): xmm626_sec_modem_fmt_recv: Message: aseq=0x1c, command=IPC_NET_SERVING_NETWORK, type=IPC_TYPE_RESP, size=11

D/RIL-IPC ( 1891): ================================= IPC FMT data =================================

D/RIL-IPC ( 1891): [0000]   02 04 FF 32 30 36 31 30  23 00 00                  ...20610 #..

D/RIL-IPC ( 1891): ================================================================================

D/RILJ    ( 2434): [0040]< QUERY_NETWORK_SELECTION_MODE {0}

D/RIL     ( 1891): 5 RIL requests in the queue (0 pending, 3 handled, 2 unhandled)

D/RIL     ( 1891): 1 RIL request data in the queue

D/RIL-IPC ( 1891): 

D/RIL-IPC ( 1891): xmm626_sec_modem_fmt_recv: Received FMT message

D/RIL-IPC ( 1891): xmm626_sec_modem_fmt_recv: Message: aseq=0x1d, command=IPC_NET_REGIST, type=IPC_TYPE_RESP, size=11

D/RILJ    ( 2434): [0037]< OPERATOR {Mobistar, Mobistar, 20610}

D/RIL-IPC ( 1891): ================================= IPC FMT data =================================

D/RIL-IPC ( 1891): [0000]   FF 03 01 00 00 00 00 00  00 00 00                  ........ ...

D/RIL-IPC ( 1891): ================================================================================

D/RIL     ( 1891): 4 RIL requests in the queue (0 pending, 2 handled, 2 unhandled)

D/RIL     ( 1891): 1 RIL request data in the queue

D/RIL-IPC ( 1891): 

D/RIL-IPC ( 1891): xmm626_sec_modem_fmt_recv: Received FMT message

D/RIL-IPC ( 1891): xmm626_sec_modem_fmt_recv: Message: aseq=0x1e, command=IPC_NET_REGIST, type=IPC_TYPE_RESP, size=11

D/RIL-IPC ( 1891): ================================= IPC FMT data =================================

D/RIL-IPC ( 1891): [0000]   FF 02 04 00 00 00 00 00  00 00 00                  ........ ...

D/RIL-IPC ( 1891): ================================================================================

D/RIL     ( 1891): 3 RIL requests in the queue (0 pending, 1 handled, 2 unhandled)

D/RIL     ( 1891): 1 RIL request data in the queue

D/RILJ    ( 2434): [0038]< DATA_REGISTRATION_STATE {0, 0, 0, 0, 3}

D/RILJ    ( 2434): [0039]< VOICE_REGISTRATION_STATE {10, 0, 0, 0, null, null, null, null, null, null, null, null, null, null, null}

D/GSM     ( 2434): [GsmSST] Poll ServiceState done:  oldSS=[1 home null null null  Unknown CSS not supported -1 -1 RoamInd=-1 DefRoamInd=-1 EmergOnly=false] newSS=[1 home Mobistar Mobistar 20610  Unknown CSS not supported -1 -1 RoamInd=-1 DefRoamInd=-1 EmergOnly=true] oldGprs=1 newData=1 oldMaxDataCalls=1 mNewMaxDataCalls=1 oldReasonDataDenied=-1 mNewReasonDataDenied=-1 oldType=Unknown newType=Unknown

D/GSM     ( 2434): [GsmSST] updateSpnDisplay: radio is on but out of service, set plmn='Emergency calls only'

D/GSM     ( 2434): [GsmSST] updateSpnDisplay: changed sending intent rule=0 showPlmn='true' plmn='Emergency calls only' showSpn='false' spn=''

D/GSM     ( 2434): [GsmSST] pollStateDone: no nitz but one TZ for iso-cc=be with zone.getID=Europe/Brussels testOneUniqueOffsetPath=false

D/GSM     ( 2434): [GsmSST] setAndBroadcastNetworkSetTimeZone: setTimeZone=Europe/Brussels

D/GSM     ( 2434): [GsmSST] setAndBroadcastNetworkSetTimeZone: call alarm.setTimeZone and broadcast zoneId=Europe/Brussels

D/GSM     ( 2434): [GsmSST] shouldFixTimeZoneNow: retVal=false iccCardExist=false operatorNumeric=20610 mcc=206 prevOperatorNumeric= prevMcc=207 needToFixTimeZone=false ltod=06-01 18:19:37.292

D/RILJ    ( 2434): [0043]> OEM_HOOK_RAW[01010007011400]

D/RIL     ( 1891): 4 RIL requests in the queue (1 pending, 1 handled, 2 unhandled)

D/RIL     ( 1891): 1 RIL request data in the queue

D/RILJ    ( 2434): [0044]> OEM_HOOK_RAW[010300063200]

D/RIL-IPC ( 1891): 

D/RIL-IPC ( 1891): xmm626_sec_modem_fmt_send: Sent FMT message

D/RIL-IPC ( 1891): xmm626_sec_modem_fmt_send: Message: mseq=0x1f, command=IPC_SVC_ENTER, type=IPC_TYPE_SET, size=3

D/RIL-IPC ( 1891): ================================= IPC FMT data =================================

D/RIL-IPC ( 1891): [0000]   01 14 10                                           ...

D/RIL-IPC ( 1891): ================================================================================

D/RIL     ( 1891): 5 RIL requests in the queue (1 pending, 2 handled, 2 unhandled)

D/RIL     ( 1891): 1 RIL request data in the queue

D/RILJ    ( 2434): [0045]> OEM_HOOK_RAW[010300063300]

D/RIL     ( 1891): 6 RIL requests in the queue (1 pending, 2 handled, 3 unhandled)

D/RIL     ( 1891): 1 RIL request data in the queue

D/RILJ    ( 2434): [0046]> OEM_HOOK_RAW[0102000501]

D/RIL     ( 1891): 7 RIL requests in the queue (1 pending, 2 handled, 4 unhandled)

D/RIL     ( 1891): 1 RIL request data in the queue

D/RIL-IPC ( 1891): 

D/RIL-IPC ( 1891): xmm626_sec_modem_fmt_recv: Received FMT message

D/RIL-IPC ( 1891): xmm626_sec_modem_fmt_recv: Message: aseq=0x1f, command=IPC_GEN_PHONE_RES, type=IPC_TYPE_RESP, size=5

D/RIL-IPC ( 1891): ================================= IPC FMT data =================================

D/RIL-IPC ( 1891): [0000]   0B 01 03 00 80                                     .....

D/RIL-IPC ( 1891): ================================================================================

D/RIL     ( 1891): Generic response was expected

D/RIL-IPC ( 1891): 

D/RIL-IPC ( 1891): xmm626_sec_modem_fmt_recv: Received FMT message

D/RIL-IPC ( 1891): xmm626_sec_modem_fmt_recv: Message: aseq=0xff, command=IPC_SVC_SCREEN_CFG, type=IPC_TYPE_NOTI, size=2

D/RIL-IPC ( 1891): ================================= IPC FMT data =================================

D/RIL-IPC ( 1891): [0000]   0B 01                                              ..

D/RIL-IPC ( 1891): ================================================================================

D/RIL-IPC ( 1891): Unhandled IPC FMT message: IPC_SVC_SCREEN_CFG

D/RIL-IPC ( 1891): 

D/RIL-IPC ( 1891): xmm626_sec_modem_fmt_recv: Received FMT message

D/RIL-IPC ( 1891): xmm626_sec_modem_fmt_recv: Message: aseq=0x00, command=IPC_SVC_DISPLAY_SCREEN, type=IPC_TYPE_NOTI, size=545

D/RIL-IPC ( 1891): ================================= IPC FMT data =================================

D/RIL-IPC ( 1891): [0000]   10 00 00 20 52 52 43 28  48 53 50 41 29 20 43 4F   ... RRC( HSPA) CO

D/RIL-IPC ( 1891): [0010]   4E 54 52 4F 4C 00 20 20  20 20 20 20 20 20 20 20   NTROL.           

D/RIL-IPC ( 1891): [0020]   20 20 00 01 00 20 5B 31  5D 20 44 49 53 50 4C 41     ... [1 ] DISPLA

D/RIL-IPC ( 1891): [0030]   59 20 52 45 56 49 53 49  4F 4E 00 20 20 20 20 20   Y REVISI ON.     

D/RIL-IPC ( 1891): [0040]   20 20 20 20 00 02 00 20  5B 32 5D 20 43 48 41 4E       ...  [2] CHAN

D/RIL-IPC ( 1891): [0050]   47 45 20 52 45 56 49 53  49 4F 4E 00 20 20 20 20   GE REVIS ION.    

D/RIL-IPC ( 1891): [0060]   20 20 20 20 20 20 00 03  00 20 20 20 20 20 20 20         .. .       

D/RIL-IPC ( 1891): [0070]   20 20 20 20 20 20 20 20  20 20 20 20 20 20 20 20                    

D/RIL-IPC ( 1891): [0080]   20 20 20 20 20 20 20 20  00 04 00 20 20 20 20 20            ...     

D/RIL-IPC ( 1891): [0090]   20 20 20 20 20 20 20 20  20 20 20 20 20 20 20 20                    

D/RIL-IPC ( 1891): [00a0]   20 20 20 20 20 20 20 20  20 20 00 05 00 20 20 20              ...   

D/RIL-IPC ( 1891): [00b0]   20 20 20 20 20 20 20 20  20 20 20 20 20 20 20 20                    

D/RIL-IPC ( 1891): [00c0]   20 20 20 20 20 20 20 20  20 20 20 20 00 06 00 20                ... 

D/RIL-IPC ( 1891): [00d0]   20 20 20 20 20 20 20 20  20 20 20 20 20 20 20 20                    

D/RIL-IPC ( 1891): [00e0]   20 20 20 20 20 20 20 20  20 20 20 20 20 20 00 07                  ..

D/RIL-IPC ( 1891): [00f0]   00 20 20 20 20 20 20 20  20 20 20 20 20 20 20 20   .                

D/RIL-IPC ( 1891): ================================================================================

D/RIL     ( 1891): 6 RIL requests in the queue (0 pending, 1 handled, 5 unhandled)

D/RIL     ( 1891): 1 RIL request data in the queue

D/RIL-IPC ( 1891): 

D/RIL-IPC ( 1891): xmm626_sec_modem_fmt_recv: Received FMT message

D/RIL-IPC ( 1891): xmm626_sec_modem_fmt_recv: Message: aseq=0x00, command=IPC_SVC_DISPLAY_SCREEN, type=IPC_TYPE_NOTI, size=35

D/RIL-IPC ( 1891): ================================= IPC FMT data =================================

D/RIL-IPC ( 1891): [0000]   01 00 01 20 52 52 43 28  48 53 50 41 29 20 43 4F   ... RRC( HSPA) CO

D/RIL-IPC ( 1891): [0010]   4E 54 52 4F 4C 00 20 20  20 20 20 20 20 20 20 20   NTROL.           

D/RIL-IPC ( 1891): [0020]   20 20 00                                             .

D/RIL-IPC ( 1891): ================================================================================

D/RIL-IPC ( 1891): 

D/RIL-IPC ( 1891): xmm626_sec_modem_fmt_send: Sent FMT message

D/RIL-IPC ( 1891): xmm626_sec_modem_fmt_send: Message: mseq=0x20, command=IPC_SVC_PRO_KEYCODE, type=IPC_TYPE_SET, size=1

D/RIL-IPC ( 1891): ================================= IPC FMT data =================================

D/RIL-IPC ( 1891): [0000]   32                                                 2

D/RIL-IPC ( 1891): ================================================================================

D/RILJ    ( 2434): [0043]< OEM_HOOK_RAW [B@41686000

D/RIL-IPC ( 1891): 

D/RIL-IPC ( 1891): xmm626_sec_modem_fmt_recv: Received FMT message

D/RIL-IPC ( 1891): xmm626_sec_modem_fmt_recv: Message: aseq=0x20, command=IPC_GEN_PHONE_RES, type=IPC_TYPE_RESP, size=5

D/RIL-IPC ( 1891): ================================= IPC FMT data =================================

D/RIL-IPC ( 1891): [0000]   0B 03 03 00 80                                     .....

D/RIL-IPC ( 1891): ================================================================================

D/RIL     ( 1891): Generic response was expected

D/RIL-IPC ( 1891): 

D/RIL-IPC ( 1891): xmm626_sec_modem_fmt_recv: Received FMT message

D/RIL-IPC ( 1891): xmm626_sec_modem_fmt_recv: Message: aseq=0xff, command=IPC_SVC_DISPLAY_SCREEN, type=IPC_TYPE_NOTI, size=35

D/RIL-IPC ( 1891): ================================= IPC FMT data =================================

D/RIL-IPC ( 1891): [0000]   01 09 00 20 32 00 20 20  20 20 20 20 20 20 20 20   ... 2.           

D/RIL-IPC ( 1891): [0010]   20 20 20 20 20 20 20 20  20 20 20 20 20 20 20 20                    

D/RIL-IPC ( 1891): [0020]   20 20 00                                             .

D/RIL-IPC ( 1891): ================================================================================

D/RIL-IPC ( 1891): 

D/RIL-IPC ( 1891): xmm626_sec_modem_fmt_recv: Received FMT message

D/RIL-IPC ( 1891): xmm626_sec_modem_fmt_recv: Message: aseq=0x00, command=IPC_SVC_DISPLAY_SCREEN, type=IPC_TYPE_NOTI, size=545

D/RIL-IPC ( 1891): ================================= IPC FMT data =================================

D/RIL-IPC ( 1891): [0000]   10 00 00 20 43 48 41 4E  47 45 20 48 53 50 41 20   ... CHAN GE HSPA 

D/RIL-IPC ( 1891): [0010]   52 45 56 49 53 49 4F 4E  00 20 20 20 20 20 20 20   REVISION .       

D/RIL-IPC ( 1891): [0020]   20 20 00 01 00 20 5B 31  5D 20 52 45 4C 45 41 53     ... [1 ] RELEAS

D/RIL-IPC ( 1891): [0030]   45 20 52 39 39 28 48 53  50 41 20 4F 46 46 29 00   E R99(HS PA OFF).

D/RIL-IPC ( 1891): [0040]   20 20 20 20 00 02 00 20  5B 32 5D 20 52 45 4C 45       ...  [2] RELE

D/RIL-IPC ( 1891): [0050]   41 53 45 20 35 28 48 53  44 50 41 20 4F 4E 4C 59   ASE 5(HS DPA ONLY

D/RIL-IPC ( 1891): [0060]   29 00 20 20 20 20 00 03  00 20 5B 33 5D 20 52 45   ).    .. . [3] RE

D/RIL-IPC ( 1891): [0070]   4C 45 41 53 45 20 36 28  48 53 44 50 41 2F 48 53   LEASE 6( HSDPA/HS

D/RIL-IPC ( 1891): [0080]   55 50 41 29 00 20 20 20  00 04 00 20 20 20 20 20   UPA).    ...     

D/RIL-IPC ( 1891): [0090]   20 20 20 20 20 20 20 20  20 20 20 20 20 20 20 20                    

D/RIL-IPC ( 1891): [00a0]   20 20 20 20 20 20 20 20  20 20 00 05 00 20 20 20              ...   

D/RIL-IPC ( 1891): [00b0]   20 20 20 20 20 20 20 20  20 20 20 20 20 20 20 20                    

D/RIL-IPC ( 1891): [00c0]   20 20 20 20 20 20 20 20  20 20 20 20 00 06 00 20                ... 

D/RIL-IPC ( 1891): [00d0]   20 20 20 20 20 20 20 20  20 20 20 20 20 20 20 20                    

D/RIL-IPC ( 1891): [00e0]   20 20 20 20 20 20 20 20  20 20 20 20 20 20 00 07                  ..

D/RIL-IPC ( 1891): [00f0]   00 20 20 20 20 20 20 20  20 20 20 20 20 20 20 20   .                

D/RIL-IPC ( 1891): ================================================================================

D/RIL     ( 1891): 5 RIL requests in the queue (0 pending, 1 handled, 4 unhandled)

D/RIL     ( 1891): 1 RIL request data in the queue

D/RIL-IPC ( 1891): 

D/RIL-IPC ( 1891): xmm626_sec_modem_fmt_recv: Received FMT message

D/RIL-IPC ( 1891): xmm626_sec_modem_fmt_recv: Message: aseq=0x00, command=IPC_SVC_DISPLAY_SCREEN, type=IPC_TYPE_NOTI, size=35

D/RIL-IPC ( 1891): ================================= IPC FMT data =================================

D/RIL-IPC ( 1891): [0000]   01 00 01 20 43 48 41 4E  47 45 20 48 53 50 41 20   ... CHAN GE HSPA 

D/RIL-IPC ( 1891): [0010]   52 45 56 49 53 49 4F 4E  00 20 20 20 20 20 20 20   REVISION .       

D/RIL-IPC ( 1891): [0020]   20 20 00                                             .

D/RIL-IPC ( 1891): ================================================================================

D/RIL-IPC ( 1891): 

D/RIL-IPC ( 1891): xmm626_sec_modem_fmt_send: Sent FMT message

D/RIL-IPC ( 1891): xmm626_sec_modem_fmt_send: Message: mseq=0x21, command=IPC_SVC_PRO_KEYCODE, type=IPC_TYPE_SET, size=1

D/RIL-IPC ( 1891): ================================= IPC FMT data =================================

D/RIL-IPC ( 1891): [0000]   33                                                 3

D/RIL-IPC ( 1891): ================================================================================

D/RIL-IPC ( 1891): 

D/RIL-IPC ( 1891): xmm626_sec_modem_fmt_recv: Received FMT message

D/RIL-IPC ( 1891): xmm626_sec_modem_fmt_recv: Message: aseq=0x21, command=IPC_GEN_PHONE_RES, type=IPC_TYPE_RESP, size=5

D/RIL-IPC ( 1891): ================================= IPC FMT data =================================

D/RIL-IPC ( 1891): [0000]   0B 03 03 00 80                                     .....

D/RIL-IPC ( 1891): ================================================================================

D/RIL     ( 1891): Generic response was expected

D/RIL-IPC ( 1891): 

D/RIL-IPC ( 1891): xmm626_sec_modem_fmt_recv: Received FMT message

D/RIL-IPC ( 1891): xmm626_sec_modem_fmt_recv: Message: aseq=0xff, command=IPC_SVC_DISPLAY_SCREEN, type=IPC_TYPE_NOTI, size=35

D/RIL-IPC ( 1891): ================================= IPC FMT data =================================

D/RIL-IPC ( 1891): [0000]   01 09 00 20 33 00 20 20  20 20 20 20 20 20 20 20   ... 3.           

D/RIL-IPC ( 1891): [0010]   20 20 20 20 20 20 20 20  20 20 20 20 20 20 20 20                    

D/RIL-IPC ( 1891): [0020]   20 20 00                                             .

D/RIL-IPC ( 1891): ================================================================================

D/RIL-IPC ( 1891): 

D/RIL-IPC ( 1891): xmm626_sec_modem_fmt_recv: Received FMT message

D/RIL-IPC ( 1891): xmm626_sec_modem_fmt_recv: Message: aseq=0x00, command=IPC_SVC_DISPLAY_SCREEN, type=IPC_TYPE_NOTI, size=545

D/RIL-IPC ( 1891): ================================= IPC FMT data =================================

D/RIL-IPC ( 1891): [0000]   10 00 00 43 48 41 4E 47  45 5F 52 45 4C 35 00 20   ...CHANG E_REL5. 

D/RIL-IPC ( 1891): [0010]   52 45 56 49 53 49 4F 4E  00 20 20 20 20 20 20 20   REVISION .       

D/RIL-IPC ( 1891): [0020]   20 20 00 01 00 48 53 44  50 41 20 4F 4E 2C 20 48     ...HSD PA ON, H

D/RIL-IPC ( 1891): [0030]   53 55 50 41 20 4F 4E 00  50 41 20 4F 46 46 29 00   SUPA ON. PA OFF).

D/RIL-IPC ( 1891): [0040]   20 20 20 20 00 02 00 20  20 20 20 20 20 20 20 20       ...          

D/RIL-IPC ( 1891): [0050]   20 20 20 20 20 20 20 20  20 20 20 20 20 20 20 20                    

D/RIL-IPC ( 1891): [0060]   20 20 20 20 20 20 00 03  00 20 20 20 20 20 20 20         .. .       

D/RIL-IPC ( 1891): [0070]   20 20 20 20 20 20 20 20  20 20 20 20 20 20 20 20                    

D/RIL-IPC ( 1891): [0080]   20 20 20 20 20 20 20 20  00 04 00 20 20 20 20 20            ...     

D/RIL-IPC ( 1891): [0090]   20 20 20 20 20 20 20 20  20 20 20 20 20 20 20 20                    

D/RIL-IPC ( 1891): [00a0]   20 20 20 20 20 20 20 20  20 20 00 05 00 20 20 20              ...   

D/RIL-IPC ( 1891): [00b0]   20 20 20 20 20 20 20 20  20 20 20 20 20 20 20 20                    

D/RIL-IPC ( 1891): [00c0]   20 20 20 20 20 20 20 20  20 20 20 20 00 06 00 20                ... 

D/RIL-IPC ( 1891): [00d0]   20 20 20 20 20 20 20 20  20 20 20 20 20 20 20 20                    

D/RIL-IPC ( 1891): [00e0]   20 20 20 20 20 20 20 20  20 20 20 20 20 20 00 07                  ..

D/RIL-IPC ( 1891): [00f0]   00 20 20 20 20 20 20 20  20 20 20 20 20 20 20 20   .                

D/RIL-IPC ( 1891): ================================================================================

D/RIL     ( 1891): 4 RIL requests in the queue (0 pending, 1 handled, 3 unhandled)

D/RIL     ( 1891): 1 RIL request data in the queue

D/RIL-IPC ( 1891): 

D/RIL-IPC ( 1891): xmm626_sec_modem_fmt_recv: Received FMT message

D/RIL-IPC ( 1891): xmm626_sec_modem_fmt_recv: Message: aseq=0x00, command=IPC_SVC_DISPLAY_SCREEN, type=IPC_TYPE_NOTI, size=35

D/RIL-IPC ( 1891): ================================= IPC FMT data =================================

D/RIL-IPC ( 1891): [0000]   01 00 01 43 48 41 4E 47  45 5F 52 45 4C 35 00 20   ...CHANG E_REL5. 

D/RIL-IPC ( 1891): [0010]   52 45 56 49 53 49 4F 4E  00 20 20 20 20 20 20 20   REVISION .       

D/RIL-IPC ( 1891): [0020]   20 20 00                                             .

D/RIL-IPC ( 1891): ================================================================================

D/RIL-IPC ( 1891): 

D/RIL-IPC ( 1891): xmm626_sec_modem_fmt_send: Sent FMT message

D/RIL-IPC ( 1891): xmm626_sec_modem_fmt_send: Message: mseq=0x22, command=IPC_SVC_END, type=IPC_TYPE_SET, size=1

D/RIL-IPC ( 1891): ================================= IPC FMT data =================================

D/RIL-IPC ( 1891): [0000]   01                                                 .

D/RIL-IPC ( 1891): ================================================================================

D/RILJ    ( 2434): [0044]< OEM_HOOK_RAW [B@416864c0

D/RILJ    ( 2434): [0045]< OEM_HOOK_RAW [B@41686948

D/RIL-IPC ( 1891): 

D/RIL-IPC ( 1891): xmm626_sec_modem_fmt_recv: Received FMT message

D/RIL-IPC ( 1891): xmm626_sec_modem_fmt_recv: Message: aseq=0x22, command=IPC_GEN_PHONE_RES, type=IPC_TYPE_RESP, size=5

D/RIL-IPC ( 1891): ================================= IPC FMT data =================================

D/RIL-IPC ( 1891): [0000]   0B 02 03 00 80                                     .....

D/RIL-IPC ( 1891): ================================================================================

D/RIL     ( 1891): Generic response was expected

D/RIL     ( 1891): 3 RIL requests in the queue (0 pending, 1 handled, 2 unhandled)

D/RIL     ( 1891): 1 RIL request data in the queue

D/RILJ    ( 2434): [0046]< OEM_HOOK_RAW [B@41686dd0

D/RIL-IPC ( 1891): 

D/RIL-IPC ( 1891): xmm626_sec_modem_fmt_recv: Received FMT message

D/RIL-IPC ( 1891): xmm626_sec_modem_fmt_recv: Message: aseq=0x22, command=IPC_GPRS_HSDPA_STATUS, type=IPC_TYPE_NOTI, size=1

D/RIL-IPC ( 1891): ================================= IPC FMT data =================================

D/RIL-IPC ( 1891): [0000]   01                                                 .

D/RIL-IPC ( 1891): ================================================================================

D/RIL-IPC ( 1891): 

D/RIL-IPC ( 1891): xmm626_sec_modem_fmt_recv: Received FMT message

D/RIL-IPC ( 1891): xmm626_sec_modem_fmt_recv: Message: aseq=0xff, command=IPC_NET_REGIST, type=IPC_TYPE_NOTI, size=11

D/RIL-IPC ( 1891): ================================= IPC FMT data =================================

D/RIL-IPC ( 1891): [0000]   04 02 04 01 CC 42 F4 A7  07 00 00                  .....B.. ...

D/RIL-IPC ( 1891): ================================================================================

D/RIL-IPC ( 1891): 

D/RIL-IPC ( 1891): xmm626_sec_modem_fmt_recv: Received FMT message

D/RIL-IPC ( 1891): xmm626_sec_modem_fmt_recv: Message: aseq=0xff, command=IPC_NET_REGIST, type=IPC_TYPE_NOTI, size=11

D/RIL-IPC ( 1891): ================================= IPC FMT data =================================

D/RIL-IPC ( 1891): [0000]   04 03 01 01 CC 42 F4 A7  07 00 00                  .....B.. ...

D/RIL-IPC ( 1891): ================================================================================

D/RIL-IPC ( 1891): 

D/RIL-IPC ( 1891): xmm626_sec_modem_fmt_recv: Received FMT message

D/RIL-IPC ( 1891): xmm626_sec_modem_fmt_recv: Message: aseq=0x00, command=IPC_NET_SERVING_NETWORK, type=IPC_TYPE_NOTI, size=11

D/RIL-IPC ( 1891): ================================= IPC FMT data =================================

D/RIL-IPC ( 1891): [0000]   02 04 04 32 30 36 31 30  23 CC 42                  ...20610 #.B

D/RIL-IPC ( 1891): ================================================================================

D/RIL-IPC ( 1891): 

D/RIL-IPC ( 1891): xmm626_sec_modem_fmt_recv: Received FMT message

D/RIL-IPC ( 1891): xmm626_sec_modem_fmt_recv: Message: aseq=0x00, command=IPC_DISP_ICON_INFO, type=IPC_TYPE_NOTI, size=4

D/RIL-IPC ( 1891): ================================= IPC FMT data =================================

D/RIL-IPC ( 1891): [0000]   FF 04 00 05                                        ....

D/RIL-IPC ( 1891): ================================================================================

D/RIL     ( 1891): Signal strength is 12

D/RIL-IPC ( 1891): 

D/RIL-IPC ( 1891): xmm626_sec_modem_fmt_recv: Received FMT message

D/RIL-IPC ( 1891): xmm626_sec_modem_fmt_recv: Message: aseq=0x00, command=IPC_DISP_RSSI_INFO, type=IPC_TYPE_NOTI, size=1

D/RIL-IPC ( 1891): ================================= IPC FMT data =================================

D/RIL-IPC ( 1891): [0000]   4B                                                 K

D/RIL-IPC ( 1891): ================================================================================

D/RIL     ( 1891): Signal strength is 19

D/RILJ    ( 2434): [UNSL]< UNSOL_RESPONSE_VOICE_NETWORK_STATE_CHANGED

D/RILJ    ( 2434): [UNSL]< UNSOL_RESPONSE_VOICE_NETWORK_STATE_CHANGED

D/RILJ    ( 2434): [UNSL]< UNSOL_RESPONSE_VOICE_NETWORK_STATE_CHANGED

D/RILJ    ( 2434): [UNSL]< UNSOL_RESPONSE_VOICE_NETWORK_STATE_CHANGED

D/RILJ    ( 2434): [0047]> OPERATOR

D/RILJ    ( 2434): [0048]> DATA_REGISTRATION_STATE

D/RIL     ( 1891): 4 RIL requests in the queue (1 pending, 1 handled, 2 unhandled)

D/RIL     ( 1891): 4 RIL requests data in the queue

D/RIL     ( 1891): 3 RIL requests in the queue (0 pending, 1 handled, 2 unhandled)

D/RIL     ( 1891): 3 RIL requests data in the queue

D/RILJ    ( 2434): [0047]< OPERATOR {Mobistar, Mobistar, 20610}

D/RILJ    ( 2434): [0049]> VOICE_REGISTRATION_STATE

D/RIL     ( 1891): 4 RIL requests in the queue (1 pending, 1 handled, 2 unhandled)

D/RIL     ( 1891): 3 RIL requests data in the queue

D/RIL     ( 1891): 3 RIL requests in the queue (0 pending, 1 handled, 2 unhandled)

D/RIL     ( 1891): 2 RIL requests data in the queue

D/RILJ    ( 2434): [0050]> QUERY_NETWORK_SELECTION_MODE

D/RILJ    ( 2434): [0051]> OPERATOR

D/RIL     ( 1891): 4 RIL requests in the queue (1 pending, 1 handled, 2 unhandled)

D/RIL     ( 1891): 2 RIL requests data in the queue

D/RIL     ( 1891): 3 RIL requests in the queue (0 pending, 1 handled, 2 unhandled)

D/RIL     ( 1891): 1 RIL request data in the queue

D/RILJ    ( 2434): [0048]< DATA_REGISTRATION_STATE {0, 42cc, 7a7f4, 9, 3}

D/RIL     ( 1891): 4 RIL requests in the queue (1 pending, 1 handled, 2 unhandled)

D/RIL     ( 1891): 1 RIL request data in the queue

D/RIL-IPC ( 1891): 

D/RIL-IPC ( 1891): xmm626_sec_modem_fmt_send: Sent FMT message

D/RIL-IPC ( 1891): xmm626_sec_modem_fmt_send: Message: mseq=0x23, command=IPC_NET_PLMN_SEL, type=IPC_TYPE_GET, size=0

D/RILJ    ( 2434): [0049]< VOICE_REGISTRATION_STATE {10, 42cc, 7a7f4, 9, null, null, null, null, null, null, null, null, null, null, null}

D/RIL     ( 1891): 5 RIL requests in the queue (1 pending, 2 handled, 2 unhandled)

D/RIL     ( 1891): 1 RIL request data in the queue

D/RIL-IPC ( 1891): 

D/RILJ    ( 2434): [0052]> DATA_REGISTRATION_STATE

D/RIL-IPC ( 1891): xmm626_sec_modem_fmt_send: Sent FMT message

D/RIL-IPC ( 1891): xmm626_sec_modem_fmt_send: Message: mseq=0x24, command=IPC_NET_SERVING_NETWORK, type=IPC_TYPE_GET, size=0

D/RILJ    ( 2434): [0053]> VOICE_REGISTRATION_STATE

D/RIL-IPC ( 1891): 

D/RIL-IPC ( 1891): xmm626_sec_modem_fmt_recv: Received FMT message

D/RIL-IPC ( 1891): xmm626_sec_modem_fmt_recv: Message: aseq=0x23, command=IPC_NET_PLMN_SEL, type=IPC_TYPE_RESP, size=1

D/RIL-IPC ( 1891): ================================= IPC FMT data =================================

D/RIL-IPC ( 1891): [0000]   02                                                 .

D/RIL-IPC ( 1891): ================================================================================

D/RIL     ( 1891): 4 RIL requests in the queue (0 pending, 2 handled, 2 unhandled)

D/RIL     ( 1891): 1 RIL request data in the queue

D/RIL     ( 1891): 5 RIL requests in the queue (1 pending, 2 handled, 2 unhandled)

D/RIL     ( 1891): 1 RIL request data in the queue

D/RIL-IPC ( 1891): 

D/RIL-IPC ( 1891): xmm626_sec_modem_fmt_send: Sent FMT message

D/RIL-IPC ( 1891): xmm626_sec_modem_fmt_send: Message: mseq=0x25, command=IPC_NET_REGIST, type=IPC_TYPE_GET, size=2

D/RIL-IPC ( 1891): ================================= IPC FMT data =================================

D/RIL-IPC ( 1891): [0000]   FF 03                                              ..

D/RIL-IPC ( 1891): ================================================================================

D/RILJ    ( 2434): [0050]< QUERY_NETWORK_SELECTION_MODE {0}

D/RIL-IPC ( 1891): 

D/RIL-IPC ( 1891): xmm626_sec_modem_fmt_recv: Received FMT message

D/RIL-IPC ( 1891): xmm626_sec_modem_fmt_recv: Message: aseq=0x24, command=IPC_NET_SERVING_NETWORK, type=IPC_TYPE_RESP, size=11

D/RIL-IPC ( 1891): ================================= IPC FMT data =================================

D/RIL-IPC ( 1891): [0000]   02 04 04 32 30 36 31 30  23 CC 42                  ...20610 #.B

D/RIL-IPC ( 1891): ================================================================================

D/RIL     ( 1891): 4 RIL requests in the queue (0 pending, 2 handled, 2 unhandled)

D/RIL     ( 1891): 1 RIL request data in the queue

D/RILJ    ( 2434): [0054]> QUERY_NETWORK_SELECTION_MODE

D/RIL     ( 1891): 5 RIL requests in the queue (1 pending, 2 handled, 2 unhandled)

D/RIL     ( 1891): 1 RIL request data in the queue

D/RIL-IPC ( 1891): 

D/RIL-IPC ( 1891): xmm626_sec_modem_fmt_send: Sent FMT message

D/RIL-IPC ( 1891): xmm626_sec_modem_fmt_send: Message: mseq=0x26, command=IPC_NET_REGIST, type=IPC_TYPE_GET, size=2

D/RIL-IPC ( 1891): ================================= IPC FMT data =================================

D/RIL-IPC ( 1891): [0000]   FF 02                                              ..

D/RIL-IPC ( 1891): ================================================================================

D/RIL-IPC ( 1891): 

D/RIL-IPC ( 1891): xmm626_sec_modem_fmt_recv: Received FMT message

D/RIL-IPC ( 1891): xmm626_sec_modem_fmt_recv: Message: aseq=0x25, command=IPC_NET_REGIST, type=IPC_TYPE_RESP, size=11

D/RIL-IPC ( 1891): ================================= IPC FMT data =================================

D/RIL-IPC ( 1891): [0000]   04 03 01 01 CC 42 F4 A7  07 00 00                  .....B.. ...

D/RIL-IPC ( 1891): ================================================================================

D/RIL     ( 1891): 4 RIL requests in the queue (0 pending, 2 handled, 2 unhandled)

D/RIL     ( 1891): 1 RIL request data in the queue

D/RIL     ( 1891): 5 RIL requests in the queue (1 pending, 2 handled, 2 unhandled)

D/RIL     ( 1891): 1 RIL request data in the queue

D/RIL-IPC ( 1891): 

D/RIL-IPC ( 1891): xmm626_sec_modem_fmt_send: Sent FMT message

D/RIL-IPC ( 1891): xmm626_sec_modem_fmt_send: Message: mseq=0x27, command=IPC_NET_PLMN_SEL, type=IPC_TYPE_GET, size=0

D/RILJ    ( 2434): [0051]< OPERATOR {Mobistar, Mobistar, 20610}

D/RILJ    ( 2434): [0052]< DATA_REGISTRATION_STATE {0, 42cc, 7a7f4, 9, 3}

D/RILJ    ( 2434): [0055]> OPERATOR

D/RIL-IPC ( 1891): 

D/RIL-IPC ( 1891): xmm626_sec_modem_fmt_recv: Received FMT message

D/RIL-IPC ( 1891): xmm626_sec_modem_fmt_recv: Message: aseq=0x26, command=IPC_NET_REGIST, type=IPC_TYPE_RESP, size=11

D/RIL-IPC ( 1891): ================================= IPC FMT data =================================

D/RIL-IPC ( 1891): [0000]   04 02 04 01 CC 42 F4 A7  07 00 00                  .....B.. ...

D/RIL-IPC ( 1891): ================================================================================

D/RIL     ( 1891): 4 RIL requests in the queue (0 pending, 2 handled, 2 unhandled)

D/RIL     ( 1891): 1 RIL request data in the queue

D/RIL-IPC ( 1891): 

D/RIL-IPC ( 1891): xmm626_sec_modem_fmt_recv: Received FMT message

D/RIL-IPC ( 1891): xmm626_sec_modem_fmt_recv: Message: aseq=0x27, command=IPC_NET_PLMN_SEL, type=IPC_TYPE_RESP, size=1

D/RIL-IPC ( 1891): ================================= IPC FMT data =================================

D/RIL-IPC ( 1891): [0000]   02                                                 .

D/RIL-IPC ( 1891): ================================================================================

D/RIL     ( 1891): 3 RIL requests in the queue (0 pending, 1 handled, 2 unhandled)

D/RIL     ( 1891): 1 RIL request data in the queue

D/RILJ    ( 2434): [0053]< VOICE_REGISTRATION_STATE {10, 42cc, 7a7f4, 9, null, null, null, null, null, null, null, null, null, null, null}

D/RILJ    ( 2434): [0056]> DATA_REGISTRATION_STATE

D/RIL     ( 1891): 4 RIL requests in the queue (1 pending, 1 handled, 2 unhandled)

D/RIL     ( 1891): 1 RIL request data in the queue

D/RIL-IPC ( 1891): 

D/RIL-IPC ( 1891): xmm626_sec_modem_fmt_send: Sent FMT message

D/RIL-IPC ( 1891): xmm626_sec_modem_fmt_send: Message: mseq=0x28, command=IPC_NET_SERVING_NETWORK, type=IPC_TYPE_GET, size=0

D/RILJ    ( 2434): [0054]< QUERY_NETWORK_SELECTION_MODE {0}

D/RILJ    ( 2434): [0057]> VOICE_REGISTRATION_STATE

D/RIL     ( 1891): 5 RIL requests in the queue (1 pending, 2 handled, 2 unhandled)

D/RIL     ( 1891): 1 RIL request data in the queue

D/RIL-IPC ( 1891): 

D/RIL-IPC ( 1891): xmm626_sec_modem_fmt_send: Sent FMT message

D/RIL-IPC ( 1891): xmm626_sec_modem_fmt_send: Message: mseq=0x29, command=IPC_NET_REGIST, type=IPC_TYPE_GET, size=2

D/RIL-IPC ( 1891): ================================= IPC FMT data =================================

D/RIL-IPC ( 1891): [0000]   FF 03                                              ..

D/RIL-IPC ( 1891): ================================================================================

D/RILJ    ( 2434): [0058]> QUERY_NETWORK_SELECTION_MODE

D/RIL-IPC ( 1891): 

D/RIL-IPC ( 1891): xmm626_sec_modem_fmt_recv: Received FMT message

D/RIL-IPC ( 1891): xmm626_sec_modem_fmt_recv: Message: aseq=0x28, command=IPC_NET_SERVING_NETWORK, type=IPC_TYPE_RESP, size=11

D/RIL-IPC ( 1891): ================================= IPC FMT data =================================

D/RIL-IPC ( 1891): [0000]   02 04 04 32 30 36 31 30  23 CC 42                  ...20610 #.B

D/RIL-IPC ( 1891): ================================================================================

D/RIL     ( 1891): 4 RIL requests in the queue (0 pending, 2 handled, 2 unhandled)

D/RIL     ( 1891): 1 RIL request data in the queue

D/RIL     ( 1891): 5 RIL requests in the queue (1 pending, 2 handled, 2 unhandled)

D/RIL     ( 1891): 1 RIL request data in the queue

D/RIL-IPC ( 1891): 

D/RIL-IPC ( 1891): xmm626_sec_modem_fmt_send: Sent FMT message

D/RIL-IPC ( 1891): xmm626_sec_modem_fmt_send: Message: mseq=0x2a, command=IPC_NET_REGIST, type=IPC_TYPE_GET, size=2

D/RIL-IPC ( 1891): ================================= IPC FMT data =================================

D/RIL-IPC ( 1891): [0000]   FF 02                                              ..

D/RIL-IPC ( 1891): ================================================================================

D/RILJ    ( 2434): [0055]< OPERATOR {Mobistar, Mobistar, 20610}

D/RILJ    ( 2434): [0059]> OPERATOR

D/RIL-IPC ( 1891): 

D/RIL-IPC ( 1891): xmm626_sec_modem_fmt_recv: Received FMT message

D/RIL-IPC ( 1891): xmm626_sec_modem_fmt_recv: Message: aseq=0x29, command=IPC_NET_REGIST, type=IPC_TYPE_RESP, size=11

D/RIL-IPC ( 1891): ================================= IPC FMT data =================================

D/RIL-IPC ( 1891): [0000]   04 03 01 01 CC 42 F4 A7  07 00 00                  .....B.. ...

D/RIL-IPC ( 1891): ================================================================================

D/RIL     ( 1891): 4 RIL requests in the queue (0 pending, 2 handled, 2 unhandled)

D/RIL     ( 1891): 1 RIL request data in the queue

D/RIL-IPC ( 1891): 

D/RIL-IPC ( 1891): xmm626_sec_modem_fmt_recv: Received FMT message

D/RIL-IPC ( 1891): xmm626_sec_modem_fmt_recv: Message: aseq=0x2a, command=IPC_NET_REGIST, type=IPC_TYPE_RESP, size=11

D/RIL-IPC ( 1891): ================================= IPC FMT data =================================

D/RIL-IPC ( 1891): [0000]   04 02 04 01 CC 42 F4 A7  07 00 00                  .....B.. ...

D/RIL-IPC ( 1891): ================================================================================

D/RIL     ( 1891): 3 RIL requests in the queue (0 pending, 1 handled, 2 unhandled)

D/RIL     ( 1891): 1 RIL request data in the queue

D/RILJ    ( 2434): [0056]< DATA_REGISTRATION_STATE {0, 42cc, 7a7f4, 9, 3}

D/RIL     ( 1891): 4 RIL requests in the queue (1 pending, 1 handled, 2 unhandled)

D/RIL     ( 1891): 1 RIL request data in the queue

D/RILJ    ( 2434): [0057]< VOICE_REGISTRATION_STATE {10, 42cc, 7a7f4, 9, null, null, null, null, null, null, null, null, null, null, null}

D/RIL-IPC ( 1891): 

D/RIL-IPC ( 1891): xmm626_sec_modem_fmt_send: Sent FMT message

D/RIL-IPC ( 1891): xmm626_sec_modem_fmt_send: Message: mseq=0x2b, command=IPC_NET_PLMN_SEL, type=IPC_TYPE_GET, size=0

D/RIL     ( 1891): 5 RIL requests in the queue (1 pending, 2 handled, 2 unhandled)

D/RIL     ( 1891): 1 RIL request data in the queue

D/RIL-IPC ( 1891): 

D/RIL-IPC ( 1891): xmm626_sec_modem_fmt_send: Sent FMT message

D/RIL-IPC ( 1891): xmm626_sec_modem_fmt_send: Message: mseq=0x2c, command=IPC_NET_SERVING_NETWORK, type=IPC_TYPE_GET, size=0

D/RILJ    ( 2434): [0060]> DATA_REGISTRATION_STATE

D/RILJ    ( 2434): [0061]> VOICE_REGISTRATION_STATE

D/RIL     ( 1891): 6 RIL requests in the queue (1 pending, 3 handled, 2 unhandled)

D/RIL     ( 1891): 1 RIL request data in the queue

D/RIL-IPC ( 1891): 

D/RIL-IPC ( 1891): xmm626_sec_modem_fmt_send: Sent FMT message

D/RIL-IPC ( 1891): xmm626_sec_modem_fmt_send: Message: mseq=0x2d, command=IPC_NET_REGIST, type=IPC_TYPE_GET, size=2

D/RIL-IPC ( 1891): ================================= IPC FMT data =================================

D/RIL-IPC ( 1891): [0000]   FF 03                                              ..

D/RIL-IPC ( 1891): ================================================================================

D/RIL-IPC ( 1891): 

D/RIL-IPC ( 1891): xmm626_sec_modem_fmt_recv: Received FMT message

D/RIL-IPC ( 1891): xmm626_sec_modem_fmt_recv: Message: aseq=0x2b, command=IPC_NET_PLMN_SEL, type=IPC_TYPE_RESP, size=1

D/RIL-IPC ( 1891): ================================= IPC FMT data =================================

D/RIL-IPC ( 1891): [0000]   02                                                 .

D/RIL-IPC ( 1891): ================================================================================

D/RIL     ( 1891): 5 RIL requests in the queue (0 pending, 3 handled, 2 unhandled)

D/RIL     ( 1891): 1 RIL request data in the queue

D/RIL-IPC ( 1891): 

D/RIL-IPC ( 1891): xmm626_sec_modem_fmt_recv: Received FMT message

D/RIL-IPC ( 1891): xmm626_sec_modem_fmt_recv: Message: aseq=0x2c, command=IPC_NET_SERVING_NETWORK, type=IPC_TYPE_RESP, size=11

D/RIL-IPC ( 1891): ================================= IPC FMT data =================================

D/RIL-IPC ( 1891): [0000]   02 04 04 32 30 36 31 30  23 CC 42                  ...20610 #.B

D/RIL-IPC ( 1891): ================================================================================

D/RILJ    ( 2434): [0062]> QUERY_NETWORK_SELECTION_MODE

D/RILJ    ( 2434): [0058]< QUERY_NETWORK_SELECTION_MODE {0}

D/RIL     ( 1891): 4 RIL requests in the queue (0 pending, 2 handled, 2 unhandled)

D/RIL     ( 1891): 1 RIL request data in the queue

D/RIL-IPC ( 1891): 

D/RIL-IPC ( 1891): xmm626_sec_modem_fmt_recv: Received FMT message

D/RIL-IPC ( 1891): xmm626_sec_modem_fmt_recv: Message: aseq=0x2d, command=IPC_NET_REGIST, type=IPC_TYPE_RESP, size=11

D/RIL-IPC ( 1891): ================================= IPC FMT data =================================

D/RIL-IPC ( 1891): [0000]   04 03 01 01 CC 42 F4 A7  07 00 00                  .....B.. ...

D/RIL-IPC ( 1891): ================================================================================

D/RIL     ( 1891): 3 RIL requests in the queue (0 pending, 1 handled, 2 unhandled)

D/RIL     ( 1891): 1 RIL request data in the queue

D/RIL     ( 1891): 4 RIL requests in the queue (1 pending, 1 handled, 2 unhandled)

D/RIL     ( 1891): 1 RIL request data in the queue

D/RIL-IPC ( 1891): 

D/RIL-IPC ( 1891): xmm626_sec_modem_fmt_send: Sent FMT message

D/RIL-IPC ( 1891): xmm626_sec_modem_fmt_send: Message: mseq=0x2e, command=IPC_NET_REGIST, type=IPC_TYPE_GET, size=2

D/RIL-IPC ( 1891): ================================= IPC FMT data =================================

D/RIL-IPC ( 1891): [0000]   FF 02                                              ..

D/RIL-IPC ( 1891): ================================================================================

D/RIL-IPC ( 1891): 

D/RIL-IPC ( 1891): xmm626_sec_modem_fmt_recv: Received FMT message

D/RIL-IPC ( 1891): xmm626_sec_modem_fmt_recv: Message: aseq=0x2e, command=IPC_NET_REGIST, type=IPC_TYPE_RESP, size=11

D/RIL-IPC ( 1891): ================================= IPC FMT data =================================

D/RIL-IPC ( 1891): [0000]   04 02 04 01 CC 42 F4 A7  07 00 00                  .....B.. ...

D/RIL-IPC ( 1891): ================================================================================

D/RIL     ( 1891): 3 RIL requests in the queue (0 pending, 1 handled, 2 unhandled)

D/RIL     ( 1891): 1 RIL request data in the queue

D/RILJ    ( 2434): [0059]< OPERATOR {Mobistar, Mobistar, 20610}

D/RILJ    ( 2434): [0060]< DATA_REGISTRATION_STATE {0, 42cc, 7a7f4, 9, 3}

D/RIL     ( 1891): 4 RIL requests in the queue (1 pending, 1 handled, 2 unhandled)

D/RIL     ( 1891): 1 RIL request data in the queue

D/RIL-IPC ( 1891): 

D/RIL-IPC ( 1891): xmm626_sec_modem_fmt_send: Sent FMT message

D/RIL-IPC ( 1891): xmm626_sec_modem_fmt_send: Message: mseq=0x2f, command=IPC_NET_PLMN_SEL, type=IPC_TYPE_GET, size=0

D/RILJ    ( 2434): [0061]< VOICE_REGISTRATION_STATE {10, 42cc, 7a7f4, 9, null, null, null, null, null, null, null, null, null, null, null}

D/RIL-IPC ( 1891): 

D/RIL-IPC ( 1891): xmm626_sec_modem_fmt_recv: Received FMT message

D/RIL-IPC ( 1891): xmm626_sec_modem_fmt_recv: Message: aseq=0x2f, command=IPC_NET_PLMN_SEL, type=IPC_TYPE_RESP, size=1

D/RIL-IPC ( 1891): ================================= IPC FMT data =================================

D/RIL-IPC ( 1891): [0000]   02                                                 .

D/RIL-IPC ( 1891): ================================================================================

D/RIL     ( 1891): 3 RIL requests in the queue (0 pending, 1 handled, 2 unhandled)

D/RIL     ( 1891): 1 RIL request data in the queue

D/RILJ    ( 2434): [0062]< QUERY_NETWORK_SELECTION_MODE {0}

D/GSM     ( 2434): [GsmSST] Poll ServiceState done:  oldSS=[1 home Mobistar Mobistar 20610  Unknown CSS not supported -1 -1 RoamInd=-1 DefRoamInd=-1 EmergOnly=true] newSS=[1 home Mobistar Mobistar 20610  HSDPA CSS not supported -1 -1 RoamInd=-1 DefRoamInd=-1 EmergOnly=true] oldGprs=1 newData=1 oldMaxDataCalls=1 mNewMaxDataCalls=1 oldReasonDataDenied=-1 mNewReasonDataDenied=-1 oldType=Unknown newType=HSDPA

D/GSM     ( 2434): [GsmSST] RAT switched Unknown -> HSDPA at cell 501748

D/GSM     ( 2434): [GsmSST] updateSpnDisplay: radio is on but out of service, set plmn='Emergency calls only'

D/GSM     ( 2434): [GsmSST] pollStateDone: no nitz but one TZ for iso-cc=be with zone.getID=Europe/Brussels testOneUniqueOffsetPath=false

D/GSM     ( 2434): [GsmSST] setAndBroadcastNetworkSetTimeZone: setTimeZone=Europe/Brussels

D/GSM     ( 2434): [GsmSST] setAndBroadcastNetworkSetTimeZone: call alarm.setTimeZone and broadcast zoneId=Europe/Brussels

D/GSM     ( 2434): [GsmSST] shouldFixTimeZoneNow: retVal=false iccCardExist=false operatorNumeric=20610 mcc=206 prevOperatorNumeric=20610 prevMcc=206 needToFixTimeZone=false ltod=06-01 18:19:42.421

D/GSM     ( 2434): [GsmDCT] get all active apn types

D/GSM     ( 2434): [GsmDCT] isDataAllowed: not allowed due to - gprs= 1 - SIM not loaded

D/GSM     ( 2434): [GsmDCT] isDataPossible(default): possible=false isDataAllowed=false apnTypePossible=true apnContextisEnabled=true apnContextState()=IDLE

D/GSM     ( 2434): [GsmDCT] get active apn string for type:default

D/GSM     ( 2434): [GsmDCT] onReceive: action=android.intent.action.SCREEN_ON

D/GSM     ( 2434): [GsmDCT] stopNetStatPoll

D/GSM     ( 2434): [GsmDCT] overall state is IDLE

D/RILJ    ( 2434): [0063]> SCREEN_STATE: true

D/RIL     ( 1891): 4 RIL requests in the queue (1 pending, 1 handled, 2 unhandled)

D/RIL     ( 1891): 1 RIL request data in the queue

D/RIL     ( 1891): 3 RIL requests in the queue (0 pending, 1 handled, 2 unhandled)

D/RIL     ( 1891): 1 RIL request data in the queue

D/RILJ    ( 2434): [UNSL]< UNSOL_RESPONSE_VOICE_NETWORK_STATE_CHANGED

D/RILJ    ( 2434): [0063]< SCREEN_STATE 

D/RILJ    ( 2434): [0064]> OPERATOR

D/RILJ    ( 2434): [0065]> DATA_REGISTRATION_STATE

D/RIL     ( 1891): 4 RIL requests in the queue (1 pending, 1 handled, 2 unhandled)

D/RIL     ( 1891): 1 RIL request data in the queue

D/RIL-IPC ( 1891): 

D/RIL-IPC ( 1891): xmm626_sec_modem_fmt_send: Sent FMT message

D/RIL-IPC ( 1891): xmm626_sec_modem_fmt_send: Message: mseq=0x30, command=IPC_NET_SERVING_NETWORK, type=IPC_TYPE_GET, size=0

D/RILJ    ( 2434): [0066]> VOICE_REGISTRATION_STATE

D/RILJ    ( 2434): [0067]> QUERY_NETWORK_SELECTION_MODE

D/RIL     ( 1891): 5 RIL requests in the queue (1 pending, 2 handled, 2 unhandled)

D/RIL     ( 1891): 1 RIL request data in the queue

D/RIL     ( 1891): 6 RIL requests in the queue (2 pending, 2 handled, 2 unhandled)

D/RIL     ( 1891): 1 RIL request data in the queue

D/RIL     ( 1891): 7 RIL requests in the queue (3 pending, 2 handled, 2 unhandled)

D/RIL     ( 1891): 1 RIL request data in the queue

D/RIL-IPC ( 1891): 

D/RIL-IPC ( 1891): xmm626_sec_modem_fmt_send: Sent FMT message

D/RIL-IPC ( 1891): xmm626_sec_modem_fmt_send: Message: mseq=0x31, command=IPC_NET_REGIST, type=IPC_TYPE_GET, size=2

D/RIL-IPC ( 1891): ================================= IPC FMT data =================================

D/RIL-IPC ( 1891): [0000]   FF 03                                              ..

D/RIL-IPC ( 1891): ================================================================================

D/RIL-IPC ( 1891): 

D/RIL-IPC ( 1891): xmm626_sec_modem_fmt_send: Sent FMT message

D/RIL-IPC ( 1891): xmm626_sec_modem_fmt_send: Message: mseq=0x32, command=IPC_NET_REGIST, type=IPC_TYPE_GET, size=2

D/RIL-IPC ( 1891): ================================= IPC FMT data =================================

D/RIL-IPC ( 1891): [0000]   FF 02                                              ..

D/RIL-IPC ( 1891): ================================================================================

D/RIL-IPC ( 1891): 

D/RIL-IPC ( 1891): xmm626_sec_modem_fmt_send: Sent FMT message

D/RIL-IPC ( 1891): xmm626_sec_modem_fmt_send: Message: mseq=0x33, command=IPC_NET_PLMN_SEL, type=IPC_TYPE_GET, size=0

D/GSM     ( 2434): [GsmDCT] onReceive: action=android.intent.action.SCREEN_OFF

D/GSM     ( 2434): [GsmDCT] stopNetStatPoll

D/GSM     ( 2434): [GsmDCT] overall state is IDLE

D/RILJ    ( 2434): [0068]> SCREEN_STATE: false

D/RIL     ( 1891): 8 RIL requests in the queue (1 pending, 5 handled, 2 unhandled)

D/RIL     ( 1891): 1 RIL request data in the queue

D/RIL     ( 1891): 7 RIL requests in the queue (0 pending, 5 handled, 2 unhandled)

D/RIL     ( 1891): 1 RIL request data in the queue

D/RILJ    ( 2434): [0068]< SCREEN_STATE 

D/RIL-IPC ( 1891): 

D/RIL-IPC ( 1891): xmm626_sec_modem_fmt_recv: Received FMT message

D/RIL-IPC ( 1891): xmm626_sec_modem_fmt_recv: Message: aseq=0x30, command=IPC_NET_SERVING_NETWORK, type=IPC_TYPE_RESP, size=11

D/RIL-IPC ( 1891): ================================= IPC FMT data =================================

D/RIL-IPC ( 1891): [0000]   02 04 04 32 30 36 31 30  23 CC 42                  ...20610 #.B

D/RIL-IPC ( 1891): ================================================================================

D/RIL     ( 1891): 6 RIL requests in the queue (0 pending, 4 handled, 2 unhandled)

D/RIL     ( 1891): 1 RIL request data in the queue

D/RILJ    ( 2434): [0064]< OPERATOR {Mobistar, Mobistar, 20610}

D/RIL-IPC ( 1891): 

D/RIL-IPC ( 1891): xmm626_sec_modem_fmt_recv: Received FMT message

D/RIL-IPC ( 1891): xmm626_sec_modem_fmt_recv: Message: aseq=0x31, command=IPC_NET_REGIST, type=IPC_TYPE_RESP, size=11

D/RIL-IPC ( 1891): ================================= IPC FMT data =================================

D/RIL-IPC ( 1891): [0000]   04 03 01 01 CC 42 F4 A7  07 00 00                  .....B.. ...

D/RIL-IPC ( 1891): ================================================================================

D/RIL     ( 1891): 5 RIL requests in the queue (0 pending, 3 handled, 2 unhandled)

D/RIL     ( 1891): 1 RIL request data in the queue

D/RILJ    ( 2434): [0065]< DATA_REGISTRATION_STATE {0, 42cc, 7a7f4, 9, 3}

D/RIL-IPC ( 1891): 

D/RIL-IPC ( 1891): xmm626_sec_modem_fmt_recv: Received FMT message

D/RIL-IPC ( 1891): xmm626_sec_modem_fmt_recv: Message: aseq=0x32, command=IPC_NET_REGIST, type=IPC_TYPE_RESP, size=11

D/RIL-IPC ( 1891): ================================= IPC FMT data =================================

D/RIL-IPC ( 1891): [0000]   04 02 04 01 CC 42 F4 A7  07 00 00                  .....B.. ...

D/RIL-IPC ( 1891): ================================================================================

D/RIL     ( 1891): 4 RIL requests in the queue (0 pending, 2 handled, 2 unhandled)

D/RIL     ( 1891): 1 RIL request data in the queue

D/RILJ    ( 2434): [0066]< VOICE_REGISTRATION_STATE {10, 42cc, 7a7f4, 9, null, null, null, null, null, null, null, null, null, null, null}

D/RIL-IPC ( 1891): 

D/RIL-IPC ( 1891): xmm626_sec_modem_fmt_recv: Received FMT message

D/RIL-IPC ( 1891): xmm626_sec_modem_fmt_recv: Message: aseq=0x33, command=IPC_NET_PLMN_SEL, type=IPC_TYPE_RESP, size=1

D/RIL-IPC ( 1891): ================================= IPC FMT data =================================

D/RIL-IPC ( 1891): [0000]   02                                                 .

D/RIL-IPC ( 1891): ================================================================================

D/RIL     ( 1891): 3 RIL requests in the queue (0 pending, 1 handled, 2 unhandled)

D/RIL     ( 1891): 1 RIL request data in the queue

D/RILJ    ( 2434): [0067]< QUERY_NETWORK_SELECTION_MODE {0}

D/GSM     ( 2434): [GsmSST] Poll ServiceState done:  oldSS=[1 home Mobistar Mobistar 20610  HSDPA CSS not supported -1 -1 RoamInd=-1 DefRoamInd=-1 EmergOnly=true] newSS=[1 home Mobistar Mobistar 20610  HSDPA CSS not supported -1 -1 RoamInd=-1 DefRoamInd=-1 EmergOnly=true] oldGprs=1 newData=1 oldMaxDataCalls=1 mNewMaxDataCalls=1 oldReasonDataDenied=-1 mNewReasonDataDenied=-1 oldType=HSDPA newType=HSDPA

D/GSM     ( 2434): [GsmDCT] onReceive: action=android.intent.action.SCREEN_ON

D/GSM     ( 2434): [GsmDCT] stopNetStatPoll

D/GSM     ( 2434): [GsmDCT] overall state is IDLE

D/RILJ    ( 2434): [0069]> SCREEN_STATE: true

D/RIL     ( 1891): 4 RIL requests in the queue (1 pending, 1 handled, 2 unhandled)

D/RIL     ( 1891): 1 RIL request data in the queue

D/RIL     ( 1891): 3 RIL requests in the queue (0 pending, 1 handled, 2 unhandled)

D/RIL     ( 1891): 1 RIL request data in the queue

D/RILJ    ( 2434): [UNSL]< UNSOL_RESPONSE_VOICE_NETWORK_STATE_CHANGED

D/RILJ    ( 2434): [0069]< SCREEN_STATE 

D/RILJ    ( 2434): [0070]> OPERATOR

D/RILJ    ( 2434): [0071]> DATA_REGISTRATION_STATE

D/RIL     ( 1891): 4 RIL requests in the queue (1 pending, 1 handled, 2 unhandled)

D/RIL     ( 1891): 1 RIL request data in the queue

D/RIL-IPC ( 1891): 

D/RIL-IPC ( 1891): xmm626_sec_modem_fmt_send: Sent FMT message

D/RIL-IPC ( 1891): xmm626_sec_modem_fmt_send: Message: mseq=0x34, command=IPC_NET_SERVING_NETWORK, type=IPC_TYPE_GET, size=0

D/RILJ    ( 2434): [0072]> VOICE_REGISTRATION_STATE

D/RILJ    ( 2434): [0073]> QUERY_NETWORK_SELECTION_MODE

D/RIL     ( 1891): 5 RIL requests in the queue (1 pending, 2 handled, 2 unhandled)

D/RIL     ( 1891): 1 RIL request data in the queue

D/RIL-IPC ( 1891): 

D/RIL-IPC ( 1891): xmm626_sec_modem_fmt_send: Sent FMT message

D/RIL-IPC ( 1891): xmm626_sec_modem_fmt_send: Message: mseq=0x35, command=IPC_NET_REGIST, type=IPC_TYPE_GET, size=2

D/RIL-IPC ( 1891): ================================= IPC FMT data =================================

D/RIL-IPC ( 1891): [0000]   FF 03                                              ..

D/RIL-IPC ( 1891): ================================================================================

D/RIL     ( 1891): 6 RIL requests in the queue (1 pending, 3 handled, 2 unhandled)

D/RIL     ( 1891): 1 RIL request data in the queue

D/RIL-IPC ( 1891): 

D/RIL-IPC ( 1891): xmm626_sec_modem_fmt_send: Sent FMT message

D/RIL-IPC ( 1891): xmm626_sec_modem_fmt_send: Message: mseq=0x36, command=IPC_NET_REGIST, type=IPC_TYPE_GET, size=2

D/RIL-IPC ( 1891): ================================= IPC FMT data =================================

D/RIL-IPC ( 1891): [0000]   FF 02                                              ..

D/RIL-IPC ( 1891): ================================================================================

D/RIL     ( 1891): 7 RIL requests in the queue (1 pending, 4 handled, 2 unhandled)

D/RIL     ( 1891): 1 RIL request data in the queue

D/RIL-IPC ( 1891): 

D/RIL-IPC ( 1891): xmm626_sec_modem_fmt_send: Sent FMT message

D/RIL-IPC ( 1891): xmm626_sec_modem_fmt_send: Message: mseq=0x37, command=IPC_NET_PLMN_SEL, type=IPC_TYPE_GET, size=0

D/RIL-IPC ( 1891): 

D/RIL-IPC ( 1891): xmm626_sec_modem_fmt_recv: Received FMT message

D/RIL-IPC ( 1891): xmm626_sec_modem_fmt_recv: Message: aseq=0x34, command=IPC_NET_SERVING_NETWORK, type=IPC_TYPE_RESP, size=11

D/RIL-IPC ( 1891): ================================= IPC FMT data =================================

D/RIL-IPC ( 1891): [0000]   02 04 04 32 30 36 31 30  23 CC 42                  ...20610 #.B

D/RIL-IPC ( 1891): ================================================================================

D/RIL     ( 1891): 6 RIL requests in the queue (0 pending, 4 handled, 2 unhandled)

D/RIL     ( 1891): 1 RIL request data in the queue

D/RIL-IPC ( 1891): 

D/RIL-IPC ( 1891): xmm626_sec_modem_fmt_recv: Received FMT message

D/RIL-IPC ( 1891): xmm626_sec_modem_fmt_recv: Message: aseq=0x35, command=IPC_NET_REGIST, type=IPC_TYPE_RESP, size=11

D/RIL-IPC ( 1891): ================================= IPC FMT data =================================

D/RIL-IPC ( 1891): [0000]   04 03 01 01 CC 42 F4 A7  07 00 00                  .....B.. ...

D/RIL-IPC ( 1891): ================================================================================

D/RIL     ( 1891): 5 RIL requests in the queue (0 pending, 3 handled, 2 unhandled)

D/RIL     ( 1891): 1 RIL request data in the queue

D/RIL-IPC ( 1891): 

D/RIL-IPC ( 1891): xmm626_sec_modem_fmt_recv: Received FMT message

D/RIL-IPC ( 1891): xmm626_sec_modem_fmt_recv: Message: aseq=0x36, command=IPC_NET_REGIST, type=IPC_TYPE_RESP, size=11

D/RIL-IPC ( 1891): ================================= IPC FMT data =================================

D/RIL-IPC ( 1891): [0000]   04 02 04 01 CC 42 F4 A7  07 00 00                  .....B.. ...

D/RIL-IPC ( 1891): ================================================================================

D/RIL     ( 1891): 4 RIL requests in the queue (0 pending, 2 handled, 2 unhandled)

D/RIL     ( 1891): 1 RIL request data in the queue

D/RIL-IPC ( 1891): 

D/RIL-IPC ( 1891): xmm626_sec_modem_fmt_recv: Received FMT message

D/RIL-IPC ( 1891): xmm626_sec_modem_fmt_recv: Message: aseq=0x37, command=IPC_NET_PLMN_SEL, type=IPC_TYPE_RESP, size=1

D/RIL-IPC ( 1891): ================================= IPC FMT data =================================

D/RIL-IPC ( 1891): [0000]   02                                                 .

D/RIL-IPC ( 1891): ================================================================================

D/RIL     ( 1891): 3 RIL requests in the queue (0 pending, 1 handled, 2 unhandled)

D/RIL     ( 1891): 1 RIL request data in the queue

D/RILJ    ( 2434): [0070]< OPERATOR {Mobistar, Mobistar, 20610}

D/RILJ    ( 2434): [0071]< DATA_REGISTRATION_STATE {0, 42cc, 7a7f4, 9, 3}

D/RILJ    ( 2434): [0072]< VOICE_REGISTRATION_STATE {10, 42cc, 7a7f4, 9, null, null, null, null, null, null, null, null, null, null, null}

D/RILJ    ( 2434): [0073]< QUERY_NETWORK_SELECTION_MODE {0}

D/GSM     ( 2434): [GsmSST] Poll ServiceState done:  oldSS=[1 home Mobistar Mobistar 20610  HSDPA CSS not supported -1 -1 RoamInd=-1 DefRoamInd=-1 EmergOnly=true] newSS=[1 home Mobistar Mobistar 20610  HSDPA CSS not supported -1 -1 RoamInd=-1 DefRoamInd=-1 EmergOnly=true] oldGprs=1 newData=1 oldMaxDataCalls=1 mNewMaxDataCalls=1 oldReasonDataDenied=-1 mNewReasonDataDenied=-1 oldType=HSDPA newType=HSDPA

D/RIL-IPC ( 1891): 

D/RIL-IPC ( 1891): xmm626_sec_modem_fmt_recv: Received FMT message

D/RIL-IPC ( 1891): xmm626_sec_modem_fmt_recv: Message: aseq=0x37, command=IPC_DISP_RSSI_INFO, type=IPC_TYPE_NOTI, size=1

D/RIL-IPC ( 1891): ================================= IPC FMT data =================================

D/RIL-IPC ( 1891): [0000]   4E                                                 N

D/RIL-IPC ( 1891): ================================================================================

D/RIL     ( 1891): Signal strength is 17

D/RIL-IPC ( 1891): 

D/RIL-IPC ( 1891): xmm626_sec_modem_fmt_recv: Received FMT message

D/RIL-IPC ( 1891): xmm626_sec_modem_fmt_recv: Message: aseq=0x37, command=IPC_DISP_RSSI_INFO, type=IPC_TYPE_NOTI, size=1

D/RIL-IPC ( 1891): ================================= IPC FMT data =================================

D/RIL-IPC ( 1891): [0000]   50                                                 P

D/RIL-IPC ( 1891): ================================================================================

D/RIL     ( 1891): Signal strength is 16

D/GSM     ( 2434): [GsmDCT] onReceive: action=android.intent.action.SCREEN_OFF

D/GSM     ( 2434): [GsmDCT] stopNetStatPoll

D/GSM     ( 2434): [GsmDCT] overall state is IDLE

D/RILJ    ( 2434): [0074]> SCREEN_STATE: false

D/RIL     ( 1891): 4 RIL requests in the queue (1 pending, 1 handled, 2 unhandled)

D/RIL     ( 1891): 1 RIL request data in the queue

D/RIL     ( 1891): 3 RIL requests in the queue (0 pending, 1 handled, 2 unhandled)

D/RIL     ( 1891): 1 RIL request data in the queue

D/RILJ    ( 2434): [0074]< SCREEN_STATE 

D/RIL-IPC ( 1891): 

D/RIL-IPC ( 1891): xmm626_sec_modem_fmt_recv: Received FMT message

D/RIL-IPC ( 1891): xmm626_sec_modem_fmt_recv: Message: aseq=0x37, command=IPC_DISP_RSSI_INFO, type=IPC_TYPE_NOTI, size=1

D/RIL-IPC ( 1891): ================================= IPC FMT data =================================

D/RIL-IPC ( 1891): [0000]   52                                                 R

D/RIL-IPC ( 1891): ================================================================================

D/RIL     ( 1891): Signal strength is 15

D/GSM     ( 2434): [GsmDCT] onReceive: action=android.intent.action.SCREEN_ON

D/GSM     ( 2434): [GsmDCT] stopNetStatPoll

D/GSM     ( 2434): [GsmDCT] overall state is IDLE

D/RILJ    ( 2434): [0075]> SCREEN_STATE: true

D/RIL     ( 1891): 4 RIL requests in the queue (1 pending, 1 handled, 2 unhandled)

D/RIL     ( 1891): 1 RIL request data in the queue

D/RIL     ( 1891): 3 RIL requests in the queue (0 pending, 1 handled, 2 unhandled)

D/RIL     ( 1891): 1 RIL request data in the queue

D/RILJ    ( 2434): [UNSL]< UNSOL_RESPONSE_VOICE_NETWORK_STATE_CHANGED

D/RILJ    ( 2434): [0075]< SCREEN_STATE 

D/RILJ    ( 2434): [0076]> OPERATOR

D/RILJ    ( 2434): [0077]> DATA_REGISTRATION_STATE

D/RIL     ( 1891): 4 RIL requests in the queue (1 pending, 1 handled, 2 unhandled)

D/RIL     ( 1891): 1 RIL request data in the queue

D/RIL-IPC ( 1891): 

D/RIL-IPC ( 1891): xmm626_sec_modem_fmt_send: Sent FMT message

D/RIL-IPC ( 1891): xmm626_sec_modem_fmt_send: Message: mseq=0x38, command=IPC_NET_SERVING_NETWORK, type=IPC_TYPE_GET, size=0

D/RILJ    ( 2434): [0078]> VOICE_REGISTRATION_STATE

D/RIL     ( 1891): 5 RIL requests in the queue (1 pending, 2 handled, 2 unhandled)

D/RIL     ( 1891): 1 RIL request data in the queue

D/RIL-IPC ( 1891): 

D/RIL-IPC ( 1891): xmm626_sec_modem_fmt_send: Sent FMT message

D/RIL-IPC ( 1891): xmm626_sec_modem_fmt_send: Message: mseq=0x39, command=IPC_NET_REGIST, type=IPC_TYPE_GET, size=2

D/RIL-IPC ( 1891): ================================= IPC FMT data =================================

D/RIL-IPC ( 1891): [0000]   FF 03                                              ..

D/RIL-IPC ( 1891): ================================================================================

D/RILJ    ( 2434): [0079]> QUERY_NETWORK_SELECTION_MODE

D/RIL     ( 1891): 6 RIL requests in the queue (1 pending, 3 handled, 2 unhandled)

D/RIL     ( 1891): 1 RIL request data in the queue

D/RIL-IPC ( 1891): 

D/RIL-IPC ( 1891): xmm626_sec_modem_fmt_send: Sent FMT message

D/RIL-IPC ( 1891): xmm626_sec_modem_fmt_send: Message: mseq=0x3a, command=IPC_NET_REGIST, type=IPC_TYPE_GET, size=2

D/RIL-IPC ( 1891): ================================= IPC FMT data =================================

D/RIL-IPC ( 1891): [0000]   FF 02                                              ..

D/RIL-IPC ( 1891): ================================================================================

D/RIL     ( 1891): 7 RIL requests in the queue (1 pending, 4 handled, 2 unhandled)

D/RIL     ( 1891): 1 RIL request data in the queue

D/RIL-IPC ( 1891): 

D/RIL-IPC ( 1891): xmm626_sec_modem_fmt_send: Sent FMT message

D/RIL-IPC ( 1891): xmm626_sec_modem_fmt_send: Message: mseq=0x3b, command=IPC_NET_PLMN_SEL, type=IPC_TYPE_GET, size=0

D/RIL-IPC ( 1891): 

D/RIL-IPC ( 1891): xmm626_sec_modem_fmt_recv: Received FMT message

D/RIL-IPC ( 1891): xmm626_sec_modem_fmt_recv: Message: aseq=0x38, command=IPC_NET_SERVING_NETWORK, type=IPC_TYPE_RESP, size=11

D/RIL-IPC ( 1891): ================================= IPC FMT data =================================

D/RIL-IPC ( 1891): [0000]   02 04 04 32 30 36 31 30  23 CC 42                  ...20610 #.B

D/RIL-IPC ( 1891): ================================================================================

D/RIL     ( 1891): 6 RIL requests in the queue (0 pending, 4 handled, 2 unhandled)

D/RIL     ( 1891): 1 RIL request data in the queue

D/RILJ    ( 2434): [0076]< OPERATOR {Mobistar, Mobistar, 20610}

D/RIL-IPC ( 1891): 

D/RIL-IPC ( 1891): xmm626_sec_modem_fmt_recv: Received FMT message

D/RIL-IPC ( 1891): xmm626_sec_modem_fmt_recv: Message: aseq=0x39, command=IPC_NET_REGIST, type=IPC_TYPE_RESP, size=11

D/RIL-IPC ( 1891): ================================= IPC FMT data =================================

D/RIL-IPC ( 1891): [0000]   04 03 01 01 CC 42 F4 A7  07 00 00                  .....B.. ...

D/RIL-IPC ( 1891): ================================================================================

D/RIL     ( 1891): 5 RIL requests in the queue (0 pending, 3 handled, 2 unhandled)

D/RIL     ( 1891): 1 RIL request data in the queue

D/RILJ    ( 2434): [0077]< DATA_REGISTRATION_STATE {0, 42cc, 7a7f4, 9, 3}

D/RIL-IPC ( 1891): 

D/RIL-IPC ( 1891): xmm626_sec_modem_fmt_recv: Received FMT message

D/RIL-IPC ( 1891): xmm626_sec_modem_fmt_recv: Message: aseq=0x3a, command=IPC_NET_REGIST, type=IPC_TYPE_RESP, size=11

D/RIL-IPC ( 1891): ================================= IPC FMT data =================================

D/RIL-IPC ( 1891): [0000]   04 02 04 01 CC 42 F4 A7  07 00 00                  .....B.. ...

D/RIL-IPC ( 1891): ================================================================================

D/RIL     ( 1891): 4 RIL requests in the queue (0 pending, 2 handled, 2 unhandled)

D/RIL     ( 1891): 1 RIL request data in the queue

D/RILJ    ( 2434): [0078]< VOICE_REGISTRATION_STATE {10, 42cc, 7a7f4, 9, null, null, null, null, null, null, null, null, null, null, null}

D/RIL-IPC ( 1891): 

D/RIL-IPC ( 1891): xmm626_sec_modem_fmt_recv: Received FMT message

D/RIL-IPC ( 1891): xmm626_sec_modem_fmt_recv: Message: aseq=0x3b, command=IPC_NET_PLMN_SEL, type=IPC_TYPE_RESP, size=1

D/RIL-IPC ( 1891): ================================= IPC FMT data =================================

D/RIL-IPC ( 1891): [0000]   02                                                 .

D/RIL-IPC ( 1891): ================================================================================

D/RIL     ( 1891): 3 RIL requests in the queue (0 pending, 1 handled, 2 unhandled)

D/RIL     ( 1891): 1 RIL request data in the queue

D/RILJ    ( 2434): [0079]< QUERY_NETWORK_SELECTION_MODE {0}

D/GSM     ( 2434): [GsmSST] Poll ServiceState done:  oldSS=[1 home Mobistar Mobistar 20610  HSDPA CSS not supported -1 -1 RoamInd=-1 DefRoamInd=-1 EmergOnly=true] newSS=[1 home Mobistar Mobistar 20610  HSDPA CSS not supported -1 -1 RoamInd=-1 DefRoamInd=-1 EmergOnly=true] oldGprs=1 newData=1 oldMaxDataCalls=1 mNewMaxDataCalls=1 oldReasonDataDenied=-1 mNewReasonDataDenied=-1 oldType=HSDPA newType=HSDPA

D/RIL-IPC ( 1891): 

D/RIL-IPC ( 1891): xmm626_sec_modem_fmt_recv: Received FMT message

D/RIL-IPC ( 1891): xmm626_sec_modem_fmt_recv: Message: aseq=0x3b, command=IPC_DISP_RSSI_INFO, type=IPC_TYPE_NOTI, size=1

D/RIL-IPC ( 1891): ================================= IPC FMT data =================================

D/RIL-IPC ( 1891): [0000]   54                                                 T

D/RIL-IPC ( 1891): ================================================================================

D/RIL     ( 1891): Signal strength is 14

D/RIL-IPC ( 1891): 

D/RIL-IPC ( 1891): xmm626_sec_modem_fmt_recv: Received FMT message

D/RIL-IPC ( 1891): xmm626_sec_modem_fmt_recv: Message: aseq=0x3b, command=IPC_DISP_RSSI_INFO, type=IPC_TYPE_NOTI, size=1

D/RIL-IPC ( 1891): ================================= IPC FMT data =================================

D/RIL-IPC ( 1891): [0000]   56                                                 V

D/RIL-IPC ( 1891): ================================================================================

D/RIL     ( 1891): Signal strength is 13

D/RIL-IPC ( 1891): 

D/RIL-IPC ( 1891): xmm626_sec_modem_fmt_recv: Received FMT message

D/RIL-IPC ( 1891): xmm626_sec_modem_fmt_recv: Message: aseq=0xff, command=IPC_NET_REGIST, type=IPC_TYPE_NOTI, size=11

D/RIL-IPC ( 1891): ================================= IPC FMT data =================================

D/RIL-IPC ( 1891): [0000]   04 02 04 01 CC 42 F2 A7  07 00 00                  .....B.. ...

D/RIL-IPC ( 1891): ================================================================================

D/RIL-IPC ( 1891): 

D/RIL-IPC ( 1891): xmm626_sec_modem_fmt_recv: Received FMT message

D/RIL-IPC ( 1891): xmm626_sec_modem_fmt_recv: Message: aseq=0xff, command=IPC_NET_REGIST, type=IPC_TYPE_NOTI, size=11

D/RIL-IPC ( 1891): ================================= IPC FMT data =================================

D/RIL-IPC ( 1891): [0000]   04 03 01 01 CC 42 F2 A7  07 00 00                  .....B.. ...

D/RIL-IPC ( 1891): ================================================================================

D/RILJ    ( 2434): [UNSL]< UNSOL_RESPONSE_VOICE_NETWORK_STATE_CHANGED

D/RILJ    ( 2434): [UNSL]< UNSOL_RESPONSE_VOICE_NETWORK_STATE_CHANGED

D/RILJ    ( 2434): [0080]> OPERATOR

D/RILJ    ( 2434): [0081]> DATA_REGISTRATION_STATE

D/RIL     ( 1891): 4 RIL requests in the queue (1 pending, 1 handled, 2 unhandled)

D/RIL     ( 1891): 3 RIL requests data in the queue

D/RIL-IPC ( 1891): 

D/RIL-IPC ( 1891): xmm626_sec_modem_fmt_send: Sent FMT message

D/RIL-IPC ( 1891): xmm626_sec_modem_fmt_send: Message: mseq=0x3c, command=IPC_NET_SERVING_NETWORK, type=IPC_TYPE_GET, size=0

D/RILJ    ( 2434): [0082]> VOICE_REGISTRATION_STATE

D/RILJ    ( 2434): [0083]> QUERY_NETWORK_SELECTION_MODE

D/RIL     ( 1891): 5 RIL requests in the queue (1 pending, 2 handled, 2 unhandled)

D/RIL     ( 1891): 3 RIL requests data in the queue

D/RIL     ( 1891): 4 RIL requests in the queue (0 pending, 2 handled, 2 unhandled)

D/RIL     ( 1891): 2 RIL requests data in the queue

D/RILJ    ( 2434): [0084]> OPERATOR

D/RILJ    ( 2434): [0081]< DATA_REGISTRATION_STATE {0, 42cc, 7a7f2, 9, 3}

D/RIL-IPC ( 1891): 

D/RIL-IPC ( 1891): xmm626_sec_modem_fmt_recv: Received FMT message

D/RIL-IPC ( 1891): xmm626_sec_modem_fmt_recv: Message: aseq=0x3c, command=IPC_NET_SERVING_NETWORK, type=IPC_TYPE_RESP, size=11

D/RIL-IPC ( 1891): ================================= IPC FMT data =================================

D/RIL-IPC ( 1891): [0000]   02 04 04 32 30 36 31 30  23 CC 42                  ...20610 #.B

D/RIL-IPC ( 1891): ================================================================================

D/RIL     ( 1891): 3 RIL requests in the queue (0 pending, 1 handled, 2 unhandled)

D/RIL     ( 1891): 2 RIL requests data in the queue

D/RILJ    ( 2434): [0085]> DATA_REGISTRATION_STATE

D/RILJ    ( 2434): [0080]< OPERATOR {Mobistar, Mobistar, 20610}

D/RILJ    ( 2434): [0086]> VOICE_REGISTRATION_STATE

D/RILJ    ( 2434): [0087]> QUERY_NETWORK_SELECTION_MODE

D/RIL     ( 1891): 4 RIL requests in the queue (1 pending, 1 handled, 2 unhandled)

D/RIL     ( 1891): 2 RIL requests data in the queue

D/RIL     ( 1891): 3 RIL requests in the queue (0 pending, 1 handled, 2 unhandled)

D/RIL     ( 1891): 1 RIL request data in the queue

D/RIL     ( 1891): 4 RIL requests in the queue (1 pending, 1 handled, 2 unhandled)

D/RIL     ( 1891): 1 RIL request data in the queue

D/RIL-IPC ( 1891): 

D/RIL-IPC ( 1891): xmm626_sec_modem_fmt_send: Sent FMT message

D/RIL-IPC ( 1891): xmm626_sec_modem_fmt_send: Message: mseq=0x3d, command=IPC_NET_PLMN_SEL, type=IPC_TYPE_GET, size=0

D/RIL     ( 1891): 5 RIL requests in the queue (1 pending, 2 handled, 2 unhandled)

D/RIL     ( 1891): 1 RIL request data in the queue

D/RIL-IPC ( 1891): 

D/RIL-IPC ( 1891): xmm626_sec_modem_fmt_send: Sent FMT message

D/RIL-IPC ( 1891): xmm626_sec_modem_fmt_send: Message: mseq=0x3e, command=IPC_NET_SERVING_NETWORK, type=IPC_TYPE_GET, size=0

D/RIL     ( 1891): 6 RIL requests in the queue (1 pending, 3 handled, 2 unhandled)

D/RIL     ( 1891): 1 RIL request data in the queue

D/RIL-IPC ( 1891): 

D/RIL-IPC ( 1891): xmm626_sec_modem_fmt_send: Sent FMT message

D/RIL-IPC ( 1891): xmm626_sec_modem_fmt_send: Message: mseq=0x3f, command=IPC_NET_REGIST, type=IPC_TYPE_GET, size=2

D/RIL-IPC ( 1891): ================================= IPC FMT data =================================

D/RIL-IPC ( 1891): [0000]   FF 03                                              ..

D/RIL-IPC ( 1891): ================================================================================

D/RIL     ( 1891): 7 RIL requests in the queue (1 pending, 4 handled, 2 unhandled)

D/RIL     ( 1891): 1 RIL request data in the queue

D/RIL-IPC ( 1891): 

D/RIL-IPC ( 1891): xmm626_sec_modem_fmt_send: Sent FMT message

D/RIL-IPC ( 1891): xmm626_sec_modem_fmt_send: Message: mseq=0x40, command=IPC_NET_REGIST, type=IPC_TYPE_GET, size=2

D/RIL-IPC ( 1891): ================================= IPC FMT data =================================

D/RIL-IPC ( 1891): [0000]   FF 02                                              ..

D/RIL-IPC ( 1891): ================================================================================

D/RILJ    ( 2434): [0082]< VOICE_REGISTRATION_STATE {10, 42cc, 7a7f2, 9, null, null, null, null, null, null, null, null, null, null, null}

D/RIL     ( 1891): 8 RIL requests in the queue (1 pending, 5 handled, 2 unhandled)

D/RIL     ( 1891): 1 RIL request data in the queue

D/RIL-IPC ( 1891): 

D/RIL-IPC ( 1891): xmm626_sec_modem_fmt_recv: Received FMT message

D/RIL-IPC ( 1891): xmm626_sec_modem_fmt_recv: Message: aseq=0x3d, command=IPC_NET_PLMN_SEL, type=IPC_TYPE_RESP, size=1

D/RIL-IPC ( 1891): ================================= IPC FMT data =================================

D/RIL-IPC ( 1891): [0000]   02                                                 .

D/RIL-IPC ( 1891): ================================================================================

D/RIL     ( 1891): 7 RIL requests in the queue (1 pending, 4 handled, 2 unhandled)

D/RIL     ( 1891): 1 RIL request data in the queue

D/RIL-IPC ( 1891): 

D/RIL-IPC ( 1891): xmm626_sec_modem_fmt_send: Sent FMT message

D/RIL-IPC ( 1891): xmm626_sec_modem_fmt_send: Message: mseq=0x41, command=IPC_NET_PLMN_SEL, type=IPC_TYPE_GET, size=0

D/RILJ    ( 2434): [0083]< QUERY_NETWORK_SELECTION_MODE {0}

D/RIL-IPC ( 1891): 

D/RIL-IPC ( 1891): xmm626_sec_modem_fmt_recv: Received FMT message

D/RIL-IPC ( 1891): xmm626_sec_modem_fmt_recv: Message: aseq=0x3e, command=IPC_NET_SERVING_NETWORK, type=IPC_TYPE_RESP, size=11

D/RIL-IPC ( 1891): ================================= IPC FMT data =================================

D/RIL-IPC ( 1891): [0000]   02 04 04 32 30 36 31 30  23 CC 42                  ...20610 #.B

D/RIL-IPC ( 1891): ================================================================================

D/RIL     ( 1891): 6 RIL requests in the queue (0 pending, 4 handled, 2 unhandled)

D/RIL     ( 1891): 1 RIL request data in the queue

D/RILJ    ( 2434): [0084]< OPERATOR {Mobistar, Mobistar, 20610}

D/RIL-IPC ( 1891): 

D/RIL-IPC ( 1891): xmm626_sec_modem_fmt_recv: Received FMT message

D/RIL-IPC ( 1891): xmm626_sec_modem_fmt_recv: Message: aseq=0x3f, command=IPC_NET_REGIST, type=IPC_TYPE_RESP, size=11

D/RIL-IPC ( 1891): ================================= IPC FMT data =================================

D/RIL-IPC ( 1891): [0000]   04 03 01 01 CC 42 F2 A7  07 00 00                  .....B.. ...

D/RIL-IPC ( 1891): ================================================================================

D/RIL     ( 1891): 5 RIL requests in the queue (0 pending, 3 handled, 2 unhandled)

D/RIL     ( 1891): 1 RIL request data in the queue

D/RILJ    ( 2434): [0085]< DATA_REGISTRATION_STATE {0, 42cc, 7a7f2, 9, 3}

D/RIL-IPC ( 1891): 

D/RIL-IPC ( 1891): xmm626_sec_modem_fmt_recv: Received FMT message

D/RIL-IPC ( 1891): xmm626_sec_modem_fmt_recv: Message: aseq=0x40, command=IPC_NET_REGIST, type=IPC_TYPE_RESP, size=11

D/RIL-IPC ( 1891): ================================= IPC FMT data =================================

D/RIL-IPC ( 1891): [0000]   04 02 04 01 CC 42 F2 A7  07 00 00                  .....B.. ...

D/RIL-IPC ( 1891): ================================================================================

D/RIL     ( 1891): 4 RIL requests in the queue (0 pending, 2 handled, 2 unhandled)

D/RIL     ( 1891): 1 RIL request data in the queue

D/RILJ    ( 2434): [0086]< VOICE_REGISTRATION_STATE {10, 42cc, 7a7f2, 9, null, null, null, null, null, null, null, null, null, null, null}

D/RIL-IPC ( 1891): 

D/RIL-IPC ( 1891): xmm626_sec_modem_fmt_recv: Received FMT message

D/RIL-IPC ( 1891): xmm626_sec_modem_fmt_recv: Message: aseq=0x41, command=IPC_NET_PLMN_SEL, type=IPC_TYPE_RESP, size=1

D/RIL-IPC ( 1891): ================================= IPC FMT data =================================

D/RIL-IPC ( 1891): [0000]   02                                                 .

D/RIL-IPC ( 1891): ================================================================================

D/RIL     ( 1891): 3 RIL requests in the queue (0 pending, 1 handled, 2 unhandled)

D/RIL     ( 1891): 1 RIL request data in the queue

D/RILJ    ( 2434): [0087]< QUERY_NETWORK_SELECTION_MODE {0}

D/GSM     ( 2434): [GsmSST] Poll ServiceState done:  oldSS=[1 home Mobistar Mobistar 20610  HSDPA CSS not supported -1 -1 RoamInd=-1 DefRoamInd=-1 EmergOnly=true] newSS=[1 home Mobistar Mobistar 20610  HSDPA CSS not supported -1 -1 RoamInd=-1 DefRoamInd=-1 EmergOnly=true] oldGprs=1 newData=1 oldMaxDataCalls=1 mNewMaxDataCalls=1 oldReasonDataDenied=-1 mNewReasonDataDenied=-1 oldType=HSDPA newType=HSDPA

D/RIL-IPC ( 1891): 

D/RIL-IPC ( 1891): xmm626_sec_modem_fmt_recv: Received FMT message

D/RIL-IPC ( 1891): xmm626_sec_modem_fmt_recv: Message: aseq=0xff, command=IPC_NET_REGIST, type=IPC_TYPE_NOTI, size=11

D/RIL-IPC ( 1891): ================================= IPC FMT data =================================

D/RIL-IPC ( 1891): [0000]   04 02 04 01 CC 42 9C AF  07 00 00                  .....B.. ...

D/RIL-IPC ( 1891): ================================================================================

D/RIL-IPC ( 1891): 

D/RIL-IPC ( 1891): xmm626_sec_modem_fmt_recv: Received FMT message

D/RIL-IPC ( 1891): xmm626_sec_modem_fmt_recv: Message: aseq=0xff, command=IPC_NET_REGIST, type=IPC_TYPE_NOTI, size=11

D/RIL-IPC ( 1891): ================================= IPC FMT data =================================

D/RIL-IPC ( 1891): [0000]   04 03 01 01 CC 42 9C AF  07 00 00                  .....B.. ...

D/RIL-IPC ( 1891): ================================================================================

D/RILJ    ( 2434): [UNSL]< UNSOL_RESPONSE_VOICE_NETWORK_STATE_CHANGED

D/RILJ    ( 2434): [UNSL]< UNSOL_RESPONSE_VOICE_NETWORK_STATE_CHANGED

D/RILJ    ( 2434): [0088]> OPERATOR

D/RILJ    ( 2434): [0089]> DATA_REGISTRATION_STATE

D/RIL     ( 1891): 4 RIL requests in the queue (1 pending, 1 handled, 2 unhandled)

D/RIL     ( 1891): 3 RIL requests data in the queue

D/RIL-IPC ( 1891): 

D/RIL-IPC ( 1891): xmm626_sec_modem_fmt_send: Sent FMT message

D/RIL-IPC ( 1891): xmm626_sec_modem_fmt_send: Message: mseq=0x42, command=IPC_NET_SERVING_NETWORK, type=IPC_TYPE_GET, size=0

D/RILJ    ( 2434): [0090]> VOICE_REGISTRATION_STATE

D/RIL     ( 1891): 5 RIL requests in the queue (1 pending, 2 handled, 2 unhandled)

D/RIL     ( 1891): 3 RIL requests data in the queue

D/RIL     ( 1891): 4 RIL requests in the queue (0 pending, 2 handled, 2 unhandled)

D/RIL     ( 1891): 2 RIL requests data in the queue

D/RILJ    ( 2434): [0089]< DATA_REGISTRATION_STATE {0, 42cc, 7af9c, 9, 3}

D/RILJ    ( 2434): [0091]> QUERY_NETWORK_SELECTION_MODE

D/RIL-IPC ( 1891): 

D/RIL-IPC ( 1891): xmm626_sec_modem_fmt_recv: Received FMT message

D/RIL-IPC ( 1891): xmm626_sec_modem_fmt_recv: Message: aseq=0x42, command=IPC_NET_SERVING_NETWORK, type=IPC_TYPE_RESP, size=11

D/RIL-IPC ( 1891): ================================= IPC FMT data =================================

D/RIL-IPC ( 1891): [0000]   02 04 04 32 30 36 31 30  23 CC 42                  ...20610 #.B

D/RIL-IPC ( 1891): ================================================================================

D/RIL     ( 1891): 3 RIL requests in the queue (0 pending, 1 handled, 2 unhandled)

D/RIL     ( 1891): 2 RIL requests data in the queue

D/RILJ    ( 2434): [0092]> OPERATOR

D/RILJ    ( 2434): [0088]< OPERATOR {Mobistar, Mobistar, 20610}

D/RIL     ( 1891): 4 RIL requests in the queue (1 pending, 1 handled, 2 unhandled)

D/RIL     ( 1891): 2 RIL requests data in the queue

D/RIL     ( 1891): 3 RIL requests in the queue (0 pending, 1 handled, 2 unhandled)

D/RIL     ( 1891): 1 RIL request data in the queue

D/RILJ    ( 2434): [0093]> DATA_REGISTRATION_STATE

D/RIL     ( 1891): 4 RIL requests in the queue (1 pending, 1 handled, 2 unhandled)

D/RIL     ( 1891): 1 RIL request data in the queue

D/RIL-IPC ( 1891): 

D/RIL-IPC ( 1891): xmm626_sec_modem_fmt_send: Sent FMT message

D/RIL-IPC ( 1891): xmm626_sec_modem_fmt_send: Message: mseq=0x43, command=IPC_NET_PLMN_SEL, type=IPC_TYPE_GET, size=0

D/RILJ    ( 2434): [0090]< VOICE_REGISTRATION_STATE {10, 42cc, 7af9c, 9, null, null, null, null, null, null, null, null, null, null, null}

D/RILJ    ( 2434): [0094]> VOICE_REGISTRATION_STATE

D/RIL     ( 1891): 5 RIL requests in the queue (1 pending, 2 handled, 2 unhandled)

D/RIL     ( 1891): 1 RIL request data in the queue

D/RIL-IPC ( 1891): 

D/RIL-IPC ( 1891): xmm626_sec_modem_fmt_send: Sent FMT message

D/RIL-IPC ( 1891): xmm626_sec_modem_fmt_send: Message: mseq=0x44, command=IPC_NET_SERVING_NETWORK, type=IPC_TYPE_GET, size=0

D/RILJ    ( 2434): [0095]> QUERY_NETWORK_SELECTION_MODE

D/RIL-IPC ( 1891): 

D/RIL-IPC ( 1891): xmm626_sec_modem_fmt_recv: Received FMT message

D/RIL-IPC ( 1891): xmm626_sec_modem_fmt_recv: Message: aseq=0x43, command=IPC_NET_PLMN_SEL, type=IPC_TYPE_RESP, size=1

D/RIL-IPC ( 1891): ================================= IPC FMT data =================================

D/RIL-IPC ( 1891): [0000]   02                                                 .

D/RIL-IPC ( 1891): ================================================================================

D/RIL     ( 1891): 4 RIL requests in the queue (0 pending, 2 handled, 2 unhandled)

D/RIL     ( 1891): 1 RIL request data in the queue

D/RIL     ( 1891): 5 RIL requests in the queue (1 pending, 2 handled, 2 unhandled)

D/RIL     ( 1891): 1 RIL request data in the queue

D/RILJ    ( 2434): [0091]< QUERY_NETWORK_SELECTION_MODE {0}

D/RIL-IPC ( 1891): 

D/RIL-IPC ( 1891): xmm626_sec_modem_fmt_send: Sent FMT message

D/RIL-IPC ( 1891): xmm626_sec_modem_fmt_send: Message: mseq=0x45, command=IPC_NET_REGIST, type=IPC_TYPE_GET, size=2

D/RIL-IPC ( 1891): ================================= IPC FMT data =================================

D/RIL-IPC ( 1891): [0000]   FF 03                                              ..

D/RIL-IPC ( 1891): ================================================================================

D/RIL     ( 1891): 6 RIL requests in the queue (1 pending, 3 handled, 2 unhandled)

D/RIL     ( 1891): 1 RIL request data in the queue

D/RIL-IPC ( 1891): 

D/RIL-IPC ( 1891): xmm626_sec_modem_fmt_send: Sent FMT message

D/RIL-IPC ( 1891): xmm626_sec_modem_fmt_send: Message: mseq=0x46, command=IPC_NET_REGIST, type=IPC_TYPE_GET, size=2

D/RIL-IPC ( 1891): ================================= IPC FMT data =================================

D/RIL-IPC ( 1891): [0000]   FF 02                                              ..

D/RIL-IPC ( 1891): ================================================================================

D/RIL-IPC ( 1891): 

D/RIL-IPC ( 1891): xmm626_sec_modem_fmt_recv: Received FMT message

D/RIL-IPC ( 1891): xmm626_sec_modem_fmt_recv: Message: aseq=0x44, command=IPC_NET_SERVING_NETWORK, type=IPC_TYPE_RESP, size=11

D/RIL-IPC ( 1891): ================================= IPC FMT data =================================

D/RIL-IPC ( 1891): [0000]   02 04 04 32 30 36 31 30  23 CC 42                  ...20610 #.B

D/RIL-IPC ( 1891): ================================================================================

D/RIL     ( 1891): 5 RIL requests in the queue (0 pending, 3 handled, 2 unhandled)

D/RIL     ( 1891): 1 RIL request data in the queue

D/RIL     ( 1891): 6 RIL requests in the queue (1 pending, 3 handled, 2 unhandled)

D/RIL     ( 1891): 1 RIL request data in the queue

D/RIL-IPC ( 1891): 

D/RIL-IPC ( 1891): xmm626_sec_modem_fmt_send: Sent FMT message

D/RIL-IPC ( 1891): xmm626_sec_modem_fmt_send: Message: mseq=0x47, command=IPC_NET_PLMN_SEL, type=IPC_TYPE_GET, size=0

D/RILJ    ( 2434): [0092]< OPERATOR {Mobistar, Mobistar, 20610}

D/RIL-IPC ( 1891): 

D/RIL-IPC ( 1891): xmm626_sec_modem_fmt_recv: Received FMT message

D/RIL-IPC ( 1891): xmm626_sec_modem_fmt_recv: Message: aseq=0x45, command=IPC_NET_REGIST, type=IPC_TYPE_RESP, size=11

D/RIL-IPC ( 1891): ================================= IPC FMT data =================================

D/RIL-IPC ( 1891): [0000]   04 03 01 01 CC 42 9C AF  07 00 00                  .....B.. ...

D/RIL-IPC ( 1891): ================================================================================

D/RIL     ( 1891): 5 RIL requests in the queue (0 pending, 3 handled, 2 unhandled)

D/RIL     ( 1891): 1 RIL request data in the queue

D/RILJ    ( 2434): [0093]< DATA_REGISTRATION_STATE {0, 42cc, 7af9c, 9, 3}

D/RIL-IPC ( 1891): 

D/RIL-IPC ( 1891): xmm626_sec_modem_fmt_recv: Received FMT message

D/RIL-IPC ( 1891): xmm626_sec_modem_fmt_recv: Message: aseq=0x46, command=IPC_NET_REGIST, type=IPC_TYPE_RESP, size=11

D/RIL-IPC ( 1891): ================================= IPC FMT data =================================

D/RIL-IPC ( 1891): [0000]   04 02 04 01 CC 42 9C AF  07 00 00                  .....B.. ...

D/RIL-IPC ( 1891): ================================================================================

D/RIL     ( 1891): 4 RIL requests in the queue (0 pending, 2 handled, 2 unhandled)

D/RIL     ( 1891): 1 RIL request data in the queue

D/RILJ    ( 2434): [0094]< VOICE_REGISTRATION_STATE {10, 42cc, 7af9c, 9, null, null, null, null, null, null, null, null, null, null, null}

D/RIL-IPC ( 1891): 

D/RIL-IPC ( 1891): xmm626_sec_modem_fmt_recv: Received FMT message

D/RIL-IPC ( 1891): xmm626_sec_modem_fmt_recv: Message: aseq=0x47, command=IPC_NET_PLMN_SEL, type=IPC_TYPE_RESP, size=1

D/RIL-IPC ( 1891): ================================= IPC FMT data =================================

D/RIL-IPC ( 1891): [0000]   02                                                 .

D/RIL-IPC ( 1891): ================================================================================

D/RIL     ( 1891): 3 RIL requests in the queue (0 pending, 1 handled, 2 unhandled)

D/RIL     ( 1891): 1 RIL request data in the queue

D/RILJ    ( 2434): [0095]< QUERY_NETWORK_SELECTION_MODE {0}

D/GSM     ( 2434): [GsmSST] Poll ServiceState done:  oldSS=[1 home Mobistar Mobistar 20610  HSDPA CSS not supported -1 -1 RoamInd=-1 DefRoamInd=-1 EmergOnly=true] newSS=[1 home Mobistar Mobistar 20610  HSDPA CSS not supported -1 -1 RoamInd=-1 DefRoamInd=-1 EmergOnly=true] oldGprs=1 newData=1 oldMaxDataCalls=1 mNewMaxDataCalls=1 oldReasonDataDenied=-1 mNewReasonDataDenied=-1 oldType=HSDPA newType=HSDPA

D/RIL-IPC ( 1891): 

D/RIL-IPC ( 1891): xmm626_sec_modem_fmt_recv: Received FMT message

D/RIL-IPC ( 1891): xmm626_sec_modem_fmt_recv: Message: aseq=0x47, command=IPC_DISP_RSSI_INFO, type=IPC_TYPE_NOTI, size=1

D/RIL-IPC ( 1891): ================================= IPC FMT data =================================

D/RIL-IPC ( 1891): [0000]   54                                                 T

D/RIL-IPC ( 1891): ================================================================================

D/RIL     ( 1891): Signal strength is 14

