06-01 10:53:31.085  1964  1964 D RILD    : **RIL Daemon Started**

06-01 10:53:31.085  1964  1964 D RILD    : **RILd param count=1**

06-01 10:53:31.120  1964  1964 W RILD    : RIL_SAP_Init not defined or exported in /system/lib/libsamsung-ril.so: undefined symbol: RIL_SAP_Init

06-01 10:53:31.120  1964  1964 D RILD    : RIL_Init argc = 5 clientId = 0

06-01 10:53:31.120  1964  1964 D use-Rlog/RLOG-RIL: Created IPC FMT client

06-01 10:53:31.120  1964  1964 D use-Rlog/RLOG-RIL: Created IPC RFS client

06-01 10:53:31.120  1964  1964 D use-Rlog/RLOG-RIL: Created SRS client

06-01 10:53:31.120  1964  1964 D use-Rlog/RLOG-RIL-IPC: Starting i9300 modem boot

06-01 10:53:31.120  1964  1964 D use-Rlog/RLOG-RIL-IPC: Opened modem image device

06-01 10:53:31.120  1964  1964 D use-Rlog/RLOG-RIL-IPC: Mapped modem image data to memory

06-01 10:53:31.120  1964  1964 D use-Rlog/RLOG-RIL-IPC: Opened modem boot device

06-01 10:53:31.120  1964  1964 D use-Rlog/RLOG-RIL-IPC: Opened modem link device

06-01 10:53:31.340  1964  1964 D use-Rlog/RLOG-RIL-IPC: Turned the modem off

06-01 10:53:31.875  1964  1964 D use-Rlog/RLOG-RIL-IPC: Turned the modem on

06-01 10:53:32.175  1964  1964 D use-Rlog/RLOG-RIL-IPC: Waited for link connected

06-01 10:53:32.175  1964  1964 D use-Rlog/RLOG-RIL-IPC: Wrote ATAT in ASCII

06-01 10:53:32.175  1964  1964 D use-Rlog/RLOG-RIL-IPC: Read chip id (0x16)

06-01 10:53:32.175  1964  1964 D use-Rlog/RLOG-RIL-IPC: Wrote PSI header

06-01 10:53:32.185  1964  1964 D use-Rlog/RLOG-RIL-IPC: Wrote PSI, CRC is 0xc8

06-01 10:53:32.185  1964  1964 D use-Rlog/RLOG-RIL-IPC: Wrote PSI CRC (0xc8)

06-01 10:53:32.215  1964  1964 D use-Rlog/RLOG-RIL-IPC: Read PSI CRC ACK

06-01 10:53:32.230  1964  1964 D use-Rlog/RLOG-RIL-IPC: Read PSI ACK

06-01 10:53:32.230  1964  1964 D use-Rlog/RLOG-RIL-IPC: Sent XMM626 HSIC PSI

06-01 10:53:32.230  1964  1964 D use-Rlog/RLOG-RIL-IPC: Wrote EBL size

06-01 10:53:32.230  1964  1964 D use-Rlog/RLOG-RIL-IPC: Wrote EBL, CRC is 0xb5

06-01 10:53:32.230  1964  1964 D use-Rlog/RLOG-RIL-IPC: Wrote EBL CRC (0xb5)

06-01 10:53:32.265  1964  1964 D use-Rlog/RLOG-RIL-IPC: Sent XMM626 HSIC EBL

06-01 10:53:32.290  1964  1964 D use-Rlog/RLOG-RIL-IPC: Read port config

06-01 10:53:32.290  1964  1964 D use-Rlog/RLOG-RIL-IPC: Sent XMM626 HSIC port config

06-01 10:53:32.300  1964  1964 D use-Rlog/RLOG-RIL-IPC: Sent XMM626 HSIC SEC start

06-01 10:53:32.660  1964  1964 D use-Rlog/RLOG-RIL-IPC: Sent XMM626 HSIC firmware

06-01 10:53:32.660  1964  1964 D use-Rlog/RLOG-RIL-IPC: Checked nv_data path

06-01 10:53:32.660  1964  1964 D use-Rlog/RLOG-RIL-IPC: Checked nv_data md5 path

06-01 10:53:32.790  1964  1964 D use-Rlog/RLOG-RIL-IPC: Calculated nv_data md5: 1455f7aaa8936eda837ebc27acf1c818

06-01 10:53:32.805  1964  1964 D use-Rlog/RLOG-RIL-IPC: Read nv_data md5: 1455f7aaa8936eda837ebc27acf1c818

06-01 10:53:32.805  1964  1964 D use-Rlog/RLOG-RIL-IPC: Checked nv_data backup path

06-01 10:53:32.815  1964  1964 D use-Rlog/RLOG-RIL-IPC: Loaded nv_data

06-01 10:53:33.055  1964  1964 D use-Rlog/RLOG-RIL-IPC: Sent XMM626 HSIC nv_data

06-01 10:53:33.170  1964  1964 D use-Rlog/RLOG-RIL-IPC: Sent XMM626 HSIC SEC end

06-01 10:53:33.170  1964  1964 D use-Rlog/RLOG-RIL-IPC: Sent XMM626 HSIC HW reset

06-01 10:53:33.970  1964  1964 D use-Rlog/RLOG-RIL-IPC: Waiting for host wake failed

06-01 10:53:34.280  1964  1964 D use-Rlog/RLOG-RIL-IPC: Waited for host wake

06-01 10:53:34.855  1964  1964 D use-Rlog/RLOG-RIL-IPC: Waited for link connected

06-01 10:53:34.865  1973  1973 D TelephonyManager: /proc/cmdline=console=ttySAC2,115200 consoleblank=0 androidboot.hardware=smdk4x12 console=ram loglevel=4 sec_debug.level=0 sec_watchdog.sec_pet=5 androidboot.debug_level=0x4f4c sec_log=0x100000@0x46000000 s3cfb.bootloaderfb=0x5ec00000 lcdtype=96 consoleblank=0 lpcharge=0 lpj=3981312 vmalloc=144m oops=panic pmic_info=65 cordon=7f16732d3788dbb1c8b4f4cdfd6c69c8 connie=GT-I9300_OPEN_EUR_217c7ff488db6c3308ffbf55e9f5d7e6 androidboot.emmc_checksum=3 androidboot.odin_download=1 androidboot.bootloader=I9300XXUGNJ2 androidboot.serialno=4df1402f279c6f81 snd_soc_core.pmdown_time=1000

06-01 10:53:35.185  1964  1964 D use-Rlog/RLOG-RIL: Opened IPC FMT client

06-01 10:53:35.185  1964  1964 D use-Rlog/RLOG-RIL: Started IPC FMT client loop

06-01 10:53:35.190  1964  1964 D use-Rlog/RLOG-RIL: Opened IPC RFS client

06-01 10:53:35.190  1964  1964 D use-Rlog/RLOG-RIL: Started IPC RFS client loop

06-01 10:53:35.190  1964  1964 D use-Rlog/RLOG-RIL-SRS: Started SRS server loop

06-01 10:53:35.190  1964  1964 D use-Rlog/RLOG-RIL: Opened SRS client

06-01 10:53:35.190  1964  1964 D use-Rlog/RLOG-RIL: Started SRS client loop

06-01 10:53:35.190  1964  1964 D RILD    : RIL_Init rilInit completed

06-01 10:53:35.190  1964  1964 I RILC    : SIM_COUNT: 1

06-01 10:53:35.190  1964  1964 E RILC    : RIL_register: RIL version 11

06-01 10:53:35.190  1964  1964 I RILC    : s_registerCalled flag set, 1

06-01 10:53:35.190  1964  1964 I RILC    : Start to listen RIL_SOCKET_1

06-01 10:53:35.190  1964  2328 D use-Rlog/RLOG-RIL-IPC: 

06-01 10:53:35.190  1964  2328 D use-Rlog/RLOG-RIL-IPC: xmm626_sec_modem_fmt_recv: Received FMT message

06-01 10:53:35.190  1964  2328 D use-Rlog/RLOG-RIL-IPC: xmm626_sec_modem_fmt_recv: Message: aseq=0xff, command=IPC_PWR_PHONE_PWR_UP, type=IPC_TYPE_NOTI, size=0

06-01 10:53:35.190  1964  1964 D RILD    : RIL_Init RIL_register completed

06-01 10:53:35.190  1964  1964 D RILD    : RIL_register_socket completed

06-01 10:53:35.190  1964  1964 D RILD    : RIL_Init starting sleep loop

06-01 10:53:35.190  1964  2328 D use-Rlog/RLOG-RIL: Updating RIL radio state to 0

06-01 10:53:35.195  1964  2328 D use-Rlog/RLOG-RIL-IPC: 

06-01 10:53:35.195  1964  2328 D use-Rlog/RLOG-RIL-IPC: xmm626_sec_modem_fmt_recv: Received FMT message

06-01 10:53:35.195  1964  2328 D use-Rlog/RLOG-RIL-IPC: xmm626_sec_modem_fmt_recv: Message: aseq=0x00, command=IPC_MISC_ME_IMSI, type=IPC_TYPE_NOTI, size=16

06-01 10:53:35.195  1964  2328 D use-Rlog/RLOG-RIL-IPC: ================================= IPC FMT data =================================

06-01 10:53:35.195  1964  2328 D use-Rlog/RLOG-RIL-IPC: [0000]   0F 30 30 30 30 30 30 30  30 30 30 30 30 30 30 30   .0000000 00000000

06-01 10:53:35.195  1964  2328 D use-Rlog/RLOG-RIL-IPC: ================================================================================

06-01 10:53:35.195  1964  2328 D use-Rlog/RLOG-RIL-IPC: 

06-01 10:53:35.195  1964  2328 D use-Rlog/RLOG-RIL-IPC: xmm626_sec_modem_fmt_recv: Received FMT message

06-01 10:53:35.195  1964  2328 D use-Rlog/RLOG-RIL-IPC: xmm626_sec_modem_fmt_recv: Message: aseq=0xff, command=IPC_NET_REGIST, type=IPC_TYPE_NOTI, size=11

06-01 10:53:35.195  1964  2328 D use-Rlog/RLOG-RIL-IPC: ================================= IPC FMT data =================================

06-01 10:53:35.195  1964  2328 D use-Rlog/RLOG-RIL-IPC: [0000]   FF 02 01 00 00 00 00 00  00 00 00                  ........ ...

06-01 10:53:35.195  1964  2328 D use-Rlog/RLOG-RIL-IPC: ================================================================================

06-01 10:53:35.195  1964  2328 D use-Rlog/RLOG-RIL-IPC: 

06-01 10:53:35.195  1964  2328 D use-Rlog/RLOG-RIL-IPC: xmm626_sec_modem_fmt_recv: Received FMT message

06-01 10:53:35.195  1964  2328 D use-Rlog/RLOG-RIL-IPC: xmm626_sec_modem_fmt_recv: Message: aseq=0xff, command=IPC_NET_REGIST, type=IPC_TYPE_NOTI, size=11

06-01 10:53:35.195  1964  2328 D use-Rlog/RLOG-RIL-IPC: ================================= IPC FMT data =================================

06-01 10:53:35.195  1964  2328 D use-Rlog/RLOG-RIL-IPC: [0000]   FF 03 01 00 00 00 00 00  00 00 00                  ........ ...

06-01 10:53:35.195  1964  2328 D use-Rlog/RLOG-RIL-IPC: ================================================================================

06-01 10:53:35.195  1964  2328 D use-Rlog/RLOG-RIL-IPC: 

06-01 10:53:35.195  1964  2328 D use-Rlog/RLOG-RIL-IPC: xmm626_sec_modem_fmt_recv: Received FMT message

06-01 10:53:35.195  1964  2328 D use-Rlog/RLOG-RIL-IPC: xmm626_sec_modem_fmt_recv: Message: aseq=0x00, command=IPC_DISP_ICON_INFO, type=IPC_TYPE_NOTI, size=4

06-01 10:53:35.195  1964  2328 D use-Rlog/RLOG-RIL-IPC: ================================= IPC FMT data =================================

06-01 10:53:35.195  1964  2328 D use-Rlog/RLOG-RIL-IPC: [0000]   FF 00 00 00                                        ....

06-01 10:53:35.195  1964  2328 D use-Rlog/RLOG-RIL-IPC: ================================================================================

06-01 10:53:41.250  1964  2328 D use-Rlog/RLOG-RIL-IPC: 

06-01 10:53:41.250  1964  2328 D use-Rlog/RLOG-RIL-IPC: xmm626_sec_modem_fmt_recv: Received FMT message

06-01 10:53:41.250  1964  2328 D use-Rlog/RLOG-RIL-IPC: xmm626_sec_modem_fmt_recv: Message: aseq=0xff, command=IPC_SEC_SIM_ICC_TYPE, type=IPC_TYPE_NOTI, size=1

06-01 10:53:41.250  1964  2328 D use-Rlog/RLOG-RIL-IPC: ================================= IPC FMT data =================================

06-01 10:53:41.250  1964  2328 D use-Rlog/RLOG-RIL-IPC: [0000]   02                                                 .

06-01 10:53:41.250  1964  2328 D use-Rlog/RLOG-RIL-IPC: ================================================================================

06-01 10:53:41.250  1964  2328 D use-Rlog/RLOG-RIL-IPC: 

06-01 10:53:41.250  1964  2328 D use-Rlog/RLOG-RIL-IPC: xmm626_sec_modem_fmt_recv: Received FMT message

06-01 10:53:41.250  1964  2328 D use-Rlog/RLOG-RIL-IPC: xmm626_sec_modem_fmt_recv: Message: aseq=0xff, command=IPC_SEC_PIN_STATUS, type=IPC_TYPE_NOTI, size=2

06-01 10:53:41.250  1964  2328 D use-Rlog/RLOG-RIL-IPC: ================================= IPC FMT data =================================

06-01 10:53:41.250  1964  2328 D use-Rlog/RLOG-RIL-IPC: [0000]   03 01                                              ..

06-01 10:53:41.250  1964  2328 D use-Rlog/RLOG-RIL-IPC: ================================================================================

06-01 10:53:41.250  1964  2328 D use-Rlog/RLOG-RIL-IPC: 

06-01 10:53:41.250  1964  2328 D use-Rlog/RLOG-RIL-IPC: xmm626_sec_modem_fmt_recv: Received FMT message

06-01 10:53:41.250  1964  2328 D use-Rlog/RLOG-RIL-IPC: xmm626_sec_modem_fmt_recv: Message: aseq=0xff, command=IPC_SAT_PROACTIVE_CMD, type=IPC_TYPE_INDI, size=13

06-01 10:53:41.250  1964  2328 D use-Rlog/RLOG-RIL-IPC: ================================= IPC FMT data =================================

06-01 10:53:41.250  1964  2328 D use-Rlog/RLOG-RIL-IPC: [0000]   0B 00 D0 09 81 03 01 02  00 82 02 81 82            ........ .....

06-01 10:53:41.250  1964  2328 D use-Rlog/RLOG-RIL-IPC: ================================================================================

06-01 10:53:41.250  1964  2328 D use-Rlog/RLOG-RIL-IPC: Unhandled IPC FMT message: IPC_SAT_PROACTIVE_CMD

06-01 10:53:48.550  2335  2347 D TelephonyRegistry: listen oscl: hasNotifySubscriptionInfoChangedOccurred==false no callback

06-01 10:53:50.035  2335  2335 D TelephonyRegistry: systemRunning register for intents

06-01 10:53:50.785  2812  2812 D TelephonyPluginDelegate: Extension = @/system/framework/

06-01 10:53:50.785  2812  2812 D TelephonyPluginDelegate: classLoader = dalvik.system.PathClassLoader[DexPathList[[directory "/system/framework"],nativeLibraryDirectories=[/vendor/lib, /system/lib]]]

06-01 10:53:50.785  2812  2812 D TelephonyPluginDelegate: No customized TelephonyPlugin available, fallback to default

06-01 10:53:50.790  2812  2812 D TelephonyPluginDelegate: cls = class com.android.internal.telephony.DefaultTelephonyPlugin

06-01 10:53:50.790  2812  2812 D TelephonyPluginDelegate: constructor method = public com.android.internal.telephony.DefaultTelephonyPlugin()

06-01 10:53:50.795  2812  2812 D TDC     : updateOrInsert: inserting: Modem { uuid=modem, state=0, rilModel=0, rat={}, maxActiveVoiceCall=1, maxActiveDataCall=1, maxStandby=1 }

06-01 10:53:50.795  2812  2812 D TDC     : updateOrInsert: inserting: Sim { uuid=sim, modemUuid=modem, state=0 }

06-01 10:53:50.800  2812  2812 D TelephonyManager: getLteOnCdmaMode=0 curVal=-1 product_type='' lteOnCdmaProductType=''

06-01 10:53:50.815  2812  2812 D CdmaSSM : subscriptionSource from settings: 0

06-01 10:53:50.815  2812  2812 I PhoneFactory: Cdma Subscription set to 0

06-01 10:53:50.835  2812  2812 I PhoneFactory: RILClassname is RIL

06-01 10:53:50.835  2812  2812 I PhoneFactory: Network Mode set to 0

06-01 10:53:50.840  2812  2812 D RILJ    : RIL(context, preferredNetworkType=0 cdmaSubscription=0)

06-01 10:53:50.850  2812  2812 D RILJ    : Starting RILReceiver0 [SUB0]

06-01 10:53:50.850  2812  2812 D RILJ    : [3648]> GET_HARDWARE_CONFIG [SUB0]

06-01 10:53:50.855  2812  2812 D RilRequest: [3648]< GET_HARDWARE_CONFIG error: com.android.internal.telephony.CommandException: RADIO_NOT_AVAILABLE ret=

06-01 10:53:50.855  2812  2812 I PhoneFactory: Creating SubscriptionController

06-01 10:53:50.855  2812  2812 D SubscriptionController: [SubscriptionController] init by Context

06-01 10:53:50.860  2812  2812 D UiccController: Creating UiccController

06-01 10:53:50.860  2812  2918 I RILJ    : (0) Connected to 'rild' socket

06-01 10:53:50.865  1964  2012 I RILC    : libril: new connection to RIL_SOCKET_1

06-01 10:53:50.865  1964  2012 I RILC    : RIL Daemon version: Samsung-RIL

06-01 10:53:50.865  2812  2918 D RILJ    : [UNSL]< UNSOL_RIL_CONNECTED {11} [SUB0]

06-01 10:53:50.870  2812  2918 D RILJ    : [3649]> RADIO_POWER off [SUB0]

06-01 10:53:50.870  2812  2918 D RILJ    : [3650]> RIL_REQUEST_CDMA_SET_SUBSCRIPTION_SOURCE : 0 [SUB0]

06-01 10:53:50.870  1964  2012 D use-Rlog/RLOG-RIL: 1 RIL request in the queue (1 pending, 0 handled, 0 unhandled)

06-01 10:53:50.870  1964  2332 D use-Rlog/RLOG-RIL: Requesting low power mode power state

06-01 10:53:50.870  1964  2332 D use-Rlog/RLOG-RIL-IPC: 

06-01 10:53:50.870  1964  2332 D use-Rlog/RLOG-RIL-IPC: xmm626_sec_modem_fmt_send: Sent FMT message

06-01 10:53:50.870  1964  2332 D use-Rlog/RLOG-RIL-IPC: xmm626_sec_modem_fmt_send: Message: mseq=0x01, command=IPC_PWR_PHONE_STATE, type=IPC_TYPE_EXEC, size=2

06-01 10:53:50.870  1964  2332 D use-Rlog/RLOG-RIL-IPC: ================================= IPC FMT data =================================

06-01 10:53:50.870  1964  2332 D use-Rlog/RLOG-RIL-IPC: [0000]   01 00                                              ..

06-01 10:53:50.870  1964  2332 D use-Rlog/RLOG-RIL-IPC: ================================================================================

06-01 10:53:50.870  2812  2918 D RILJ    : setCellInfoListRate: 2147483647 [SUB0]

06-01 10:53:50.870  2812  2918 D RILJ    : [3651]> RIL_REQUEST_SET_CELL_INFO_LIST_RATE [SUB0]

06-01 10:53:50.870  1964  2012 D use-Rlog/RLOG-RIL: 2 RIL requests in the queue (1 pending, 1 handled, 0 unhandled)

06-01 10:53:50.870  1964  2332 D use-Rlog/RLOG-RIL: Unhandled RIL request: 77

06-01 10:53:50.870  1964  2332 D use-Rlog/RLOG-RIL: 1 RIL request in the queue (0 pending, 1 handled, 0 unhandled)

06-01 10:53:50.870  2812  2918 D RILJ    : [UNSL]< UNSOL_RESPONSE_RADIO_STATE_CHANGED RADIO_OFF [SUB0]

06-01 10:53:50.870  2812  2918 D RILJ    : [3652]> SCREEN_STATE: true [SUB0]

06-01 10:53:50.870  1964  2012 D use-Rlog/RLOG-RIL: 2 RIL requests in the queue (1 pending, 1 handled, 0 unhandled)

06-01 10:53:50.870  1964  2332 D use-Rlog/RLOG-RIL: Unhandled RIL request: 110

06-01 10:53:50.870  1964  2332 D use-Rlog/RLOG-RIL: 1 RIL request in the queue (0 pending, 1 handled, 0 unhandled)

06-01 10:53:50.885  2812  2918 D RilRequest: [3650]< RIL_REQUEST_CDMA_SET_SUBSCRIPTION_SOURCE error: com.android.internal.telephony.CommandException: REQUEST_NOT_SUPPORTED ret=

06-01 10:53:50.885  2812  2918 D RilRequest: [3651]< RIL_REQUEST_SET_CELL_INFO_LIST_RATE error: com.android.internal.telephony.CommandException: REQUEST_NOT_SUPPORTED ret=

06-01 10:53:50.885  1964  2012 D use-Rlog/RLOG-RIL: 2 RIL requests in the queue (1 pending, 1 handled, 0 unhandled)

06-01 10:53:50.890  2812  2812 D TelephonyTester: register for intent action=com.android.internal.telephony.gsm.action_detached

06-01 10:53:50.890  2812  2812 D TelephonyTester: register for intent action=com.android.internal.telephony.gsm.action_attached

06-01 10:53:50.935  2812  2812 D PhoneBase: mDoesRilSendMultipleCallRing=false

06-01 10:53:50.935  2812  2812 D PhoneBase: mCallRingDelay=3000

06-01 10:53:50.960  2812  2812 D RILJ    : [3653]> RIL_REQUEST_START_LCE [SUB0]

06-01 10:53:50.960  2812  2812 D PhoneBase: mOosIsDisconnect=true

06-01 10:53:50.960  2812  2812 D RILJ    : setPhoneType=1 old value=0 [SUB0]

06-01 10:53:50.970  1964  2012 D use-Rlog/RLOG-RIL: 3 RIL requests in the queue (1 pending, 1 handled, 1 unhandled)

06-01 10:53:50.970  1964  2332 D use-Rlog/RLOG-RIL: Unhandled RIL request: 132

06-01 10:53:50.970  1964  2332 D use-Rlog/RLOG-RIL: 2 RIL requests in the queue (0 pending, 1 handled, 1 unhandled)

06-01 10:53:50.970  2812  2918 D RilRequest: [3653]< RIL_REQUEST_START_LCE error: com.android.internal.telephony.CommandException: REQUEST_NOT_SUPPORTED ret=

06-01 10:53:50.970  1964  2328 D use-Rlog/RLOG-RIL-IPC: 

06-01 10:53:50.970  1964  2328 D use-Rlog/RLOG-RIL-IPC: xmm626_sec_modem_fmt_recv: Received FMT message

06-01 10:53:50.970  1964  2328 D use-Rlog/RLOG-RIL-IPC: xmm626_sec_modem_fmt_recv: Message: aseq=0x01, command=IPC_GEN_PHONE_RES, type=IPC_TYPE_RESP, size=5

06-01 10:53:50.970  1964  2328 D use-Rlog/RLOG-RIL-IPC: ================================= IPC FMT data =================================

06-01 10:53:50.970  1964  2328 D use-Rlog/RLOG-RIL-IPC: [0000]   01 07 01 00 80                                     .....

06-01 10:53:50.970  1964  2328 D use-Rlog/RLOG-RIL-IPC: ================================================================================

06-01 10:53:50.970  1964  2328 D use-Rlog/RLOG-RIL: Generic response was expected

06-01 10:53:50.970  1964  2328 D use-Rlog/RLOG-RIL-IPC: 

06-01 10:53:50.970  1964  2328 D use-Rlog/RLOG-RIL-IPC: xmm626_sec_modem_fmt_recv: Received FMT message

06-01 10:53:50.970  1964  2328 D use-Rlog/RLOG-RIL-IPC: xmm626_sec_modem_fmt_recv: Message: aseq=0x01, command=IPC_PWR_PHONE_STATE, type=IPC_TYPE_NOTI, size=1

06-01 10:53:50.970  1964  2328 D use-Rlog/RLOG-RIL-IPC: ================================= IPC FMT data =================================

06-01 10:53:50.970  1964  2328 D use-Rlog/RLOG-RIL-IPC: [0000]   01                                                 .

06-01 10:53:50.970  1964  2328 D use-Rlog/RLOG-RIL-IPC: ================================================================================

06-01 10:53:50.970  1964  2328 D use-Rlog/RLOG-RIL: Power state is low power mode

06-01 10:53:50.970  1964  2328 D use-Rlog/RLOG-RIL: 1 RIL request in the queue (0 pending, 0 handled, 1 unhandled)

06-01 10:53:50.970  2812  2918 D RILJ    : [3649]< RADIO_POWER  [SUB0]

06-01 10:53:50.995  2335  2807 D TelephonyRegistry: listen oscl: hasNotifySubscriptionInfoChangedOccurred==false no callback

06-01 10:53:50.995  2812  2812 D TelephonyManager: setTelephonyProperty: success phoneId=0 property=gsm.network.type value: Unknown propVal=Unknown

06-01 10:53:51.010  2812  2812 D RILJ    : [3654]> SIGNAL_STRENGTH [SUB0]

06-01 10:53:51.020  1964  2012 D use-Rlog/RLOG-RIL: 2 RIL requests in the queue (1 pending, 0 handled, 1 unhandled)

06-01 10:53:51.040  2812  2812 D         : [0]DCT.constructor

06-01 10:53:51.040  2812  2812 D SubscriptionController: [getSubId]- sSlotIdxToSubId.size == 0, return DummySubIds slotIdx=0

06-01 10:53:51.045  2812  2812 D         : [0]getDataEnabled: getIntWithSubId retVal=true

06-01 10:53:51.045  2335  2515 D TelephonyRegistry: listen oscl: hasNotifySubscriptionInfoChangedOccurred==false no callback

06-01 10:53:51.050  2812  2812 D Dcc     : E ctor

06-01 10:53:51.050  2812  2812 D Dcc     : X ctor

06-01 10:53:51.065  2812  2812 D SubscriptionController: [getPhoneId] asked for default subId=-1

06-01 10:53:51.065  2812  2812 D SubscriptionController: [getPhoneId]- invalid subId return=-1

06-01 10:53:51.070  2812  2950 D DcTesterDeacativeAll: register for intent action=com.android.internal.telephony.dataconnection.action_deactivate_all

06-01 10:53:51.070  2812  2950 D DcTesterDeacativeAll: register for intent action=com.android.internal.telephony.gsm.action_detached

06-01 10:53:51.070  2812  2812 D DcTesterFailBrinupAll: register for intent action=com.android.internal.telephony.dataconnection.action_fail_bringup

06-01 10:53:51.070  2812  2812 D DcTesterFailBrinupAll: register for intent action=com.android.internal.telephony.gsm.action_detached

06-01 10:53:51.070  2812  2812 D DcTesterFailBrinupAll: register for intent action=com.android.internal.telephony.gsm.action_attached

06-01 10:53:51.070  2812  2950 D Dcc     : DccDefaultState: msg.what=EVENT_RIL_CONNECTED mRilVersion=11

06-01 10:53:51.075  2812  2812 D DCT     : [0]GsmDCT.constructor

06-01 10:53:51.075  2812  2812 D GsmSST  : [GsmSST] notifyDataRegStateRilRadioTechnologyChanged: drs=1 rat=0

06-01 10:53:51.075  2812  2812 D TelephonyManager: setTelephonyProperty: success phoneId=0 property=gsm.network.type value: Unknown propVal=Unknown

06-01 10:53:51.075  2812  2812 D SubscriptionController: [getSubId]- sSlotIdxToSubId.size == 0, return DummySubIds slotIdx=0

06-01 10:53:51.075  2812  2812 D DCT     : [0]update sub = -2

06-01 10:53:51.075  2812  2812 D DCT     : [0]update(): Active DDS, register for all events now!

06-01 10:53:51.075  2812  2812 D DCT     : [0]onUpdateIcc: newIccRecords null

06-01 10:53:51.075  2812  2812 D DCT     : [0]getDataEnabled: getIntWithSubId retVal=true

06-01 10:53:51.085  2812  2812 D SubscriptionController: [getSubId]- sSlotIdxToSubId.size == 0, return DummySubIds slotIdx=0

06-01 10:53:51.085  2812  2812 D GSMPhone: [GSMPhone] updateCurrentCarrierInProvider: mSubId = -2 currentDds = -1 operatorNumeric = null

06-01 10:53:51.090  2812  2812 D DCT     : [0]initApnContexts: E

06-01 10:53:51.090  2812  2812 D DCT     : [0]initApnContexts: skipping unknown type=1

06-01 10:53:51.090  2812  2812 D DCT     : [0]initApnContexts: apnContext={mApnType=default mState=IDLE mWaitingApns={null} mWaitingApnsPermanentFailureCountDown=0 mApnSetting={null} mReason=dataEnabled mDataEnabled=false mDependencyMet=true}

06-01 10:53:51.090  2812  2812 D DCT     : [0]initApnContexts: apnContext={mApnType=mms mState=IDLE mWaitingApns={null} mWaitingApnsPermanentFailureCountDown=0 mApnSetting={null} mReason=dataEnabled mDataEnabled=false mDependencyMet=true}

06-01 10:53:51.090  2812  2812 D DCT     : [0]initApnContexts: apnContext={mApnType=supl mState=IDLE mWaitingApns={null} mWaitingApnsPermanentFailureCountDown=0 mApnSetting={null} mReason=dataEnabled mDataEnabled=false mDependencyMet=true}

06-01 10:53:51.090  2812  2812 D DCT     : [0]initApnContexts: apnContext={mApnType=dun mState=IDLE mWaitingApns={null} mWaitingApnsPermanentFailureCountDown=0 mApnSetting={null} mReason=dataEnabled mDataEnabled=false mDependencyMet=true}

06-01 10:53:51.090  2812  2812 D DCT     : [0]initApnContexts: apnContext={mApnType=hipri mState=IDLE mWaitingApns={null} mWaitingApnsPermanentFailureCountDown=0 mApnSetting={null} mReason=dataEnabled mDataEnabled=false mDependencyMet=true}

06-01 10:53:51.090  2812  2812 D DCT     : [0]initApnContexts: skipping unknown type=7

06-01 10:53:51.090  2812  2812 D DCT     : [0]initApnContexts: skipping unknown type=13

06-01 10:53:51.090  2812  2812 D DCT     : [0]initApnContexts: X mApnContexts={default={mApnType=default mState=IDLE mWaitingApns={null} mWaitingApnsPermanentFailureCountDown=0 mApnSetting={null} mReason=dataEnabled mDataEnabled=false mDependencyMet=true}, mms={mApnType=mms mState=IDLE mWaitingApns={null} mWaitingApnsPermanentFailureCountDown=0 mApnSetting={null} mReason=dataEnabled mDataEnabled=false mDependencyMet=true}, supl={mApnType=supl mState=IDLE mWaitingApns={null} mWaitingApnsPermanentFailureCountDown=0 mApnSetting={null} mReason=dataEnabled mDataEnabled=false mDependencyMet=true}, dun={mApnType=dun mState=IDLE mWaitingApns={null} mWaitingApnsPermanentFailureCountDown=0 mApnSetting={null} mReason=dataEnabled mDataEnabled=false mDependencyMet=true}, hipri={mApnType=hipri mState=IDLE mWaitingApns={null} mWaitingApnsPermanentFailureCountDown=0 mApnSetting={null} mReason=dataEnabled mDataEnabled=false mDependencyMet=true}}

06-01 10:53:51.185  2812  2812 D TelephonyManager: setTelephonyProperty: success phoneId=0 property=gsm.current.phone-type value: 1 propVal=1

06-01 10:53:51.185  2812  2812 D GSMPhone: [GSMPhone] GSMPhone: constructor: sub = 0

06-01 10:53:51.185  2812  2812 D TelephonyManager: setTelephonyProperty: success phoneId=0 property=gsm.current.phone-type value: 1 propVal=1

06-01 10:53:51.185  2812  2812 D SubscriptionController: [getSubId]- sSlotIdxToSubId.size == 0, return DummySubIds slotIdx=0

06-01 10:53:51.200  2812  2812 I PhoneFactory: Creating Phone with type = 1 sub = 0

06-01 10:53:51.205  2812  2812 E RIL_ImsSms: getFormat should never be called from here!

06-01 10:53:51.205  2812  2812 D SMSDispatcher: SMSDispatcher: ctor mSmsCapable=true format=unknown mSmsSendDisabled=false

06-01 10:53:51.205  2812  2812 D RIL_ImsSms: ImsSMSDispatcher created

06-01 10:53:51.205  2812  2812 D SMSDispatcher: SMSDispatcher: ctor mSmsCapable=true format=3gpp2 mSmsSendDisabled=false

06-01 10:53:51.205  2812  2812 D CdmaSMSDispatcher: CdmaSMSDispatcher created

06-01 10:53:51.240  2812  2812 D GsmInboundSmsHandler: created InboundSmsHandler

06-01 10:53:51.285  2812  2812 D CdmaInboundSmsHandler: created InboundSmsHandler

06-01 10:53:51.295  2812  2812 D SMSDispatcher: SMSDispatcher: ctor mSmsCapable=true format=3gpp mSmsSendDisabled=false

06-01 10:53:51.295  2812  2812 D GsmSMSDispatcher: GsmSMSDispatcher created

06-01 10:53:51.300  2812  2991 D SmsBroadcastUndelivered: scanning raw table for undelivered messages

06-01 10:53:51.305  2812  2812 D IccCardProxy: ctor: ci=com.android.internal.telephony.RIL@4cc13b5 phoneId=0

06-01 10:53:51.305  2812  2812 D CdmaSSM : subscriptionSource from settings: 0

06-01 10:53:51.305  2812  2812 D CdmaSSM : cdmaSSM constructor: 0

06-01 10:53:51.305  2812  2812 D IccCardProxy: update icc_operator_numeric=

06-01 10:53:51.305  2812  2812 D TelephonyManager: setTelephonyProperty: success phoneId=0 property=gsm.sim.operator.numeric value:  propVal=

06-01 10:53:51.305  2812  2812 D TelephonyManager: setTelephonyProperty: success phoneId=0 property=gsm.sim.operator.iso-country value:  propVal=

06-01 10:53:51.305  2812  2812 D TelephonyManager: setTelephonyProperty: success phoneId=0 property=gsm.sim.operator.alpha value:  propVal=

06-01 10:53:51.305  2812  2812 E IccCardProxy: setExternalState: set mPhoneId=0 mExternalState=NOT_READY

06-01 10:53:51.305  2812  2812 D TelephonyManager: setTelephonyProperty: success phoneId=0 property=gsm.sim.state value: NOT_READY propVal=NOT_READY

06-01 10:53:51.305  2812  2812 D SubscriptionController: [getSubId]- sSlotIdxToSubId.size == 0, return DummySubIds slotIdx=0

06-01 10:53:51.305  2812  2812 D IccCardProxy: broadcastIccStateChangedIntent intent ACTION_SIM_STATE_CHANGED value=NOT_READY reason=null for mPhoneId=0

06-01 10:53:51.315  2812  2812 D IccCardProxy: Setting radio tech UMTS

06-01 10:53:51.315  2812  2812 D IccCardProxy: updateQuietMode: 3GPP subscription -> newQuietMode=false

06-01 10:53:51.315  2812  2812 D IccCardProxy: updateQuietMode: no changes don't setExternalState

06-01 10:53:51.315  2812  2812 D IccCardProxy: updateQuietMode: QuietMode is false (app_type=1 cdmaSource=-1)

06-01 10:53:51.320  2812  2812 D ProxyController: Constructor - Enter

06-01 10:53:51.320  2812  2812 D DctController: makeDctController: new DctController phones.length=1

06-01 10:53:51.320  2812  2812 D DctController: DctController(): phones.length=1

06-01 10:53:51.345  2812  2812 D DcSwitchSM: [DcSwitchStateMachine-0] DcSwitchState constructor E

06-01 10:53:51.345  2812  2812 D DcSwitchSM: [DcSwitchStateMachine-0] DcSwitchState constructor X

06-01 10:53:51.345  2812  2992 D DcSwitchSM: [DcSwitchStateMachine-0] IdleState: enter

06-01 10:53:51.350  2812  2991 D SmsBroadcastUndelivered: finished scanning raw table in 48 ms

06-01 10:53:51.350  2812  2969 D GsmInboundSmsHandler: StartupState.processMessage:6

06-01 10:53:51.350  2812  2981 D CdmaInboundSmsHandler: StartupState.processMessage:6

06-01 10:53:51.350  2812  2981 D CdmaInboundSmsHandler: entering Idle state

06-01 10:53:51.350  2812  2969 D GsmInboundSmsHandler: entering Idle state

06-01 10:53:51.350  2812  2969 D GsmInboundSmsHandler: IdleState.processMessage:5

06-01 10:53:51.350  2812  2981 D CdmaInboundSmsHandler: IdleState.processMessage:5

06-01 10:53:51.350  2812  2969 D GsmInboundSmsHandler: Idle state processing message type 5

06-01 10:53:51.350  2812  2981 D CdmaInboundSmsHandler: Idle state processing message type 5

06-01 10:53:51.350  2812  2812 D DctController: DctController(phones): Connect success: 0

06-01 10:53:51.350  2812  2812 D DctController: updatePhoneBaseForIndex for phone index=0

06-01 10:53:51.350  2812  2812 D DctController: unregister TelephonyNetworkFactory for phone index=0

06-01 10:53:51.355  2812  2812 D SubscriptionController: [getSubId]- sSlotIdxToSubId.size == 0, return DummySubIds slotIdx=0

06-01 10:53:51.355  2812  2812 D DctController: [TNF -2]NetworkCapabilities: [ Transports: CELLULAR Capabilities: MMS&SUPL&DUN&FOTA&IMS&CBS&IA&RCS&XCAP&EIMS&INTERNET&NOT_RESTRICTED&TRUSTED&NOT_VPN]

06-01 10:53:51.355  2335  2787 D TelephonyRegistry: listen oscl: hasNotifySubscriptionInfoChangedOccurred==false no callback

06-01 10:53:51.360  2812  2812 D DctController: makeDctController: X sDctController=Handler (com.android.internal.telephony.dataconnection.DctController) {68758f}

06-01 10:53:51.365  2812  2812 D ProxyController: clearTransaction

06-01 10:53:51.365  2812  2812 D ProxyController: clearTransaction: phoneId=0 status=IDLE

06-01 10:53:51.365  2812  2812 D ProxyController: Constructor - Exit

06-01 10:53:51.365  2812  2981 D CdmaInboundSmsHandler: mWakeLock released wakelockcount = 0

06-01 10:53:51.370  2812  2969 D GsmInboundSmsHandler: mWakeLock released wakelockcount = 0

06-01 10:53:51.400  2812  2812 I PhoneFactory: defaultSmsApplication: com.android.messaging

06-01 10:53:51.405  2812  2812 I PhoneFactory: Creating SubInfoRecordUpdater 

06-01 10:53:51.405  2812  2812 D SubscriptionInfoUpdater: Constructor invoked

06-01 10:53:51.420  2812  2812 D SubscriptionController: [getSubId]- sSlotIdxToSubId.size == 0, return DummySubIds slotIdx=0

06-01 10:53:51.420  2812  2812 D SubscriptionController: [getActiveSubInfoList]+

06-01 10:53:51.420  2812  2812 D SubscriptionController: selection:sim_id>=0 null

06-01 10:53:51.420  2812  2812 D SubscriptionController: [getActiveSubInfoList]- no info return

06-01 10:53:51.420  2812  2812 D SubscriptionController: [getActiveSubInfoForSubscriber]- subId=-2 subList=null subInfo=null

06-01 10:53:51.420  2812  2812 E SubscriptionController: getUserNwMode: invalid subId = -2

06-01 10:53:51.425  2812  2812 D CallManager: registerPhone(GSM Handler (com.android.internal.telephony.PhoneProxy) {b8dd208})

06-01 10:53:51.425  2812  2812 D RILJ    : [3655]> SET_SUPP_SVC_NOTIFICATION [SUB0]

06-01 10:53:51.425  1964  2012 D use-Rlog/RLOG-RIL: 3 RIL requests in the queue (1 pending, 0 handled, 2 unhandled)

06-01 10:53:51.425  1964  2332 D use-Rlog/RLOG-RIL: Unhandled RIL request: 62

06-01 10:53:51.425  1964  2332 D use-Rlog/RLOG-RIL: 2 RIL requests in the queue (0 pending, 0 handled, 2 unhandled)

06-01 10:53:51.425  2812  2918 D RilRequest: [3655]< SET_SUPP_SVC_NOTIFICATION error: com.android.internal.telephony.CommandException: REQUEST_NOT_SUPPORTED ret=

06-01 10:53:51.465  2335  2871 D TelephonyRegistry: listen oscl: hasNotifySubscriptionInfoChangedOccurred==false no callback

06-01 10:53:51.530  2812  2812 D RILJ    : [3656]> RIL_REQUEST_SET_TTY_MODE : 0 [SUB0]

06-01 10:53:51.535  1964  2012 D use-Rlog/RLOG-RIL: 3 RIL requests in the queue (1 pending, 0 handled, 2 unhandled)

06-01 10:53:51.535  1964  2332 D use-Rlog/RLOG-RIL: Unhandled RIL request: 80

06-01 10:53:51.535  1964  2332 D use-Rlog/RLOG-RIL: 2 RIL requests in the queue (0 pending, 0 handled, 2 unhandled)

06-01 10:53:51.535  2812  2918 D RilRequest: [3656]< RIL_REQUEST_SET_TTY_MODE error: com.android.internal.telephony.CommandException: REQUEST_NOT_SUPPORTED ret=

06-01 10:53:51.540  2335  2787 D TelephonyRegistry: listen oscl: hasNotifySubscriptionInfoChangedOccurred==false no callback

06-01 10:53:51.540  2812  2812 D SubscriptionController: [getPhoneId] asked for default subId=-1

06-01 10:53:51.540  2812  2812 D SubscriptionController: [getPhoneId]- invalid subId return=-1

06-01 10:53:51.540  2812  2812 D UiccController: EVENT_RADIO_UNAVAILABLE, dispose card

06-01 10:53:51.540  2812  2812 D PhoneBase: config LCE service failed: com.android.internal.telephony.CommandException: REQUEST_NOT_SUPPORTED

06-01 10:53:51.540  2812  2812 D GsmSST  : [GsmSST] mDeviceShuttingDown = false

06-01 10:53:51.540  2812  2812 D GsmSST  : [GsmSST] mDesiredPowerState = true

06-01 10:53:51.540  2812  2812 D GsmSST  : [GsmSST] getRadioState = RADIO_OFF

06-01 10:53:51.540  2812  2812 D GsmSST  : [GsmSST] mPowerOffDelayNeed = true

06-01 10:53:51.540  2812  2812 D GsmSST  : [GsmSST] mAlarmSwitch = false

06-01 10:53:51.540  2812  2812 D RILJ    : [3657]> RADIO_POWER on [SUB0]

06-01 10:53:51.545  1964  2012 D use-Rlog/RLOG-RIL: 3 RIL requests in the queue (1 pending, 0 handled, 2 unhandled)

06-01 10:53:51.545  1964  2332 D use-Rlog/RLOG-RIL: Requesting normal power state

06-01 10:53:51.545  1964  2332 D use-Rlog/RLOG-RIL-IPC: 

06-01 10:53:51.545  1964  2332 D use-Rlog/RLOG-RIL-IPC: xmm626_sec_modem_fmt_send: Sent FMT message

06-01 10:53:51.545  1964  2332 D use-Rlog/RLOG-RIL-IPC: xmm626_sec_modem_fmt_send: Message: mseq=0x02, command=IPC_PWR_PHONE_STATE, type=IPC_TYPE_EXEC, size=2

06-01 10:53:51.545  1964  2332 D use-Rlog/RLOG-RIL-IPC: ================================= IPC FMT data =================================

06-01 10:53:51.545  1964  2332 D use-Rlog/RLOG-RIL-IPC: [0000]   02 02                                              ..

06-01 10:53:51.545  1964  2332 D use-Rlog/RLOG-RIL-IPC: ================================================================================

06-01 10:53:51.545  2812  2812 D PHONE   : [ServiceState] setNullState=3

06-01 10:53:51.545  2812  2812 D GsmSST  : [GsmSST] set service state as POWER_OFF

06-01 10:53:51.545  2812  2812 D PHONE   : [ServiceState] setNullState=3

06-01 10:53:51.545  2812  2812 D GsmSST  : [GsmSST] Poll ServiceState done:  oldSS=[1 1 voice home data home null null null null null null  Unknown Unknown CSS not supported 0 0 RoamInd=0 DefRoamInd=0 EmergOnly=false IsDataRoamingFromRegistration=false] newSS=[3 3 voice home data home null null null null null null  Unknown Unknown CSS not supported -1 -1 RoamInd=-1 DefRoamInd=-1 EmergOnly=false IsDataRoamingFromRegistration=false] oldMaxDataCalls=1 mNewMaxDataCalls=1 oldReasonDataDenied=-1 mNewReasonDataDenied=-1

06-01 10:53:51.545  2812  2812 D PHONE   : [ServiceState] setNullState=1

06-01 10:53:51.545  2812  2812 D GsmSST  : [GsmSST] updateSpnDisplay: radio is off w/ showPlmn=true plmn=No service.

06-01 10:53:51.545  2812  2812 D SubscriptionController: [getSubId]- sSlotIdxToSubId.size == 0, return DummySubIds slotIdx=0

06-01 10:53:51.545  2812  2812 D GsmSST  : [GsmSST] updateSpnDisplay: changed sending intent rule=0 showPlmn='true' plmn='No service.' showSpn='false' spn='null' dataSpn='' subId='-2'

06-01 10:53:51.545  2812  2812 D SubscriptionController: [getSubId]- sSlotIdxToSubId.size == 0, return DummySubIds slotIdx=0

06-01 10:53:51.545  2812  2812 D SubscriptionController: [getSubId]- sSlotIdxToSubId.size == 0, return DummySubIds slotIdx=0

06-01 10:53:51.545  2812  2812 D SubscriptionController: [setPlmnSpn] No valid subscription to store info

06-01 10:53:51.545  2812  2812 D SubscriptionController: notifySubscriptionInfoChanged:

06-01 10:53:51.545  2335  2837 D TelephonyRegistry: notifySubscriptionInfoChanged: first invocation mRecords.size=12

06-01 10:53:51.550  2812  2812 D TelephonyManager: setTelephonyProperty: success phoneId=0 property=gsm.operator.alpha value:  propVal=

06-01 10:53:51.600  2812  2812 D TelephonyManager: setTelephonyProperty: success phoneId=0 property=gsm.operator.numeric value:  propVal=

06-01 10:53:51.600  2812  2812 D GsmSST  : [GsmSST] operatorNumeric is null

06-01 10:53:51.600  2812  2812 D TelephonyManager: setTelephonyProperty: success phoneId=0 property=gsm.operator.iso-country value:  propVal=

06-01 10:53:51.605  2812  2812 D TelephonyManager: setTelephonyProperty: success phoneId=0 property=gsm.operator.isroaming value: false propVal=false

06-01 10:53:51.605  2812  2812 D GsmSST  : [GsmSST] Broadcasting ServiceState : 3 3 voice home data home null null null null null null  Unknown Unknown CSS not supported -1 -1 RoamInd=-1 DefRoamInd=-1 EmergOnly=false IsDataRoamingFromRegistration=false

06-01 10:53:51.605  2812  2812 D SubscriptionController: [getSubId]- sSlotIdxToSubId.size == 0, return DummySubIds slotIdx=0

06-01 10:53:51.605  2812  2812 D DefaultPhoneNotifier: nofityServiceState: mRegistry=com.android.internal.telephony.ITelephonyRegistry$Stub$Proxy@d42da20 ss=3 3 voice home data home null null null null null null  Unknown Unknown CSS not supported -1 -1 RoamInd=-1 DefRoamInd=-1 EmergOnly=false IsDataRoamingFromRegistration=false sender=Handler (com.android.internal.telephony.gsm.GSMPhone) {b910da1} phondId=0 subId=-2

06-01 10:53:51.615  2812  2812 D SubscriptionController: [getSlotId]- subId invalid

06-01 10:53:51.615  2812  2812 D SubscriptionController: getSimStateForSlotIdx:  simState=NOT_READY ordinal=6

06-01 10:53:51.615  2335  2346 D SubscriptionManager: getSimStateForSubscriber: simState=6 slotIdx=0

06-01 10:53:51.615  2335  2346 D TelephonyManager: getSimState: default sim:-1, sim state for slotIdx=0 is 6, return state as unknown

06-01 10:53:51.615  2812  2812 D GsmSST  : [GsmSST] notifyDataRegStateRilRadioTechnologyChanged: drs=3 rat=0

06-01 10:53:51.615  2812  2812 D TelephonyManager: setTelephonyProperty: success phoneId=0 property=gsm.network.type value: Unknown propVal=Unknown

06-01 10:53:51.615  2812  2812 D DCT     : [0]get all active apn types

06-01 10:53:51.615  2812  2812 D RILJ    : [3658]> OPERATOR [SUB0]

06-01 10:53:51.635  2812  2812 D RILJ    : [3659]> DATA_REGISTRATION_STATE [SUB0]

06-01 10:53:51.635  1964  2012 D use-Rlog/RLOG-RIL: 4 RIL requests in the queue (1 pending, 1 handled, 2 unhandled)

06-01 10:53:51.635  2812  2812 D RILJ    : [3660]> VOICE_REGISTRATION_STATE [SUB0]

06-01 10:53:51.635  1964  2012 D use-Rlog/RLOG-RIL: 5 RIL requests in the queue (1 pending, 1 handled, 3 unhandled)

06-01 10:53:51.635  2812  2812 D RILJ    : [3661]> QUERY_NETWORK_SELECTION_MODE [SUB0]

06-01 10:53:51.635  1964  2012 D use-Rlog/RLOG-RIL: 6 RIL requests in the queue (1 pending, 1 handled, 4 unhandled)

06-01 10:53:51.640  2812  2812 D DCT     : [0]handleMessage msg={ when=-595ms what=270369 obj=android.os.AsyncResult@8accfd9 target=com.android.internal.telephony.dataconnection.DcTracker }

06-01 10:53:51.640  2812  2812 D DCT     : [0]onUpdateIcc: newIccRecords null

06-01 10:53:51.640  2812  2812 D DCT     : [0]handleMessage msg={ when=-565ms what=270337 obj=android.os.AsyncResult@3becd9e target=com.android.internal.telephony.dataconnection.DcTracker }

06-01 10:53:51.640  2812  2812 D DCT     : [0]onRadioAvailable

06-01 10:53:51.640  2812  2812 D DCT     : [0]overall state is IDLE

06-01 10:53:51.640  2812  2812 D DCT     : [0]handleMessage msg={ when=-566ms what=270342 obj=android.os.AsyncResult@117e07f target=com.android.internal.telephony.dataconnection.DcTracker }

06-01 10:53:51.640  2812  2812 D DCT     : [0]onRadioOffOrNotAvailable: is off and clean up all connections

06-01 10:53:51.640  2812  2812 D DCT     : [0]cleanUpAllConnections: tearDown=false reason=radioTurnedOff

06-01 10:53:51.640  2812  2812 D DCT     : [0]cleanUpConnection: tearDown=false reason=radioTurnedOff apnContext={mApnType=default mState=IDLE mWaitingApns={null} mWaitingApnsPermanentFailureCountDown=0 mApnSetting={null} mReason=radioTurnedOff mDataEnabled=false mDependencyMet=true}

06-01 10:53:51.640  2812  2812 D GSMPhone: getDataConnectionState: Data is Out of Service. ret = DISCONNECTED

06-01 10:53:51.640  2812  2812 D SubscriptionController: [getSubId]- sSlotIdxToSubId.size == 0, return DummySubIds slotIdx=0

06-01 10:53:51.640  1964  2012 D use-Rlog/RLOG-RIL: 7 RIL requests in the queue (1 pending, 1 handled, 5 unhandled)

06-01 10:53:51.640  2812  2812 D DCT     : [0]isDataAllowed: not allowed due to - Attached= false - SIM not loaded - SIM not loaded and not NV subscription - defaultDataSelected= false

06-01 10:53:51.645  2812  2812 D SubscriptionController: [getPhoneId]- invalid subId return=-1

06-01 10:53:51.650  2812  2812 D DCT     : [0]setupDataForSinglePdn: reason = radioTurnedOff isDisconnected = true

06-01 10:53:51.650  2812  2812 D DCT     : [0]isOnlySingleDcAllowed(0): false

06-01 10:53:51.650  2812  2812 D DCT     : [0]cleanUpConnection: X tearDown=false reason=radioTurnedOff apnContext={mApnType=default mState=IDLE mWaitingApns={null} mWaitingApnsPermanentFailureCountDown=0 mApnSetting={null} mReason=radioTurnedOff mDataEnabled=false mDependencyMet=true} dcac=null

06-01 10:53:51.650  2812  2812 D DCT     : [0]cleanUpConnection: tearDown=false reason=radioTurnedOff apnContext={mApnType=mms mState=IDLE mWaitingApns={null} mWaitingApnsPermanentFailureCountDown=0 mApnSetting={null} mReason=radioTurnedOff mDataEnabled=false mDependencyMet=true}

06-01 10:53:51.650  2812  2812 D GSMPhone: getDataConnectionState: Data is Out of Service. ret = DISCONNECTED

06-01 10:53:51.650  2812  2812 D SubscriptionController: [getSubId]- sSlotIdxToSubId.size == 0, return DummySubIds slotIdx=0

06-01 10:53:51.650  2812  2812 D DCT     : [0]isDataAllowed: not allowed due to - Attached= false - SIM not loaded - SIM not loaded and not NV subscription - defaultDataSelected= false

06-01 10:53:51.650  2812  2812 D SubscriptionController: [getPhoneId]- invalid subId return=-1

06-01 10:53:51.650  2812  2812 D DCT     : [0]setupDataForSinglePdn: reason = radioTurnedOff isDisconnected = true

06-01 10:53:51.650  2812  2812 D DCT     : [0]isOnlySingleDcAllowed(0): false

06-01 10:53:51.650  2812  2812 D DCT     : [0]cleanUpConnection: X tearDown=false reason=radioTurnedOff apnContext={mApnType=mms mState=IDLE mWaitingApns={null} mWaitingApnsPermanentFailureCountDown=0 mApnSetting={null} mReason=radioTurnedOff mDataEnabled=false mDependencyMet=true} dcac=null

06-01 10:53:51.650  2812  2812 D DCT     : [0]cleanUpConnection: tearDown=false reason=radioTurnedOff apnContext={mApnType=supl mState=IDLE mWaitingApns={null} mWaitingApnsPermanentFailureCountDown=0 mApnSetting={null} mReason=radioTurnedOff mDataEnabled=false mDependencyMet=true}

06-01 10:53:51.650  2812  2812 D GSMPhone: getDataConnectionState: Data is Out of Service. ret = DISCONNECTED

06-01 10:53:51.655  2812  2812 D SubscriptionController: [getSubId]- sSlotIdxToSubId.size == 0, return DummySubIds slotIdx=0

06-01 10:53:51.655  2812  2812 D DCT     : [0]isDataAllowed: not allowed due to - Attached= false - SIM not loaded - SIM not loaded and not NV subscription - defaultDataSelected= false

06-01 10:53:51.655  2812  2812 D SubscriptionController: [getPhoneId]- invalid subId return=-1

06-01 10:53:51.655  1964  2328 D use-Rlog/RLOG-RIL-IPC: 

06-01 10:53:51.655  1964  2328 D use-Rlog/RLOG-RIL-IPC: xmm626_sec_modem_fmt_recv: Received FMT message

06-01 10:53:51.655  1964  2328 D use-Rlog/RLOG-RIL-IPC: xmm626_sec_modem_fmt_recv: Message: aseq=0x02, command=IPC_GEN_PHONE_RES, type=IPC_TYPE_RESP, size=5

06-01 10:53:51.655  1964  2328 D use-Rlog/RLOG-RIL-IPC: ================================= IPC FMT data =================================

06-01 10:53:51.655  2812  2812 D DCT     : [0]setupDataForSinglePdn: reason = radioTurnedOff isDisconnected = true

06-01 10:53:51.655  1964  2328 D use-Rlog/RLOG-RIL-IPC: [0000]   01 07 01 00 80                                     .....

06-01 10:53:51.655  1964  2328 D use-Rlog/RLOG-RIL-IPC: ================================================================================

06-01 10:53:51.655  2812  2812 D DCT     : [0]isOnlySingleDcAllowed(0): false

06-01 10:53:51.655  1964  2328 D use-Rlog/RLOG-RIL: Generic response was expected

06-01 10:53:51.655  2812  2812 D DCT     : [0]cleanUpConnection: X tearDown=false reason=radioTurnedOff apnContext={mApnType=supl mState=IDLE mWaitingApns={null} mWaitingApnsPermanentFailureCountDown=0 mApnSetting={null} mReason=radioTurnedOff mDataEnabled=false mDependencyMet=true} dcac=null

06-01 10:53:51.655  2812  2812 D DCT     : [0]cleanUpConnection: tearDown=false reason=radioTurnedOff apnContext={mApnType=dun mState=IDLE mWaitingApns={null} mWaitingApnsPermanentFailureCountDown=0 mApnSetting={null} mReason=radioTurnedOff mDataEnabled=false mDependencyMet=true}

06-01 10:53:51.655  2812  2812 D GSMPhone: getDataConnectionState: Data is Out of Service. ret = DISCONNECTED

06-01 10:53:51.655  1964  2328 D use-Rlog/RLOG-RIL-IPC: 

06-01 10:53:51.655  2812  2812 D SubscriptionController: [getSubId]- sSlotIdxToSubId.size == 0, return DummySubIds slotIdx=0

06-01 10:53:51.655  1964  2328 D use-Rlog/RLOG-RIL-IPC: xmm626_sec_modem_fmt_recv: Received FMT message

06-01 10:53:51.655  1964  2328 D use-Rlog/RLOG-RIL-IPC: xmm626_sec_modem_fmt_recv: Message: aseq=0x02, command=IPC_PWR_PHONE_STATE, type=IPC_TYPE_NOTI, size=1

06-01 10:53:51.655  1964  2328 D use-Rlog/RLOG-RIL-IPC: ================================= IPC FMT data =================================

06-01 10:53:51.655  1964  2328 D use-Rlog/RLOG-RIL-IPC: [0000]   02                                                 .

06-01 10:53:51.655  1964  2328 D use-Rlog/RLOG-RIL-IPC: ================================================================================

06-01 10:53:51.655  1964  2328 D use-Rlog/RLOG-RIL: Power state is normal

06-01 10:53:51.655  1964  2328 D use-Rlog/RLOG-RIL: 6 RIL requests in the queue (0 pending, 0 handled, 6 unhandled)

06-01 10:53:51.655  1964  2328 D use-Rlog/RLOG-RIL: Updating RIL radio state to 2

06-01 10:53:51.655  1964  2328 D use-Rlog/RLOG-RIL-IPC: 

06-01 10:53:51.655  1964  2328 D use-Rlog/RLOG-RIL-IPC: xmm626_sec_modem_fmt_recv: Received FMT message

06-01 10:53:51.655  1964  2328 D use-Rlog/RLOG-RIL-IPC: xmm626_sec_modem_fmt_recv: Message: aseq=0x02, command=IPC_SEC_SIM_ICC_TYPE, type=IPC_TYPE_NOTI, size=1

06-01 10:53:51.655  1964  2328 D use-Rlog/RLOG-RIL-IPC: ================================= IPC FMT data =================================

06-01 10:53:51.655  1964  2328 D use-Rlog/RLOG-RIL-IPC: [0000]   02                                                 .

06-01 10:53:51.655  1964  2328 D use-Rlog/RLOG-RIL-IPC: ================================================================================

06-01 10:53:51.660  1964  2328 D use-Rlog/RLOG-RIL-IPC: 

06-01 10:53:51.660  1964  2328 D use-Rlog/RLOG-RIL-IPC: xmm626_sec_modem_fmt_recv: Received FMT message

06-01 10:53:51.660  1964  2328 D use-Rlog/RLOG-RIL-IPC: xmm626_sec_modem_fmt_recv: Message: aseq=0x02, command=IPC_SEC_PIN_STATUS, type=IPC_TYPE_NOTI, size=2

06-01 10:53:51.660  1964  2328 D use-Rlog/RLOG-RIL-IPC: ================================= IPC FMT data =================================

06-01 10:53:51.660  1964  2328 D use-Rlog/RLOG-RIL-IPC: [0000]   03 01                                              ..

06-01 10:53:51.660  1964  2328 D use-Rlog/RLOG-RIL-IPC: ================================================================================

06-01 10:53:51.660  1964  2328 D use-Rlog/RLOG-RIL: ipc2ril_sec_pin_status_response: Selecting status application 3 on 10

06-01 10:53:51.660  1964  2328 D use-Rlog/RLOG-RIL: Updating RIL radio state to 3

06-01 10:53:51.660  1964  2328 D use-Rlog/RLOG-RIL-IPC: 

06-01 10:53:51.660  1964  2328 D use-Rlog/RLOG-RIL-IPC: xmm626_sec_modem_fmt_recv: Received FMT message

06-01 10:53:51.660  1964  2328 D use-Rlog/RLOG-RIL-IPC: xmm626_sec_modem_fmt_recv: Message: aseq=0x02, command=IPC_SAT_PROACTIVE_CMD, type=IPC_TYPE_INDI, size=13

06-01 10:53:51.660  1964  2328 D use-Rlog/RLOG-RIL-IPC: ================================= IPC FMT data =================================

06-01 10:53:51.660  1964  2328 D use-Rlog/RLOG-RIL-IPC: [0000]   0B 00 D0 09 81 03 01 02  00 82 02 81 82            ........ .....

06-01 10:53:51.660  2812  2918 D RILJ    : [3657]< RADIO_POWER  [SUB0]

06-01 10:53:51.660  1964  2328 D use-Rlog/RLOG-RIL-IPC: ================================================================================

06-01 10:53:51.660  1964  2328 D use-Rlog/RLOG-RIL-IPC: Unhandled IPC FMT message: IPC_SAT_PROACTIVE_CMD

06-01 10:53:51.660  1964  2328 D use-Rlog/RLOG-RIL-IPC: 

06-01 10:53:51.660  1964  2328 D use-Rlog/RLOG-RIL-IPC: xmm626_sec_modem_fmt_recv: Received FMT message

06-01 10:53:51.660  1964  2328 D use-Rlog/RLOG-RIL-IPC: xmm626_sec_modem_fmt_recv: Message: aseq=0xff, command=IPC_NET_REGIST, type=IPC_TYPE_NOTI, size=11

06-01 10:53:51.660  2812  2918 D RILJ    : [UNSL]< UNSOL_VOICE_RADIO_TECH_CHANGED {3} [SUB0]

06-01 10:53:51.660  1964  2328 D use-Rlog/RLOG-RIL-IPC: ================================= IPC FMT data =================================

06-01 10:53:51.660  1964  2328 D use-Rlog/RLOG-RIL-IPC: [0000]   FF 02 01 00 00 00 00 00  00 00 00                  ........ ...

06-01 10:53:51.660  1964  2328 D use-Rlog/RLOG-RIL-IPC: ================================================================================

06-01 10:53:51.660  2812  2918 D RILJ    : [UNSL]< UNSOL_RESPONSE_RADIO_STATE_CHANGED RADIO_ON [SUB0]

06-01 10:53:51.660  1964  2328 D use-Rlog/RLOG-RIL-IPC: 

06-01 10:53:51.660  1964  2328 D use-Rlog/RLOG-RIL-IPC: xmm626_sec_modem_fmt_recv: Received FMT message

06-01 10:53:51.660  1964  2328 D use-Rlog/RLOG-RIL-IPC: xmm626_sec_modem_fmt_recv: Message: aseq=0xff, command=IPC_NET_REGIST, type=IPC_TYPE_NOTI, size=11

06-01 10:53:51.660  1964  2328 D use-Rlog/RLOG-RIL-IPC: ================================= IPC FMT data =================================

06-01 10:53:51.660  1964  2328 D use-Rlog/RLOG-RIL-IPC: [0000]   FF 03 01 00 00 00 00 00  00 00 00                  ........ ...

06-01 10:53:51.660  2812  2918 D RILJ    : [UNSL]< UNSOL_RESPONSE_SIM_STATUS_CHANGED [SUB0]

06-01 10:53:51.660  1964  2328 D use-Rlog/RLOG-RIL-IPC: ================================================================================

06-01 10:53:51.660  1964  2328 D use-Rlog/RLOG-RIL-IPC: 

06-01 10:53:51.660  1964  2328 D use-Rlog/RLOG-RIL-IPC: xmm626_sec_modem_fmt_recv: Received FMT message

06-01 10:53:51.660  2812  2918 D RILJ    : [UNSL]< UNSOL_RESPONSE_RADIO_STATE_CHANGED RADIO_ON [SUB0]

06-01 10:53:51.660  1964  2328 D use-Rlog/RLOG-RIL-IPC: xmm626_sec_modem_fmt_recv: Message: aseq=0x00, command=IPC_DISP_ICON_INFO, type=IPC_TYPE_NOTI, size=4

06-01 10:53:51.660  1964  2328 D use-Rlog/RLOG-RIL-IPC: ================================= IPC FMT data =================================

06-01 10:53:51.660  1964  2328 D use-Rlog/RLOG-RIL-IPC: [0000]   FF 00 00 04                                        ....

06-01 10:53:51.660  2812  2918 D RILJ    : [UNSL]< UNSOL_RESPONSE_SIM_STATUS_CHANGED [SUB0]

06-01 10:53:51.660  1964  2328 D use-Rlog/RLOG-RIL-IPC: ================================================================================

06-01 10:53:51.660  1964  2328 D use-Rlog/RLOG-RIL: Signal strength is 1

06-01 10:53:51.660  1964  2328 D use-Rlog/RLOG-RIL-IPC: 

06-01 10:53:51.660  2812  2918 D RILJ    : [UNSL]< UNSOL_RESPONSE_VOICE_NETWORK_STATE_CHANGED [SUB0]

06-01 10:53:51.660  1964  2328 D use-Rlog/RLOG-RIL-IPC: xmm626_sec_modem_fmt_recv: Received FMT message

06-01 10:53:51.660  1964  2328 D use-Rlog/RLOG-RIL-IPC: xmm626_sec_modem_fmt_recv: Message: aseq=0xff, command=IPC_NET_REGIST, type=IPC_TYPE_NOTI, size=11

06-01 10:53:51.660  1964  2328 D use-Rlog/RLOG-RIL-IPC: ================================= IPC FMT data =================================

06-01 10:53:51.660  2812  2918 D RILJ    : [UNSL]< UNSOL_RESPONSE_VOICE_NETWORK_STATE_CHANGED [SUB0]

06-01 10:53:51.660  1964  2328 D use-Rlog/RLOG-RIL-IPC: [0000]   FF 02 04 00 00 00 00 00  00 00 00                  ........ ...

06-01 10:53:51.660  1964  2328 D use-Rlog/RLOG-RIL-IPC: ================================================================================

06-01 10:53:51.660  1964  2328 D use-Rlog/RLOG-RIL-IPC: 

06-01 10:53:51.660  1964  2328 D use-Rlog/RLOG-RIL-IPC: xmm626_sec_modem_fmt_recv: Received FMT message

06-01 10:53:51.660  1964  2328 D use-Rlog/RLOG-RIL-IPC: xmm626_sec_modem_fmt_recv: Message: aseq=0xff, command=IPC_NET_REGIST, type=IPC_TYPE_NOTI, size=11

06-01 10:53:51.660  1964  2328 D use-Rlog/RLOG-RIL-IPC: ================================= IPC FMT data =================================

06-01 10:53:51.660  1964  2328 D use-Rlog/RLOG-RIL-IPC: [0000]   FF 03 01 00 00 00 00 00  00 00 00                  ........ ...

06-01 10:53:51.660  1964  2328 D use-Rlog/RLOG-RIL-IPC: ================================================================================

06-01 10:53:51.660  2812  2918 D RILJ    : [UNSL]< UNSOL_RESPONSE_VOICE_NETWORK_STATE_CHANGED [SUB0]

06-01 10:53:51.660  1964  2328 D use-Rlog/RLOG-RIL-IPC: 

06-01 10:53:51.660  1964  2328 D use-Rlog/RLOG-RIL-IPC: xmm626_sec_modem_fmt_recv: Received FMT message

06-01 10:53:51.660  1964  2328 D use-Rlog/RLOG-RIL-IPC: xmm626_sec_modem_fmt_recv: Message: aseq=0x00, command=IPC_NET_SERVING_NETWORK, type=IPC_TYPE_NOTI, size=11

06-01 10:53:51.660  1964  2328 D use-Rlog/RLOG-RIL-IPC: ================================= IPC FMT data =================================

06-01 10:53:51.660  2812  2918 D RILJ    : [UNSL]< UNSOL_RESPONSE_VOICE_NETWORK_STATE_CHANGED [SUB0]

06-01 10:53:51.660  1964  2328 D use-Rlog/RLOG-RIL-IPC: [0000]   02 04 FF 32 30 36 31 30  23 00 00                  ...20610 #..

06-01 10:53:51.660  1964  2328 D use-Rlog/RLOG-RIL-IPC: ================================================================================

06-01 10:53:51.660  1964  2332 D use-Rlog/RLOG-RIL: 5 RIL requests in the queue (5 pending, 0 handled, 0 unhandled)

06-01 10:53:51.660  1964  2332 D use-Rlog/RLOG-RIL: 6 RIL requests data in the queue

06-01 10:53:51.660  1964  2332 D use-Rlog/RLOG-RIL-IPC: 

06-01 10:53:51.660  1964  2332 D use-Rlog/RLOG-RIL-IPC: xmm626_sec_modem_fmt_send: Sent FMT message

06-01 10:53:51.660  1964  2332 D use-Rlog/RLOG-RIL-IPC: xmm626_sec_modem_fmt_send: Message: mseq=0x03, command=IPC_DISP_ICON_INFO, type=IPC_TYPE_GET, size=1

06-01 10:53:51.660  1964  2332 D use-Rlog/RLOG-RIL-IPC: ================================= IPC FMT data =================================

06-01 10:53:51.660  1964  2332 D use-Rlog/RLOG-RIL-IPC: [0000]   01                                                 .

06-01 10:53:51.660  1964  2332 D use-Rlog/RLOG-RIL-IPC: ================================================================================

06-01 10:53:51.660  1964  2332 D use-Rlog/RLOG-RIL: 4 RIL requests in the queue (3 pending, 1 handled, 0 unhandled)

06-01 10:53:51.660  1964  2332 D use-Rlog/RLOG-RIL: 5 RIL requests data in the queue

06-01 10:53:51.660  1964  2332 D use-Rlog/RLOG-RIL: 3 RIL requests in the queue (2 pending, 1 handled, 0 unhandled)

06-01 10:53:51.660  1964  2332 D use-Rlog/RLOG-RIL: 4 RIL requests data in the queue

06-01 10:53:51.660  1964  2332 D use-Rlog/RLOG-RIL: 2 RIL requests in the queue (1 pending, 1 handled, 0 unhandled)

06-01 10:53:51.660  1964  2332 D use-Rlog/RLOG-RIL: 3 RIL requests data in the queue

06-01 10:53:51.660  1964  2332 D use-Rlog/RLOG-RIL-IPC: 

06-01 10:53:51.660  1964  2332 D use-Rlog/RLOG-RIL-IPC: xmm626_sec_modem_fmt_send: Sent FMT message

06-01 10:53:51.660  1964  2332 D use-Rlog/RLOG-RIL-IPC: xmm626_sec_modem_fmt_send: Message: mseq=0x04, command=IPC_NET_PLMN_SEL, type=IPC_TYPE_GET, size=0

06-01 10:53:51.660  2812  2812 D DCT     : [0]isDataAllowed: not allowed due to - Attached= false - SIM not loaded - SIM not loaded and not NV subscription - defaultDataSelected= false

06-01 10:53:51.660  2812  2812 D SubscriptionController: [getPhoneId]- invalid subId return=-1

06-01 10:53:51.660  1964  2328 D use-Rlog/RLOG-RIL-IPC: 

06-01 10:53:51.660  1964  2328 D use-Rlog/RLOG-RIL-IPC: xmm626_sec_modem_fmt_recv: Received FMT message

06-01 10:53:51.660  1964  2328 D use-Rlog/RLOG-RIL-IPC: xmm626_sec_modem_fmt_recv: Message: aseq=0x03, command=IPC_DISP_ICON_INFO, type=IPC_TYPE_RESP, size=4

06-01 10:53:51.660  1964  2328 D use-Rlog/RLOG-RIL-IPC: ================================= IPC FMT data =================================

06-01 10:53:51.660  1964  2328 D use-Rlog/RLOG-RIL-IPC: [0000]   01 00 00 04                                        ....

06-01 10:53:51.660  1964  2328 D use-Rlog/RLOG-RIL-IPC: ================================================================================

06-01 10:53:51.660  1964  2328 D use-Rlog/RLOG-RIL: Signal strength is 1

06-01 10:53:51.660  1964  2328 D use-Rlog/RLOG-RIL: 1 RIL request in the queue (0 pending, 1 handled, 0 unhandled)

06-01 10:53:51.660  1964  2328 D use-Rlog/RLOG-RIL: 3 RIL requests data in the queue

06-01 10:53:51.660  1964  2328 D use-Rlog/RLOG-RIL-IPC: 

06-01 10:53:51.660  1964  2328 D use-Rlog/RLOG-RIL-IPC: xmm626_sec_modem_fmt_recv: Received FMT message

06-01 10:53:51.660  1964  2328 D use-Rlog/RLOG-RIL-IPC: xmm626_sec_modem_fmt_recv: Message: aseq=0x04, command=IPC_NET_PLMN_SEL, type=IPC_TYPE_RESP, size=1

06-01 10:53:51.660  2812  2918 D RILJ    : [UNSL]< UNSOL_RESPONSE_VOICE_NETWORK_STATE_CHANGED [SUB0]

06-01 10:53:51.660  1964  2328 D use-Rlog/RLOG-RIL-IPC: ================================= IPC FMT data =================================

06-01 10:53:51.660  1964  2328 D use-Rlog/RLOG-RIL-IPC: [0000]   02                                                 .

06-01 10:53:51.660  1964  2328 D use-Rlog/RLOG-RIL-IPC: ================================================================================

06-01 10:53:51.660  1964  2328 D use-Rlog/RLOG-RIL: 0 RIL request in the queue (0 pending, 0 handled, 0 unhandled)

06-01 10:53:51.660  1964  2328 D use-Rlog/RLOG-RIL: 3 RIL requests data in the queue

06-01 10:53:51.660  2812  2918 D RILJ    : [UNSL]< UNSOL_RESPONSE_VOICE_NETWORK_STATE_CHANGED [SUB0]

06-01 10:53:51.660  2812  2918 D RILJ    : [3652]< SCREEN_STATE  [SUB0]

06-01 10:53:51.660  2812  2918 D RILJ    : [3658]< OPERATOR {Mobistar, Mobistar, 20610} [SUB0]

06-01 10:53:51.665  2812  2918 D RILJ    : [3659]< DATA_REGISTRATION_STATE {0, 0, 0, 0, 3} [SUB0]

06-01 10:53:51.665  1964  2329 D use-Rlog/RLOG-RIL-IPC: 

06-01 10:53:51.665  1964  2329 D use-Rlog/RLOG-RIL-IPC: xmm626_sec_modem_rfs_recv: Received RFS message

06-01 10:53:51.665  1964  2329 D use-Rlog/RLOG-RIL-IPC: xmm626_sec_modem_rfs_recv: Message: aseq=0x01, command=IPC_RFS_NV_WRITE_ITEM, size=12

06-01 10:53:51.665  1964  2329 D use-Rlog/RLOG-RIL-IPC: ================================= IPC RFS data =================================

06-01 10:53:51.665  1964  2329 D use-Rlog/RLOG-RIL-IPC: [0000]   09 00 1A 00 04 00 00 00  0F 00 93 40               ........ ...@

06-01 10:53:51.665  1964  2329 D use-Rlog/RLOG-RIL-IPC: ================================================================================

06-01 10:53:51.665  2812  2918 D RILJ    : [3660]< VOICE_REGISTRATION_STATE {0, 0, 0, 0, null, null, null, null, null, null, null, null, null, null, null} [SUB0]

06-01 10:53:51.665  1964  2329 D use-Rlog/RLOG-RIL-IPC: Checked nv_data path

06-01 10:53:51.665  2812  2918 D RILJ    : [3654]< SIGNAL_STRENGTH SignalStrength: 1 99 -1 -1 -1 -1 -1 -1 -1 -1 -1 -1 2147483647 gsm|lte [SUB0]

06-01 10:53:51.665  2812  2918 D RILJ    : [3661]< QUERY_NETWORK_SELECTION_MODE {0} [SUB0]

06-01 10:53:51.665  2812  2812 D DCT     : [0]setupDataForSinglePdn: reason = radioTurnedOff isDisconnected = true

06-01 10:53:51.665  2812  2812 D DCT     : [0]isOnlySingleDcAllowed(0): false

06-01 10:53:51.665  2812  2812 D DCT     : [0]cleanUpConnection: X tearDown=false reason=radioTurnedOff apnContext={mApnType=dun mState=IDLE mWaitingApns={null} mWaitingApnsPermanentFailureCountDown=0 mApnSetting={null} mReason=radioTurnedOff mDataEnabled=false mDependencyMet=true} dcac=null

06-01 10:53:51.665  2812  2812 D DCT     : [0]cleanUpConnection: tearDown=false reason=radioTurnedOff apnContext={mApnType=hipri mState=IDLE mWaitingApns={null} mWaitingApnsPermanentFailureCountDown=0 mApnSetting={null} mReason=radioTurnedOff mDataEnabled=false mDependencyMet=true}

06-01 10:53:51.665  2812  2812 D GSMPhone: getDataConnectionState: Data is Out of Service. ret = DISCONNECTED

06-01 10:53:51.665  2812  2812 D SubscriptionController: [getSubId]- sSlotIdxToSubId.size == 0, return DummySubIds slotIdx=0

06-01 10:53:51.665  2812  2812 D DCT     : [0]isDataAllowed: not allowed due to - Attached= false - SIM not loaded - SIM not loaded and not NV subscription - defaultDataSelected= false

06-01 10:53:51.665  2812  2812 D SubscriptionController: [getPhoneId]- invalid subId return=-1

06-01 10:53:51.665  2812  2812 D DCT     : [0]setupDataForSinglePdn: reason = radioTurnedOff isDisconnected = true

06-01 10:53:51.665  2812  2812 D DCT     : [0]isOnlySingleDcAllowed(0): false

06-01 10:53:51.665  2812  2812 D DCT     : [0]cleanUpConnection: X tearDown=false reason=radioTurnedOff apnContext={mApnType=hipri mState=IDLE mWaitingApns={null} mWaitingApnsPermanentFailureCountDown=0 mApnSetting={null} mReason=radioTurnedOff mDataEnabled=false mDependencyMet=true} dcac=null

06-01 10:53:51.665  2812  2812 D DCT     : [0]stopNetStatPoll

06-01 10:53:51.665  2812  2812 D SubscriptionController: [getSubId]- sSlotIdxToSubId.size == 0, return DummySubIds slotIdx=0

06-01 10:53:51.670  2812  2812 D DCT     : [0]cleanUpConnection: mDisconnectPendingCount = 0

06-01 10:53:51.670  2812  2812 D SubscriptionController: [getSubId]- sSlotIdxToSubId.size == 0, return DummySubIds slotIdx=0

06-01 10:53:51.670  2812  2812 D DCT     : [0]isDataAllowed: not allowed due to - Attached= false - SIM not loaded - SIM not loaded and not NV subscription - defaultDataSelected= false

06-01 10:53:51.670  2812  2812 D SubscriptionController: [getPhoneId]- invalid subId return=-1

06-01 10:53:51.670  2812  2812 D SubscriptionController: [getSubId]- sSlotIdxToSubId.size == 0, return DummySubIds slotIdx=0

06-01 10:53:51.670  2812  2812 D DCT     : [0]isDataAllowed: not allowed due to - Attached= false - SIM not loaded - SIM not loaded and not NV subscription - defaultDataSelected= false

06-01 10:53:51.670  2812  2812 D SubscriptionController: [getPhoneId]- invalid subId return=-1

06-01 10:53:51.675  2812  2812 D SubscriptionController: [getSubId]- sSlotIdxToSubId.size == 0, return DummySubIds slotIdx=0

06-01 10:53:51.675  2812  2812 D DCT     : [0]isDataAllowed: not allowed due to - Attached= false - SIM not loaded - SIM not loaded and not NV subscription - defaultDataSelected= false

06-01 10:53:51.675  2812  2812 D SubscriptionController: [getPhoneId]- invalid subId return=-1

06-01 10:53:51.675  2812  2812 D SubscriptionController: [getSubId]- sSlotIdxToSubId.size == 0, return DummySubIds slotIdx=0

06-01 10:53:51.675  2812  2812 D DCT     : [0]isDataAllowed: not allowed due to - Attached= false - SIM not loaded - SIM not loaded and not NV subscription - defaultDataSelected= false

06-01 10:53:51.680  2812  2812 D SubscriptionController: [getPhoneId]- invalid subId return=-1

06-01 10:53:51.680  2812  2812 D SubscriptionController: [getSubId]- sSlotIdxToSubId.size == 0, return DummySubIds slotIdx=0

06-01 10:53:51.680  2812  2812 D DCT     : [0]isDataAllowed: not allowed due to - Attached= false - SIM not loaded - SIM not loaded and not NV subscription - defaultDataSelected= false

06-01 10:53:51.685  2812  2812 D SubscriptionController: [getPhoneId]- invalid subId return=-1

06-01 10:53:51.685  2812  2812 D DCT     : [0]handleMessage msg={ when=-613ms what=270345 obj=android.os.AsyncResult@ecb784c target=com.android.internal.telephony.dataconnection.DcTracker }

06-01 10:53:51.685  2812  2812 D DCT     : [0]onDataConnectionDetached: stop polling and notify detached

06-01 10:53:51.685  2812  2812 D DCT     : [0]stopNetStatPoll

06-01 10:53:51.685  2812  2812 D SubscriptionController: [getSubId]- sSlotIdxToSubId.size == 0, return DummySubIds slotIdx=0

06-01 10:53:51.685  2812  2812 D DCT     : [0]notifyDataConnection: reason=dataDetached

06-01 10:53:51.685  2812  2812 D SubscriptionController: [getSubId]- sSlotIdxToSubId.size == 0, return DummySubIds slotIdx=0

06-01 10:53:51.695  2812  2812 D DCT     : [0]isDataAllowed: not allowed due to - Attached= false - SIM not loaded - SIM not loaded and not NV subscription - defaultDataSelected= false

06-01 10:53:51.695  2812  2812 D SubscriptionController: [getPhoneId]- invalid subId return=-1

06-01 10:53:51.700  2812  2812 D SubscriptionController: [getSubId]- sSlotIdxToSubId.size == 0, return DummySubIds slotIdx=0

06-01 10:53:51.700  2812  2812 D DCT     : [0]isDataAllowed: not allowed due to - Attached= false - SIM not loaded - SIM not loaded and not NV subscription - defaultDataSelected= false

06-01 10:53:51.700  2812  2812 D SubscriptionController: [getPhoneId]- invalid subId return=-1

06-01 10:53:51.700  2812  2812 D SubscriptionController: [getSubId]- sSlotIdxToSubId.size == 0, return DummySubIds slotIdx=0

06-01 10:53:51.700  2812  2812 D DCT     : [0]isDataAllowed: not allowed due to - Attached= false - SIM not loaded - SIM not loaded and not NV subscription - defaultDataSelected= false

06-01 10:53:51.705  2812  2812 D SubscriptionController: [getPhoneId]- invalid subId return=-1

06-01 10:53:51.705  2812  2812 D SubscriptionController: [getSubId]- sSlotIdxToSubId.size == 0, return DummySubIds slotIdx=0

06-01 10:53:51.715  2812  2812 D DCT     : [0]isDataAllowed: not allowed due to - Attached= false - SIM not loaded - SIM not loaded and not NV subscription - defaultDataSelected= false

06-01 10:53:51.735  2812  2812 D SubscriptionController: [getPhoneId]- invalid subId return=-1

06-01 10:53:51.740  2812  2812 D SubscriptionController: [getSubId]- sSlotIdxToSubId.size == 0, return DummySubIds slotIdx=0

06-01 10:53:51.740  2812  2812 D DCT     : [0]isDataAllowed: not allowed due to - Attached= false - SIM not loaded - SIM not loaded and not NV subscription - defaultDataSelected= false

06-01 10:53:51.745  2812  2812 D SubscriptionController: [getPhoneId]- invalid subId return=-1

06-01 10:53:51.745  2812  2812 D DCT     : [0]handleMessage msg={ when=-672ms what=270348 obj=android.os.AsyncResult@2119095 target=com.android.internal.telephony.dataconnection.DcTracker }

06-01 10:53:51.745  2812  2812 D DCT     : [0]onRoamingOff

06-01 10:53:51.745  2812  2812 D SubscriptionController: [getSubId]- sSlotIdxToSubId.size == 0, return DummySubIds slotIdx=0

06-01 10:53:51.745  2812  2812 D DCT     : [0]getDataOnRoamingEnabled: phoneSubId=-2 isDataRoamingEnabled=false

06-01 10:53:51.745  2812  2812 D SubscriptionController: [getSubId]- sSlotIdxToSubId.size == 0, return DummySubIds slotIdx=0

06-01 10:53:51.745  2812  2812 D DCT     : [0]isDataAllowed: not allowed due to - Attached= false - SIM not loaded - SIM not loaded and not NV subscription - defaultDataSelected= false

06-01 10:53:51.750  2812  2812 D SubscriptionController: [getPhoneId]- invalid subId return=-1

06-01 10:53:51.750  2812  2812 D SubscriptionController: [getSubId]- sSlotIdxToSubId.size == 0, return DummySubIds slotIdx=0

06-01 10:53:51.755  2812  2812 D DCT     : [0]isDataAllowed: not allowed due to - Attached= false - SIM not loaded - SIM not loaded and not NV subscription - defaultDataSelected= false

06-01 10:53:51.760  2812  2812 D SubscriptionController: [getPhoneId]- invalid subId return=-1

06-01 10:53:51.765  1964  2329 D use-Rlog/RLOG-RIL-RFS: Wrote 4 nv_data byte(s) at offset 0x1a0009

06-01 10:53:51.765  1964  2329 D use-Rlog/RLOG-RIL-IPC: 

06-01 10:53:51.765  1964  2329 D use-Rlog/RLOG-RIL-IPC: xmm626_sec_modem_rfs_send: Sent RFS message

06-01 10:53:51.765  1964  2329 D use-Rlog/RLOG-RIL-IPC: xmm626_sec_modem_rfs_send: Message: mseq=0x01, command=IPC_RFS_NV_WRITE_ITEM, size=9

06-01 10:53:51.765  1964  2329 D use-Rlog/RLOG-RIL-IPC: ================================= IPC RFS data =================================

06-01 10:53:51.765  1964  2329 D use-Rlog/RLOG-RIL-IPC: [0000]   01 09 00 1A 00 04 00 00  00                        ........ .

06-01 10:53:51.765  1964  2329 D use-Rlog/RLOG-RIL-IPC: ================================================================================

06-01 10:53:51.770  1964  2329 D use-Rlog/RLOG-RIL-IPC: 

06-01 10:53:51.770  1964  2329 D use-Rlog/RLOG-RIL-IPC: xmm626_sec_modem_rfs_recv: Received RFS message

06-01 10:53:51.770  1964  2329 D use-Rlog/RLOG-RIL-IPC: xmm626_sec_modem_rfs_recv: Message: aseq=0x01, command=IPC_RFS_NV_WRITE_ITEM, size=9

06-01 10:53:51.770  1964  2329 D use-Rlog/RLOG-RIL-IPC: ================================= IPC RFS data =================================

06-01 10:53:51.770  1964  2329 D use-Rlog/RLOG-RIL-IPC: [0000]   10 00 1A 00 01 00 00 00  02                        ........ .

06-01 10:53:51.770  1964  2329 D use-Rlog/RLOG-RIL-IPC: ================================================================================

06-01 10:53:51.770  1964  2329 D use-Rlog/RLOG-RIL-IPC: Checked nv_data path

06-01 10:53:51.775  2812  2812 D SubscriptionController: [getSubId]- sSlotIdxToSubId.size == 0, return DummySubIds slotIdx=0

06-01 10:53:51.780  2812  2812 D DCT     : [0]isDataAllowed: not allowed due to - Attached= false - SIM not loaded - SIM not loaded and not NV subscription - defaultDataSelected= false

06-01 10:53:51.785  2812  2812 D SubscriptionController: [getPhoneId]- invalid subId return=-1

06-01 10:53:51.815  2812  2812 D SubscriptionController: [getSubId]- sSlotIdxToSubId.size == 0, return DummySubIds slotIdx=0

06-01 10:53:51.815  2335  2335 D TelephonyRegistry: notifyCellLocationForSubscriber: subId=0 cellLocation=Bundle[{}]

06-01 10:53:51.815  2812  2812 D DCT     : [0]isDataAllowed: not allowed due to - Attached= false - SIM not loaded - SIM not loaded and not NV subscription - defaultDataSelected= false

06-01 10:53:51.830  2812  2846 D SubscriptionController: [getPhoneId]- no sims, returning default phoneId=2147483647

06-01 10:53:51.830  2812  2812 D SubscriptionController: [getPhoneId]- invalid subId return=-1

06-01 10:53:51.835  2812  2812 D SubscriptionController: [getSubId]- sSlotIdxToSubId.size == 0, return DummySubIds slotIdx=0

06-01 10:53:51.835  2812  2812 D DCT     : [0]isDataAllowed: not allowed due to - Attached= false - SIM not loaded - SIM not loaded and not NV subscription - defaultDataSelected= false

06-01 10:53:51.835  2812  2812 D SubscriptionController: [getPhoneId]- invalid subId return=-1

06-01 10:53:51.835  2812  2812 D DCT     : [0]setupDataOnConnectableApns: roamingOff

06-01 10:53:51.835  2812  2812 D DCT     : [0]setupDataOnConnectableApns: apnContext {mApnType=dun mState=IDLE mWaitingApns={null} mWaitingApnsPermanentFailureCountDown=0 mApnSetting={null} mReason=radioTurnedOff mDataEnabled=false mDependencyMet=true}

06-01 10:53:51.835  2812  2812 D DCT     : [0]setupDataOnConnectableApns: apnContext {mApnType=hipri mState=IDLE mWaitingApns={null} mWaitingApnsPermanentFailureCountDown=0 mApnSetting={null} mReason=radioTurnedOff mDataEnabled=false mDependencyMet=true}

06-01 10:53:51.835  2812  2812 D DCT     : [0]setupDataOnConnectableApns: apnContext {mApnType=supl mState=IDLE mWaitingApns={null} mWaitingApnsPermanentFailureCountDown=0 mApnSetting={null} mReason=radioTurnedOff mDataEnabled=false mDependencyMet=true}

06-01 10:53:51.835  2812  2812 D DCT     : [0]setupDataOnConnectableApns: apnContext {mApnType=default mState=IDLE mWaitingApns={null} mWaitingApnsPermanentFailureCountDown=0 mApnSetting={null} mReason=radioTurnedOff mDataEnabled=false mDependencyMet=true}

06-01 10:53:51.835  2812  2812 D DCT     : [0]setupDataOnConnectableApns: apnContext {mApnType=mms mState=IDLE mWaitingApns={null} mWaitingApnsPermanentFailureCountDown=0 mApnSetting={null} mReason=radioTurnedOff mDataEnabled=false mDependencyMet=true}

06-01 10:53:51.835  2812  2812 D DCT     : [0]handleMessage msg={ when=-762ms what=270377 obj=android.os.AsyncResult@654059b target=com.android.internal.telephony.dataconnection.DcTracker }

06-01 10:53:51.835  2812  2812 D DCT     : [0]onUpdateIcc: newIccRecords null

06-01 10:53:51.835  2812  2812 D DCT     : [0]setupDataOnConnectableApns: nwTypeChanged

06-01 10:53:51.835  2812  2812 D DCT     : [0]setupDataOnConnectableApns: apnContext {mApnType=dun mState=IDLE mWaitingApns={null} mWaitingApnsPermanentFailureCountDown=0 mApnSetting={null} mReason=radioTurnedOff mDataEnabled=false mDependencyMet=true}

06-01 10:53:51.835  2812  2812 D DCT     : [0]setupDataOnConnectableApns: apnContext {mApnType=hipri mState=IDLE mWaitingApns={null} mWaitingApnsPermanentFailureCountDown=0 mApnSetting={null} mReason=radioTurnedOff mDataEnabled=false mDependencyMet=true}

06-01 10:53:51.835  2812  2812 D DCT     : [0]setupDataOnConnectableApns: apnContext {mApnType=supl mState=IDLE mWaitingApns={null} mWaitingApnsPermanentFailureCountDown=0 mApnSetting={null} mReason=radioTurnedOff mDataEnabled=false mDependencyMet=true}

06-01 10:53:51.835  2812  2812 D DCT     : [0]setupDataOnConnectableApns: apnContext {mApnType=default mState=IDLE mWaitingApns={null} mWaitingApnsPermanentFailureCountDown=0 mApnSetting={null} mReason=radioTurnedOff mDataEnabled=false mDependencyMet=true}

06-01 10:53:51.835  2812  2812 D DCT     : [0]setupDataOnConnectableApns: apnContext {mApnType=mms mState=IDLE mWaitingApns={null} mWaitingApnsPermanentFailureCountDown=0 mApnSetting={null} mReason=radioTurnedOff mDataEnabled=false mDependencyMet=true}

06-01 10:53:51.835  2812  2812 D RILJ    : [3662]> BASEBAND_VERSION [SUB0]

06-01 10:53:51.840  2812  2812 D RILJ    : [3663]> GET_IMEI [SUB0]

06-01 10:53:51.840  2812  2812 D RILJ    : [3664]> GET_IMEISV [SUB0]

06-01 10:53:51.840  2812  2812 D RILJ    : [3665]> RIL_REQUEST_GET_RADIO_CAPABILITY [SUB0]

06-01 10:53:51.840  2812  2812 D RILJ    : [3666]> RIL_REQUEST_START_LCE [SUB0]

06-01 10:53:51.845  2812  2812 D RILJ    : [3667]> RIL_REQUEST_VOICE_RADIO_TECH [SUB0]

06-01 10:53:51.845  2812  2812 D SubscriptionController: [getSubId]- sSlotIdxToSubId.size == 0, return DummySubIds slotIdx=0

06-01 10:53:51.845  2812  2812 D GsmSMSDispatcher: GsmSMSDispatcher: subId = -2 slotId = 0

06-01 10:53:51.845  2812  2812 E IccCardProxy: setExternalState: !override and newstate unchanged from NOT_READY

06-01 10:53:51.845  2812  2812 E IccCardProxy: setExternalState: !override and newstate unchanged from NOT_READY

06-01 10:53:51.845  2812  2812 D DctController: EVENT_PHONE1_DATA_DETACH.

06-01 10:53:51.845  2812  2992 D DcSwitchSM: [DcSwitchStateMachine-0] DefaultState: shouldn't happen but ignore msg.what=0x44008

06-01 10:53:51.845  2812  2812 D SubscriptionController: [getSubId]- sSlotIdxToSubId.size == 0, return DummySubIds slotIdx=0

06-01 10:53:51.845  2812  2812 D DctController: [TNF -2]got request NetworkRequest [ id=1, legacyType=-1, [ Capabilities: INTERNET&NOT_RESTRICTED&TRUSTED&NOT_VPN] ] with score 0

06-01 10:53:51.845  2812  2812 D SubscriptionController: [getSubId]- sSlotIdxToSubId.size == 0, return DummySubIds slotIdx=0

06-01 10:53:51.845  2812  2812 D DctController: [TNF -2]Cellular needs Network for NetworkRequest [ id=1, legacyType=-1, [ Capabilities: INTERNET&NOT_RESTRICTED&TRUSTED&NOT_VPN] ]

06-01 10:53:51.845  2812  2812 D SubscriptionController: [getSubId]- sSlotIdxToSubId.size == 0, return DummySubIds slotIdx=0

06-01 10:53:51.845  2812  2812 D SubscriptionController: [getSubId]- sSlotIdxToSubId.size == 0, return DummySubIds slotIdx=0

06-01 10:53:51.845  2812  2812 D DctController: [TNF -2]Request not useable, pending request.

06-01 10:53:51.845  2812  2812 D SubscriptionInfoUpdater: [Receiver]+

06-01 10:53:51.845  2812  2812 D SubscriptionInfoUpdater: Action: android.intent.action.SIM_STATE_CHANGED

06-01 10:53:51.845  2812  2812 D SubscriptionInfoUpdater: slotId: 0

06-01 10:53:51.845  2812  2812 D SubscriptionInfoUpdater: simStatus: NOT_READY

06-01 10:53:51.845  2812  2812 D SubscriptionInfoUpdater: Ignoring simStatus: NOT_READY

06-01 10:53:51.845  2812  2812 D SubscriptionInfoUpdater: Wait for SIM1 IccId

06-01 10:53:51.845  2812  2812 D SubscriptionInfoUpdater: [Receiver]-

06-01 10:53:51.845  2812  2812 D DebugService: DebugService DebugService:

06-01 10:53:51.865  2812  2812 D SipService: SipService: started!

06-01 10:53:51.895  2812  2812 D SipService: start:

06-01 10:53:51.895  2812  2812 D RILJ    : [3668]> RIL_REQUEST_QUERY_TTY_MODE [SUB0]

06-01 10:53:51.895  2812  2812 D DCT     : [0]handleMessage msg={ when=-353ms what=270369 obj=android.os.AsyncResult@138f276 target=com.android.internal.telephony.dataconnection.DcTracker }

06-01 10:53:51.895  2812  2812 D DCT     : [0]onUpdateIcc: newIccRecords null

06-01 10:53:51.895  2812  2812 D SubscriptionController: [getSubId]- sSlotIdxToSubId.size == 0, return DummySubIds slotIdx=0

06-01 10:53:51.895  2812  2812 D GsmSMSDispatcher: GsmSMSDispatcher: subId = -2 slotId = 0

06-01 10:53:51.895  2812  2812 E IccCardProxy: setExternalState: !override and newstate unchanged from NOT_READY

06-01 10:53:51.895  2812  2812 D GsmSST  : [GsmSST] SubscriptionListener.onSubscriptionInfoChanged

06-01 10:53:51.895  2812  2812 D SubscriptionController: [getSubId]- sSlotIdxToSubId.size == 0, return DummySubIds slotIdx=0

06-01 10:53:51.895  2812  2812 D DCT     : [0]SubscriptionListener.onSubscriptionInfoChanged

06-01 10:53:51.895  2812  2812 D SubscriptionController: [getSubId]- sSlotIdxToSubId.size == 0, return DummySubIds slotIdx=0

06-01 10:53:51.895  2812  2812 D SubscriptionController: [getActiveSubInfoList]+

06-01 10:53:51.905  2812  2812 D SubscriptionController: selection:sim_id>=0 null

06-01 10:53:51.965  2812  2850 D SubscriptionController: [getActiveSubInfoList]+

06-01 10:53:51.970  2812  2850 D SubscriptionController: selection:sim_id>=0 null

06-01 10:53:51.975  2812  2812 D SubscriptionController: [getActiveSubInfoList]- no info return

06-01 10:53:51.980  2812  2812 D SubscriptionController: [getSubId]- sSlotIdxToSubId.size == 0, return DummySubIds slotIdx=0

06-01 10:53:51.985  2812  2812 D SubscriptionController: [getSubId]- sSlotIdxToSubId.size == 0, return DummySubIds slotIdx=0

06-01 10:53:51.985  1964  2329 D use-Rlog/RLOG-RIL-RFS: Wrote 1 nv_data byte(s) at offset 0x1a0010

06-01 10:53:51.985  1964  2329 D use-Rlog/RLOG-RIL-IPC: 

06-01 10:53:51.985  1964  2329 D use-Rlog/RLOG-RIL-IPC: xmm626_sec_modem_rfs_send: Sent RFS message

06-01 10:53:51.985  1964  2329 D use-Rlog/RLOG-RIL-IPC: xmm626_sec_modem_rfs_send: Message: mseq=0x01, command=IPC_RFS_NV_WRITE_ITEM, size=9

06-01 10:53:51.985  1964  2329 D use-Rlog/RLOG-RIL-IPC: ================================= IPC RFS data =================================

06-01 10:53:51.985  1964  2329 D use-Rlog/RLOG-RIL-IPC: [0000]   01 10 00 1A 00 01 00 00  00                        ........ .

06-01 10:53:51.985  1964  2329 D use-Rlog/RLOG-RIL-IPC: ================================================================================

06-01 10:53:51.985  1964  2012 D use-Rlog/RLOG-RIL: 1 RIL request in the queue (1 pending, 0 handled, 0 unhandled)

06-01 10:53:51.985  1964  2012 D use-Rlog/RLOG-RIL: 3 RIL requests data in the queue

06-01 10:53:51.985  1964  2012 D use-Rlog/RLOG-RIL: 2 RIL requests in the queue (2 pending, 0 handled, 0 unhandled)

06-01 10:53:51.985  1964  2012 D use-Rlog/RLOG-RIL: 3 RIL requests data in the queue

06-01 10:53:51.985  1964  2012 D use-Rlog/RLOG-RIL: 3 RIL requests in the queue (3 pending, 0 handled, 0 unhandled)

06-01 10:53:51.985  1964  2012 D use-Rlog/RLOG-RIL: 3 RIL requests data in the queue

06-01 10:53:51.985  1964  2012 D use-Rlog/RLOG-RIL: 4 RIL requests in the queue (4 pending, 0 handled, 0 unhandled)

06-01 10:53:51.985  1964  2012 D use-Rlog/RLOG-RIL: 3 RIL requests data in the queue

06-01 10:53:51.985  1964  2012 D use-Rlog/RLOG-RIL: 5 RIL requests in the queue (5 pending, 0 handled, 0 unhandled)

06-01 10:53:51.985  1964  2012 D use-Rlog/RLOG-RIL: 3 RIL requests data in the queue

06-01 10:53:51.985  1964  2012 D use-Rlog/RLOG-RIL: 6 RIL requests in the queue (6 pending, 0 handled, 0 unhandled)

06-01 10:53:51.985  1964  2012 D use-Rlog/RLOG-RIL: 3 RIL requests data in the queue

06-01 10:53:51.985  2812  2918 D RILJ    : [3667]< RIL_REQUEST_VOICE_RADIO_TECH {3} [SUB0]

06-01 10:53:51.985  1964  2332 D use-Rlog/RLOG-RIL-IPC: 

06-01 10:53:51.985  1964  2332 D use-Rlog/RLOG-RIL-IPC: xmm626_sec_modem_fmt_send: Sent FMT message

06-01 10:53:51.985  1964  2332 D use-Rlog/RLOG-RIL-IPC: xmm626_sec_modem_fmt_send: Message: mseq=0x05, command=IPC_MISC_ME_VERSION, type=IPC_TYPE_GET, size=1

06-01 10:53:51.985  1964  2332 D use-Rlog/RLOG-RIL-IPC: ================================= IPC FMT data =================================

06-01 10:53:51.985  1964  2332 D use-Rlog/RLOG-RIL-IPC: [0000]   FF                                                 .

06-01 10:53:51.985  1964  2332 D use-Rlog/RLOG-RIL-IPC: ================================================================================

06-01 10:53:51.985  1964  2332 D use-Rlog/RLOG-RIL-IPC: 

06-01 10:53:51.985  1964  2332 D use-Rlog/RLOG-RIL-IPC: xmm626_sec_modem_fmt_send: Sent FMT message

06-01 10:53:51.985  1964  2332 D use-Rlog/RLOG-RIL-IPC: xmm626_sec_modem_fmt_send: Message: mseq=0x06, command=IPC_MISC_ME_SN, type=IPC_TYPE_GET, size=1

06-01 10:53:51.985  1964  2332 D use-Rlog/RLOG-RIL-IPC: ================================= IPC FMT data =================================

06-01 10:53:51.985  1964  2332 D use-Rlog/RLOG-RIL-IPC: [0000]   01                                                 .

06-01 10:53:51.985  1964  2332 D use-Rlog/RLOG-RIL-IPC: ================================================================================

06-01 10:53:51.985  1964  2332 D use-Rlog/RLOG-RIL: Unhandled RIL request: 130

06-01 10:53:51.985  1964  2332 D use-Rlog/RLOG-RIL: 5 RIL requests in the queue (2 pending, 3 handled, 0 unhandled)

06-01 10:53:51.985  1964  2332 D use-Rlog/RLOG-RIL: 3 RIL requests data in the queue

06-01 10:53:51.985  1964  2332 D use-Rlog/RLOG-RIL: Unhandled RIL request: 132

06-01 10:53:51.985  1964  2332 D use-Rlog/RLOG-RIL: 4 RIL requests in the queue (1 pending, 3 handled, 0 unhandled)

06-01 10:53:51.985  1964  2332 D use-Rlog/RLOG-RIL: 3 RIL requests data in the queue

06-01 10:53:51.985  1964  2332 D use-Rlog/RLOG-RIL: Unhandled RIL request: 81

06-01 10:53:51.985  1964  2332 D use-Rlog/RLOG-RIL: 3 RIL requests in the queue (0 pending, 3 handled, 0 unhandled)

06-01 10:53:51.985  1964  2332 D use-Rlog/RLOG-RIL: 3 RIL requests data in the queue

06-01 10:53:51.990  2812  2918 D RILJ    : Faking RIL_REQUEST_GET_RADIO_CAPABILITY response using 36366 [SUB0]

06-01 10:53:51.990  2812  2918 D RILJ    : [3665]< RIL_REQUEST_GET_RADIO_CAPABILITY {mPhoneId = 0 mVersion=1 mSession=0 mPhase=0 mRadioAccessFamily=36366 mLogicModemId= mStatus=1} [SUB0]

06-01 10:53:51.990  2812  2918 D RilRequest: [3666]< RIL_REQUEST_START_LCE error: com.android.internal.telephony.CommandException: REQUEST_NOT_SUPPORTED ret=

06-01 10:53:51.990  2812  2918 D RilRequest: [3668]< RIL_REQUEST_QUERY_TTY_MODE error: com.android.internal.telephony.CommandException: REQUEST_NOT_SUPPORTED ret=

06-01 10:53:51.990  2812  2850 D SubscriptionController: [getActiveSubInfoList]- no info return

06-01 10:53:51.995  2812  3017 D SubscriptionController: [getActiveSubInfoList]+

06-01 10:53:51.995  2812  3017 D SubscriptionController: selection:sim_id>=0 null

06-01 10:53:52.000  2812  2812 D SubscriptionController: [getPhoneId]- invalid subId return=-1

06-01 10:53:52.000  2812  2812 D SubscriptionController: [getSubId]- sSlotIdxToSubId.size == 0, return DummySubIds slotIdx=0

06-01 10:53:52.005  2812  2812 D SubscriptionController: [getSubId]- sSlotIdxToSubId.size == 0, return DummySubIds slotIdx=0

06-01 10:53:52.005  2812  2812 D SubscriptionController: [getSubId]- sSlotIdxToSubId.size == 0, return DummySubIds slotIdx=0

06-01 10:53:52.040  2812  3017 D SubscriptionController: [getActiveSubInfoList]- no info return

06-01 10:53:52.040  1964  2328 D use-Rlog/RLOG-RIL-IPC: 

06-01 10:53:52.040  1964  2328 D use-Rlog/RLOG-RIL-IPC: xmm626_sec_modem_fmt_recv: Received FMT message

06-01 10:53:52.040  1964  2328 D use-Rlog/RLOG-RIL-IPC: xmm626_sec_modem_fmt_recv: Message: aseq=0x05, command=IPC_MISC_ME_VERSION, type=IPC_TYPE_RESP, size=148

06-01 10:53:52.040  1964  2328 D use-Rlog/RLOG-RIL-IPC: ================================= IPC FMT data =================================

06-01 10:53:52.040  1964  2328 D use-Rlog/RLOG-RIL-IPC: [0000]   1F 49 39 33 30 30 58 58  55 47 4E 41 38 00 00 00   .I9300XX UGNA8...

06-01 10:53:52.040  1964  2328 D use-Rlog/RLOG-RIL-IPC: [0010]   00 00 00 00 00 00 00 00  00 00 00 00 00 00 00 00   ........ ........

06-01 10:53:52.040  1964  2328 D use-Rlog/RLOG-RIL-IPC: [0020]   00 4D 50 20 31 2E 31 30  30 00 00 00 00 00 00 00   .MP 1.10 0.......

06-01 10:53:52.040  1964  2328 D use-Rlog/RLOG-RIL-IPC: [0030]   00 00 00 00 00 00 00 00  00 00 00 00 00 00 00 00   ........ ........

06-01 10:53:52.040  1964  2328 D use-Rlog/RLOG-RIL-IPC: [0040]   00 32 30 31 32 2E 37 2E  34 00 00 00 00 00 00 00   .2012.7. 4.......

06-01 10:53:52.040  1964  2328 D use-Rlog/RLOG-RIL-IPC: [0050]   00 00 00 00 00 00 00 00  00 00 00 00 00 00 00 00   ........ ........

06-01 10:53:52.040  1964  2328 D use-Rlog/RLOG-RIL-IPC: [0060]   00 47 54 2D 49 39 33 30  30 4D 42 44 43 59 4F 00   .GT-I930 0MBDCYO.

06-01 10:53:52.040  1964  2328 D use-Rlog/RLOG-RIL-IPC: [0070]   00 00 00 00 00 00 00 00  00 00 00 00 00 00 00 00   ........ ........

06-01 10:53:52.040  1964  2328 D use-Rlog/RLOG-RIL-IPC: [0080]   00 49 39 33 30 30 00 00  00 00 00 00 00 00 00 00   .I9300.. ........

06-01 10:53:52.040  1964  2328 D use-Rlog/RLOG-RIL-IPC: [0090]   00 00 00 00                                        ....

06-01 10:53:52.040  1964  2328 D use-Rlog/RLOG-RIL-IPC: ================================================================================

06-01 10:53:52.040  1964  2328 D use-Rlog/RLOG-RIL: 2 RIL requests in the queue (0 pending, 2 handled, 0 unhandled)

06-01 10:53:52.040  1964  2328 D use-Rlog/RLOG-RIL: 3 RIL requests data in the queue

06-01 10:53:52.040  1964  2328 D use-Rlog/RLOG-RIL-IPC: 

06-01 10:53:52.040  1964  2328 D use-Rlog/RLOG-RIL-IPC: xmm626_sec_modem_fmt_recv: Received FMT message

06-01 10:53:52.040  1964  2328 D use-Rlog/RLOG-RIL-IPC: xmm626_sec_modem_fmt_recv: Message: aseq=0x06, command=IPC_MISC_ME_SN, type=IPC_TYPE_RESP, size=34

06-01 10:53:52.040  1964  2328 D use-Rlog/RLOG-RIL-IPC: ================================= IPC FMT data =================================

06-01 10:53:52.040  1964  2328 D use-Rlog/RLOG-RIL-IPC: [0000]   01 11 33 35 33 38 31 37  30 35 31 38 32 38 37 31   ..353817 05182871

06-01 10:53:52.040  1964  2328 D use-Rlog/RLOG-RIL-IPC: [0010]   33 30 31 00 00 00 00 00  00 00 00 00 00 00 00 00   301..... ........

06-01 10:53:52.040  1964  2328 D use-Rlog/RLOG-RIL-IPC: [0020]   00 4D                                              .M

06-01 10:53:52.040  1964  2328 D use-Rlog/RLOG-RIL-IPC: ================================================================================

06-01 10:53:52.045  1964  2328 D use-Rlog/RLOG-RIL: 1 RIL request in the queue (0 pending, 1 handled, 0 unhandled)

06-01 10:53:52.045  1964  2328 D use-Rlog/RLOG-RIL: 3 RIL requests data in the queue

06-01 10:53:52.045  1964  2328 D use-Rlog/RLOG-RIL: 0 RIL request in the queue (0 pending, 0 handled, 0 unhandled)

06-01 10:53:52.045  1964  2328 D use-Rlog/RLOG-RIL: 3 RIL requests data in the queue

06-01 10:53:52.045  2812  2918 D RILJ    : [3662]< BASEBAND_VERSION I9300XXUGNA8 [SUB0]

06-01 10:53:52.045  2812  2918 D RILJ    : [3663]< GET_IMEI  [SUB0]

06-01 10:53:52.045  2812  2918 D RILJ    : [3664]< GET_IMEISV  [SUB0]

06-01 10:53:52.045  2812  2850 D SubscriptionController: [getActiveSubInfoList]+

06-01 10:53:52.060  2812  2850 D SubscriptionController: selection:sim_id>=0 null

06-01 10:53:52.115  2812  2850 D SubscriptionController: [getActiveSubInfoList]- no info return

06-01 10:53:52.150  2812  2812 E PhoneBase: Error! registerForCallWaiting() in PhoneBase should not be called, CDMAPhone inactive.

06-01 10:53:52.210  2812  2812 D SubscriptionController: [getSubId]- sSlotIdxToSubId.size == 0, return DummySubIds slotIdx=0

06-01 10:53:52.210  2812  2812 D DCT     : [0]handleMessage msg={ when=-595ms what=270377 obj=android.os.AsyncResult@f76f8dc target=com.android.internal.telephony.dataconnection.DcTracker }

06-01 10:53:52.210  2812  2812 D DCT     : [0]onUpdateIcc: newIccRecords null

06-01 10:53:52.210  2812  2812 D DCT     : [0]setupDataOnConnectableApns: nwTypeChanged

06-01 10:53:52.210  2812  2812 D DCT     : [0]setupDataOnConnectableApns: apnContext {mApnType=dun mState=IDLE mWaitingApns={null} mWaitingApnsPermanentFailureCountDown=0 mApnSetting={null} mReason=radioTurnedOff mDataEnabled=false mDependencyMet=true}

06-01 10:53:52.210  2812  2812 D DCT     : [0]setupDataOnConnectableApns: apnContext {mApnType=hipri mState=IDLE mWaitingApns={null} mWaitingApnsPermanentFailureCountDown=0 mApnSetting={null} mReason=radioTurnedOff mDataEnabled=false mDependencyMet=true}

06-01 10:53:52.210  2812  2812 D DCT     : [0]setupDataOnConnectableApns: apnContext {mApnType=supl mState=IDLE mWaitingApns={null} mWaitingApnsPermanentFailureCountDown=0 mApnSetting={null} mReason=radioTurnedOff mDataEnabled=false mDependencyMet=true}

06-01 10:53:52.210  2812  2812 D DCT     : [0]setupDataOnConnectableApns: apnContext {mApnType=default mState=IDLE mWaitingApns={null} mWaitingApnsPermanentFailureCountDown=0 mApnSetting={null} mReason=radioTurnedOff mDataEnabled=false mDependencyMet=true}

06-01 10:53:52.210  2812  2812 D DCT     : [0]setupDataOnConnectableApns: apnContext {mApnType=mms mState=IDLE mWaitingApns={null} mWaitingApnsPermanentFailureCountDown=0 mApnSetting={null} mReason=radioTurnedOff mDataEnabled=false mDependencyMet=true}

06-01 10:53:52.210  2812  2812 D SubscriptionController: [getSubId]- sSlotIdxToSubId.size == 0, return DummySubIds slotIdx=0

06-01 10:53:52.210  2812  2812 D DCT     : [0]getDataOnRoamingEnabled: phoneSubId=-2 isDataRoamingEnabled=false

06-01 10:53:52.210  2812  2812 D SubscriptionController: [getSubId]- sSlotIdxToSubId.size == 0, return DummySubIds slotIdx=0

06-01 10:53:52.210  2812  2812 D DCT     : [0]getDataOnRoamingEnabled: phoneSubId=-2 isDataRoamingEnabled=false

06-01 10:53:52.210  2812  2812 D PhoneProxy: [PhoneProxy] EVENT_VOICE_RADIO_TECH_CHANGED: newVoiceTech=3

06-01 10:53:52.210  2812  2812 D PhoneProxy: [PhoneProxy] phoneObjectUpdater: newVoiceRadioTech=3

06-01 10:53:52.210  2812  2812 D PhoneProxy: [PhoneProxy] phoneObjectUpdater: No change ignore, newVoiceRadioTech=3 mActivePhone=GSM

06-01 10:53:52.210  2812  2812 D GsmSST  : [GsmSST] mDeviceShuttingDown = false

06-01 10:53:52.210  2812  2812 D GsmSST  : [GsmSST] mDesiredPowerState = true

06-01 10:53:52.210  2812  2812 D GsmSST  : [GsmSST] getRadioState = RADIO_ON

06-01 10:53:52.210  2812  2812 D GsmSST  : [GsmSST] mPowerOffDelayNeed = true

06-01 10:53:52.210  2812  2812 D GsmSST  : [GsmSST] mAlarmSwitch = false

06-01 10:53:52.210  2812  2812 D RILJ    : [3669]> OPERATOR [SUB0]

06-01 10:53:52.215  1964  2012 D use-Rlog/RLOG-RIL: 1 RIL request in the queue (1 pending, 0 handled, 0 unhandled)

06-01 10:53:52.215  1964  2012 D use-Rlog/RLOG-RIL: 3 RIL requests data in the queue

06-01 10:53:52.215  1964  2332 D use-Rlog/RLOG-RIL-IPC: 

06-01 10:53:52.215  1964  2332 D use-Rlog/RLOG-RIL-IPC: xmm626_sec_modem_fmt_send: Sent FMT message

06-01 10:53:52.215  1964  2332 D use-Rlog/RLOG-RIL-IPC: xmm626_sec_modem_fmt_send: Message: mseq=0x07, command=IPC_NET_SERVING_NETWORK, type=IPC_TYPE_GET, size=0

06-01 10:53:52.215  2812  2812 D RILJ    : [3670]> DATA_REGISTRATION_STATE [SUB0]

06-01 10:53:52.215  1964  2012 D use-Rlog/RLOG-RIL: 2 RIL requests in the queue (1 pending, 1 handled, 0 unhandled)

06-01 10:53:52.215  1964  2012 D use-Rlog/RLOG-RIL: 3 RIL requests data in the queue

06-01 10:53:52.215  1964  2332 D use-Rlog/RLOG-RIL: 1 RIL request in the queue (0 pending, 1 handled, 0 unhandled)

06-01 10:53:52.215  1964  2332 D use-Rlog/RLOG-RIL: 2 RIL requests data in the queue

06-01 10:53:52.215  2812  2918 D RILJ    : [3670]< DATA_REGISTRATION_STATE {0, 0, 0, 0, 3} [SUB0]

06-01 10:53:52.215  1964  2328 D use-Rlog/RLOG-RIL-IPC: 

06-01 10:53:52.215  1964  2328 D use-Rlog/RLOG-RIL-IPC: xmm626_sec_modem_fmt_recv: Received FMT message

06-01 10:53:52.215  1964  2328 D use-Rlog/RLOG-RIL-IPC: xmm626_sec_modem_fmt_recv: Message: aseq=0x07, command=IPC_NET_SERVING_NETWORK, type=IPC_TYPE_RESP, size=11

06-01 10:53:52.215  1964  2328 D use-Rlog/RLOG-RIL-IPC: ================================= IPC FMT data =================================

06-01 10:53:52.215  1964  2328 D use-Rlog/RLOG-RIL-IPC: [0000]   02 04 FF 32 30 36 31 30  23 00 00                  ...20610 #..

06-01 10:53:52.215  1964  2328 D use-Rlog/RLOG-RIL-IPC: ================================================================================

06-01 10:53:52.215  1964  2328 D use-Rlog/RLOG-RIL: 0 RIL request in the queue (0 pending, 0 handled, 0 unhandled)

06-01 10:53:52.215  1964  2328 D use-Rlog/RLOG-RIL: 2 RIL requests data in the queue

06-01 10:53:52.215  2812  2918 D RILJ    : [3669]< OPERATOR {Mobistar, Mobistar, 20610} [SUB0]

06-01 10:53:52.215  2812  2812 D RILJ    : [3671]> VOICE_REGISTRATION_STATE [SUB0]

06-01 10:53:52.220  1964  2012 D use-Rlog/RLOG-RIL: 1 RIL request in the queue (1 pending, 0 handled, 0 unhandled)

06-01 10:53:52.220  1964  2012 D use-Rlog/RLOG-RIL: 2 RIL requests data in the queue

06-01 10:53:52.220  1964  2332 D use-Rlog/RLOG-RIL: 0 RIL request in the queue (0 pending, 0 handled, 0 unhandled)

06-01 10:53:52.220  1964  2332 D use-Rlog/RLOG-RIL: 1 RIL request data in the queue

06-01 10:53:52.220  2812  2918 D RILJ    : [3671]< VOICE_REGISTRATION_STATE {10, 0, 0, 0, null, null, null, null, null, null, null, null, null, null, null} [SUB0]

06-01 10:53:52.220  2812  2812 D RILJ    : [3672]> QUERY_NETWORK_SELECTION_MODE [SUB0]

06-01 10:53:52.225  2812  2812 D UiccController: Received EVENT_ICC_STATUS_CHANGED, calling getIccCardStatus

06-01 10:53:52.225  2812  2812 D RILJ    : [3673]> GET_SIM_STATUS [SUB0]

06-01 10:53:52.225  1964  2012 D use-Rlog/RLOG-RIL: 1 RIL request in the queue (1 pending, 0 handled, 0 unhandled)

06-01 10:53:52.225  1964  2012 D use-Rlog/RLOG-RIL: 1 RIL request data in the queue

06-01 10:53:52.225  1964  2332 D use-Rlog/RLOG-RIL-IPC: 

06-01 10:53:52.225  1964  2332 D use-Rlog/RLOG-RIL-IPC: xmm626_sec_modem_fmt_send: Sent FMT message

06-01 10:53:52.225  1964  2332 D use-Rlog/RLOG-RIL-IPC: xmm626_sec_modem_fmt_send: Message: mseq=0x08, command=IPC_NET_PLMN_SEL, type=IPC_TYPE_GET, size=0

06-01 10:53:52.225  2812  2812 D RILJ    : [3674]> GET_CURRENT_CALLS [SUB0]

06-01 10:53:52.225  1964  2328 D use-Rlog/RLOG-RIL-IPC: 

06-01 10:53:52.225  1964  2328 D use-Rlog/RLOG-RIL-IPC: xmm626_sec_modem_fmt_recv: Received FMT message

06-01 10:53:52.225  1964  2328 D use-Rlog/RLOG-RIL-IPC: xmm626_sec_modem_fmt_recv: Message: aseq=0x08, command=IPC_NET_PLMN_SEL, type=IPC_TYPE_RESP, size=1

06-01 10:53:52.225  1964  2328 D use-Rlog/RLOG-RIL-IPC: ================================= IPC FMT data =================================

06-01 10:53:52.225  1964  2328 D use-Rlog/RLOG-RIL-IPC: [0000]   02                                                 .

06-01 10:53:52.225  1964  2328 D use-Rlog/RLOG-RIL-IPC: ================================================================================

06-01 10:53:52.225  1964  2328 D use-Rlog/RLOG-RIL: 0 RIL request in the queue (0 pending, 0 handled, 0 unhandled)

06-01 10:53:52.225  1964  2328 D use-Rlog/RLOG-RIL: 1 RIL request data in the queue

06-01 10:53:52.225  2812  2918 D RILJ    : [3672]< QUERY_NETWORK_SELECTION_MODE {0} [SUB0]

06-01 10:53:52.225  1964  2012 D use-Rlog/RLOG-RIL: 1 RIL request in the queue (1 pending, 0 handled, 0 unhandled)

06-01 10:53:52.225  1964  2012 D use-Rlog/RLOG-RIL: 1 RIL request data in the queue

06-01 10:53:52.225  1964  2332 D use-Rlog/RLOG-RIL: 0 RIL request in the queue (0 pending, 0 handled, 0 unhandled)

06-01 10:53:52.225  2812  2812 D SubscriptionController: [getSubId]- sSlotIdxToSubId.size == 0, return DummySubIds slotIdx=0

06-01 10:53:52.225  2812  2812 D RILJ    : [3675]> RIL_REQUEST_VOICE_RADIO_TECH [SUB0]

06-01 10:53:52.225  1964  2012 D use-Rlog/RLOG-RIL: 1 RIL request in the queue (1 pending, 0 handled, 0 unhandled)

06-01 10:53:52.225  1964  2332 D use-Rlog/RLOG-RIL-IPC: 

06-01 10:53:52.225  1964  2332 D use-Rlog/RLOG-RIL-IPC: xmm626_sec_modem_fmt_send: Sent FMT message

06-01 10:53:52.225  1964  2332 D use-Rlog/RLOG-RIL-IPC: xmm626_sec_modem_fmt_send: Message: mseq=0x09, command=IPC_CALL_LIST, type=IPC_TYPE_GET, size=0

06-01 10:53:52.225  2812  2812 D RILJ    : [3676]> RIL_REQUEST_IMS_REGISTRATION_STATE [SUB0]

06-01 10:53:52.230  1964  2328 D use-Rlog/RLOG-RIL-IPC: 

06-01 10:53:52.230  1964  2328 D use-Rlog/RLOG-RIL-IPC: xmm626_sec_modem_fmt_recv: Received FMT message

06-01 10:53:52.230  1964  2328 D use-Rlog/RLOG-RIL-IPC: xmm626_sec_modem_fmt_recv: Message: aseq=0x09, command=IPC_CALL_LIST, type=IPC_TYPE_RESP, size=1

06-01 10:53:52.230  1964  2328 D use-Rlog/RLOG-RIL-IPC: ================================= IPC FMT data =================================

06-01 10:53:52.230  1964  2328 D use-Rlog/RLOG-RIL-IPC: [0000]   00                                                 .

06-01 10:53:52.230  1964  2328 D use-Rlog/RLOG-RIL-IPC: ================================================================================

06-01 10:53:52.230  1964  2328 D use-Rlog/RLOG-RIL: 0 RIL request in the queue (0 pending, 0 handled, 0 unhandled)

06-01 10:53:52.230  2812  2812 D RILJ    : [3677]> RIL_REQUEST_CDMA_GET_SUBSCRIPTION_SOURCE [SUB0]

06-01 10:53:52.230  1964  2012 D use-Rlog/RLOG-RIL: 1 RIL request in the queue (1 pending, 0 handled, 0 unhandled)

06-01 10:53:52.230  1964  2332 D use-Rlog/RLOG-RIL: Unhandled RIL request: 112

06-01 10:53:52.230  1964  2332 D use-Rlog/RLOG-RIL: 0 RIL request in the queue (0 pending, 0 handled, 0 unhandled)

06-01 10:53:52.235  2812  2812 D UiccController: Received EVENT_ICC_STATUS_CHANGED, calling getIccCardStatus

06-01 10:53:52.235  2812  2812 D RILJ    : [3678]> GET_SIM_STATUS [SUB0]

06-01 10:53:52.235  2812  2812 D UiccController: Received EVENT_ICC_STATUS_CHANGED, calling getIccCardStatus

06-01 10:53:52.235  2812  2812 D RILJ    : [3679]> GET_SIM_STATUS [SUB0]

06-01 10:53:52.240  1964  2012 D use-Rlog/RLOG-RIL: 1 RIL request in the queue (1 pending, 0 handled, 0 unhandled)

06-01 10:53:52.240  1964  2332 D use-Rlog/RLOG-RIL-IPC: 

06-01 10:53:52.240  1964  2332 D use-Rlog/RLOG-RIL-IPC: xmm626_sec_modem_fmt_send: Sent FMT message

06-01 10:53:52.240  1964  2332 D use-Rlog/RLOG-RIL-IPC: xmm626_sec_modem_fmt_send: Message: mseq=0x0a, command=IPC_SEC_PIN_STATUS, type=IPC_TYPE_GET, size=0

06-01 10:53:52.240  2812  2918 D RILJ    : [3673]< GET_SIM_STATUS IccCardState {CARDSTATE_PRESENT,PINSTATE_UNKNOWN,num_apps=1,gsm_id=0{APPTYPE_SIM,APPSTATE_PIN},cdma_id=-1,ims_id=-1} [SUB0]

06-01 10:53:52.240  1964  2328 D use-Rlog/RLOG-RIL-IPC: 

06-01 10:53:52.240  1964  2328 D use-Rlog/RLOG-RIL-IPC: xmm626_sec_modem_fmt_recv: Received FMT message

06-01 10:53:52.240  1964  2328 D use-Rlog/RLOG-RIL-IPC: xmm626_sec_modem_fmt_recv: Message: aseq=0x0a, command=IPC_SEC_PIN_STATUS, type=IPC_TYPE_RESP, size=2

06-01 10:53:52.240  1964  2328 D use-Rlog/RLOG-RIL-IPC: ================================= IPC FMT data =================================

06-01 10:53:52.240  1964  2328 D use-Rlog/RLOG-RIL-IPC: [0000]   03 01                                              ..

06-01 10:53:52.240  1964  2328 D use-Rlog/RLOG-RIL-IPC: ================================================================================

06-01 10:53:52.240  1964  2328 D use-Rlog/RLOG-RIL: ipc2ril_sec_pin_status_response: Selecting status application 3 on 10

06-01 10:53:52.240  1964  2328 D use-Rlog/RLOG-RIL: 0 RIL request in the queue (0 pending, 0 handled, 0 unhandled)

06-01 10:53:52.245  2812  2812 D RILJ    : [3680]> OPERATOR [SUB0]

06-01 10:53:52.245  1964  2012 D use-Rlog/RLOG-RIL: 1 RIL request in the queue (1 pending, 0 handled, 0 unhandled)

06-01 10:53:52.245  1964  2332 D use-Rlog/RLOG-RIL-IPC: 

06-01 10:53:52.245  1964  2332 D use-Rlog/RLOG-RIL-IPC: xmm626_sec_modem_fmt_send: Sent FMT message

06-01 10:53:52.245  1964  2332 D use-Rlog/RLOG-RIL-IPC: xmm626_sec_modem_fmt_send: Message: mseq=0x0b, command=IPC_SEC_PIN_STATUS, type=IPC_TYPE_GET, size=0

06-01 10:53:52.250  2812  2812 D RILJ    : [3681]> DATA_REGISTRATION_STATE [SUB0]

06-01 10:53:52.250  2812  2812 D RILJ    : [3682]> VOICE_REGISTRATION_STATE [SUB0]

06-01 10:53:52.250  1964  2012 D use-Rlog/RLOG-RIL: 2 RIL requests in the queue (1 pending, 1 handled, 0 unhandled)

06-01 10:53:52.250  1964  2012 D use-Rlog/RLOG-RIL: 3 RIL requests in the queue (2 pending, 1 handled, 0 unhandled)

06-01 10:53:52.250  1964  2332 D use-Rlog/RLOG-RIL-IPC: 

06-01 10:53:52.250  1964  2332 D use-Rlog/RLOG-RIL-IPC: xmm626_sec_modem_fmt_send: Sent FMT message

06-01 10:53:52.250  1964  2332 D use-Rlog/RLOG-RIL-IPC: xmm626_sec_modem_fmt_send: Message: mseq=0x0c, command=IPC_NET_SERVING_NETWORK, type=IPC_TYPE_GET, size=0

06-01 10:53:52.250  1964  2332 D use-Rlog/RLOG-RIL-IPC: 

06-01 10:53:52.250  1964  2332 D use-Rlog/RLOG-RIL-IPC: xmm626_sec_modem_fmt_send: Sent FMT message

06-01 10:53:52.250  1964  2332 D use-Rlog/RLOG-RIL-IPC: xmm626_sec_modem_fmt_send: Message: mseq=0x0d, command=IPC_NET_REGIST, type=IPC_TYPE_GET, size=2

06-01 10:53:52.250  1964  2332 D use-Rlog/RLOG-RIL-IPC: ================================= IPC FMT data =================================

06-01 10:53:52.250  1964  2332 D use-Rlog/RLOG-RIL-IPC: [0000]   FF 03                                              ..

06-01 10:53:52.250  1964  2332 D use-Rlog/RLOG-RIL-IPC: ================================================================================

06-01 10:53:52.250  2812  2812 D RILJ    : [3683]> QUERY_NETWORK_SELECTION_MODE [SUB0]

06-01 10:53:52.250  1964  2012 D use-Rlog/RLOG-RIL: 4 RIL requests in the queue (1 pending, 3 handled, 0 unhandled)

06-01 10:53:52.250  1964  2332 D use-Rlog/RLOG-RIL-IPC: 

06-01 10:53:52.250  1964  2332 D use-Rlog/RLOG-RIL-IPC: xmm626_sec_modem_fmt_send: Sent FMT message

06-01 10:53:52.250  1964  2332 D use-Rlog/RLOG-RIL-IPC: xmm626_sec_modem_fmt_send: Message: mseq=0x0e, command=IPC_NET_REGIST, type=IPC_TYPE_GET, size=2

06-01 10:53:52.250  1964  2332 D use-Rlog/RLOG-RIL-IPC: ================================= IPC FMT data =================================

06-01 10:53:52.250  1964  2332 D use-Rlog/RLOG-RIL-IPC: [0000]   FF 02                                              ..

06-01 10:53:52.250  1964  2332 D use-Rlog/RLOG-RIL-IPC: ================================================================================

06-01 10:53:52.250  2812  2812 D RILJ    : [3684]> OPERATOR [SUB0]

06-01 10:53:52.255  1964  2012 D use-Rlog/RLOG-RIL: 5 RIL requests in the queue (1 pending, 4 handled, 0 unhandled)

06-01 10:53:52.255  1964  2332 D use-Rlog/RLOG-RIL-IPC: 

06-01 10:53:52.255  1964  2332 D use-Rlog/RLOG-RIL-IPC: xmm626_sec_modem_fmt_send: Sent FMT message

06-01 10:53:52.255  1964  2332 D use-Rlog/RLOG-RIL-IPC: xmm626_sec_modem_fmt_send: Message: mseq=0x0f, command=IPC_NET_PLMN_SEL, type=IPC_TYPE_GET, size=0

06-01 10:53:52.255  1964  2328 D use-Rlog/RLOG-RIL-IPC: 

06-01 10:53:52.255  1964  2328 D use-Rlog/RLOG-RIL-IPC: xmm626_sec_modem_fmt_recv: Received FMT message

06-01 10:53:52.255  1964  2328 D use-Rlog/RLOG-RIL-IPC: xmm626_sec_modem_fmt_recv: Message: aseq=0x0b, command=IPC_SEC_PIN_STATUS, type=IPC_TYPE_RESP, size=2

06-01 10:53:52.255  1964  2328 D use-Rlog/RLOG-RIL-IPC: ================================= IPC FMT data =================================

06-01 10:53:52.255  1964  2328 D use-Rlog/RLOG-RIL-IPC: [0000]   03 01                                              ..

06-01 10:53:52.255  1964  2328 D use-Rlog/RLOG-RIL-IPC: ================================================================================

06-01 10:53:52.255  1964  2328 D use-Rlog/RLOG-RIL: ipc2ril_sec_pin_status_response: Selecting status application 3 on 10

06-01 10:53:52.255  1964  2328 D use-Rlog/RLOG-RIL: 4 RIL requests in the queue (0 pending, 4 handled, 0 unhandled)

06-01 10:53:52.255  2812  2812 D RILJ    : [3685]> DATA_REGISTRATION_STATE [SUB0]

06-01 10:53:52.255  1964  2012 D use-Rlog/RLOG-RIL: 5 RIL requests in the queue (1 pending, 4 handled, 0 unhandled)

06-01 10:53:52.255  2812  2812 D RILJ    : [3686]> VOICE_REGISTRATION_STATE [SUB0]

06-01 10:53:52.255  1964  2328 D use-Rlog/RLOG-RIL-IPC: 

06-01 10:53:52.255  1964  2328 D use-Rlog/RLOG-RIL-IPC: xmm626_sec_modem_fmt_recv: Received FMT message

06-01 10:53:52.255  1964  2328 D use-Rlog/RLOG-RIL-IPC: xmm626_sec_modem_fmt_recv: Message: aseq=0x0c, command=IPC_NET_SERVING_NETWORK, type=IPC_TYPE_RESP, size=11

06-01 10:53:52.255  1964  2328 D use-Rlog/RLOG-RIL-IPC: ================================= IPC FMT data =================================

06-01 10:53:52.255  1964  2328 D use-Rlog/RLOG-RIL-IPC: [0000]   02 04 FF 32 30 36 31 30  23 00 00                  ...20610 #..

06-01 10:53:52.255  1964  2328 D use-Rlog/RLOG-RIL-IPC: ================================================================================

06-01 10:53:52.255  1964  2328 D use-Rlog/RLOG-RIL: 4 RIL requests in the queue (0 pending, 3 handled, 1 unhandled)

06-01 10:53:52.255  1964  2328 D use-Rlog/RLOG-RIL-IPC: 

06-01 10:53:52.255  1964  2328 D use-Rlog/RLOG-RIL-IPC: xmm626_sec_modem_fmt_recv: Received FMT message

06-01 10:53:52.255  1964  2328 D use-Rlog/RLOG-RIL-IPC: xmm626_sec_modem_fmt_recv: Message: aseq=0x0d, command=IPC_NET_REGIST, type=IPC_TYPE_RESP, size=11

06-01 10:53:52.255  1964  2328 D use-Rlog/RLOG-RIL-IPC: ================================= IPC FMT data =================================

06-01 10:53:52.255  1964  2328 D use-Rlog/RLOG-RIL-IPC: [0000]   FF 03 01 00 00 00 00 00  00 00 00                  ........ ...

06-01 10:53:52.255  1964  2328 D use-Rlog/RLOG-RIL-IPC: ================================================================================

06-01 10:53:52.255  1964  2328 D use-Rlog/RLOG-RIL: 3 RIL requests in the queue (0 pending, 2 handled, 1 unhandled)

06-01 10:53:52.255  1964  2332 D use-Rlog/RLOG-RIL-IPC: 

06-01 10:53:52.255  1964  2332 D use-Rlog/RLOG-RIL-IPC: xmm626_sec_modem_fmt_send: Sent FMT message

06-01 10:53:52.255  1964  2332 D use-Rlog/RLOG-RIL-IPC: xmm626_sec_modem_fmt_send: Message: mseq=0x10, command=IPC_NET_SERVING_NETWORK, type=IPC_TYPE_GET, size=0

06-01 10:53:52.255  1964  2328 D use-Rlog/RLOG-RIL-IPC: 

06-01 10:53:52.255  1964  2328 D use-Rlog/RLOG-RIL-IPC: xmm626_sec_modem_fmt_recv: Received FMT message

06-01 10:53:52.255  1964  2328 D use-Rlog/RLOG-RIL-IPC: xmm626_sec_modem_fmt_recv: Message: aseq=0x0e, command=IPC_NET_REGIST, type=IPC_TYPE_RESP, size=11

06-01 10:53:52.255  1964  2328 D use-Rlog/RLOG-RIL-IPC: ================================= IPC FMT data =================================

06-01 10:53:52.255  1964  2328 D use-Rlog/RLOG-RIL-IPC: [0000]   FF 02 04 00 00 00 00 00  00 00 00                  ........ ...

06-01 10:53:52.255  1964  2328 D use-Rlog/RLOG-RIL-IPC: ================================================================================

06-01 10:53:52.255  1964  2328 D use-Rlog/RLOG-RIL: 2 RIL requests in the queue (0 pending, 2 handled, 0 unhandled)

06-01 10:53:52.255  1964  2012 D use-Rlog/RLOG-RIL: 3 RIL requests in the queue (1 pending, 2 handled, 0 unhandled)

06-01 10:53:52.255  1964  2332 D use-Rlog/RLOG-RIL-IPC: 

06-01 10:53:52.255  1964  2332 D use-Rlog/RLOG-RIL-IPC: xmm626_sec_modem_fmt_send: Sent FMT message

06-01 10:53:52.255  1964  2332 D use-Rlog/RLOG-RIL-IPC: xmm626_sec_modem_fmt_send: Message: mseq=0x11, command=IPC_NET_REGIST, type=IPC_TYPE_GET, size=2

06-01 10:53:52.255  1964  2332 D use-Rlog/RLOG-RIL-IPC: ================================= IPC FMT data =================================

06-01 10:53:52.255  1964  2332 D use-Rlog/RLOG-RIL-IPC: [0000]   FF 03                                              ..

06-01 10:53:52.255  1964  2332 D use-Rlog/RLOG-RIL-IPC: ================================================================================

06-01 10:53:52.255  2812  2812 D RILJ    : [3687]> QUERY_NETWORK_SELECTION_MODE [SUB0]

06-01 10:53:52.255  1964  2012 D use-Rlog/RLOG-RIL: 4 RIL requests in the queue (1 pending, 3 handled, 0 unhandled)

06-01 10:53:52.255  1964  2332 D use-Rlog/RLOG-RIL-IPC: 

06-01 10:53:52.255  1964  2332 D use-Rlog/RLOG-RIL-IPC: xmm626_sec_modem_fmt_send: Sent FMT message

06-01 10:53:52.255  1964  2332 D use-Rlog/RLOG-RIL-IPC: xmm626_sec_modem_fmt_send: Message: mseq=0x12, command=IPC_NET_REGIST, type=IPC_TYPE_GET, size=2

06-01 10:53:52.255  1964  2332 D use-Rlog/RLOG-RIL-IPC: ================================= IPC FMT data =================================

06-01 10:53:52.255  1964  2332 D use-Rlog/RLOG-RIL-IPC: [0000]   FF 02                                              ..

06-01 10:53:52.255  1964  2332 D use-Rlog/RLOG-RIL-IPC: ================================================================================

06-01 10:53:52.255  1964  2328 D use-Rlog/RLOG-RIL-IPC: 

06-01 10:53:52.255  1964  2328 D use-Rlog/RLOG-RIL-IPC: xmm626_sec_modem_fmt_recv: Received FMT message

06-01 10:53:52.255  1964  2328 D use-Rlog/RLOG-RIL-IPC: xmm626_sec_modem_fmt_recv: Message: aseq=0x0f, command=IPC_NET_PLMN_SEL, type=IPC_TYPE_RESP, size=1

06-01 10:53:52.255  1964  2328 D use-Rlog/RLOG-RIL-IPC: ================================= IPC FMT data =================================

06-01 10:53:52.255  1964  2328 D use-Rlog/RLOG-RIL-IPC: [0000]   02                                                 .

06-01 10:53:52.255  1964  2328 D use-Rlog/RLOG-RIL-IPC: ================================================================================

06-01 10:53:52.255  1964  2328 D use-Rlog/RLOG-RIL: 3 RIL requests in the queue (0 pending, 3 handled, 0 unhandled)

06-01 10:53:52.255  1964  2328 D use-Rlog/RLOG-RIL-IPC: 

06-01 10:53:52.255  1964  2328 D use-Rlog/RLOG-RIL-IPC: xmm626_sec_modem_fmt_recv: Received FMT message

06-01 10:53:52.255  1964  2328 D use-Rlog/RLOG-RIL-IPC: xmm626_sec_modem_fmt_recv: Message: aseq=0x10, command=IPC_NET_SERVING_NETWORK, type=IPC_TYPE_RESP, size=11

06-01 10:53:52.255  1964  2328 D use-Rlog/RLOG-RIL-IPC: ================================= IPC FMT data =================================

06-01 10:53:52.255  1964  2328 D use-Rlog/RLOG-RIL-IPC: [0000]   02 04 FF 32 30 36 31 30  23 00 00                  ...20610 #..

06-01 10:53:52.255  1964  2328 D use-Rlog/RLOG-RIL-IPC: ================================================================================

06-01 10:53:52.255  1964  2328 D use-Rlog/RLOG-RIL: 2 RIL requests in the queue (0 pending, 2 handled, 0 unhandled)

06-01 10:53:52.260  2812  2812 D SubscriptionController: [getSubId]- sSlotIdxToSubId.size == 0, return DummySubIds slotIdx=0

06-01 10:53:52.260  2812  2812 D DefaultPhoneNotifier: notifySignalStrength: mRegistry=com.android.internal.telephony.ITelephonyRegistry$Stub$Proxy@d42da20 ss=SignalStrength: 1 99 -120 -160 -120 -1 -1 99 2147483647 2147483647 2147483647 -1 2147483647 gsm|lte sender=Handler (com.android.internal.telephony.gsm.GSMPhone) {b910da1}

06-01 10:53:52.260  2812  2918 D RILJ    : [3675]< RIL_REQUEST_VOICE_RADIO_TECH {3} [SUB0]

06-01 10:53:52.260  2812  2918 D RILJ    : [3674]< GET_CURRENT_CALLS {} [SUB0]

06-01 10:53:52.260  2812  2918 D RilRequest: [3676]< RIL_REQUEST_IMS_REGISTRATION_STATE error: com.android.internal.telephony.CommandException: REQUEST_NOT_SUPPORTED ret=

06-01 10:53:52.260  2812  2918 D RILJ    : [3677]< RIL_REQUEST_CDMA_GET_SUBSCRIPTION_SOURCE {0} [SUB0]

06-01 10:53:52.260  2812  2918 D RILJ    : [3678]< GET_SIM_STATUS IccCardState {CARDSTATE_PRESENT,PINSTATE_UNKNOWN,num_apps=1,gsm_id=0{APPTYPE_SIM,APPSTATE_PIN},cdma_id=-1,ims_id=-1} [SUB0]

06-01 10:53:52.260  2812  2918 D RILJ    : [3679]< GET_SIM_STATUS IccCardState {CARDSTATE_PRESENT,PINSTATE_UNKNOWN,num_apps=1,gsm_id=0{APPTYPE_SIM,APPSTATE_PIN},cdma_id=-1,ims_id=-1} [SUB0]

06-01 10:53:52.260  2812  2918 D RILJ    : [3680]< OPERATOR {Mobistar, Mobistar, 20610} [SUB0]

06-01 10:53:52.260  2812  2918 D RILJ    : [3681]< DATA_REGISTRATION_STATE {0, 0, 0, 0, 3} [SUB0]

06-01 10:53:52.260  2812  2918 D RILJ    : [3682]< VOICE_REGISTRATION_STATE {10, 0, 0, 0, null, null, null, null, null, null, null, null, null, null, null} [SUB0]

06-01 10:53:52.260  2812  2918 D RILJ    : [3683]< QUERY_NETWORK_SELECTION_MODE {0} [SUB0]

06-01 10:53:52.260  2812  2918 D RILJ    : [3684]< OPERATOR {Mobistar, Mobistar, 20610} [SUB0]

06-01 10:53:52.260  1964  2012 D use-Rlog/RLOG-RIL: 3 RIL requests in the queue (1 pending, 2 handled, 0 unhandled)

06-01 10:53:52.260  1964  2332 D use-Rlog/RLOG-RIL-IPC: 

06-01 10:53:52.260  1964  2332 D use-Rlog/RLOG-RIL-IPC: xmm626_sec_modem_fmt_send: Sent FMT message

06-01 10:53:52.260  1964  2332 D use-Rlog/RLOG-RIL-IPC: xmm626_sec_modem_fmt_send: Message: mseq=0x13, command=IPC_NET_PLMN_SEL, type=IPC_TYPE_GET, size=0

06-01 10:53:52.260  1964  2328 D use-Rlog/RLOG-RIL-IPC: 

06-01 10:53:52.260  1964  2328 D use-Rlog/RLOG-RIL-IPC: xmm626_sec_modem_fmt_recv: Received FMT message

06-01 10:53:52.260  1964  2328 D use-Rlog/RLOG-RIL-IPC: xmm626_sec_modem_fmt_recv: Message: aseq=0x11, command=IPC_NET_REGIST, type=IPC_TYPE_RESP, size=11

06-01 10:53:52.260  1964  2328 D use-Rlog/RLOG-RIL-IPC: ================================= IPC FMT data =================================

06-01 10:53:52.260  1964  2328 D use-Rlog/RLOG-RIL-IPC: [0000]   FF 03 01 00 00 00 00 00  00 00 00                  ........ ...

06-01 10:53:52.260  1964  2328 D use-Rlog/RLOG-RIL-IPC: ================================================================================

06-01 10:53:52.260  1964  2328 D use-Rlog/RLOG-RIL: 2 RIL requests in the queue (0 pending, 2 handled, 0 unhandled)

06-01 10:53:52.260  1964  2328 D use-Rlog/RLOG-RIL-IPC: 

06-01 10:53:52.260  1964  2328 D use-Rlog/RLOG-RIL-IPC: xmm626_sec_modem_fmt_recv: Received FMT message

06-01 10:53:52.260  1964  2328 D use-Rlog/RLOG-RIL-IPC: xmm626_sec_modem_fmt_recv: Message: aseq=0x12, command=IPC_NET_REGIST, type=IPC_TYPE_RESP, size=11

06-01 10:53:52.260  1964  2328 D use-Rlog/RLOG-RIL-IPC: ================================= IPC FMT data =================================

06-01 10:53:52.260  1964  2328 D use-Rlog/RLOG-RIL-IPC: [0000]   FF 02 04 00 00 00 00 00  00 00 00                  ........ ...

06-01 10:53:52.260  1964  2328 D use-Rlog/RLOG-RIL-IPC: ================================================================================

06-01 10:53:52.260  1964  2328 D use-Rlog/RLOG-RIL: 1 RIL request in the queue (0 pending, 1 handled, 0 unhandled)

06-01 10:53:52.260  2812  2918 D RILJ    : [3685]< DATA_REGISTRATION_STATE {0, 0, 0, 0, 3} [SUB0]

06-01 10:53:52.260  2812  2918 D RILJ    : [3686]< VOICE_REGISTRATION_STATE {10, 0, 0, 0, null, null, null, null, null, null, null, null, null, null, null} [SUB0]

06-01 10:53:52.260  1964  2328 D use-Rlog/RLOG-RIL-IPC: 

06-01 10:53:52.260  1964  2328 D use-Rlog/RLOG-RIL-IPC: xmm626_sec_modem_fmt_recv: Received FMT message

06-01 10:53:52.260  1964  2328 D use-Rlog/RLOG-RIL-IPC: xmm626_sec_modem_fmt_recv: Message: aseq=0x13, command=IPC_NET_PLMN_SEL, type=IPC_TYPE_RESP, size=1

06-01 10:53:52.260  1964  2328 D use-Rlog/RLOG-RIL-IPC: ================================= IPC FMT data =================================

06-01 10:53:52.260  1964  2328 D use-Rlog/RLOG-RIL-IPC: [0000]   02                                                 .

06-01 10:53:52.260  1964  2328 D use-Rlog/RLOG-RIL-IPC: ================================================================================

06-01 10:53:52.260  1964  2328 D use-Rlog/RLOG-RIL: 0 RIL request in the queue (0 pending, 0 handled, 0 unhandled)

06-01 10:53:52.260  2812  2918 D RILJ    : [3687]< QUERY_NETWORK_SELECTION_MODE {0} [SUB0]

06-01 10:53:52.260  2335  2837 D TelephonyRegistry: notifySignalStrengthForSubscriber: invalid phoneId=-1

06-01 10:53:52.265  2812  2812 D RILJ    : [3688]> OPERATOR [SUB0]

06-01 10:53:52.265  2812  2812 D RILJ    : [3689]> DATA_REGISTRATION_STATE [SUB0]

06-01 10:53:52.265  1964  2012 D use-Rlog/RLOG-RIL: 1 RIL request in the queue (1 pending, 0 handled, 0 unhandled)

06-01 10:53:52.270  1964  2332 D use-Rlog/RLOG-RIL-IPC: 

06-01 10:53:52.270  1964  2332 D use-Rlog/RLOG-RIL-IPC: xmm626_sec_modem_fmt_send: Sent FMT message

06-01 10:53:52.270  1964  2332 D use-Rlog/RLOG-RIL-IPC: xmm626_sec_modem_fmt_send: Message: mseq=0x14, command=IPC_NET_SERVING_NETWORK, type=IPC_TYPE_GET, size=0

06-01 10:53:52.270  2812  2812 D RILJ    : [3690]> VOICE_REGISTRATION_STATE [SUB0]

06-01 10:53:52.270  1964  2012 D use-Rlog/RLOG-RIL: 2 RIL requests in the queue (1 pending, 1 handled, 0 unhandled)

06-01 10:53:52.270  1964  2332 D use-Rlog/RLOG-RIL-IPC: 

06-01 10:53:52.270  1964  2332 D use-Rlog/RLOG-RIL-IPC: xmm626_sec_modem_fmt_send: Sent FMT message

06-01 10:53:52.270  1964  2332 D use-Rlog/RLOG-RIL-IPC: xmm626_sec_modem_fmt_send: Message: mseq=0x15, command=IPC_NET_REGIST, type=IPC_TYPE_GET, size=2

06-01 10:53:52.270  1964  2332 D use-Rlog/RLOG-RIL-IPC: ================================= IPC FMT data =================================

06-01 10:53:52.270  1964  2332 D use-Rlog/RLOG-RIL-IPC: [0000]   FF 03                                              ..

06-01 10:53:52.270  1964  2332 D use-Rlog/RLOG-RIL-IPC: ================================================================================

06-01 10:53:52.270  1964  2328 D use-Rlog/RLOG-RIL-IPC: 

06-01 10:53:52.270  1964  2328 D use-Rlog/RLOG-RIL-IPC: xmm626_sec_modem_fmt_recv: Received FMT message

06-01 10:53:52.270  1964  2328 D use-Rlog/RLOG-RIL-IPC: xmm626_sec_modem_fmt_recv: Message: aseq=0x14, command=IPC_NET_SERVING_NETWORK, type=IPC_TYPE_RESP, size=11

06-01 10:53:52.270  1964  2328 D use-Rlog/RLOG-RIL-IPC: ================================= IPC FMT data =================================

06-01 10:53:52.270  1964  2328 D use-Rlog/RLOG-RIL-IPC: [0000]   02 04 FF 32 30 36 31 30  23 00 00                  ...20610 #..

06-01 10:53:52.270  1964  2328 D use-Rlog/RLOG-RIL-IPC: ================================================================================

06-01 10:53:52.270  1964  2328 D use-Rlog/RLOG-RIL: 1 RIL request in the queue (0 pending, 1 handled, 0 unhandled)

06-01 10:53:52.270  2812  2918 D RILJ    : [3688]< OPERATOR {Mobistar, Mobistar, 20610} [SUB0]

06-01 10:53:52.280  1964  2328 D use-Rlog/RLOG-RIL-IPC: 

06-01 10:53:52.280  1964  2328 D use-Rlog/RLOG-RIL-IPC: xmm626_sec_modem_fmt_recv: Received FMT message

06-01 10:53:52.280  1964  2328 D use-Rlog/RLOG-RIL-IPC: xmm626_sec_modem_fmt_recv: Message: aseq=0x15, command=IPC_NET_REGIST, type=IPC_TYPE_RESP, size=11

06-01 10:53:52.280  1964  2328 D use-Rlog/RLOG-RIL-IPC: ================================= IPC FMT data =================================

06-01 10:53:52.280  1964  2328 D use-Rlog/RLOG-RIL-IPC: [0000]   FF 03 01 00 00 00 00 00  00 00 00                  ........ ...

06-01 10:53:52.280  1964  2328 D use-Rlog/RLOG-RIL-IPC: ================================================================================

06-01 10:53:52.280  1964  2328 D use-Rlog/RLOG-RIL: 0 RIL request in the queue (0 pending, 0 handled, 0 unhandled)

06-01 10:53:52.280  2812  2812 D RILJ    : [3691]> QUERY_NETWORK_SELECTION_MODE [SUB0]

06-01 10:53:52.280  1964  2012 D use-Rlog/RLOG-RIL: 1 RIL request in the queue (1 pending, 0 handled, 0 unhandled)

06-01 10:53:52.280  1964  2332 D use-Rlog/RLOG-RIL-IPC: 

06-01 10:53:52.280  1964  2332 D use-Rlog/RLOG-RIL-IPC: xmm626_sec_modem_fmt_send: Sent FMT message

06-01 10:53:52.280  1964  2332 D use-Rlog/RLOG-RIL-IPC: xmm626_sec_modem_fmt_send: Message: mseq=0x16, command=IPC_NET_REGIST, type=IPC_TYPE_GET, size=2

06-01 10:53:52.280  1964  2332 D use-Rlog/RLOG-RIL-IPC: ================================= IPC FMT data =================================

06-01 10:53:52.280  1964  2332 D use-Rlog/RLOG-RIL-IPC: [0000]   FF 02                                              ..

06-01 10:53:52.280  1964  2332 D use-Rlog/RLOG-RIL-IPC: ================================================================================

06-01 10:53:52.280  2812  2812 D RILJ    : [3692]> OPERATOR [SUB0]

06-01 10:53:52.280  1964  2012 D use-Rlog/RLOG-RIL: 2 RIL requests in the queue (1 pending, 1 handled, 0 unhandled)

06-01 10:53:52.280  1964  2332 D use-Rlog/RLOG-RIL-IPC: 

06-01 10:53:52.280  1964  2332 D use-Rlog/RLOG-RIL-IPC: xmm626_sec_modem_fmt_send: Sent FMT message

06-01 10:53:52.280  1964  2332 D use-Rlog/RLOG-RIL-IPC: xmm626_sec_modem_fmt_send: Message: mseq=0x17, command=IPC_NET_PLMN_SEL, type=IPC_TYPE_GET, size=0

06-01 10:53:52.280  2812  2812 D RILJ    : [3693]> DATA_REGISTRATION_STATE [SUB0]

06-01 10:53:52.285  1964  2328 D use-Rlog/RLOG-RIL-IPC: 

06-01 10:53:52.285  1964  2328 D use-Rlog/RLOG-RIL-IPC: xmm626_sec_modem_fmt_recv: Received FMT message

06-01 10:53:52.285  1964  2328 D use-Rlog/RLOG-RIL-IPC: xmm626_sec_modem_fmt_recv: Message: aseq=0x16, command=IPC_NET_REGIST, type=IPC_TYPE_RESP, size=11

06-01 10:53:52.285  1964  2328 D use-Rlog/RLOG-RIL-IPC: ================================= IPC FMT data =================================

06-01 10:53:52.285  1964  2328 D use-Rlog/RLOG-RIL-IPC: [0000]   FF 02 04 00 00 00 00 00  00 00 00                  ........ ...

06-01 10:53:52.285  1964  2328 D use-Rlog/RLOG-RIL-IPC: ================================================================================

06-01 10:53:52.285  1964  2328 D use-Rlog/RLOG-RIL: 1 RIL request in the queue (0 pending, 1 handled, 0 unhandled)

06-01 10:53:52.285  2812  2812 D RILJ    : [3694]> VOICE_REGISTRATION_STATE [SUB0]

06-01 10:53:52.285  1964  2012 D use-Rlog/RLOG-RIL: 2 RIL requests in the queue (1 pending, 1 handled, 0 unhandled)

06-01 10:53:52.285  1964  2332 D use-Rlog/RLOG-RIL-IPC: 

06-01 10:53:52.285  1964  2332 D use-Rlog/RLOG-RIL-IPC: xmm626_sec_modem_fmt_send: Sent FMT message

06-01 10:53:52.285  1964  2332 D use-Rlog/RLOG-RIL-IPC: xmm626_sec_modem_fmt_send: Message: mseq=0x18, command=IPC_NET_SERVING_NETWORK, type=IPC_TYPE_GET, size=0

06-01 10:53:52.285  1964  2328 D use-Rlog/RLOG-RIL-IPC: 

06-01 10:53:52.285  1964  2328 D use-Rlog/RLOG-RIL-IPC: xmm626_sec_modem_fmt_recv: Received FMT message

06-01 10:53:52.285  1964  2328 D use-Rlog/RLOG-RIL-IPC: xmm626_sec_modem_fmt_recv: Message: aseq=0x17, command=IPC_NET_PLMN_SEL, type=IPC_TYPE_RESP, size=1

06-01 10:53:52.285  1964  2328 D use-Rlog/RLOG-RIL-IPC: ================================= IPC FMT data =================================

06-01 10:53:52.285  1964  2328 D use-Rlog/RLOG-RIL-IPC: [0000]   02                                                 .

06-01 10:53:52.285  1964  2328 D use-Rlog/RLOG-RIL-IPC: ================================================================================

06-01 10:53:52.285  1964  2328 D use-Rlog/RLOG-RIL: 1 RIL request in the queue (0 pending, 1 handled, 0 unhandled)

06-01 10:53:52.285  1964  2012 D use-Rlog/RLOG-RIL: 2 RIL requests in the queue (1 pending, 1 handled, 0 unhandled)

06-01 10:53:52.285  1964  2328 D use-Rlog/RLOG-RIL-IPC: 

06-01 10:53:52.285  1964  2328 D use-Rlog/RLOG-RIL-IPC: xmm626_sec_modem_fmt_recv: Received FMT message

06-01 10:53:52.285  1964  2328 D use-Rlog/RLOG-RIL-IPC: xmm626_sec_modem_fmt_recv: Message: aseq=0x18, command=IPC_NET_SERVING_NETWORK, type=IPC_TYPE_RESP, size=11

06-01 10:53:52.285  1964  2328 D use-Rlog/RLOG-RIL-IPC: ================================= IPC FMT data =================================

06-01 10:53:52.285  1964  2328 D use-Rlog/RLOG-RIL-IPC: [0000]   02 04 FF 32 30 36 31 30  23 00 00                  ...20610 #..

06-01 10:53:52.285  1964  2328 D use-Rlog/RLOG-RIL-IPC: ================================================================================

06-01 10:53:52.285  1964  2328 D use-Rlog/RLOG-RIL: 1 RIL request in the queue (1 pending, 0 handled, 0 unhandled)

06-01 10:53:52.285  2812  2812 D RILJ    : [3695]> QUERY_NETWORK_SELECTION_MODE [SUB0]

06-01 10:53:52.285  1964  2332 D use-Rlog/RLOG-RIL-IPC: 

06-01 10:53:52.285  1964  2332 D use-Rlog/RLOG-RIL-IPC: xmm626_sec_modem_fmt_send: Sent FMT message

06-01 10:53:52.285  1964  2332 D use-Rlog/RLOG-RIL-IPC: xmm626_sec_modem_fmt_send: Message: mseq=0x19, command=IPC_NET_REGIST, type=IPC_TYPE_GET, size=2

06-01 10:53:52.285  1964  2332 D use-Rlog/RLOG-RIL-IPC: ================================= IPC FMT data =================================

06-01 10:53:52.285  1964  2332 D use-Rlog/RLOG-RIL-IPC: [0000]   FF 03                                              ..

06-01 10:53:52.285  1964  2332 D use-Rlog/RLOG-RIL-IPC: ================================================================================

06-01 10:53:52.285  1964  2012 D use-Rlog/RLOG-RIL: 2 RIL requests in the queue (1 pending, 1 handled, 0 unhandled)

06-01 10:53:52.285  1964  2332 D use-Rlog/RLOG-RIL-IPC: 

06-01 10:53:52.285  1964  2332 D use-Rlog/RLOG-RIL-IPC: xmm626_sec_modem_fmt_send: Sent FMT message

06-01 10:53:52.285  1964  2332 D use-Rlog/RLOG-RIL-IPC: xmm626_sec_modem_fmt_send: Message: mseq=0x1a, command=IPC_NET_REGIST, type=IPC_TYPE_GET, size=2

06-01 10:53:52.285  1964  2332 D use-Rlog/RLOG-RIL-IPC: ================================= IPC FMT data =================================

06-01 10:53:52.285  1964  2332 D use-Rlog/RLOG-RIL-IPC: [0000]   FF 02                                              ..

06-01 10:53:52.285  1964  2332 D use-Rlog/RLOG-RIL-IPC: ================================================================================

06-01 10:53:52.285  2812  2812 D SubscriptionController: [getSubId]- sSlotIdxToSubId.size == 0, return DummySubIds slotIdx=0

06-01 10:53:52.285  2812  2812 D DCT     : [0]getDataOnRoamingEnabled: phoneSubId=-2 isDataRoamingEnabled=false

06-01 10:53:52.285  2812  2812 D SubscriptionController: [getSubId]- sSlotIdxToSubId.size == 0, return DummySubIds slotIdx=0

06-01 10:53:52.285  2812  2812 D DCT     : [0]getDataOnRoamingEnabled: phoneSubId=-2 isDataRoamingEnabled=false

06-01 10:53:52.285  2812  2812 D RILJ    : [3696]> OPERATOR [SUB0]

06-01 10:53:52.290  1964  2012 D use-Rlog/RLOG-RIL: 3 RIL requests in the queue (1 pending, 2 handled, 0 unhandled)

06-01 10:53:52.290  1964  2332 D use-Rlog/RLOG-RIL-IPC: 

06-01 10:53:52.290  1964  2332 D use-Rlog/RLOG-RIL-IPC: xmm626_sec_modem_fmt_send: Sent FMT message

06-01 10:53:52.290  1964  2332 D use-Rlog/RLOG-RIL-IPC: xmm626_sec_modem_fmt_send: Message: mseq=0x1b, command=IPC_NET_PLMN_SEL, type=IPC_TYPE_GET, size=0

06-01 10:53:52.290  1964  2328 D use-Rlog/RLOG-RIL-IPC: 

06-01 10:53:52.290  1964  2328 D use-Rlog/RLOG-RIL-IPC: xmm626_sec_modem_fmt_recv: Received FMT message

06-01 10:53:52.290  1964  2328 D use-Rlog/RLOG-RIL-IPC: xmm626_sec_modem_fmt_recv: Message: aseq=0x19, command=IPC_NET_REGIST, type=IPC_TYPE_RESP, size=11

06-01 10:53:52.290  1964  2328 D use-Rlog/RLOG-RIL-IPC: ================================= IPC FMT data =================================

06-01 10:53:52.290  1964  2328 D use-Rlog/RLOG-RIL-IPC: [0000]   FF 03 01 00 00 00 00 00  00 00 00                  ........ ...

06-01 10:53:52.290  1964  2328 D use-Rlog/RLOG-RIL-IPC: ================================================================================

06-01 10:53:52.290  1964  2328 D use-Rlog/RLOG-RIL: 2 RIL requests in the queue (0 pending, 2 handled, 0 unhandled)

06-01 10:53:52.290  2812  2918 D RILJ    : [3689]< DATA_REGISTRATION_STATE {0, 0, 0, 0, 3} [SUB0]

06-01 10:53:52.290  1964  2328 D use-Rlog/RLOG-RIL-IPC: 

06-01 10:53:52.290  1964  2328 D use-Rlog/RLOG-RIL-IPC: xmm626_sec_modem_fmt_recv: Received FMT message

06-01 10:53:52.290  1964  2328 D use-Rlog/RLOG-RIL-IPC: xmm626_sec_modem_fmt_recv: Message: aseq=0x1a, command=IPC_NET_REGIST, type=IPC_TYPE_RESP, size=11

06-01 10:53:52.290  1964  2328 D use-Rlog/RLOG-RIL-IPC: ================================= IPC FMT data =================================

06-01 10:53:52.290  1964  2328 D use-Rlog/RLOG-RIL-IPC: [0000]   FF 02 04 00 00 00 00 00  00 00 00                  ........ ...

06-01 10:53:52.290  1964  2328 D use-Rlog/RLOG-RIL-IPC: ================================================================================

06-01 10:53:52.290  2812  2918 D RILJ    : [3690]< VOICE_REGISTRATION_STATE {10, 0, 0, 0, null, null, null, null, null, null, null, null, null, null, null} [SUB0]

06-01 10:53:52.290  1964  2328 D use-Rlog/RLOG-RIL: 1 RIL request in the queue (0 pending, 1 handled, 0 unhandled)

06-01 10:53:52.290  2812  2918 D RILJ    : [3691]< QUERY_NETWORK_SELECTION_MODE {0} [SUB0]

06-01 10:53:52.290  2812  2918 D RILJ    : [3692]< OPERATOR {Mobistar, Mobistar, 20610} [SUB0]

06-01 10:53:52.290  2812  2918 D RILJ    : [3693]< DATA_REGISTRATION_STATE {0, 0, 0, 0, 3} [SUB0]

06-01 10:53:52.290  2812  2918 D RILJ    : [3694]< VOICE_REGISTRATION_STATE {10, 0, 0, 0, null, null, null, null, null, null, null, null, null, null, null} [SUB0]

06-01 10:53:52.290  1964  2012 D use-Rlog/RLOG-RIL: 2 RIL requests in the queue (1 pending, 1 handled, 0 unhandled)

06-01 10:53:52.290  2812  2812 D RILJ    : [3697]> DATA_REGISTRATION_STATE [SUB0]

06-01 10:53:52.290  1964  2328 D use-Rlog/RLOG-RIL-IPC: 

06-01 10:53:52.290  1964  2328 D use-Rlog/RLOG-RIL-IPC: xmm626_sec_modem_fmt_recv: Received FMT message

06-01 10:53:52.290  1964  2328 D use-Rlog/RLOG-RIL-IPC: xmm626_sec_modem_fmt_recv: Message: aseq=0x1b, command=IPC_NET_PLMN_SEL, type=IPC_TYPE_RESP, size=1

06-01 10:53:52.290  1964  2328 D use-Rlog/RLOG-RIL-IPC: ================================= IPC FMT data =================================

06-01 10:53:52.290  1964  2328 D use-Rlog/RLOG-RIL-IPC: [0000]   02                                                 .

06-01 10:53:52.290  1964  2328 D use-Rlog/RLOG-RIL-IPC: ================================================================================

06-01 10:53:52.290  1964  2328 D use-Rlog/RLOG-RIL: 1 RIL request in the queue (1 pending, 0 handled, 0 unhandled)

06-01 10:53:52.290  1964  2332 D use-Rlog/RLOG-RIL-IPC: 

06-01 10:53:52.290  1964  2332 D use-Rlog/RLOG-RIL-IPC: xmm626_sec_modem_fmt_send: Sent FMT message

06-01 10:53:52.290  1964  2332 D use-Rlog/RLOG-RIL-IPC: xmm626_sec_modem_fmt_send: Message: mseq=0x1c, command=IPC_NET_SERVING_NETWORK, type=IPC_TYPE_GET, size=0

06-01 10:53:52.290  2812  2918 D RILJ    : [3695]< QUERY_NETWORK_SELECTION_MODE {0} [SUB0]

06-01 10:53:52.290  1964  2012 D use-Rlog/RLOG-RIL: 2 RIL requests in the queue (1 pending, 1 handled, 0 unhandled)

06-01 10:53:52.290  1964  2332 D use-Rlog/RLOG-RIL-IPC: 

06-01 10:53:52.290  1964  2332 D use-Rlog/RLOG-RIL-IPC: xmm626_sec_modem_fmt_send: Sent FMT message

06-01 10:53:52.290  1964  2332 D use-Rlog/RLOG-RIL-IPC: xmm626_sec_modem_fmt_send: Message: mseq=0x1d, command=IPC_NET_REGIST, type=IPC_TYPE_GET, size=2

06-01 10:53:52.290  2812  2812 D RILJ    : [3698]> VOICE_REGISTRATION_STATE [SUB0]

06-01 10:53:52.290  1964  2332 D use-Rlog/RLOG-RIL-IPC: ================================= IPC FMT data =================================

06-01 10:53:52.290  1964  2332 D use-Rlog/RLOG-RIL-IPC: [0000]   FF 03                                              ..

06-01 10:53:52.290  1964  2332 D use-Rlog/RLOG-RIL-IPC: ================================================================================

06-01 10:53:52.290  1964  2328 D use-Rlog/RLOG-RIL-IPC: 

06-01 10:53:52.290  1964  2328 D use-Rlog/RLOG-RIL-IPC: xmm626_sec_modem_fmt_recv: Received FMT message

06-01 10:53:52.290  1964  2328 D use-Rlog/RLOG-RIL-IPC: xmm626_sec_modem_fmt_recv: Message: aseq=0x1c, command=IPC_NET_SERVING_NETWORK, type=IPC_TYPE_RESP, size=11

06-01 10:53:52.290  1964  2328 D use-Rlog/RLOG-RIL-IPC: ================================= IPC FMT data =================================

06-01 10:53:52.290  1964  2328 D use-Rlog/RLOG-RIL-IPC: [0000]   02 04 FF 32 30 36 31 30  23 00 00                  ...20610 #..

06-01 10:53:52.290  1964  2328 D use-Rlog/RLOG-RIL-IPC: ================================================================================

06-01 10:53:52.290  1964  2328 D use-Rlog/RLOG-RIL: 1 RIL request in the queue (0 pending, 1 handled, 0 unhandled)

06-01 10:53:52.290  2812  2918 D RILJ    : [3696]< OPERATOR {Mobistar, Mobistar, 20610} [SUB0]

06-01 10:53:52.290  1964  2328 D use-Rlog/RLOG-RIL-IPC: 

06-01 10:53:52.290  1964  2328 D use-Rlog/RLOG-RIL-IPC: xmm626_sec_modem_fmt_recv: Received FMT message

06-01 10:53:52.290  1964  2328 D use-Rlog/RLOG-RIL-IPC: xmm626_sec_modem_fmt_recv: Message: aseq=0x1d, command=IPC_NET_REGIST, type=IPC_TYPE_RESP, size=11

06-01 10:53:52.290  1964  2328 D use-Rlog/RLOG-RIL-IPC: ================================= IPC FMT data =================================

06-01 10:53:52.290  1964  2328 D use-Rlog/RLOG-RIL-IPC: [0000]   FF 03 01 00 00 00 00 00  00 00 00                  ........ ...

06-01 10:53:52.290  1964  2328 D use-Rlog/RLOG-RIL-IPC: ================================================================================

06-01 10:53:52.290  1964  2328 D use-Rlog/RLOG-RIL: 0 RIL request in the queue (0 pending, 0 handled, 0 unhandled)

06-01 10:53:52.290  2812  2812 D RILJ    : [3699]> QUERY_NETWORK_SELECTION_MODE [SUB0]

06-01 10:53:52.290  1964  2012 D use-Rlog/RLOG-RIL: 1 RIL request in the queue (1 pending, 0 handled, 0 unhandled)

06-01 10:53:52.295  1964  2332 D use-Rlog/RLOG-RIL-IPC: 

06-01 10:53:52.295  1964  2332 D use-Rlog/RLOG-RIL-IPC: xmm626_sec_modem_fmt_send: Sent FMT message

06-01 10:53:52.295  1964  2332 D use-Rlog/RLOG-RIL-IPC: xmm626_sec_modem_fmt_send: Message: mseq=0x1e, command=IPC_NET_REGIST, type=IPC_TYPE_GET, size=2

06-01 10:53:52.295  1964  2332 D use-Rlog/RLOG-RIL-IPC: ================================= IPC FMT data =================================

06-01 10:53:52.295  1964  2332 D use-Rlog/RLOG-RIL-IPC: [0000]   FF 02                                              ..

06-01 10:53:52.295  1964  2332 D use-Rlog/RLOG-RIL-IPC: ================================================================================

06-01 10:53:52.295  2812  2812 D RILJ    : [3700]> OPERATOR [SUB0]

06-01 10:53:52.295  2812  2918 D RILJ    : [3697]< DATA_REGISTRATION_STATE {0, 0, 0, 0, 3} [SUB0]

06-01 10:53:52.295  1964  2012 D use-Rlog/RLOG-RIL: 2 RIL requests in the queue (1 pending, 1 handled, 0 unhandled)

06-01 10:53:52.295  1964  2332 D use-Rlog/RLOG-RIL-IPC: 

06-01 10:53:52.295  1964  2332 D use-Rlog/RLOG-RIL-IPC: xmm626_sec_modem_fmt_send: Sent FMT message

06-01 10:53:52.295  1964  2332 D use-Rlog/RLOG-RIL-IPC: xmm626_sec_modem_fmt_send: Message: mseq=0x1f, command=IPC_NET_PLMN_SEL, type=IPC_TYPE_GET, size=0

06-01 10:53:52.295  2812  2812 D RILJ    : [3701]> DATA_REGISTRATION_STATE [SUB0]

06-01 10:53:52.295  1964  2328 D use-Rlog/RLOG-RIL-IPC: 

06-01 10:53:52.295  1964  2328 D use-Rlog/RLOG-RIL-IPC: xmm626_sec_modem_fmt_recv: Received FMT message

06-01 10:53:52.295  1964  2328 D use-Rlog/RLOG-RIL-IPC: xmm626_sec_modem_fmt_recv: Message: aseq=0x1e, command=IPC_NET_REGIST, type=IPC_TYPE_RESP, size=11

06-01 10:53:52.295  1964  2328 D use-Rlog/RLOG-RIL-IPC: ================================= IPC FMT data =================================

06-01 10:53:52.295  1964  2328 D use-Rlog/RLOG-RIL-IPC: [0000]   FF 02 04 00 00 00 00 00  00 00 00                  ........ ...

06-01 10:53:52.295  1964  2328 D use-Rlog/RLOG-RIL-IPC: ================================================================================

06-01 10:53:52.295  1964  2328 D use-Rlog/RLOG-RIL: 1 RIL request in the queue (0 pending, 1 handled, 0 unhandled)

06-01 10:53:52.295  1964  2328 D use-Rlog/RLOG-RIL-IPC: 

06-01 10:53:52.295  2812  2812 D RILJ    : [3702]> VOICE_REGISTRATION_STATE [SUB0]

06-01 10:53:52.295  1964  2328 D use-Rlog/RLOG-RIL-IPC: xmm626_sec_modem_fmt_recv: Received FMT message

06-01 10:53:52.295  1964  2328 D use-Rlog/RLOG-RIL-IPC: xmm626_sec_modem_fmt_recv: Message: aseq=0x1f, command=IPC_NET_PLMN_SEL, type=IPC_TYPE_RESP, size=1

06-01 10:53:52.295  1964  2328 D use-Rlog/RLOG-RIL-IPC: ================================= IPC FMT data =================================

06-01 10:53:52.295  1964  2328 D use-Rlog/RLOG-RIL-IPC: [0000]   02                                                 .

06-01 10:53:52.295  1964  2328 D use-Rlog/RLOG-RIL-IPC: ================================================================================

06-01 10:53:52.295  1964  2328 D use-Rlog/RLOG-RIL: 0 RIL request in the queue (0 pending, 0 handled, 0 unhandled)

06-01 10:53:52.295  1964  2012 D use-Rlog/RLOG-RIL: 1 RIL request in the queue (1 pending, 0 handled, 0 unhandled)

06-01 10:53:52.295  1964  2332 D use-Rlog/RLOG-RIL-IPC: 

06-01 10:53:52.295  1964  2332 D use-Rlog/RLOG-RIL-IPC: xmm626_sec_modem_fmt_send: Sent FMT message

06-01 10:53:52.295  1964  2332 D use-Rlog/RLOG-RIL-IPC: xmm626_sec_modem_fmt_send: Message: mseq=0x20, command=IPC_NET_SERVING_NETWORK, type=IPC_TYPE_GET, size=0

06-01 10:53:52.295  2812  2812 D RILJ    : [3703]> QUERY_NETWORK_SELECTION_MODE [SUB0]

06-01 10:53:52.295  1964  2012 D use-Rlog/RLOG-RIL: 2 RIL requests in the queue (1 pending, 1 handled, 0 unhandled)

06-01 10:53:52.295  1964  2012 D use-Rlog/RLOG-RIL: 3 RIL requests in the queue (2 pending, 1 handled, 0 unhandled)

06-01 10:53:52.295  1964  2332 D use-Rlog/RLOG-RIL-IPC: 

06-01 10:53:52.295  1964  2332 D use-Rlog/RLOG-RIL-IPC: xmm626_sec_modem_fmt_send: Sent FMT message

06-01 10:53:52.295  1964  2332 D use-Rlog/RLOG-RIL-IPC: xmm626_sec_modem_fmt_send: Message: mseq=0x21, command=IPC_NET_REGIST, type=IPC_TYPE_GET, size=2

06-01 10:53:52.295  1964  2332 D use-Rlog/RLOG-RIL-IPC: ================================= IPC FMT data =================================

06-01 10:53:52.295  1964  2332 D use-Rlog/RLOG-RIL-IPC: [0000]   FF 03                                              ..

06-01 10:53:52.295  1964  2332 D use-Rlog/RLOG-RIL-IPC: ================================================================================

06-01 10:53:52.295  2812  2812 D SubscriptionController: [getSubId]- sSlotIdxToSubId.size == 0, return DummySubIds slotIdx=0

06-01 10:53:52.295  2812  2812 D DefaultPhoneNotifier: notifySignalStrength: mRegistry=com.android.internal.telephony.ITelephonyRegistry$Stub$Proxy@d42da20 ss=SignalStrength: 1 99 -120 -160 -120 -1 -1 99 2147483647 2147483647 2147483647 -1 2147483647 gsm|lte sender=Handler (com.android.internal.telephony.gsm.GSMPhone) {b910da1}

06-01 10:53:52.295  2812  2918 D RILJ    : [3698]< VOICE_REGISTRATION_STATE {10, 0, 0, 0, null, null, null, null, null, null, null, null, null, null, null} [SUB0]

06-01 10:53:52.295  1964  2332 D use-Rlog/RLOG-RIL-IPC: 

06-01 10:53:52.295  1964  2332 D use-Rlog/RLOG-RIL-IPC: xmm626_sec_modem_fmt_send: Sent FMT message

06-01 10:53:52.295  1964  2332 D use-Rlog/RLOG-RIL-IPC: xmm626_sec_modem_fmt_send: Message: mseq=0x22, command=IPC_NET_REGIST, type=IPC_TYPE_GET, size=2

06-01 10:53:52.295  1964  2332 D use-Rlog/RLOG-RIL-IPC: ================================= IPC FMT data =================================

06-01 10:53:52.295  1964  2332 D use-Rlog/RLOG-RIL-IPC: [0000]   FF 02                                              ..

06-01 10:53:52.295  1964  2332 D use-Rlog/RLOG-RIL-IPC: ================================================================================

06-01 10:53:52.295  2812  2918 D RILJ    : [3699]< QUERY_NETWORK_SELECTION_MODE {0} [SUB0]

06-01 10:53:52.295  1964  2328 D use-Rlog/RLOG-RIL-IPC: 

06-01 10:53:52.295  2335  2847 D TelephonyRegistry: notifySignalStrengthForSubscriber: invalid phoneId=-1

06-01 10:53:52.295  1964  2328 D use-Rlog/RLOG-RIL-IPC: xmm626_sec_modem_fmt_recv: Received FMT message

06-01 10:53:52.295  1964  2328 D use-Rlog/RLOG-RIL-IPC: xmm626_sec_modem_fmt_recv: Message: aseq=0x20, command=IPC_NET_SERVING_NETWORK, type=IPC_TYPE_RESP, size=11

06-01 10:53:52.295  1964  2328 D use-Rlog/RLOG-RIL-IPC: ================================= IPC FMT data =================================

06-01 10:53:52.300  1964  2328 D use-Rlog/RLOG-RIL-IPC: [0000]   02 04 FF 32 30 36 31 30  23 00 00                  ...20610 #..

06-01 10:53:52.300  1964  2328 D use-Rlog/RLOG-RIL-IPC: ================================================================================

06-01 10:53:52.300  1964  2328 D use-Rlog/RLOG-RIL: 2 RIL requests in the queue (0 pending, 2 handled, 0 unhandled)

06-01 10:53:52.300  1964  2012 D use-Rlog/RLOG-RIL: 3 RIL requests in the queue (1 pending, 2 handled, 0 unhandled)

06-01 10:53:52.300  2812  2918 D RILJ    : [3700]< OPERATOR {Mobistar, Mobistar, 20610} [SUB0]

06-01 10:53:52.300  2812  2812 D SubscriptionController: [getSubId]- sSlotIdxToSubId.size == 0, return DummySubIds slotIdx=0

06-01 10:53:52.300  2812  2812 D DCT     : [0]getDataOnRoamingEnabled: phoneSubId=-2 isDataRoamingEnabled=false

06-01 10:53:52.300  2812  2812 D SubscriptionController: [getSubId]- sSlotIdxToSubId.size == 0, return DummySubIds slotIdx=0

06-01 10:53:52.300  1964  2332 D use-Rlog/RLOG-RIL-IPC: 

06-01 10:53:52.300  1964  2332 D use-Rlog/RLOG-RIL-IPC: xmm626_sec_modem_fmt_send: Sent FMT message

06-01 10:53:52.300  2812  2812 D DCT     : [0]getDataOnRoamingEnabled: phoneSubId=-2 isDataRoamingEnabled=false

06-01 10:53:52.300  1964  2332 D use-Rlog/RLOG-RIL-IPC: xmm626_sec_modem_fmt_send: Message: mseq=0x23, command=IPC_NET_PLMN_SEL, type=IPC_TYPE_GET, size=0

06-01 10:53:52.300  2812  2812 D SubscriptionController: [getSubId]- sSlotIdxToSubId.size == 0, return DummySubIds slotIdx=0

06-01 10:53:52.300  2812  2812 D DCT     : [0]getDataOnRoamingEnabled: phoneSubId=-2 isDataRoamingEnabled=false

06-01 10:53:52.300  2812  2812 D SubscriptionController: [getSubId]- sSlotIdxToSubId.size == 0, return DummySubIds slotIdx=0

06-01 10:53:52.300  2812  2812 D DCT     : [0]getDataOnRoamingEnabled: phoneSubId=-2 isDataRoamingEnabled=false

06-01 10:53:52.300  2812  2812 D SubscriptionController: [getSubId]- sSlotIdxToSubId.size == 0, return DummySubIds slotIdx=0

06-01 10:53:52.300  2812  2812 D DCT     : [0]getDataOnRoamingEnabled: phoneSubId=-2 isDataRoamingEnabled=false

06-01 10:53:52.300  2812  2812 D SubscriptionController: [getSubId]- sSlotIdxToSubId.size == 0, return DummySubIds slotIdx=0

06-01 10:53:52.300  2812  2812 D DCT     : [0]getDataOnRoamingEnabled: phoneSubId=-2 isDataRoamingEnabled=false

06-01 10:53:52.300  2812  2812 D SubscriptionController: [getSubId]- sSlotIdxToSubId.size == 0, return DummySubIds slotIdx=0

06-01 10:53:52.300  1964  2328 D use-Rlog/RLOG-RIL-IPC: 

06-01 10:53:52.300  1964  2328 D use-Rlog/RLOG-RIL-IPC: xmm626_sec_modem_fmt_recv: Received FMT message

06-01 10:53:52.300  2812  2812 D DCT     : [0]getDataOnRoamingEnabled: phoneSubId=-2 isDataRoamingEnabled=false

06-01 10:53:52.300  1964  2328 D use-Rlog/RLOG-RIL-IPC: xmm626_sec_modem_fmt_recv: Message: aseq=0x21, command=IPC_NET_REGIST, type=IPC_TYPE_RESP, size=11

06-01 10:53:52.300  1964  2328 D use-Rlog/RLOG-RIL-IPC: ================================= IPC FMT data =================================

06-01 10:53:52.300  1964  2328 D use-Rlog/RLOG-RIL-IPC: [0000]   FF 03 01 00 00 00 00 00  00 00 00                  ........ ...

06-01 10:53:52.300  2812  2812 D SubscriptionController: [getSubId]- sSlotIdxToSubId.size == 0, return DummySubIds slotIdx=0

06-01 10:53:52.300  1964  2328 D use-Rlog/RLOG-RIL-IPC: ================================================================================

06-01 10:53:52.300  2812  2812 D DCT     : [0]getDataOnRoamingEnabled: phoneSubId=-2 isDataRoamingEnabled=false

06-01 10:53:52.300  1964  2328 D use-Rlog/RLOG-RIL: 2 RIL requests in the queue (0 pending, 2 handled, 0 unhandled)

06-01 10:53:52.300  2812  2812 D SubscriptionController: [getSubId]- sSlotIdxToSubId.size == 0, return DummySubIds slotIdx=0

06-01 10:53:52.300  2812  2812 D DCT     : [0]getDataOnRoamingEnabled: phoneSubId=-2 isDataRoamingEnabled=false

06-01 10:53:52.300  2812  2812 D SubscriptionController: [getSubId]- sSlotIdxToSubId.size == 0, return DummySubIds slotIdx=0

06-01 10:53:52.300  2812  2918 D RILJ    : [3701]< DATA_REGISTRATION_STATE {0, 0, 0, 0, 3} [SUB0]

06-01 10:53:52.300  2812  2812 D DCT     : [0]getDataOnRoamingEnabled: phoneSubId=-2 isDataRoamingEnabled=false

06-01 10:53:52.300  2812  2812 D SubscriptionController: [getSubId]- sSlotIdxToSubId.size == 0, return DummySubIds slotIdx=0

06-01 10:53:52.300  2812  2812 D DCT     : [0]getDataOnRoamingEnabled: phoneSubId=-2 isDataRoamingEnabled=false

06-01 10:53:52.300  2812  2812 D SubscriptionController: [getSubId]- sSlotIdxToSubId.size == 0, return DummySubIds slotIdx=0

06-01 10:53:52.300  2812  2812 D DCT     : [0]getDataOnRoamingEnabled: phoneSubId=-2 isDataRoamingEnabled=false

06-01 10:53:52.300  2812  2812 D SubscriptionController: [getSubId]- sSlotIdxToSubId.size == 0, return DummySubIds slotIdx=0

06-01 10:53:52.300  2812  2812 D DCT     : [0]getDataOnRoamingEnabled: phoneSubId=-2 isDataRoamingEnabled=false

06-01 10:53:52.300  2812  2812 D SubscriptionController: [getSubId]- sSlotIdxToSubId.size == 0, return DummySubIds slotIdx=0

06-01 10:53:52.300  2812  2812 D DCT     : [0]getDataOnRoamingEnabled: phoneSubId=-2 isDataRoamingEnabled=false

06-01 10:53:52.300  2812  2812 D SubscriptionController: [getSubId]- sSlotIdxToSubId.size == 0, return DummySubIds slotIdx=0

06-01 10:53:52.300  2812  2812 D DCT     : [0]getDataOnRoamingEnabled: phoneSubId=-2 isDataRoamingEnabled=false

06-01 10:53:52.300  1964  2328 D use-Rlog/RLOG-RIL-IPC: 

06-01 10:53:52.300  1964  2328 D use-Rlog/RLOG-RIL-IPC: xmm626_sec_modem_fmt_recv: Received FMT message

06-01 10:53:52.300  1964  2328 D use-Rlog/RLOG-RIL-IPC: xmm626_sec_modem_fmt_recv: Message: aseq=0x22, command=IPC_NET_REGIST, type=IPC_TYPE_RESP, size=11

06-01 10:53:52.300  1964  2328 D use-Rlog/RLOG-RIL-IPC: ================================= IPC FMT data =================================

06-01 10:53:52.300  2812  2812 D SubscriptionController: [getSubId]- sSlotIdxToSubId.size == 0, return DummySubIds slotIdx=0

06-01 10:53:52.300  1964  2328 D use-Rlog/RLOG-RIL-IPC: [0000]   FF 02 04 00 00 00 00 00  00 00 00                  ........ ...

06-01 10:53:52.300  1964  2328 D use-Rlog/RLOG-RIL-IPC: ================================================================================

06-01 10:53:52.300  2812  2812 D DCT     : [0]getDataOnRoamingEnabled: phoneSubId=-2 isDataRoamingEnabled=false

06-01 10:53:52.300  1964  2328 D use-Rlog/RLOG-RIL: 1 RIL request in the queue (0 pending, 1 handled, 0 unhandled)

06-01 10:53:52.300  2812  2812 D DctController: handleMessage msg={ when=-404ms what=107 target=com.android.internal.telephony.dataconnection.DctController }

06-01 10:53:52.300  2812  2812 D DctController: onSubInfoReady mPhoneNum=1

06-01 10:53:52.300  1964  2328 D use-Rlog/RLOG-RIL-IPC: 

06-01 10:53:52.300  1964  2328 D use-Rlog/RLOG-RIL-IPC: xmm626_sec_modem_fmt_recv: Received FMT message

06-01 10:53:52.300  2812  2812 D SubscriptionController: [getSubId]- sSlotIdxToSubId.size == 0, return DummySubIds slotIdx=0

06-01 10:53:52.300  1964  2328 D use-Rlog/RLOG-RIL-IPC: xmm626_sec_modem_fmt_recv: Message: aseq=0x23, command=IPC_NET_PLMN_SEL, type=IPC_TYPE_RESP, size=1

06-01 10:53:52.300  2812  2812 D DctController: onSubInfoReady handle pending requests subId=-2

06-01 10:53:52.300  2812  2812 D DctController: onSubInfoReady: SIM card absent on phoneId = 0

06-01 10:53:52.300  1964  2328 D use-Rlog/RLOG-RIL-IPC: ================================= IPC FMT data =================================

06-01 10:53:52.300  1964  2328 D use-Rlog/RLOG-RIL-IPC: [0000]   02                                                 .

06-01 10:53:52.300  1964  2328 D use-Rlog/RLOG-RIL-IPC: ================================================================================

06-01 10:53:52.300  1964  2328 D use-Rlog/RLOG-RIL: 0 RIL request in the queue (0 pending, 0 handled, 0 unhandled)

06-01 10:53:52.300  2812  2812 D SubscriptionController: [getSubId]- sSlotIdxToSubId.size == 0, return DummySubIds slotIdx=0

06-01 10:53:52.300  2812  2812 D DctController: [TNF -2]evalPendingRequest, pending request size is 1

06-01 10:53:52.300  2812  2812 D SubscriptionController: [getSubId]- sSlotIdxToSubId.size == 0, return DummySubIds slotIdx=0

06-01 10:53:52.300  2812  2918 D RILJ    : [3702]< VOICE_REGISTRATION_STATE {10, 0, 0, 0, null, null, null, null, null, null, null, null, null, null, null} [SUB0]

06-01 10:53:52.300  2812  2812 D DctController: [TNF -2]evalPendingRequest: request = NetworkRequest [ id=1, legacyType=-1, [ Capabilities: INTERNET&NOT_RESTRICTED&TRUSTED&NOT_VPN] ]

06-01 10:53:52.300  2812  2812 D SubscriptionController: [getSubId]- sSlotIdxToSubId.size == 0, return DummySubIds slotIdx=0

06-01 10:53:52.300  2812  2812 D DctController: [TNF -2]Cellular needs Network for NetworkRequest [ id=1, legacyType=-1, [ Capabilities: INTERNET&NOT_RESTRICTED&TRUSTED&NOT_VPN] ]

06-01 10:53:52.300  2812  2918 D RILJ    : [3703]< QUERY_NETWORK_SELECTION_MODE {0} [SUB0]

06-01 10:53:52.300  2812  2812 D SubscriptionController: [getSubId]- sSlotIdxToSubId.size == 0, return DummySubIds slotIdx=0

06-01 10:53:52.300  2812  2812 D SubscriptionController: [getSubId]- sSlotIdxToSubId.size == 0, return DummySubIds slotIdx=0

06-01 10:53:52.300  2812  2812 D DctController: [TNF -2]Request not useable, pending request.

06-01 10:53:52.300  2812  2812 D DctController: processRequests

06-01 10:53:52.300  2812  2812 D PhoneProxy: [PhoneProxy] EVENT_REQUEST_VOICE_RADIO_TECH_DONE: newVoiceTech=3

06-01 10:53:52.300  2812  2812 D PhoneProxy: [PhoneProxy] phoneObjectUpdater: newVoiceRadioTech=3

06-01 10:53:52.300  2812  2812 D PhoneProxy: [PhoneProxy] phoneObjectUpdater: No change ignore, newVoiceRadioTech=3 mActivePhone=GSM

06-01 10:53:52.300  2812  2812 D SubscriptionController: [getSubId]- sSlotIdxToSubId.size == 0, return DummySubIds slotIdx=0

06-01 10:53:52.300  2812  2812 D PhoneBase: EVENT_GET_RADIO_CAPABILITY :phone rc : {mPhoneId = 0 mVersion=1 mSession=0 mPhase=0 mRadioAccessFamily=36366 mLogicModemId= mStatus=1}

06-01 10:53:52.300  2812  2812 D PhoneBase: config LCE service failed: com.android.internal.telephony.CommandException: REQUEST_NOT_SUPPORTED

06-01 10:53:52.300  2812  2812 D GSMPhone: Baseband version: I9300XXUGNA8

06-01 10:53:52.305  2812  2812 D SubscriptionController: [getSubId]- sSlotIdxToSubId.size == 0, return DummySubIds slotIdx=0

06-01 10:53:52.310  2812  2812 D UiccController: Received EVENT_GET_ICC_STATUS_DONE

06-01 10:53:52.320  2812  2812 D UiccCard: 1 applications

06-01 10:53:52.320  2812  2812 D UiccCardApplication: Creating UiccApp: {APPTYPE_SIM,APPSTATE_PIN}

06-01 10:53:52.325  2812  2812 D SpnOverride: No SPN in OEM image = /oem/telephony/spn-conf.xml Load SPN from system image

06-01 10:53:52.325  2812  2812 W SpnOverride: Can not open /system/etc/spn-conf.xml

06-01 10:53:52.325  2812  2812 W VoiceMailConstants: Can't open /system/etc/voicemail-conf.xml

06-01 10:53:52.325  2812  2812 D SIMRecords: [SIMRecords] setting0 mMncLength-1

06-01 10:53:52.325  2812  2812 D SIMRecords: [SIMRecords] SIMRecords: onRadioOffOrNotAvailable set 'gsm.sim.operator.numeric' to operator=null

06-01 10:53:52.325  2812  2812 D SIMRecords: [SIMRecords] update icc_operator_numeric=null

06-01 10:53:52.325  2812  2812 D TelephonyManager: setTelephonyProperty: success phoneId=0 property=gsm.sim.operator.numeric value:  propVal=

06-01 10:53:52.325  2812  2812 D TelephonyManager: setTelephonyProperty: success phoneId=0 property=gsm.sim.operator.alpha value:  propVal=

06-01 10:53:52.325  2812  2812 D TelephonyManager: setTelephonyProperty: success phoneId=0 property=gsm.sim.operator.iso-country value:  propVal=

06-01 10:53:52.330  2812  2812 D UiccCardApplication: Notifying 1 registrant: LOCKED

06-01 10:53:52.330  2812  2812 D SIMRecords: [SIMRecords] getOperatorNumeric: IMSI == null

06-01 10:53:52.330  2812  2812 D SIMRecords: [SIMRecords] SIMRecords X ctor this=SimRecords: mDestroyed=false mContext=com.android.phone.PhoneGlobals@ba32de5 mCi=com.android.internal.telephony.RIL@4cc13b5 mFh=Handler (com.android.internal.telephony.uicc.SIMFileHandler) {9480ba} mParentApp=com.android.internal.telephony.uicc.UiccCardApplication@84fab6b mSpnOverride=mSpnOverride recordsLoadedRegistrants=android.os.RegistrantList@fe8c6c8 mImsiReadyRegistrants=android.os.RegistrantList@95dc361 mRecordsEventsRegistrants=android.os.RegistrantList@c79ee86 mNewSmsRegistrants=android.os.RegistrantList@83b9347 mNetworkSelectionModeAutomaticRegistrants=android.os.RegistrantList@8278774 recordsToLoad=0 adnCache=Handler (com.android.internal.telephony.uicc.AdnRecordCache) {bd2349d} recordsRequested=false iccid=null msisdnTag=null voiceMailNum=null voiceMailTag=null newVoiceMailNum=null newVoiceMailTag=null isVoiceMailFixed=false mncLength=-1 mailboxIndex=0 spn=null mVmConfigcom.android.internal.telephony.uicc.VoiceMailConstants@2f66d12 callForwardingEnabled=0 spnState=null mCphsInfo=null mCspPlmnEnabled=true efMWIS=null efCPHS_MWI=null mEfCff=null mEfCfis=null getOperatorNumeric=null

06-01 10:53:52.355  2812  2812 D CAT     : CatService: registerForRecordsLoaded slotid=0 instance:Handler (com.android.internal.telephony.cat.CatService) {f61a43f}

06-01 10:53:52.355  2812  2812 D CAT     : CatService: Running CAT service on Slotid: 0. STK app installed:true

06-01 10:53:52.355  2812  2812 D UiccCard: Before privilege rules: null : CARDSTATE_PRESENT

06-01 10:53:52.355  2812  2812 D RILJ    : [3704]> RIL_REQUEST_SIM_OPEN_CHANNEL [SUB0]

06-01 10:53:52.355  1964  2012 D use-Rlog/RLOG-RIL: Detected string with a size of 19 bytes

06-01 10:53:52.355  1964  2012 D use-Rlog/RLOG-RIL: 1 RIL request in the queue (1 pending, 0 handled, 0 unhandled)

06-01 10:53:52.355  1964  2332 D use-Rlog/RLOG-RIL: Unhandled RIL request: 115

06-01 10:53:52.355  1964  2332 D use-Rlog/RLOG-RIL: 0 RIL request in the queue (0 pending, 0 handled, 0 unhandled)

06-01 10:53:52.355  2812  2812 D UiccCard: update: radioState=RADIO_ON mLastRadioState=RADIO_UNAVAILABLE

06-01 10:53:52.355  2812  2812 D UiccController: Notifying IccChangedRegistrants

06-01 10:53:52.355  2812  2918 D RilRequest: [3704]< RIL_REQUEST_SIM_OPEN_CHANNEL error: com.android.internal.telephony.CommandException: REQUEST_NOT_SUPPORTED ret=

06-01 10:53:52.360  2812  2812 D PhoneProxy: [PhoneProxy] EVENT_REQUEST_VOICE_RADIO_TECH_DONE: newVoiceTech=3

06-01 10:53:52.360  2812  2812 D PhoneProxy: [PhoneProxy] phoneObjectUpdater: newVoiceRadioTech=3

06-01 10:53:52.360  2812  2812 D PhoneProxy: [PhoneProxy] phoneObjectUpdater: No change ignore, newVoiceRadioTech=3 mActivePhone=GSM

06-01 10:53:52.365  2812  2812 E RIL_ImsSms: IMS State query failed with exp com.android.internal.telephony.CommandException: REQUEST_NOT_SUPPORTED

06-01 10:53:52.365  2812  2812 D CdmaSSM : CDMA_SUBSCRIPTION_SOURCE event = 2

06-01 10:53:52.365  2812  2812 D UiccController: Received EVENT_GET_ICC_STATUS_DONE

06-01 10:53:52.365  2812  2812 D UiccCard: 1 applications

06-01 10:53:52.365  2812  2812 D UiccCardApplication: APPTYPE_SIM update. New {APPTYPE_SIM,APPSTATE_PIN}

06-01 10:53:52.365  2812  2812 D UiccCard: Before privilege rules: Handler (com.android.internal.telephony.uicc.UiccCarrierPrivilegeRules) {458510c} : CARDSTATE_PRESENT

06-01 10:53:52.365  2812  2812 D UiccCard: update: radioState=RADIO_ON mLastRadioState=RADIO_ON

06-01 10:53:52.365  2812  2812 D UiccController: Notifying IccChangedRegistrants

06-01 10:53:52.365  2812  2812 D UiccController: Received EVENT_GET_ICC_STATUS_DONE

06-01 10:53:52.365  2812  2812 D UiccCard: 1 applications

06-01 10:53:52.365  2812  2812 D UiccCardApplication: APPTYPE_SIM update. New {APPTYPE_SIM,APPSTATE_PIN}

06-01 10:53:52.365  2812  2812 D UiccCard: Before privilege rules: Handler (com.android.internal.telephony.uicc.UiccCarrierPrivilegeRules) {458510c} : CARDSTATE_PRESENT

06-01 10:53:52.365  2812  2812 D UiccCard: update: radioState=RADIO_ON mLastRadioState=RADIO_ON

06-01 10:53:52.365  2812  2812 D UiccController: Notifying IccChangedRegistrants

06-01 10:53:52.365  2812  2812 D PHONE   : [ServiceState] setDataRegState=1

06-01 10:53:52.365  2812  2812 D PHONE   : [ServiceState] setDataRadioTechnology=0

06-01 10:53:52.365  2812  2812 D GsmSST  : [GsmSST] handlPollStateResultMessage: GsmSST setDataRegState=1 regState=0 dataRadioTechnology=0

06-01 10:53:52.365  2812  2812 D PHONE   : [ServiceState] setVoiceRegState=1

06-01 10:53:52.365  2812  2812 E PHONE   : [ServiceState] setState deprecated use setVoiceRegState()

06-01 10:53:52.370  2812  2812 D SubscriptionController: [getSubId]- sSlotIdxToSubId.size == 0, return DummySubIds slotIdx=0

06-01 10:53:52.370  2812  2812 D GsmSST  : [GsmSST] Poll ServiceState done:  oldSS=[3 3 voice home data home null null null null null null  Unknown Unknown CSS not supported -1 -1 RoamInd=-1 DefRoamInd=-1 EmergOnly=false IsDataRoamingFromRegistration=false] newSS=[1 1 voice home data home Mobistar Mobistar 20610 Mobistar Mobistar 20610  Unknown Unknown CSS not supported -1 -1 RoamInd=-1 DefRoamInd=-1 EmergOnly=true IsDataRoamingFromRegistration=false] oldMaxDataCalls=1 mNewMaxDataCalls=1 oldReasonDataDenied=-1 mNewReasonDataDenied=-1

06-01 10:53:52.370  2812  2812 D PHONE   : [ServiceState] setNullState=1

06-01 10:53:52.370  2812  2812 D GsmSST  : [GsmSST] updateSpnDisplay: radio is on but out of service, set plmn='Emergency calls only'

06-01 10:53:52.370  2812  2812 D SubscriptionController: [getSubId]- sSlotIdxToSubId.size == 0, return DummySubIds slotIdx=0

06-01 10:53:52.370  2812  2812 D GsmSST  : [GsmSST] updateSpnDisplay: changed sending intent rule=0 showPlmn='true' plmn='Emergency calls only' showSpn='false' spn='' dataSpn='' subId='-2'

06-01 10:53:52.370  2812  2812 D SubscriptionController: [getSubId]- sSlotIdxToSubId.size == 0, return DummySubIds slotIdx=0

06-01 10:53:52.375  2812  2812 D SubscriptionController: [getSubId]- sSlotIdxToSubId.size == 0, return DummySubIds slotIdx=0

06-01 10:53:52.380  2812  2812 D SubscriptionController: [setPlmnSpn] No valid subscription to store info

06-01 10:53:52.380  2812  2812 D SubscriptionController: notifySubscriptionInfoChanged:

06-01 10:53:52.380  2812  2812 D TelephonyManager: setTelephonyProperty: success phoneId=0 property=gsm.operator.alpha value: Mobistar propVal=Mobistar

06-01 10:53:52.380  2812  2812 D TelephonyManager: setTelephonyProperty: success phoneId=0 property=gsm.operator.numeric value: 20610 propVal=20610

06-01 10:53:52.380  2812  2812 D GsmSST  : [GsmSST] update mccmnc=20610 fromServiceState=true

06-01 10:53:52.395  2812  2850 D SubscriptionController: [getActiveSubInfoList]+

06-01 10:53:52.400  2812  2812 D TelephonyManager: setTelephonyProperty: success phoneId=0 property=gsm.operator.iso-country value: be propVal=be

06-01 10:53:52.400  2812  2850 D SubscriptionController: selection:sim_id>=0 null

06-01 10:53:52.410  2812  2812 D GsmSST  : [GsmSST] pollStateDone: no nitz but one TZ for iso-cc=be with zone.getID=Europe/Brussels testOneUniqueOffsetPath=false

06-01 10:53:52.410  2812  2812 D GsmSST  : [GsmSST] setAndBroadcastNetworkSetTimeZone: setTimeZone=Europe/Brussels

06-01 10:53:52.415  2812  2812 D GsmSST  : [GsmSST] setAndBroadcastNetworkSetTimeZone: call alarm.setTimeZone and broadcast zoneId=Europe/Brussels

06-01 10:53:52.415  2812  2812 D GsmSST  : [GsmSST] shouldFixTimeZoneNow: retVal=false iccCardExist=false operatorNumeric=20610 mcc=206 prevOperatorNumeric= prevMcc=207 needToFixTimeZone=false ltod=06-01 10:53:52.421

06-01 10:53:52.415  2812  2812 D TelephonyManager: setTelephonyProperty: success phoneId=0 property=gsm.operator.isroaming value: false propVal=false

06-01 10:53:52.415  2812  2812 D GsmSST  : [GsmSST] Broadcasting ServiceState : 1 1 voice home data home Mobistar Mobistar 20610 Mobistar Mobistar 20610  Unknown Unknown CSS not supported -1 -1 RoamInd=-1 DefRoamInd=-1 EmergOnly=true IsDataRoamingFromRegistration=false

06-01 10:53:52.415  2812  2812 D SubscriptionController: [getSubId]- sSlotIdxToSubId.size == 0, return DummySubIds slotIdx=0

06-01 10:53:52.415  2812  2812 D DefaultPhoneNotifier: nofityServiceState: mRegistry=com.android.internal.telephony.ITelephonyRegistry$Stub$Proxy@d42da20 ss=1 1 voice home data home Mobistar Mobistar 20610 Mobistar Mobistar 20610  Unknown Unknown CSS not supported -1 -1 RoamInd=-1 DefRoamInd=-1 EmergOnly=true IsDataRoamingFromRegistration=false sender=Handler (com.android.internal.telephony.gsm.GSMPhone) {b910da1} phondId=0 subId=-2

06-01 10:53:52.420  2812  2812 D SubscriptionController: [getSlotId]- subId invalid

06-01 10:53:52.425  2812  2812 D SubscriptionController: getSimStateForSlotIdx:  simState=NOT_READY ordinal=6

06-01 10:53:52.425  2335  2381 D SubscriptionManager: getSimStateForSubscriber: simState=6 slotIdx=0

06-01 10:53:52.425  2335  2381 D TelephonyManager: getSimState: default sim:-1, sim state for slotIdx=0 is 6, return state as unknown

06-01 10:53:52.425  2812  2812 D GsmSST  : [GsmSST] notifyDataRegStateRilRadioTechnologyChanged: drs=1 rat=0

06-01 10:53:52.425  2812  2812 D TelephonyManager: setTelephonyProperty: success phoneId=0 property=gsm.network.type value: Unknown propVal=Unknown

06-01 10:53:52.425  2812  2812 D DCT     : [0]get all active apn types

06-01 10:53:52.425  2812  2812 D SubscriptionController: [getSubId]- sSlotIdxToSubId.size == 0, return DummySubIds slotIdx=0

06-01 10:53:52.425  2812  2812 D GsmSST  : [GsmSST] getCellLocation(): X good mCellLoc=[0,0,-1]

06-01 10:53:52.425  2335  2851 D TelephonyRegistry: notifyCellLocationForSubscriber: subId=-2 cellLocation=Bundle[mParcelledData.dataSize=64]

06-01 10:53:52.425  2812  2812 D DctController: handleMessage msg={ when=-124ms what=100 target=com.android.internal.telephony.dataconnection.DctController }

06-01 10:53:52.425  2812  2812 D DcSwitchAsyncChannel: [DcSwitchAsyncChannel-0]: rspIsIdle=true

06-01 10:53:52.425  2812  2812 D SubscriptionController: [getPhoneId]- invalid subId return=-1

06-01 10:53:52.425  2812  2812 D DcSwitchAsyncChannel: [DcSwitchAsyncChannel-0]: rspIsIdle=true

06-01 10:53:52.425  2812  2812 D DctController: onProcessRequest requestedPhoneId=-1, activePhoneId=-1

06-01 10:53:52.425  2812  2812 D SIMRecords: [SIMRecords] only fetch EF_LI and EF_PL in lock state

06-01 10:53:52.425  2812  2812 D CAT     : CatService: handleMessage[8]

06-01 10:53:52.425  2812  2812 D CAT     : CatService: MSG_ID_ICC_CHANGED

06-01 10:53:52.425  2812  2812 D CAT     : CatService: New Card State = CARDSTATE_PRESENT Old Card State = CARDSTATE_ABSENT

06-01 10:53:52.425  2812  2812 D RILJ    : [3705]> RIL_REQUEST_REPORT_STK_SERVICE_IS_RUNNING [SUB0]

06-01 10:53:52.430  2812  2812 D GSMPhone: [GSMPhone] New Uicc application found

06-01 10:53:52.430  2812  2812 D GsmSST  : [GsmSST] New card found

06-01 10:53:52.430  2812  2812 D DCT     : [0]handleMessage msg={ when=-71ms what=270369 obj=android.os.AsyncResult@e6e8c6a target=com.android.internal.telephony.dataconnection.DcTracker }

06-01 10:53:52.430  2812  2812 D DCT     : [0]onUpdateIcc: newIccRecords null

06-01 10:53:52.430  2812  2812 D SubscriptionController: [getSubId]- sSlotIdxToSubId.size == 0, return DummySubIds slotIdx=0

06-01 10:53:52.430  2812  2812 D GsmSMSDispatcher: GsmSMSDispatcher: subId = -2 slotId = 0

06-01 10:53:52.430  2812  2812 D GsmSMSDispatcher: New Uicc application found

06-01 10:53:52.430  2812  2812 D IccCardProxy: Icc changed. Reregestering.

06-01 10:53:52.430  2812  2812 D UiccCardApplication: Notifying 1 registrant: LOCKED

06-01 10:53:52.430  2812  2812 E IccCardProxy: setExternalState: set mPhoneId=0 mExternalState=PIN_REQUIRED

06-01 10:53:52.430  2812  2812 D TelephonyManager: setTelephonyProperty: success phoneId=0 property=gsm.sim.state value: PIN_REQUIRED propVal=PIN_REQUIRED

06-01 10:53:52.430  1964  2012 D use-Rlog/RLOG-RIL: 1 RIL request in the queue (1 pending, 0 handled, 0 unhandled)

06-01 10:53:52.430  1964  2332 D use-Rlog/RLOG-RIL: Unhandled RIL request: 103

06-01 10:53:52.430  1964  2332 D use-Rlog/RLOG-RIL: 0 RIL request in the queue (0 pending, 0 handled, 0 unhandled)

06-01 10:53:52.430  2812  2918 D RilRequest: [3705]< RIL_REQUEST_REPORT_STK_SERVICE_IS_RUNNING error: com.android.internal.telephony.CommandException: REQUEST_NOT_SUPPORTED ret=

06-01 10:53:52.430  2812  2812 D IccCardProxy: Sending intent ACTION_INTERNAL_SIM_STATE_CHANGED for mPhoneId : 0

06-01 10:53:52.430  2812  2812 D CAT     : CatService: handleMessage[8]

06-01 10:53:52.430  2812  2812 D CAT     : CatService: MSG_ID_ICC_CHANGED

06-01 10:53:52.430  2812  2812 D CAT     : CatService: New Card State = CARDSTATE_PRESENT Old Card State = CARDSTATE_PRESENT

06-01 10:53:52.430  2812  2812 D UiccCard: Error in SIM access with exceptioncom.android.internal.telephony.CommandException: REQUEST_NOT_SUPPORTED

06-01 10:53:52.430  2812  2812 D DCT     : [0]handleMessage msg={ when=-65ms what=270369 obj=android.os.AsyncResult@7d6455b target=com.android.internal.telephony.dataconnection.DcTracker }

06-01 10:53:52.430  2812  2812 D DCT     : [0]onUpdateIcc: newIccRecords null

06-01 10:53:52.430  2812  2812 D SubscriptionController: [getSubId]- sSlotIdxToSubId.size == 0, return DummySubIds slotIdx=0

06-01 10:53:52.430  2812  2812 D GsmSMSDispatcher: GsmSMSDispatcher: subId = -2 slotId = 0

06-01 10:53:52.430  2812  2812 E IccCardProxy: setExternalState: !override and newstate unchanged from PIN_REQUIRED

06-01 10:53:52.430  2812  2812 D CAT     : CatService: handleMessage[8]

06-01 10:53:52.430  2812  2812 D CAT     : CatService: MSG_ID_ICC_CHANGED

06-01 10:53:52.430  2812  2812 D CAT     : CatService: New Card State = CARDSTATE_PRESENT Old Card State = CARDSTATE_PRESENT

06-01 10:53:52.430  2812  2812 D DCT     : [0]handleMessage msg={ when=-65ms what=270369 obj=android.os.AsyncResult@ebf71f8 target=com.android.internal.telephony.dataconnection.DcTracker }

06-01 10:53:52.430  2812  2812 D DCT     : [0]onUpdateIcc: newIccRecords null

06-01 10:53:52.430  2812  2812 D SubscriptionController: [getSubId]- sSlotIdxToSubId.size == 0, return DummySubIds slotIdx=0

06-01 10:53:52.430  2812  2812 D GsmSMSDispatcher: GsmSMSDispatcher: subId = -2 slotId = 0

06-01 10:53:52.430  2812  2812 E IccCardProxy: setExternalState: !override and newstate unchanged from PIN_REQUIRED

06-01 10:53:52.430  2812  2812 D CAT     : CatService: handleMessage[8]

06-01 10:53:52.430  2812  2812 D CAT     : CatService: MSG_ID_ICC_CHANGED

06-01 10:53:52.430  2812  2812 D CAT     : CatService: New Card State = CARDSTATE_PRESENT Old Card State = CARDSTATE_PRESENT

06-01 10:53:52.430  2812  2812 D GsmSST  : [GsmSST] SubscriptionListener.onSubscriptionInfoChanged

06-01 10:53:52.430  2812  2812 D SubscriptionController: [getSubId]- sSlotIdxToSubId.size == 0, return DummySubIds slotIdx=0

06-01 10:53:52.430  2812  2812 D DCT     : [0]SubscriptionListener.onSubscriptionInfoChanged

06-01 10:53:52.430  2812  2812 D SubscriptionController: [getSubId]- sSlotIdxToSubId.size == 0, return DummySubIds slotIdx=0

06-01 10:53:52.430  2812  2812 D SubscriptionController: [getActiveSubInfoList]+

06-01 10:53:52.435  2812  2812 D SubscriptionController: selection:sim_id>=0 null

06-01 10:53:52.455  2812  2812 D SubscriptionController: [getActiveSubInfoList]- no info return

06-01 10:53:52.455  2812  2812 E PhoneBase: Error! unregisterForCallWaiting() in PhoneBase should not be called, CDMAPhone inactive.

06-01 10:53:52.460  2812  2812 D SubscriptionController: [getSubId]- sSlotIdxToSubId.size == 0, return DummySubIds slotIdx=0

06-01 10:53:52.460  2812  2812 D SubscriptionController: [getSubId]- sSlotIdxToSubId.size == 0, return DummySubIds slotIdx=0

06-01 10:53:52.460  2812  2812 D SubscriptionController: [getPhoneId]- invalid subId return=-1

06-01 10:53:52.465  2812  2812 D SubscriptionController: [getSubId]- sSlotIdxToSubId.size == 0, return DummySubIds slotIdx=0

06-01 10:53:52.465  2812  2812 D SubscriptionController: [getSubId]- sSlotIdxToSubId.size == 0, return DummySubIds slotIdx=0

06-01 10:53:52.465  2812  2812 D SubscriptionController: [getSubId]- sSlotIdxToSubId.size == 0, return DummySubIds slotIdx=0

06-01 10:53:52.530  2812  2850 D SubscriptionController: [getActiveSubInfoList]- no info return

06-01 10:53:52.540  2812  2812 E PhoneBase: Error! registerForCallWaiting() in PhoneBase should not be called, CDMAPhone inactive.

06-01 10:53:52.560  2812  2812 D DCT     : [0]handleMessage msg={ when=-135ms what=270377 obj=android.os.AsyncResult@229dc37 target=com.android.internal.telephony.dataconnection.DcTracker }

06-01 10:53:52.560  2812  2812 D DCT     : [0]onUpdateIcc: newIccRecords null

06-01 10:53:52.560  2812  2812 D DCT     : [0]setupDataOnConnectableApns: nwTypeChanged

06-01 10:53:52.560  2812  2812 D DCT     : [0]setupDataOnConnectableApns: apnContext {mApnType=dun mState=IDLE mWaitingApns={null} mWaitingApnsPermanentFailureCountDown=0 mApnSetting={null} mReason=radioTurnedOff mDataEnabled=false mDependencyMet=true}

06-01 10:53:52.560  2812  2812 D DCT     : [0]setupDataOnConnectableApns: apnContext {mApnType=hipri mState=IDLE mWaitingApns={null} mWaitingApnsPermanentFailureCountDown=0 mApnSetting={null} mReason=radioTurnedOff mDataEnabled=false mDependencyMet=true}

06-01 10:53:52.560  2812  2812 D DCT     : [0]setupDataOnConnectableApns: apnContext {mApnType=supl mState=IDLE mWaitingApns={null} mWaitingApnsPermanentFailureCountDown=0 mApnSetting={null} mReason=radioTurnedOff mDataEnabled=false mDependencyMet=true}

06-01 10:53:52.560  2812  2812 D DCT     : [0]setupDataOnConnectableApns: apnContext {mApnType=default mState=IDLE mWaitingApns={null} mWaitingApnsPermanentFailureCountDown=0 mApnSetting={null} mReason=radioTurnedOff mDataEnabled=false mDependencyMet=true}

06-01 10:53:52.560  2812  2812 D DCT     : [0]setupDataOnConnectableApns: apnContext {mApnType=mms mState=IDLE mWaitingApns={null} mWaitingApnsPermanentFailureCountDown=0 mApnSetting={null} mReason=radioTurnedOff mDataEnabled=false mDependencyMet=true}

06-01 10:53:52.560  2812  2812 D SubscriptionController: [getSubId]- sSlotIdxToSubId.size == 0, return DummySubIds slotIdx=0

06-01 10:53:52.560  2812  2812 D SubscriptionController: [getSubId]- sSlotIdxToSubId.size == 0, return DummySubIds slotIdx=0

06-01 10:53:52.560  2812  2812 D PhoneBase: Get callforwarding info from perferences

06-01 10:53:52.560  2812  2812 D PhoneBase: ProvisionStatus: 1

06-01 10:53:52.560  2812  2812 D SubscriptionController: [getSubId]- sSlotIdxToSubId.size == 0, return DummySubIds slotIdx=0

06-01 10:53:52.560  2812  2812 D PhoneBase: Get video call forwarding info from preferences

06-01 10:53:52.560  2812  2812 D SubscriptionController: [getSubId]- sSlotIdxToSubId.size == 0, return DummySubIds slotIdx=0

06-01 10:53:52.560  2812  2812 D SubscriptionController: [getSubId]- sSlotIdxToSubId.size == 0, return DummySubIds slotIdx=0

06-01 10:53:52.565  2812  2812 E IccCardProxy: setExternalState: !override and newstate unchanged from PIN_REQUIRED

06-01 10:53:52.565  2812  2812 D SubscriptionInfoUpdater: [Receiver]+

06-01 10:53:52.565  2812  2812 D SubscriptionInfoUpdater: Action: android.intent.action.internal_sim_state_changed

06-01 10:53:52.565  2812  2812 D SubscriptionInfoUpdater: slotId: 0

06-01 10:53:52.565  2812  2812 D SubscriptionInfoUpdater: simStatus: LOCKED

06-01 10:53:52.565  2812  2812 D SubscriptionInfoUpdater: Wait for SIM1 IccId

06-01 10:53:52.565  2812  2812 D SubscriptionInfoUpdater: [Receiver]-

06-01 10:53:52.565  2812  2812 D DctController: handleMessage msg={ when=-133ms what=107 target=com.android.internal.telephony.dataconnection.DctController }

06-01 10:53:52.565  2812  2812 D DctController: onSubInfoReady mPhoneNum=1

06-01 10:53:52.565  2812  2812 D SubscriptionController: [getSubId]- sSlotIdxToSubId.size == 0, return DummySubIds slotIdx=0

06-01 10:53:52.565  2812  2812 D DctController: onSubInfoReady handle pending requests subId=-2

06-01 10:53:52.565  2812  2812 D SubscriptionController: [getSubId]- sSlotIdxToSubId.size == 0, return DummySubIds slotIdx=0

06-01 10:53:52.565  2812  2812 D DctController: [TNF -2]evalPendingRequest, pending request size is 1

06-01 10:53:52.565  2812  2812 D SubscriptionController: [getSubId]- sSlotIdxToSubId.size == 0, return DummySubIds slotIdx=0

06-01 10:53:52.565  2812  2812 D DctController: [TNF -2]evalPendingRequest: request = NetworkRequest [ id=1, legacyType=-1, [ Capabilities: INTERNET&NOT_RESTRICTED&TRUSTED&NOT_VPN] ]

06-01 10:53:52.565  2812  2812 D SubscriptionController: [getSubId]- sSlotIdxToSubId.size == 0, return DummySubIds slotIdx=0

06-01 10:53:52.565  2812  2812 D DctController: [TNF -2]Cellular needs Network for NetworkRequest [ id=1, legacyType=-1, [ Capabilities: INTERNET&NOT_RESTRICTED&TRUSTED&NOT_VPN] ]

06-01 10:53:52.565  2812  2812 D SubscriptionController: [getSubId]- sSlotIdxToSubId.size == 0, return DummySubIds slotIdx=0

06-01 10:53:52.565  2812  2812 D SubscriptionController: [getSubId]- sSlotIdxToSubId.size == 0, return DummySubIds slotIdx=0

06-01 10:53:52.565  2812  2812 D DctController: [TNF -2]Request not useable, pending request.

06-01 10:53:52.565  2812  2812 D DctController: processRequests

06-01 10:53:52.565  2812  2812 D SubscriptionController: [getSubId]- sSlotIdxToSubId.size == 0, return DummySubIds slotIdx=0

06-01 10:53:52.565  2812  2812 D SubscriptionInfoUpdater: Querying IccId

06-01 10:53:52.565  2812  2812 D RILJ    : [3706]> iccIO: SIM_IO 0xc0 0x2fe2  path: 3F00,0,0,0 aid: null [SUB0]

06-01 10:53:52.570  1964  2012 D use-Rlog/RLOG-RIL: 1 RIL request in the queue (1 pending, 0 handled, 0 unhandled)

06-01 10:53:52.570  1964  2332 E use-Rlog/RLOG-RIL: ril_request_sim_io: SIM is locked or absent.

06-01 10:53:52.570  1964  2332 D use-Rlog/RLOG-RIL-IPC: 

06-01 10:53:52.570  1964  2332 D use-Rlog/RLOG-RIL-IPC: xmm626_sec_modem_fmt_send: Sent FMT message

06-01 10:53:52.570  1964  2332 D use-Rlog/RLOG-RIL-IPC: xmm626_sec_modem_fmt_send: Message: mseq=0x24, command=IPC_SEC_RSIM_ACCESS, type=IPC_TYPE_GET, size=6

06-01 10:53:52.570  1964  2332 D use-Rlog/RLOG-RIL-IPC: ================================= IPC FMT data =================================

06-01 10:53:52.570  1964  2332 D use-Rlog/RLOG-RIL-IPC: [0000]   C0 E2 2F 00 00 00                                  ../...

06-01 10:53:52.570  1964  2332 D use-Rlog/RLOG-RIL-IPC: ================================================================================

06-01 10:53:52.570  2812  2812 D SubscriptionInfoUpdater: Wait for SIM1 IccId

06-01 10:53:52.570  2812  2812 D DctController: handleMessage msg={ when=-6ms what=100 target=com.android.internal.telephony.dataconnection.DctController }

06-01 10:53:52.575  2812  2812 D DcSwitchAsyncChannel: [DcSwitchAsyncChannel-0]: rspIsIdle=true

06-01 10:53:52.575  2812  2812 D SubscriptionController: [getPhoneId]- invalid subId return=-1

06-01 10:53:52.575  2812  2812 D DcSwitchAsyncChannel: [DcSwitchAsyncChannel-0]: rspIsIdle=true

06-01 10:53:52.575  2812  2812 D DctController: onProcessRequest requestedPhoneId=-1, activePhoneId=-1

06-01 10:53:52.640  1964  2328 D use-Rlog/RLOG-RIL-IPC: 

06-01 10:53:52.640  1964  2328 D use-Rlog/RLOG-RIL-IPC: xmm626_sec_modem_fmt_recv: Received FMT message

06-01 10:53:52.640  1964  2328 D use-Rlog/RLOG-RIL-IPC: xmm626_sec_modem_fmt_recv: Message: aseq=0x24, command=IPC_SEC_RSIM_ACCESS, type=IPC_TYPE_RESP, size=37

06-01 10:53:52.640  1964  2328 D use-Rlog/RLOG-RIL-IPC: ================================= IPC FMT data =================================

06-01 10:53:52.640  1964  2328 D use-Rlog/RLOG-RIL-IPC: [0000]   90 00 22 62 20 82 02 41  21 83 02 2F E2 A5 03 C0   .."b ..A !../....

06-01 10:53:52.640  1964  2328 D use-Rlog/RLOG-RIL-IPC: [0010]   01 40 8A 01 05 8B 06 2F  06 01 01 00 00 80 02 00   .@...../ ........

06-01 10:53:52.640  1964  2328 D use-Rlog/RLOG-RIL-IPC: [0020]   0A 81 02 00 1C                                     .....

06-01 10:53:52.640  1964  2328 D use-Rlog/RLOG-RIL-IPC: ================================================================================

06-01 10:53:52.640  1964  2328 D use-Rlog/RLOG-RIL: 0 RIL request in the queue (0 pending, 0 handled, 0 unhandled)

06-01 10:53:52.640  2812  2918 D RILJ    : [3706]< SIM_IO IccIoResponse sw1:0x90 sw2:0x0 [SUB0]

06-01 10:53:52.645  2812  2812 D SubscriptionInfoUpdater: handleMessage : <EVENT_SIM_LOCKED_QUERY_ICCID_DONE> SIM1

06-01 10:53:52.645  2812  2812 D SubscriptionInfoUpdater: Query IccId fail: java.lang.NullPointerException: Attempt to read from null array

06-01 10:53:52.645  2812  2812 D SubscriptionInfoUpdater: sIccId[0] = 

06-01 10:53:52.645  2812  2812 D SubscriptionInfoUpdater: All IccIds query complete

06-01 10:53:52.645  2812  2812 D SubscriptionInfoUpdater: updateSubscriptionInfoByIccId:+ Start

06-01 10:53:52.645  2812  2812 D SubscriptionInfoUpdater: insertedSimCount = 0

06-01 10:53:52.645  2812  2812 D SubscriptionController: [getSubInfoUsingSlotIdWithCheck]+ slotId:0

06-01 10:53:52.655  2812  2812 D SubscriptionController: [getSubInfoUsingSlotId]- null info return

06-01 10:53:52.655  2812  2812 D SubscriptionInfoUpdater: updateSubscriptionInfoByIccId: No SIM in slot 0 last time

06-01 10:53:52.655  2812  2812 D SubscriptionInfoUpdater: updateSubscriptionInfoByIccId: oldIccId[0] = , sIccId[0] = 

06-01 10:53:52.655  2812  2812 D SubscriptionInfoUpdater: updateSubscriptionInfoByIccId: No SIM inserted in slot 0 this time

06-01 10:53:52.655  2812  2812 D SubscriptionInfoUpdater: updateSubscriptionInfoByIccId: sInsertSimState[0] = -99

06-01 10:53:52.655  2812  2812 D SubscriptionController: [getActiveSubInfoList]+

06-01 10:53:52.655  2812  2812 D SubscriptionController: selection:sim_id>=0 null

06-01 10:53:52.660  2812  2812 D SubscriptionController: [getActiveSubInfoList]- no info return

06-01 10:53:52.660  2812  2812 D SubscriptionInfoUpdater: updateSubscriptionInfoByIccId: nSubCount = 0

06-01 10:53:52.660  2812  2812 D SubscriptionInfoUpdater: updateSubscriptionInfoByIccId:- SsubscriptionInfo update complete

06-01 10:53:52.660  2812  2812 D SubscriptionController: [getSubId]- sSlotIdxToSubId.size == 0, return DummySubIds slotIdx=0

06-01 10:53:52.660  2812  2812 D SubscriptionInfoUpdater: Broadcasting intent ACTION_SIM_STATE_CHANGED LOADED reason null for mCardIndex : 0

06-01 10:53:52.670  2812  2812 D SubscriptionInfoUpdater: [Receiver]+

06-01 10:53:52.670  2812  2812 D SubscriptionInfoUpdater: Action: android.intent.action.SIM_STATE_CHANGED

06-01 10:53:52.670  2812  2812 D SubscriptionInfoUpdater: slotId: 0

06-01 10:53:52.670  2812  2812 D SubscriptionInfoUpdater: simStatus: LOCKED

06-01 10:53:52.670  2812  2812 D SubscriptionInfoUpdater: Ignoring simStatus: LOCKED

06-01 10:53:52.670  2812  2812 D SubscriptionInfoUpdater: All IccIds query complete

06-01 10:53:52.670  2812  2812 D SubscriptionInfoUpdater: All IccIds query complete

06-01 10:53:52.670  2812  2812 D SubscriptionInfoUpdater: updateSubscriptionInfoByIccId:+ Start

06-01 10:53:52.670  2812  2812 D SubscriptionInfoUpdater: insertedSimCount = 0

06-01 10:53:52.670  2812  2812 D SubscriptionController: [getSubInfoUsingSlotIdWithCheck]+ slotId:0

06-01 10:53:52.680  2812  2812 D SubscriptionController: [getSubInfoUsingSlotId]- null info return

06-01 10:53:52.680  2812  2812 D SubscriptionInfoUpdater: updateSubscriptionInfoByIccId: No SIM in slot 0 last time

06-01 10:53:52.680  2812  2812 D SubscriptionInfoUpdater: updateSubscriptionInfoByIccId: oldIccId[0] = , sIccId[0] = 

06-01 10:53:52.680  2812  2812 D SubscriptionInfoUpdater: updateSubscriptionInfoByIccId: No SIM inserted in slot 0 this time

06-01 10:53:52.680  2812  2812 D SubscriptionInfoUpdater: updateSubscriptionInfoByIccId: sInsertSimState[0] = -99

06-01 10:53:52.680  2812  2812 D SubscriptionController: [getActiveSubInfoList]+

06-01 10:53:52.680  2812  2812 D SubscriptionController: selection:sim_id>=0 null

06-01 10:53:52.690  2812  3017 D SubscriptionController: [getActiveSubInfoList]+

06-01 10:53:52.690  2812  2812 D SubscriptionController: [getActiveSubInfoList]- no info return

06-01 10:53:52.690  2812  2812 D SubscriptionInfoUpdater: updateSubscriptionInfoByIccId: nSubCount = 0

06-01 10:53:52.690  2812  2812 D SubscriptionInfoUpdater: updateSubscriptionInfoByIccId:- SsubscriptionInfo update complete

06-01 10:53:52.690  2812  2812 D SubscriptionInfoUpdater: [Receiver]-

06-01 10:53:52.695  2812  2812 D SubscriptionController: [getPhoneId]- invalid subId return=-1

06-01 10:53:52.695  2812  2812 D SubscriptionController: [getSubId]- sSlotIdxToSubId.size == 0, return DummySubIds slotIdx=0

06-01 10:53:52.700  2812  3017 D SubscriptionController: selection:sim_id>=0 null

06-01 10:53:52.725  2812  3017 D SubscriptionController: [getActiveSubInfoList]- no info return

06-01 10:53:52.970  2812  2812 D SubscriptionController: [getPhoneId]- invalid subId return=-1

06-01 10:53:52.970  2812  2812 D SubscriptionController: [getSubId]- sSlotIdxToSubId.size == 0, return DummySubIds slotIdx=0

06-01 10:53:53.070  2812  2812 D SubscriptionInfoUpdater: EVENT_UPDATE_INSERTED_SIM_COUNT: locked sims: 1

06-01 10:53:53.070  2812  2812 D SubscriptionInfoUpdater: All IccIds query complete

06-01 10:53:53.145  2812  2812 D SubscriptionInfoUpdater: EVENT_UPDATE_INSERTED_SIM_COUNT: locked sims: 1

06-01 10:53:53.145  2812  2812 D SubscriptionInfoUpdater: All IccIds query complete

06-01 10:53:53.170  2812  2812 D SubscriptionInfoUpdater: EVENT_UPDATE_INSERTED_SIM_COUNT: locked sims: 1

06-01 10:53:53.170  2812  2812 D SubscriptionInfoUpdater: All IccIds query complete

06-01 10:53:53.170  2812  2812 D SubscriptionInfoUpdater: updateSubscriptionInfoByIccId:+ Start

06-01 10:53:53.170  2812  2812 D SubscriptionController: [clearSubInfo]+

06-01 10:53:53.170  2812  2812 D SubscriptionController: [clearSubInfo]- no simInfo size=0

06-01 10:53:53.170  2812  2812 D SubscriptionInfoUpdater: insertedSimCount = 0

06-01 10:53:53.170  2812  2812 D SubscriptionController: [getSubInfoUsingSlotIdWithCheck]+ slotId:0

06-01 10:53:53.175  2812  2812 D SubscriptionController: [getSubInfoUsingSlotId]- null info return

06-01 10:53:53.175  2812  2812 D SubscriptionInfoUpdater: updateSubscriptionInfoByIccId: No SIM in slot 0 last time

06-01 10:53:53.175  2812  2812 D SubscriptionInfoUpdater: updateSubscriptionInfoByIccId: oldIccId[0] = , sIccId[0] = 

06-01 10:53:53.175  2812  2812 D SubscriptionInfoUpdater: updateSubscriptionInfoByIccId: No SIM inserted in slot 0 this time

06-01 10:53:53.175  2812  2812 D SubscriptionInfoUpdater: updateSubscriptionInfoByIccId: sInsertSimState[0] = -99

06-01 10:53:53.175  2812  2812 D SubscriptionController: [getActiveSubInfoList]+

06-01 10:53:53.180  2812  2812 D SubscriptionController: selection:sim_id>=0 null

06-01 10:53:53.180  2812  2812 D SubscriptionController: [getActiveSubInfoList]- no info return

06-01 10:53:53.180  2812  2812 D SubscriptionInfoUpdater: updateSubscriptionInfoByIccId: nSubCount = 0

06-01 10:53:53.180  2812  2812 D SubscriptionController: notifySubscriptionInfoChanged:

06-01 10:53:53.185  2812  2812 D SubscriptionInfoUpdater: updateSubscriptionInfoByIccId:- SsubscriptionInfo update complete

06-01 10:53:53.185  2812  2812 D SubscriptionInfoUpdater: update inserted sim count, current sim count: 0

06-01 10:53:53.185  2812  3017 D SubscriptionController: [getActiveSubInfoList]+

06-01 10:53:53.195  2812  3017 D SubscriptionController: selection:sim_id>=0 null

06-01 10:53:53.200  2812  2812 D GsmSST  : [GsmSST] SubscriptionListener.onSubscriptionInfoChanged

06-01 10:53:53.200  2812  2812 D SubscriptionController: [getSubId]- sSlotIdxToSubId.size == 0, return DummySubIds slotIdx=0

06-01 10:53:53.200  2812  2812 D DCT     : [0]SubscriptionListener.onSubscriptionInfoChanged

06-01 10:53:53.200  2812  2812 D SubscriptionController: [getSubId]- sSlotIdxToSubId.size == 0, return DummySubIds slotIdx=0

06-01 10:53:53.200  2812  2812 D SubscriptionController: [getActiveSubInfoList]+

06-01 10:53:53.200  2812  2812 D SubscriptionController: selection:sim_id>=0 null

06-01 10:53:53.245  2812  3017 D SubscriptionController: [getActiveSubInfoList]- no info return

06-01 10:53:53.270  2812  2812 D SubscriptionController: [getActiveSubInfoList]- no info return

06-01 10:53:53.275  2812  2812 E PhoneBase: Error! unregisterForCallWaiting() in PhoneBase should not be called, CDMAPhone inactive.

06-01 10:53:53.275  2812  2812 D SubscriptionController: [getSubId]- sSlotIdxToSubId.size == 0, return DummySubIds slotIdx=0

06-01 10:53:53.275  2812  2812 D SubscriptionController: [getSubId]- sSlotIdxToSubId.size == 0, return DummySubIds slotIdx=0

06-01 10:53:53.275  2812  2812 D SubscriptionController: [getPhoneId]- invalid subId return=-1

06-01 10:53:53.280  2812  2812 D SubscriptionController: [getSubId]- sSlotIdxToSubId.size == 0, return DummySubIds slotIdx=0

06-01 10:53:53.280  2812  2812 D SubscriptionController: [getSubId]- sSlotIdxToSubId.size == 0, return DummySubIds slotIdx=0

06-01 10:53:53.280  2812  2812 D SubscriptionController: [getSubId]- sSlotIdxToSubId.size == 0, return DummySubIds slotIdx=0

06-01 10:53:53.310  2812  2812 E PhoneBase: Error! registerForCallWaiting() in PhoneBase should not be called, CDMAPhone inactive.

06-01 10:53:53.315  2812  2812 D DctController: handleMessage msg={ when=-116ms what=107 target=com.android.internal.telephony.dataconnection.DctController }

06-01 10:53:53.315  2812  2812 D DctController: onSubInfoReady mPhoneNum=1

06-01 10:53:53.315  2812  2812 D SubscriptionController: [getSubId]- sSlotIdxToSubId.size == 0, return DummySubIds slotIdx=0

06-01 10:53:53.315  2812  2812 D DctController: onSubInfoReady handle pending requests subId=-2

06-01 10:53:53.315  2812  2812 D SubscriptionController: [getSubId]- sSlotIdxToSubId.size == 0, return DummySubIds slotIdx=0

06-01 10:53:53.315  2812  2812 D DctController: [TNF -2]evalPendingRequest, pending request size is 1

06-01 10:53:53.315  2812  2812 D SubscriptionController: [getSubId]- sSlotIdxToSubId.size == 0, return DummySubIds slotIdx=0

06-01 10:53:53.315  2812  2812 D DctController: [TNF -2]evalPendingRequest: request = NetworkRequest [ id=1, legacyType=-1, [ Capabilities: INTERNET&NOT_RESTRICTED&TRUSTED&NOT_VPN] ]

06-01 10:53:53.315  2812  2812 D SubscriptionController: [getSubId]- sSlotIdxToSubId.size == 0, return DummySubIds slotIdx=0

06-01 10:53:53.315  2812  2812 D DctController: [TNF -2]Cellular needs Network for NetworkRequest [ id=1, legacyType=-1, [ Capabilities: INTERNET&NOT_RESTRICTED&TRUSTED&NOT_VPN] ]

06-01 10:53:53.315  2812  2812 D SubscriptionController: [getSubId]- sSlotIdxToSubId.size == 0, return DummySubIds slotIdx=0

06-01 10:53:53.315  2812  2812 D SubscriptionController: [getSubId]- sSlotIdxToSubId.size == 0, return DummySubIds slotIdx=0

06-01 10:53:53.315  2812  2812 D DctController: [TNF -2]Request not useable, pending request.

06-01 10:53:53.315  2812  2812 D DctController: processRequests

06-01 10:53:53.315  2812  2812 D SubscriptionController: [getSubId]- sSlotIdxToSubId.size == 0, return DummySubIds slotIdx=0

06-01 10:53:53.315  2812  2812 D DctController: handleMessage msg={ when=-1ms what=100 target=com.android.internal.telephony.dataconnection.DctController }

06-01 10:53:53.315  2812  2812 D DcSwitchAsyncChannel: [DcSwitchAsyncChannel-0]: rspIsIdle=true

06-01 10:53:53.315  2812  2812 D SubscriptionController: [getPhoneId]- invalid subId return=-1

06-01 10:53:53.320  2812  2812 D DcSwitchAsyncChannel: [DcSwitchAsyncChannel-0]: rspIsIdle=true

06-01 10:53:53.320  2812  2812 D DctController: onProcessRequest requestedPhoneId=-1, activePhoneId=-1

06-01 10:53:54.225  2812  2968 D GsmCellBroadcastHandler: mWakeLock released

06-01 10:53:54.265  2812  2977 D CellBroadcastHandler: mWakeLock released

06-01 10:53:54.300  2812  2988 D CdmaServiceCategoryProgramHandler: mWakeLock released

06-01 10:53:56.110  2812  2846 D SubscriptionController: [getSlotId]- subId invalid

06-01 10:53:56.110  2812  3063 D SubscriptionController: getSimStateForSlotIdx:  simState=PIN_REQUIRED ordinal=2

06-01 10:53:56.110  2457  3212 D SubscriptionManager: getSimStateForSubscriber: simState=2 slotIdx=0

06-01 10:53:56.110  2457  3212 D TelephonyManager: getSimState: default sim:-1, sim state for slotIdx=0 is 2, return state as unknown

06-01 10:53:56.115  2812  2850 D SubscriptionController: [getSlotId]- subId invalid

06-01 10:53:56.115  2812  2846 D SubscriptionController: getSimStateForSlotIdx:  simState=PIN_REQUIRED ordinal=2

06-01 10:53:56.115  2457  3212 D SubscriptionManager: getSimStateForSubscriber: simState=2 slotIdx=0

06-01 10:53:56.115  2457  3212 D TelephonyManager: getSimState: default sim:-1, sim state for slotIdx=0 is 2, return state as unknown

06-01 10:53:56.140  2812  3063 D DCT     : [0]hasMatchedTetherApnSetting: APN=null

06-01 10:53:56.145  2812  3017 D DCT     : [0]hasMatchedTetherApnSetting: APN=null

06-01 10:53:56.155  2812  2846 D SubscriptionController: [getSlotId]- subId invalid

06-01 10:53:56.160  2812  3063 D SubscriptionController: getSimStateForSlotIdx:  simState=PIN_REQUIRED ordinal=2

06-01 10:53:56.160  2457  3212 D SubscriptionManager: getSimStateForSubscriber: simState=2 slotIdx=0

06-01 10:53:56.160  2457  3212 D TelephonyManager: getSimState: default sim:-1, sim state for slotIdx=0 is 2, return state as unknown

06-01 10:53:56.170  2812  3017 D DCT     : [0]hasMatchedTetherApnSetting: APN=null

06-01 10:53:56.460  1964  2328 D use-Rlog/RLOG-RIL-IPC: 

06-01 10:53:56.460  1964  2328 D use-Rlog/RLOG-RIL-IPC: xmm626_sec_modem_fmt_recv: Received FMT message

06-01 10:53:56.460  1964  2328 D use-Rlog/RLOG-RIL-IPC: xmm626_sec_modem_fmt_recv: Message: aseq=0x24, command=IPC_GPRS_HSDPA_STATUS, type=IPC_TYPE_NOTI, size=1

06-01 10:53:56.460  1964  2328 D use-Rlog/RLOG-RIL-IPC: ================================= IPC FMT data =================================

06-01 10:53:56.460  1964  2328 D use-Rlog/RLOG-RIL-IPC: [0000]   01                                                 .

06-01 10:53:56.460  1964  2328 D use-Rlog/RLOG-RIL-IPC: ================================================================================

06-01 10:53:56.460  1964  2328 D use-Rlog/RLOG-RIL-IPC: 

06-01 10:53:56.460  1964  2328 D use-Rlog/RLOG-RIL-IPC: xmm626_sec_modem_fmt_recv: Received FMT message

06-01 10:53:56.460  1964  2328 D use-Rlog/RLOG-RIL-IPC: xmm626_sec_modem_fmt_recv: Message: aseq=0xff, command=IPC_NET_REGIST, type=IPC_TYPE_NOTI, size=11

06-01 10:53:56.460  1964  2328 D use-Rlog/RLOG-RIL-IPC: ================================= IPC FMT data =================================

06-01 10:53:56.460  1964  2328 D use-Rlog/RLOG-RIL-IPC: [0000]   04 02 04 01 CC 42 F4 A7  07 00 00                  .....B.. ...

06-01 10:53:56.460  1964  2328 D use-Rlog/RLOG-RIL-IPC: ================================================================================

06-01 10:53:56.460  1964  2328 D use-Rlog/RLOG-RIL-IPC: 

06-01 10:53:56.460  1964  2328 D use-Rlog/RLOG-RIL-IPC: xmm626_sec_modem_fmt_recv: Received FMT message

06-01 10:53:56.460  1964  2328 D use-Rlog/RLOG-RIL-IPC: xmm626_sec_modem_fmt_recv: Message: aseq=0xff, command=IPC_NET_REGIST, type=IPC_TYPE_NOTI, size=11

06-01 10:53:56.460  1964  2328 D use-Rlog/RLOG-RIL-IPC: ================================= IPC FMT data =================================

06-01 10:53:56.460  1964  2328 D use-Rlog/RLOG-RIL-IPC: [0000]   04 03 01 01 CC 42 F4 A7  07 00 00                  .....B.. ...

06-01 10:53:56.460  1964  2328 D use-Rlog/RLOG-RIL-IPC: ================================================================================

06-01 10:53:56.460  1964  2328 D use-Rlog/RLOG-RIL-IPC: 

06-01 10:53:56.460  1964  2328 D use-Rlog/RLOG-RIL-IPC: xmm626_sec_modem_fmt_recv: Received FMT message

06-01 10:53:56.460  1964  2328 D use-Rlog/RLOG-RIL-IPC: xmm626_sec_modem_fmt_recv: Message: aseq=0x00, command=IPC_NET_SERVING_NETWORK, type=IPC_TYPE_NOTI, size=11

06-01 10:53:56.460  1964  2328 D use-Rlog/RLOG-RIL-IPC: ================================= IPC FMT data =================================

06-01 10:53:56.460  1964  2328 D use-Rlog/RLOG-RIL-IPC: [0000]   02 04 04 32 30 36 31 30  23 CC 42                  ...20610 #.B

06-01 10:53:56.460  1964  2328 D use-Rlog/RLOG-RIL-IPC: ================================================================================

06-01 10:53:56.460  1964  2328 D use-Rlog/RLOG-RIL-IPC: 

06-01 10:53:56.460  1964  2328 D use-Rlog/RLOG-RIL-IPC: xmm626_sec_modem_fmt_recv: Received FMT message

06-01 10:53:56.460  1964  2328 D use-Rlog/RLOG-RIL-IPC: xmm626_sec_modem_fmt_recv: Message: aseq=0x00, command=IPC_DISP_ICON_INFO, type=IPC_TYPE_NOTI, size=4

06-01 10:53:56.460  1964  2328 D use-Rlog/RLOG-RIL-IPC: ================================= IPC FMT data =================================

06-01 10:53:56.460  1964  2328 D use-Rlog/RLOG-RIL-IPC: [0000]   FF 04 00 04                                        ....

06-01 10:53:56.460  1964  2328 D use-Rlog/RLOG-RIL-IPC: ================================================================================

06-01 10:53:56.460  1964  2328 D use-Rlog/RLOG-RIL: Signal strength is 12

06-01 10:53:56.460  1964  2328 D use-Rlog/RLOG-RIL-IPC: 

06-01 10:53:56.460  1964  2328 D use-Rlog/RLOG-RIL-IPC: xmm626_sec_modem_fmt_recv: Received FMT message

06-01 10:53:56.460  1964  2328 D use-Rlog/RLOG-RIL-IPC: xmm626_sec_modem_fmt_recv: Message: aseq=0x00, command=IPC_DISP_RSSI_INFO, type=IPC_TYPE_NOTI, size=1

06-01 10:53:56.460  1964  2328 D use-Rlog/RLOG-RIL-IPC: ================================= IPC FMT data =================================

06-01 10:53:56.460  1964  2328 D use-Rlog/RLOG-RIL-IPC: [0000]   4B                                                 K

06-01 10:53:56.460  1964  2328 D use-Rlog/RLOG-RIL-IPC: ================================================================================

06-01 10:53:56.460  1964  2328 D use-Rlog/RLOG-RIL: Signal strength is 19

06-01 10:53:56.460  2812  2918 D RILJ    : [UNSL]< UNSOL_RESPONSE_VOICE_NETWORK_STATE_CHANGED [SUB0]

06-01 10:53:56.465  2812  2918 D RILJ    : [UNSL]< UNSOL_RESPONSE_VOICE_NETWORK_STATE_CHANGED [SUB0]

06-01 10:53:56.465  2812  2812 D RILJ    : [3707]> OPERATOR [SUB0]

06-01 10:53:56.465  2812  2918 D RILJ    : [UNSL]< UNSOL_RESPONSE_VOICE_NETWORK_STATE_CHANGED [SUB0]

06-01 10:53:56.465  2812  2918 D RILJ    : [UNSL]< UNSOL_RESPONSE_VOICE_NETWORK_STATE_CHANGED [SUB0]

06-01 10:53:56.465  2812  2812 D RILJ    : [3708]> DATA_REGISTRATION_STATE [SUB0]

06-01 10:53:56.465  1964  2012 D use-Rlog/RLOG-RIL: 1 RIL request in the queue (1 pending, 0 handled, 0 unhandled)

06-01 10:53:56.465  1964  2012 D use-Rlog/RLOG-RIL: 3 RIL requests data in the queue

06-01 10:53:56.465  1964  2332 D use-Rlog/RLOG-RIL: 0 RIL request in the queue (0 pending, 0 handled, 0 unhandled)

06-01 10:53:56.465  1964  2332 D use-Rlog/RLOG-RIL: 2 RIL requests data in the queue

06-01 10:53:56.465  2812  2918 D RILJ    : [3707]< OPERATOR {Mobistar, Mobistar, 20610} [SUB0]

06-01 10:53:56.465  2812  2812 D RILJ    : [3709]> VOICE_REGISTRATION_STATE [SUB0]

06-01 10:53:56.465  1964  2012 D use-Rlog/RLOG-RIL: 1 RIL request in the queue (1 pending, 0 handled, 0 unhandled)

06-01 10:53:56.465  1964  2012 D use-Rlog/RLOG-RIL: 2 RIL requests data in the queue

06-01 10:53:56.465  1964  2332 D use-Rlog/RLOG-RIL: 0 RIL request in the queue (0 pending, 0 handled, 0 unhandled)

06-01 10:53:56.465  1964  2332 D use-Rlog/RLOG-RIL: 1 RIL request data in the queue

06-01 10:53:56.465  2812  2850 D SubscriptionController: [getSubId]- sSlotIdxToSubId.size == 0, return DummySubIds slotIdx=0

06-01 10:53:56.465  2812  2812 D RILJ    : [3710]> QUERY_NETWORK_SELECTION_MODE [SUB0]

06-01 10:53:56.465  2812  2918 D RILJ    : [3708]< DATA_REGISTRATION_STATE {0, 42cc, 7a7f4, 9, 3} [SUB0]

06-01 10:53:56.470  1964  2012 D use-Rlog/RLOG-RIL: 1 RIL request in the queue (1 pending, 0 handled, 0 unhandled)

06-01 10:53:56.470  1964  2012 D use-Rlog/RLOG-RIL: 1 RIL request data in the queue

06-01 10:53:56.470  2812  2812 D RILJ    : [3711]> OPERATOR [SUB0]

06-01 10:53:56.470  1964  2332 D use-Rlog/RLOG-RIL: 0 RIL request in the queue (0 pending, 0 handled, 0 unhandled)

06-01 10:53:56.470  1964  2012 D use-Rlog/RLOG-RIL: 1 RIL request in the queue (1 pending, 0 handled, 0 unhandled)

06-01 10:53:56.470  1964  2332 D use-Rlog/RLOG-RIL-IPC: 

06-01 10:53:56.470  1964  2332 D use-Rlog/RLOG-RIL-IPC: xmm626_sec_modem_fmt_send: Sent FMT message

06-01 10:53:56.470  1964  2332 D use-Rlog/RLOG-RIL-IPC: xmm626_sec_modem_fmt_send: Message: mseq=0x25, command=IPC_NET_PLMN_SEL, type=IPC_TYPE_GET, size=0

06-01 10:53:56.470  2812  2812 D RILJ    : [3712]> DATA_REGISTRATION_STATE [SUB0]

06-01 10:53:56.470  2812  2918 D RILJ    : [3709]< VOICE_REGISTRATION_STATE {10, 42cc, 7a7f4, 9, null, null, null, null, null, null, null, null, null, null, null} [SUB0]

06-01 10:53:56.470  1964  2012 D use-Rlog/RLOG-RIL: 2 RIL requests in the queue (1 pending, 1 handled, 0 unhandled)

06-01 10:53:56.470  1964  2332 D use-Rlog/RLOG-RIL-IPC: 

06-01 10:53:56.470  1964  2332 D use-Rlog/RLOG-RIL-IPC: xmm626_sec_modem_fmt_send: Sent FMT message

06-01 10:53:56.470  1964  2332 D use-Rlog/RLOG-RIL-IPC: xmm626_sec_modem_fmt_send: Message: mseq=0x26, command=IPC_NET_SERVING_NETWORK, type=IPC_TYPE_GET, size=0

06-01 10:53:56.470  2812  2812 D RILJ    : [3713]> VOICE_REGISTRATION_STATE [SUB0]

06-01 10:53:56.470  1964  2012 D use-Rlog/RLOG-RIL: 3 RIL requests in the queue (1 pending, 2 handled, 0 unhandled)

06-01 10:53:56.470  1964  2332 D use-Rlog/RLOG-RIL-IPC: 

06-01 10:53:56.470  1964  2332 D use-Rlog/RLOG-RIL-IPC: xmm626_sec_modem_fmt_send: Sent FMT message

06-01 10:53:56.470  1964  2332 D use-Rlog/RLOG-RIL-IPC: xmm626_sec_modem_fmt_send: Message: mseq=0x27, command=IPC_NET_REGIST, type=IPC_TYPE_GET, size=2

06-01 10:53:56.470  1964  2332 D use-Rlog/RLOG-RIL-IPC: ================================= IPC FMT data =================================

06-01 10:53:56.470  1964  2332 D use-Rlog/RLOG-RIL-IPC: [0000]   FF 03                                              ..

06-01 10:53:56.470  1964  2332 D use-Rlog/RLOG-RIL-IPC: ================================================================================

06-01 10:53:56.470  1964  2328 D use-Rlog/RLOG-RIL-IPC: 

06-01 10:53:56.470  1964  2328 D use-Rlog/RLOG-RIL-IPC: xmm626_sec_modem_fmt_recv: Received FMT message

06-01 10:53:56.470  1964  2328 D use-Rlog/RLOG-RIL-IPC: xmm626_sec_modem_fmt_recv: Message: aseq=0x25, command=IPC_NET_PLMN_SEL, type=IPC_TYPE_RESP, size=1

06-01 10:53:56.470  1964  2328 D use-Rlog/RLOG-RIL-IPC: ================================= IPC FMT data =================================

06-01 10:53:56.470  1964  2328 D use-Rlog/RLOG-RIL-IPC: [0000]   02                                                 .

06-01 10:53:56.470  1964  2328 D use-Rlog/RLOG-RIL-IPC: ================================================================================

06-01 10:53:56.470  2812  2812 D RILJ    : [3714]> QUERY_NETWORK_SELECTION_MODE [SUB0]

06-01 10:53:56.470  1964  2328 D use-Rlog/RLOG-RIL: 2 RIL requests in the queue (0 pending, 2 handled, 0 unhandled)

06-01 10:53:56.470  1964  2328 D use-Rlog/RLOG-RIL-IPC: 

06-01 10:53:56.470  1964  2328 D use-Rlog/RLOG-RIL-IPC: xmm626_sec_modem_fmt_recv: Received FMT message

06-01 10:53:56.470  1964  2328 D use-Rlog/RLOG-RIL-IPC: xmm626_sec_modem_fmt_recv: Message: aseq=0x26, command=IPC_NET_SERVING_NETWORK, type=IPC_TYPE_RESP, size=11

06-01 10:53:56.475  1964  2328 D use-Rlog/RLOG-RIL-IPC: ================================= IPC FMT data =================================

06-01 10:53:56.475  1964  2328 D use-Rlog/RLOG-RIL-IPC: [0000]   02 04 04 32 30 36 31 30  23 CC 42                  ...20610 #.B

06-01 10:53:56.475  1964  2328 D use-Rlog/RLOG-RIL-IPC: ================================================================================

06-01 10:53:56.475  1964  2328 D use-Rlog/RLOG-RIL: 1 RIL request in the queue (0 pending, 1 handled, 0 unhandled)

06-01 10:53:56.475  1964  2012 D use-Rlog/RLOG-RIL: 2 RIL requests in the queue (1 pending, 1 handled, 0 unhandled)

06-01 10:53:56.475  1964  2332 D use-Rlog/RLOG-RIL-IPC: 

06-01 10:53:56.475  1964  2332 D use-Rlog/RLOG-RIL-IPC: xmm626_sec_modem_fmt_send: Sent FMT message

06-01 10:53:56.475  2812  2918 D RILJ    : [3710]< QUERY_NETWORK_SELECTION_MODE {0} [SUB0]

06-01 10:53:56.475  1964  2332 D use-Rlog/RLOG-RIL-IPC: xmm626_sec_modem_fmt_send: Message: mseq=0x28, command=IPC_NET_REGIST, type=IPC_TYPE_GET, size=2

06-01 10:53:56.475  1964  2332 D use-Rlog/RLOG-RIL-IPC: ================================= IPC FMT data =================================

06-01 10:53:56.475  1964  2332 D use-Rlog/RLOG-RIL-IPC: [0000]   FF 02                                              ..

06-01 10:53:56.475  1964  2332 D use-Rlog/RLOG-RIL-IPC: ================================================================================

06-01 10:53:56.475  2812  2918 D RILJ    : [3711]< OPERATOR {Mobistar, Mobistar, 20610} [SUB0]

06-01 10:53:56.475  1964  2328 D use-Rlog/RLOG-RIL-IPC: 

06-01 10:53:56.475  1964  2328 D use-Rlog/RLOG-RIL-IPC: xmm626_sec_modem_fmt_recv: Received FMT message

06-01 10:53:56.475  1964  2328 D use-Rlog/RLOG-RIL-IPC: xmm626_sec_modem_fmt_recv: Message: aseq=0x27, command=IPC_NET_REGIST, type=IPC_TYPE_RESP, size=11

06-01 10:53:56.475  1964  2328 D use-Rlog/RLOG-RIL-IPC: ================================= IPC FMT data =================================

06-01 10:53:56.475  1964  2328 D use-Rlog/RLOG-RIL-IPC: [0000]   04 03 01 01 CC 42 F4 A7  07 00 00                  .....B.. ...

06-01 10:53:56.475  1964  2328 D use-Rlog/RLOG-RIL-IPC: ================================================================================

06-01 10:53:56.475  2812  2812 D RILJ    : [3715]> OPERATOR [SUB0]

06-01 10:53:56.475  1964  2328 D use-Rlog/RLOG-RIL: 1 RIL request in the queue (0 pending, 1 handled, 0 unhandled)

06-01 10:53:56.475  1964  2012 D use-Rlog/RLOG-RIL: 2 RIL requests in the queue (1 pending, 1 handled, 0 unhandled)

06-01 10:53:56.475  2812  2918 D RILJ    : [3712]< DATA_REGISTRATION_STATE {0, 42cc, 7a7f4, 9, 3} [SUB0]

06-01 10:53:56.475  1964  2332 D use-Rlog/RLOG-RIL-IPC: 

06-01 10:53:56.475  1964  2332 D use-Rlog/RLOG-RIL-IPC: xmm626_sec_modem_fmt_send: Sent FMT message

06-01 10:53:56.475  1964  2332 D use-Rlog/RLOG-RIL-IPC: xmm626_sec_modem_fmt_send: Message: mseq=0x29, command=IPC_NET_PLMN_SEL, type=IPC_TYPE_GET, size=0

06-01 10:53:56.475  1964  2328 D use-Rlog/RLOG-RIL-IPC: 

06-01 10:53:56.475  2812  2812 D RILJ    : [3716]> DATA_REGISTRATION_STATE [SUB0]

06-01 10:53:56.475  1964  2328 D use-Rlog/RLOG-RIL-IPC: xmm626_sec_modem_fmt_recv: Received FMT message

06-01 10:53:56.475  1964  2328 D use-Rlog/RLOG-RIL-IPC: xmm626_sec_modem_fmt_recv: Message: aseq=0x28, command=IPC_NET_REGIST, type=IPC_TYPE_RESP, size=11

06-01 10:53:56.475  1964  2328 D use-Rlog/RLOG-RIL-IPC: ================================= IPC FMT data =================================

06-01 10:53:56.475  1964  2328 D use-Rlog/RLOG-RIL-IPC: [0000]   04 02 04 01 CC 42 F4 A7  07 00 00                  .....B.. ...

06-01 10:53:56.475  1964  2328 D use-Rlog/RLOG-RIL-IPC: ================================================================================

06-01 10:53:56.475  1964  2328 D use-Rlog/RLOG-RIL: 1 RIL request in the queue (0 pending, 1 handled, 0 unhandled)

06-01 10:53:56.475  1964  2328 D use-Rlog/RLOG-RIL-IPC: 

06-01 10:53:56.475  1964  2328 D use-Rlog/RLOG-RIL-IPC: xmm626_sec_modem_fmt_recv: Received FMT message

06-01 10:53:56.475  1964  2328 D use-Rlog/RLOG-RIL-IPC: xmm626_sec_modem_fmt_recv: Message: aseq=0x29, command=IPC_NET_PLMN_SEL, type=IPC_TYPE_RESP, size=1

06-01 10:53:56.475  1964  2328 D use-Rlog/RLOG-RIL-IPC: ================================= IPC FMT data =================================

06-01 10:53:56.475  1964  2328 D use-Rlog/RLOG-RIL-IPC: [0000]   02                                                 .

06-01 10:53:56.475  1964  2328 D use-Rlog/RLOG-RIL-IPC: ================================================================================

06-01 10:53:56.475  1964  2328 D use-Rlog/RLOG-RIL: 0 RIL request in the queue (0 pending, 0 handled, 0 unhandled)

06-01 10:53:56.475  2812  2812 D RILJ    : [3717]> VOICE_REGISTRATION_STATE [SUB0]

06-01 10:53:56.475  1964  2012 D use-Rlog/RLOG-RIL: 1 RIL request in the queue (1 pending, 0 handled, 0 unhandled)

06-01 10:53:56.475  1964  2012 D use-Rlog/RLOG-RIL: 2 RIL requests in the queue (2 pending, 0 handled, 0 unhandled)

06-01 10:53:56.480  1964  2332 D use-Rlog/RLOG-RIL-IPC: 

06-01 10:53:56.480  1964  2332 D use-Rlog/RLOG-RIL-IPC: xmm626_sec_modem_fmt_send: Sent FMT message

06-01 10:53:56.480  1964  2332 D use-Rlog/RLOG-RIL-IPC: xmm626_sec_modem_fmt_send: Message: mseq=0x2a, command=IPC_NET_SERVING_NETWORK, type=IPC_TYPE_GET, size=0

06-01 10:53:56.480  1964  2332 D use-Rlog/RLOG-RIL-IPC: 

06-01 10:53:56.480  1964  2332 D use-Rlog/RLOG-RIL-IPC: xmm626_sec_modem_fmt_send: Sent FMT message

06-01 10:53:56.480  1964  2332 D use-Rlog/RLOG-RIL-IPC: xmm626_sec_modem_fmt_send: Message: mseq=0x2b, command=IPC_NET_REGIST, type=IPC_TYPE_GET, size=2

06-01 10:53:56.480  1964  2332 D use-Rlog/RLOG-RIL-IPC: ================================= IPC FMT data =================================

06-01 10:53:56.480  1964  2332 D use-Rlog/RLOG-RIL-IPC: [0000]   FF 03                                              ..

06-01 10:53:56.480  1964  2332 D use-Rlog/RLOG-RIL-IPC: ================================================================================

06-01 10:53:56.480  2812  2812 D RILJ    : [3718]> QUERY_NETWORK_SELECTION_MODE [SUB0]

06-01 10:53:56.480  1964  2012 D use-Rlog/RLOG-RIL: 3 RIL requests in the queue (1 pending, 2 handled, 0 unhandled)

06-01 10:53:56.480  1964  2332 D use-Rlog/RLOG-RIL-IPC: 

06-01 10:53:56.480  1964  2332 D use-Rlog/RLOG-RIL-IPC: xmm626_sec_modem_fmt_send: Sent FMT message

06-01 10:53:56.480  1964  2332 D use-Rlog/RLOG-RIL-IPC: xmm626_sec_modem_fmt_send: Message: mseq=0x2c, command=IPC_NET_REGIST, type=IPC_TYPE_GET, size=2

06-01 10:53:56.480  1964  2332 D use-Rlog/RLOG-RIL-IPC: ================================= IPC FMT data =================================

06-01 10:53:56.480  1964  2332 D use-Rlog/RLOG-RIL-IPC: [0000]   FF 02                                              ..

06-01 10:53:56.480  1964  2332 D use-Rlog/RLOG-RIL-IPC: ================================================================================

06-01 10:53:56.480  2812  2812 D RILJ    : [3719]> OPERATOR [SUB0]

06-01 10:53:56.480  1964  2012 D use-Rlog/RLOG-RIL: 4 RIL requests in the queue (1 pending, 3 handled, 0 unhandled)

06-01 10:53:56.480  1964  2332 D use-Rlog/RLOG-RIL-IPC: 

06-01 10:53:56.480  1964  2332 D use-Rlog/RLOG-RIL-IPC: xmm626_sec_modem_fmt_send: Sent FMT message

06-01 10:53:56.480  1964  2332 D use-Rlog/RLOG-RIL-IPC: xmm626_sec_modem_fmt_send: Message: mseq=0x2d, command=IPC_NET_PLMN_SEL, type=IPC_TYPE_GET, size=0

06-01 10:53:56.480  1964  2328 D use-Rlog/RLOG-RIL-IPC: 

06-01 10:53:56.480  1964  2328 D use-Rlog/RLOG-RIL-IPC: xmm626_sec_modem_fmt_recv: Received FMT message

06-01 10:53:56.480  1964  2328 D use-Rlog/RLOG-RIL-IPC: xmm626_sec_modem_fmt_recv: Message: aseq=0x2a, command=IPC_NET_SERVING_NETWORK, type=IPC_TYPE_RESP, size=11

06-01 10:53:56.480  1964  2328 D use-Rlog/RLOG-RIL-IPC: ================================= IPC FMT data =================================

06-01 10:53:56.480  1964  2328 D use-Rlog/RLOG-RIL-IPC: [0000]   02 04 04 32 30 36 31 30  23 CC 42                  ...20610 #.B

06-01 10:53:56.480  1964  2328 D use-Rlog/RLOG-RIL-IPC: ================================================================================

06-01 10:53:56.480  2812  2812 D RILJ    : [3720]> DATA_REGISTRATION_STATE [SUB0]

06-01 10:53:56.480  1964  2328 D use-Rlog/RLOG-RIL: 3 RIL requests in the queue (0 pending, 3 handled, 0 unhandled)

06-01 10:53:56.480  1964  2012 D use-Rlog/RLOG-RIL: 4 RIL requests in the queue (1 pending, 3 handled, 0 unhandled)

06-01 10:53:56.480  1964  2328 D use-Rlog/RLOG-RIL-IPC: 

06-01 10:53:56.480  1964  2328 D use-Rlog/RLOG-RIL-IPC: xmm626_sec_modem_fmt_recv: Received FMT message

06-01 10:53:56.480  1964  2328 D use-Rlog/RLOG-RIL-IPC: xmm626_sec_modem_fmt_recv: Message: aseq=0x2b, command=IPC_NET_REGIST, type=IPC_TYPE_RESP, size=11

06-01 10:53:56.480  1964  2328 D use-Rlog/RLOG-RIL-IPC: ================================= IPC FMT data =================================

06-01 10:53:56.480  1964  2328 D use-Rlog/RLOG-RIL-IPC: [0000]   04 03 01 01 CC 42 F4 A7  07 00 00                  .....B.. ...

06-01 10:53:56.480  1964  2328 D use-Rlog/RLOG-RIL-IPC: ================================================================================

06-01 10:53:56.480  1964  2328 D use-Rlog/RLOG-RIL: 3 RIL requests in the queue (1 pending, 2 handled, 0 unhandled)

06-01 10:53:56.480  1964  2332 D use-Rlog/RLOG-RIL-IPC: 

06-01 10:53:56.480  1964  2332 D use-Rlog/RLOG-RIL-IPC: xmm626_sec_modem_fmt_send: Sent FMT message

06-01 10:53:56.480  1964  2332 D use-Rlog/RLOG-RIL-IPC: xmm626_sec_modem_fmt_send: Message: mseq=0x2e, command=IPC_NET_SERVING_NETWORK, type=IPC_TYPE_GET, size=0

06-01 10:53:56.480  1964  2328 D use-Rlog/RLOG-RIL-IPC: 

06-01 10:53:56.480  1964  2328 D use-Rlog/RLOG-RIL-IPC: xmm626_sec_modem_fmt_recv: Received FMT message

06-01 10:53:56.480  1964  2328 D use-Rlog/RLOG-RIL-IPC: xmm626_sec_modem_fmt_recv: Message: aseq=0x2c, command=IPC_NET_REGIST, type=IPC_TYPE_RESP, size=11

06-01 10:53:56.480  1964  2328 D use-Rlog/RLOG-RIL-IPC: ================================= IPC FMT data =================================

06-01 10:53:56.480  1964  2328 D use-Rlog/RLOG-RIL-IPC: [0000]   04 02 04 01 CC 42 F4 A7  07 00 00                  .....B.. ...

06-01 10:53:56.480  1964  2328 D use-Rlog/RLOG-RIL-IPC: ================================================================================

06-01 10:53:56.480  1964  2328 D use-Rlog/RLOG-RIL: 2 RIL requests in the queue (0 pending, 2 handled, 0 unhandled)

06-01 10:53:56.485  2812  2918 D RILJ    : [3713]< VOICE_REGISTRATION_STATE {10, 42cc, 7a7f4, 9, null, null, null, null, null, null, null, null, null, null, null} [SUB0]

06-01 10:53:56.485  1964  2328 D use-Rlog/RLOG-RIL-IPC: 

06-01 10:53:56.485  1964  2328 D use-Rlog/RLOG-RIL-IPC: xmm626_sec_modem_fmt_recv: Received FMT message

06-01 10:53:56.485  2812  2812 D RILJ    : [3721]> VOICE_REGISTRATION_STATE [SUB0]

06-01 10:53:56.485  1964  2328 D use-Rlog/RLOG-RIL-IPC: xmm626_sec_modem_fmt_recv: Message: aseq=0x2d, command=IPC_NET_PLMN_SEL, type=IPC_TYPE_RESP, size=1

06-01 10:53:56.485  1964  2328 D use-Rlog/RLOG-RIL-IPC: ================================= IPC FMT data =================================

06-01 10:53:56.485  1964  2328 D use-Rlog/RLOG-RIL-IPC: [0000]   02                                                 .

06-01 10:53:56.485  2812  2918 D RILJ    : [3714]< QUERY_NETWORK_SELECTION_MODE {0} [SUB0]

06-01 10:53:56.485  1964  2328 D use-Rlog/RLOG-RIL-IPC: ================================================================================

06-01 10:53:56.485  1964  2328 D use-Rlog/RLOG-RIL: 1 RIL request in the queue (0 pending, 1 handled, 0 unhandled)

06-01 10:53:56.485  1964  2328 D use-Rlog/RLOG-RIL-IPC: 

06-01 10:53:56.485  1964  2328 D use-Rlog/RLOG-RIL-IPC: xmm626_sec_modem_fmt_recv: Received FMT message

06-01 10:53:56.485  1964  2328 D use-Rlog/RLOG-RIL-IPC: xmm626_sec_modem_fmt_recv: Message: aseq=0x2e, command=IPC_NET_SERVING_NETWORK, type=IPC_TYPE_RESP, size=11

06-01 10:53:56.485  1964  2328 D use-Rlog/RLOG-RIL-IPC: ================================= IPC FMT data =================================

06-01 10:53:56.485  1964  2328 D use-Rlog/RLOG-RIL-IPC: [0000]   02 04 04 32 30 36 31 30  23 CC 42                  ...20610 #.B

06-01 10:53:56.485  1964  2328 D use-Rlog/RLOG-RIL-IPC: ================================================================================

06-01 10:53:56.485  1964  2328 D use-Rlog/RLOG-RIL: 0 RIL request in the queue (0 pending, 0 handled, 0 unhandled)

06-01 10:53:56.485  1964  2012 D use-Rlog/RLOG-RIL: 1 RIL request in the queue (1 pending, 0 handled, 0 unhandled)

06-01 10:53:56.485  2812  2918 D RILJ    : [3715]< OPERATOR {Mobistar, Mobistar, 20610} [SUB0]

06-01 10:53:56.485  1964  2012 D use-Rlog/RLOG-RIL: 2 RIL requests in the queue (2 pending, 0 handled, 0 unhandled)

06-01 10:53:56.485  2812  2812 D RILJ    : [3722]> QUERY_NETWORK_SELECTION_MODE [SUB0]

06-01 10:53:56.485  2812  2918 D RILJ    : [3716]< DATA_REGISTRATION_STATE {0, 42cc, 7a7f4, 9, 3} [SUB0]

06-01 10:53:56.485  1964  2332 D use-Rlog/RLOG-RIL-IPC: 

06-01 10:53:56.485  1964  2332 D use-Rlog/RLOG-RIL-IPC: xmm626_sec_modem_fmt_send: Sent FMT message

06-01 10:53:56.485  1964  2332 D use-Rlog/RLOG-RIL-IPC: xmm626_sec_modem_fmt_send: Message: mseq=0x2f, command=IPC_NET_REGIST, type=IPC_TYPE_GET, size=2

06-01 10:53:56.485  1964  2332 D use-Rlog/RLOG-RIL-IPC: ================================= IPC FMT data =================================

06-01 10:53:56.485  1964  2332 D use-Rlog/RLOG-RIL-IPC: [0000]   FF 03                                              ..

06-01 10:53:56.485  1964  2332 D use-Rlog/RLOG-RIL-IPC: ================================================================================

06-01 10:53:56.485  1964  2332 D use-Rlog/RLOG-RIL-IPC: 

06-01 10:53:56.485  1964  2332 D use-Rlog/RLOG-RIL-IPC: xmm626_sec_modem_fmt_send: Sent FMT message

06-01 10:53:56.485  1964  2332 D use-Rlog/RLOG-RIL-IPC: xmm626_sec_modem_fmt_send: Message: mseq=0x30, command=IPC_NET_REGIST, type=IPC_TYPE_GET, size=2

06-01 10:53:56.485  1964  2332 D use-Rlog/RLOG-RIL-IPC: ================================= IPC FMT data =================================

06-01 10:53:56.485  1964  2332 D use-Rlog/RLOG-RIL-IPC: [0000]   FF 02                                              ..

06-01 10:53:56.485  1964  2332 D use-Rlog/RLOG-RIL-IPC: ================================================================================

06-01 10:53:56.485  2812  2918 D RILJ    : [3717]< VOICE_REGISTRATION_STATE {10, 42cc, 7a7f4, 9, null, null, null, null, null, null, null, null, null, null, null} [SUB0]

06-01 10:53:56.485  2812  2918 D RILJ    : [3718]< QUERY_NETWORK_SELECTION_MODE {0} [SUB0]

06-01 10:53:56.485  2812  2918 D RILJ    : [3719]< OPERATOR {Mobistar, Mobistar, 20610} [SUB0]

06-01 10:53:56.490  1964  2328 D use-Rlog/RLOG-RIL-IPC: 

06-01 10:53:56.490  1964  2328 D use-Rlog/RLOG-RIL-IPC: xmm626_sec_modem_fmt_recv: Received FMT message

06-01 10:53:56.490  1964  2328 D use-Rlog/RLOG-RIL-IPC: xmm626_sec_modem_fmt_recv: Message: aseq=0x2f, command=IPC_NET_REGIST, type=IPC_TYPE_RESP, size=11

06-01 10:53:56.490  1964  2328 D use-Rlog/RLOG-RIL-IPC: ================================= IPC FMT data =================================

06-01 10:53:56.490  2812  2812 D SubscriptionController: [getSubId]- sSlotIdxToSubId.size == 0, return DummySubIds slotIdx=0

06-01 10:53:56.490  2812  2812 D DefaultPhoneNotifier: notifySignalStrength: mRegistry=com.android.internal.telephony.ITelephonyRegistry$Stub$Proxy@d42da20 ss=SignalStrength: 12 99 -120 -160 -120 -1 -1 99 2147483647 2147483647 2147483647 -1 2147483647 gsm|lte sender=Handler (com.android.internal.telephony.gsm.GSMPhone) {b910da1}

06-01 10:53:56.490  1964  2328 D use-Rlog/RLOG-RIL-IPC: [0000]   04 03 01 01 CC 42 F4 A7  07 00 00                  .....B.. ...

06-01 10:53:56.490  1964  2328 D use-Rlog/RLOG-RIL-IPC: ================================================================================

06-01 10:53:56.490  1964  2328 D use-Rlog/RLOG-RIL: 1 RIL request in the queue (0 pending, 1 handled, 0 unhandled)

06-01 10:53:56.490  1964  2328 D use-Rlog/RLOG-RIL-IPC: 

06-01 10:53:56.490  1964  2328 D use-Rlog/RLOG-RIL-IPC: xmm626_sec_modem_fmt_recv: Received FMT message

06-01 10:53:56.490  1964  2328 D use-Rlog/RLOG-RIL-IPC: xmm626_sec_modem_fmt_recv: Message: aseq=0x30, command=IPC_NET_REGIST, type=IPC_TYPE_RESP, size=11

06-01 10:53:56.490  1964  2328 D use-Rlog/RLOG-RIL-IPC: ================================= IPC FMT data =================================

06-01 10:53:56.490  2335  3091 D TelephonyRegistry: notifySignalStrengthForSubscriber: invalid phoneId=-1

06-01 10:53:56.490  1964  2328 D use-Rlog/RLOG-RIL-IPC: [0000]   04 02 04 01 CC 42 F4 A7  07 00 00                  .....B.. ...

06-01 10:53:56.490  1964  2328 D use-Rlog/RLOG-RIL-IPC: ================================================================================

06-01 10:53:56.490  1964  2328 D use-Rlog/RLOG-RIL: 0 RIL request in the queue (0 pending, 0 handled, 0 unhandled)

06-01 10:53:56.490  2812  2918 D RILJ    : [3720]< DATA_REGISTRATION_STATE {0, 42cc, 7a7f4, 9, 3} [SUB0]

06-01 10:53:56.490  1964  2012 D use-Rlog/RLOG-RIL: 1 RIL request in the queue (1 pending, 0 handled, 0 unhandled)

06-01 10:53:56.490  2812  2918 D RILJ    : [3721]< VOICE_REGISTRATION_STATE {10, 42cc, 7a7f4, 9, null, null, null, null, null, null, null, null, null, null, null} [SUB0]

06-01 10:53:56.490  1964  2332 D use-Rlog/RLOG-RIL-IPC: 

06-01 10:53:56.490  1964  2332 D use-Rlog/RLOG-RIL-IPC: xmm626_sec_modem_fmt_send: Sent FMT message

06-01 10:53:56.490  1964  2332 D use-Rlog/RLOG-RIL-IPC: xmm626_sec_modem_fmt_send: Message: mseq=0x31, command=IPC_NET_PLMN_SEL, type=IPC_TYPE_GET, size=0

06-01 10:53:56.490  2812  2812 D SubscriptionController: [getSubId]- sSlotIdxToSubId.size == 0, return DummySubIds slotIdx=0

06-01 10:53:56.490  2812  2812 D DefaultPhoneNotifier: notifySignalStrength: mRegistry=com.android.internal.telephony.ITelephonyRegistry$Stub$Proxy@d42da20 ss=SignalStrength: 19 99 -120 -160 -120 -1 -1 99 2147483647 2147483647 2147483647 -1 2147483647 gsm|lte sender=Handler (com.android.internal.telephony.gsm.GSMPhone) {b910da1}

06-01 10:53:56.490  2335  2807 D TelephonyRegistry: notifySignalStrengthForSubscriber: invalid phoneId=-1

06-01 10:53:56.490  2812  2812 D PHONE   : [ServiceState] setDataRegState=1

06-01 10:53:56.490  1964  2328 D use-Rlog/RLOG-RIL-IPC: 

06-01 10:53:56.490  1964  2328 D use-Rlog/RLOG-RIL-IPC: xmm626_sec_modem_fmt_recv: Received FMT message

06-01 10:53:56.490  2812  2812 D PHONE   : [ServiceState] setDataRadioTechnology=9

06-01 10:53:56.490  1964  2328 D use-Rlog/RLOG-RIL-IPC: xmm626_sec_modem_fmt_recv: Message: aseq=0x31, command=IPC_NET_PLMN_SEL, type=IPC_TYPE_RESP, size=1

06-01 10:53:56.490  1964  2328 D use-Rlog/RLOG-RIL-IPC: ================================= IPC FMT data =================================

06-01 10:53:56.490  2812  2812 D GsmSST  : [GsmSST] handlPollStateResultMessage: GsmSST setDataRegState=1 regState=0 dataRadioTechnology=9

06-01 10:53:56.490  1964  2328 D use-Rlog/RLOG-RIL-IPC: [0000]   02                                                 .

06-01 10:53:56.490  2812  2812 D PHONE   : [ServiceState] setVoiceRegState=1

06-01 10:53:56.490  2812  2812 E PHONE   : [ServiceState] setState deprecated use setVoiceRegState()

06-01 10:53:56.490  1964  2328 D use-Rlog/RLOG-RIL-IPC: ================================================================================

06-01 10:53:56.490  1964  2328 D use-Rlog/RLOG-RIL: 0 RIL request in the queue (0 pending, 0 handled, 0 unhandled)

06-01 10:53:56.495  2812  2918 D RILJ    : [3722]< QUERY_NETWORK_SELECTION_MODE {0} [SUB0]

06-01 10:53:56.495  2812  2812 D SubscriptionController: [getSubId]- sSlotIdxToSubId.size == 0, return DummySubIds slotIdx=0

06-01 10:53:56.495  2812  2812 D GsmSST  : [GsmSST] Poll ServiceState done:  oldSS=[1 1 voice home data home Mobistar Mobistar 20610 Mobistar Mobistar 20610  Unknown Unknown CSS not supported -1 -1 RoamInd=-1 DefRoamInd=-1 EmergOnly=true IsDataRoamingFromRegistration=false] newSS=[1 1 voice home data home Mobistar Mobistar 20610 Mobistar Mobistar 20610  HSDPA HSDPA CSS not supported -1 -1 RoamInd=-1 DefRoamInd=-1 EmergOnly=true IsDataRoamingFromRegistration=false] oldMaxDataCalls=1 mNewMaxDataCalls=1 oldReasonDataDenied=-1 mNewReasonDataDenied=-1

06-01 10:53:56.495  2812  2812 D GsmSST  : [GsmSST] RAT switched Unknown -> HSDPA at cell 501748

06-01 10:53:56.495  2812  2812 D PHONE   : [ServiceState] setNullState=1

06-01 10:53:56.495  2812  2812 D SST     : updatePhoneObject: Ignore update

06-01 10:53:56.495  2812  2812 D TelephonyManager: setTelephonyProperty: success phoneId=0 property=gsm.network.type value: HSDPA propVal=HSDPA

06-01 10:53:56.495  2812  2812 D SIMRecords: [SIMRecords] getServiceProviderName: no brandOverride

06-01 10:53:56.495  2812  2812 D SIMRecords: [SIMRecords] getServiceProviderName: providerName=null

06-01 10:53:56.500  2812  2812 D GsmSST  : [GsmSST] updateSpnDisplay: radio is on but out of service, set plmn='Emergency calls only'

06-01 10:53:56.500  2812  2812 D SIMRecords: [SIMRecords] getServiceProviderName: no brandOverride

06-01 10:53:56.500  2812  2812 D SIMRecords: [SIMRecords] getServiceProviderName: providerName=null

06-01 10:53:56.500  2812  2812 D SubscriptionController: [getSubId]- sSlotIdxToSubId.size == 0, return DummySubIds slotIdx=0

06-01 10:53:56.500  2812  2812 D GsmSST  : [GsmSST] updateSpnDisplay: changed sending intent rule=2 showPlmn='true' plmn='Emergency calls only' showSpn='false' spn='null' dataSpn='null' subId='-2'

06-01 10:53:56.500  2812  2812 D SubscriptionController: [getSubId]- sSlotIdxToSubId.size == 0, return DummySubIds slotIdx=0

06-01 10:53:56.500  2812  2812 D SubscriptionController: [getSubId]- sSlotIdxToSubId.size == 0, return DummySubIds slotIdx=0

06-01 10:53:56.505  2812  2812 D SubscriptionController: [setPlmnSpn] No valid subscription to store info

06-01 10:53:56.505  2812  2812 D SubscriptionController: notifySubscriptionInfoChanged:

06-01 10:53:56.510  2812  2850 D SubscriptionController: [getActiveSubInfoList]+

06-01 10:53:56.510  2812  2812 D TelephonyManager: setTelephonyProperty: success phoneId=0 property=gsm.operator.alpha value: Mobistar propVal=Mobistar

06-01 10:53:56.510  2812  2850 D SubscriptionController: selection:sim_id>=0 null

06-01 10:53:56.510  2812  2812 D TelephonyManager: setTelephonyProperty: success phoneId=0 property=gsm.operator.numeric value: 20610 propVal=20610

06-01 10:53:56.510  2812  2812 D TelephonyManager: setTelephonyProperty: success phoneId=0 property=gsm.operator.iso-country value: be propVal=be

06-01 10:53:56.510  2812  2812 D GsmSST  : [GsmSST] pollStateDone: no nitz but one TZ for iso-cc=be with zone.getID=Europe/Brussels testOneUniqueOffsetPath=false

06-01 10:53:56.510  2812  2812 D GsmSST  : [GsmSST] setAndBroadcastNetworkSetTimeZone: setTimeZone=Europe/Brussels

06-01 10:53:56.515  2812  2812 D GsmSST  : [GsmSST] setAndBroadcastNetworkSetTimeZone: call alarm.setTimeZone and broadcast zoneId=Europe/Brussels

06-01 10:53:56.515  2812  2812 D GsmSST  : [GsmSST] shouldFixTimeZoneNow: retVal=false iccCardExist=true operatorNumeric=20610 mcc=206 prevOperatorNumeric=20610 prevMcc=206 needToFixTimeZone=false ltod=06-01 10:53:56.522

06-01 10:53:56.515  2812  2812 D TelephonyManager: setTelephonyProperty: success phoneId=0 property=gsm.operator.isroaming value: false propVal=false

06-01 10:53:56.515  2812  2850 D SubscriptionController: [getActiveSubInfoList]- no info return

06-01 10:53:56.520  2812  2812 D GsmSST  : [GsmSST] Broadcasting ServiceState : 1 1 voice home data home Mobistar Mobistar 20610 Mobistar Mobistar 20610  HSDPA HSDPA CSS not supported -1 -1 RoamInd=-1 DefRoamInd=-1 EmergOnly=true IsDataRoamingFromRegistration=false

06-01 10:53:56.520  2812  2812 D SubscriptionController: [getSubId]- sSlotIdxToSubId.size == 0, return DummySubIds slotIdx=0

06-01 10:53:56.520  2812  2812 D DefaultPhoneNotifier: nofityServiceState: mRegistry=com.android.internal.telephony.ITelephonyRegistry$Stub$Proxy@d42da20 ss=1 1 voice home data home Mobistar Mobistar 20610 Mobistar Mobistar 20610  HSDPA HSDPA CSS not supported -1 -1 RoamInd=-1 DefRoamInd=-1 EmergOnly=true IsDataRoamingFromRegistration=false sender=Handler (com.android.internal.telephony.gsm.GSMPhone) {b910da1} phondId=0 subId=-2

06-01 10:53:56.520  2812  2812 D SubscriptionController: [getSlotId]- subId invalid

06-01 10:53:56.520  2812  2812 D SubscriptionController: getSimStateForSlotIdx:  simState=PIN_REQUIRED ordinal=2

06-01 10:53:56.520  2335  2807 D SubscriptionManager: getSimStateForSubscriber: simState=2 slotIdx=0

06-01 10:53:56.520  2335  2807 D TelephonyManager: getSimState: default sim:-1, sim state for slotIdx=0 is 2, return state as unknown

06-01 10:53:56.525  2812  2812 D GsmSST  : [GsmSST] notifyDataRegStateRilRadioTechnologyChanged: drs=1 rat=9

06-01 10:53:56.525  2812  2812 D TelephonyManager: setTelephonyProperty: success phoneId=0 property=gsm.network.type value: HSDPA propVal=HSDPA

06-01 10:53:56.530  2812  2812 D DCT     : [0]get all active apn types

06-01 10:53:56.530  2812  2812 D SubscriptionController: [getSubId]- sSlotIdxToSubId.size == 0, return DummySubIds slotIdx=0

06-01 10:53:56.530  2812  2812 D GsmSST  : [GsmSST] getCellLocation(): X good mCellLoc=[17100,501748,-1]

06-01 10:53:56.530  2335  2851 D TelephonyRegistry: notifyCellLocationForSubscriber: subId=-2 cellLocation=Bundle[mParcelledData.dataSize=64]

06-01 10:53:56.530  2812  2812 D GsmSST  : [GsmSST] SubscriptionListener.onSubscriptionInfoChanged

06-01 10:53:56.530  2812  2812 D SubscriptionController: [getSubId]- sSlotIdxToSubId.size == 0, return DummySubIds slotIdx=0

06-01 10:53:56.530  2812  2812 D DCT     : [0]SubscriptionListener.onSubscriptionInfoChanged

06-01 10:53:56.530  2812  2812 D SubscriptionController: [getSubId]- sSlotIdxToSubId.size == 0, return DummySubIds slotIdx=0

06-01 10:53:56.530  2812  2812 D SubscriptionController: [getActiveSubInfoList]+

06-01 10:53:56.530  2812  2812 D SubscriptionController: selection:sim_id>=0 null

06-01 10:53:56.545  2812  2812 D SubscriptionController: [getActiveSubInfoList]- no info return

06-01 10:53:56.545  2812  2812 E PhoneBase: Error! unregisterForCallWaiting() in PhoneBase should not be called, CDMAPhone inactive.

06-01 10:53:56.545  2812  2812 D SubscriptionController: [getSubId]- sSlotIdxToSubId.size == 0, return DummySubIds slotIdx=0

06-01 10:53:56.545  2812  2812 D SubscriptionController: [getSubId]- sSlotIdxToSubId.size == 0, return DummySubIds slotIdx=0

06-01 10:53:56.550  2812  2812 D SubscriptionController: [getPhoneId]- invalid subId return=-1

06-01 10:53:56.550  2812  2812 D SubscriptionController: [getSubId]- sSlotIdxToSubId.size == 0, return DummySubIds slotIdx=0

06-01 10:53:56.550  2812  2812 D SubscriptionController: [getSubId]- sSlotIdxToSubId.size == 0, return DummySubIds slotIdx=0

06-01 10:53:56.550  2812  2812 D SubscriptionController: [getSubId]- sSlotIdxToSubId.size == 0, return DummySubIds slotIdx=0

06-01 10:53:56.595  2812  2812 E PhoneBase: Error! registerForCallWaiting() in PhoneBase should not be called, CDMAPhone inactive.

06-01 10:53:56.615  2812  2812 D SubscriptionController: [getSubId]- sSlotIdxToSubId.size == 0, return DummySubIds slotIdx=0

06-01 10:53:56.615  2812  2812 D DCT     : [0]handleMessage msg={ when=-90ms what=270377 obj=android.os.AsyncResult@32a8810 target=com.android.internal.telephony.dataconnection.DcTracker }

06-01 10:53:56.615  2812  2812 D DCT     : [0]onUpdateIcc: newIccRecords com.android.internal.telephony.uicc.SIMRecords

06-01 10:53:56.615  2812  2812 D SubscriptionController: [getSubId]- sSlotIdxToSubId.size == 0, return DummySubIds slotIdx=0

06-01 10:53:56.620  2812  2812 D DCT     : [0]onUpdateIcc: tryRestartDataConnections nwTypeChanged

06-01 10:53:56.620  2812  2812 D DCT     : [0]overall state is IDLE

06-01 10:53:56.620  2812  2812 D SIMRecords: [SIMRecords] getOperatorNumeric: IMSI == null

06-01 10:53:56.620  2812  2812 D SubscriptionController: [getSubId]- sSlotIdxToSubId.size == 0, return DummySubIds slotIdx=0

06-01 10:53:56.620  2812  2812 D GSMPhone: [GSMPhone] updateCurrentCarrierInProvider: mSubId = -2 currentDds = -1 operatorNumeric = null

06-01 10:53:56.620  2812  2812 D DCT     : [0]tryRestartDataConnections: createAllApnList and cleanUpAllConnections

06-01 10:53:56.620  2812  2812 D DCT     : [0]getOperatorNumberic - returning from card: 

06-01 10:53:56.620  2812  2812 D DCT     : [0]isDummyProfileNeeded: radioTechFam = 1

06-01 10:53:56.620  2812  2812 D DCT     : [0]createAllApnList: No APN found for carrier: 

06-01 10:53:56.620  2812  2812 D DCT     : [0]createAllApnList: X mAllApnSettings=[]

06-01 10:53:56.620  2812  2812 D DCT     : [0]setDataProfilesAsNeeded

06-01 10:53:56.620  2812  2812 D DCT     : [0]setInitialApn: E preferredApn=null

06-01 10:53:56.620  2812  2812 D DCT     : [0]setInitialAttachApn: X There in no available apn

06-01 10:53:56.620  2812  2812 D DCT     : [0]cleanUpAllConnections: tearDown=false reason=nwTypeChanged

06-01 10:53:56.620  2812  2812 D DCT     : [0]cleanUpConnection: tearDown=false reason=nwTypeChanged apnContext={mApnType=default mState=IDLE mWaitingApns={null} mWaitingApnsPermanentFailureCountDown=0 mApnSetting={null} mReason=nwTypeChanged mDataEnabled=false mDependencyMet=true}

06-01 10:53:56.620  2812  2812 D GSMPhone: getDataConnectionState: Data is Out of Service. ret = DISCONNECTED

06-01 10:53:56.620  2812  2812 D SubscriptionController: [getSubId]- sSlotIdxToSubId.size == 0, return DummySubIds slotIdx=0

06-01 10:53:56.620  2812  2812 D DCT     : [0]isDataAllowed: not allowed due to - Attached= false - SIM not loaded - SIM not loaded and not NV subscription - defaultDataSelected= false

06-01 10:53:56.625  2812  2812 D SubscriptionController: [getPhoneId]- invalid subId return=-1

06-01 10:53:56.625  2812  2812 D DCT     : [0]setupDataForSinglePdn: reason = nwTypeChanged isDisconnected = true

06-01 10:53:56.625  2812  2812 D DCT     : [0]isOnlySingleDcAllowed(9): false

06-01 10:53:56.625  2812  2812 D DCT     : [0]cleanUpConnection: X tearDown=false reason=nwTypeChanged apnContext={mApnType=default mState=IDLE mWaitingApns={null} mWaitingApnsPermanentFailureCountDown=0 mApnSetting={null} mReason=nwTypeChanged mDataEnabled=false mDependencyMet=true} dcac=null

06-01 10:53:56.630  2812  2812 D DCT     : [0]cleanUpConnection: tearDown=false reason=nwTypeChanged apnContext={mApnType=mms mState=IDLE mWaitingApns={null} mWaitingApnsPermanentFailureCountDown=0 mApnSetting={null} mReason=nwTypeChanged mDataEnabled=false mDependencyMet=true}

06-01 10:53:56.630  2812  2812 D GSMPhone: getDataConnectionState: Data is Out of Service. ret = DISCONNECTED

06-01 10:53:56.630  2812  2812 D SubscriptionController: [getSubId]- sSlotIdxToSubId.size == 0, return DummySubIds slotIdx=0

06-01 10:53:56.630  2812  2812 D DCT     : [0]isDataAllowed: not allowed due to - Attached= false - SIM not loaded - SIM not loaded and not NV subscription - defaultDataSelected= false

06-01 10:53:56.630  2812  2812 D SubscriptionController: [getPhoneId]- invalid subId return=-1

06-01 10:53:56.635  2812  2812 D DCT     : [0]setupDataForSinglePdn: reason = nwTypeChanged isDisconnected = true

06-01 10:53:56.635  2812  2812 D DCT     : [0]isOnlySingleDcAllowed(9): false

06-01 10:53:56.635  2812  2812 D DCT     : [0]cleanUpConnection: X tearDown=false reason=nwTypeChanged apnContext={mApnType=mms mState=IDLE mWaitingApns={null} mWaitingApnsPermanentFailureCountDown=0 mApnSetting={null} mReason=nwTypeChanged mDataEnabled=false mDependencyMet=true} dcac=null

06-01 10:53:56.635  2812  2812 D DCT     : [0]cleanUpConnection: tearDown=false reason=nwTypeChanged apnContext={mApnType=supl mState=IDLE mWaitingApns={null} mWaitingApnsPermanentFailureCountDown=0 mApnSetting={null} mReason=nwTypeChanged mDataEnabled=false mDependencyMet=true}

06-01 10:53:56.635  2812  2812 D GSMPhone: getDataConnectionState: Data is Out of Service. ret = DISCONNECTED

06-01 10:53:56.635  2812  2812 D SubscriptionController: [getSubId]- sSlotIdxToSubId.size == 0, return DummySubIds slotIdx=0

06-01 10:53:56.635  2812  2812 D DCT     : [0]isDataAllowed: not allowed due to - Attached= false - SIM not loaded - SIM not loaded and not NV subscription - defaultDataSelected= false

06-01 10:53:56.635  2812  2812 D SubscriptionController: [getPhoneId]- invalid subId return=-1

06-01 10:53:56.640  2812  2812 D DCT     : [0]setupDataForSinglePdn: reason = nwTypeChanged isDisconnected = true

06-01 10:53:56.640  2812  2812 D DCT     : [0]isOnlySingleDcAllowed(9): false

06-01 10:53:56.640  2812  2812 D DCT     : [0]cleanUpConnection: X tearDown=false reason=nwTypeChanged apnContext={mApnType=supl mState=IDLE mWaitingApns={null} mWaitingApnsPermanentFailureCountDown=0 mApnSetting={null} mReason=nwTypeChanged mDataEnabled=false mDependencyMet=true} dcac=null

06-01 10:53:56.640  2812  2812 D DCT     : [0]cleanUpConnection: tearDown=false reason=nwTypeChanged apnContext={mApnType=dun mState=IDLE mWaitingApns={null} mWaitingApnsPermanentFailureCountDown=0 mApnSetting={null} mReason=nwTypeChanged mDataEnabled=false mDependencyMet=true}

06-01 10:53:56.640  2812  2812 D GSMPhone: getDataConnectionState: Data is Out of Service. ret = DISCONNECTED

06-01 10:53:56.640  2812  2812 D SubscriptionController: [getSubId]- sSlotIdxToSubId.size == 0, return DummySubIds slotIdx=0

06-01 10:53:56.640  2812  2812 D DCT     : [0]isDataAllowed: not allowed due to - Attached= false - SIM not loaded - SIM not loaded and not NV subscription - defaultDataSelected= false

06-01 10:53:56.640  2812  2812 D SubscriptionController: [getPhoneId]- invalid subId return=-1

06-01 10:53:56.645  2812  2812 D DCT     : [0]setupDataForSinglePdn: reason = nwTypeChanged isDisconnected = true

06-01 10:53:56.645  2812  2812 D DCT     : [0]isOnlySingleDcAllowed(9): false

06-01 10:53:56.645  2812  2812 D DCT     : [0]cleanUpConnection: X tearDown=false reason=nwTypeChanged apnContext={mApnType=dun mState=IDLE mWaitingApns={null} mWaitingApnsPermanentFailureCountDown=0 mApnSetting={null} mReason=nwTypeChanged mDataEnabled=false mDependencyMet=true} dcac=null

06-01 10:53:56.645  2812  2812 D DCT     : [0]cleanUpConnection: tearDown=false reason=nwTypeChanged apnContext={mApnType=hipri mState=IDLE mWaitingApns={null} mWaitingApnsPermanentFailureCountDown=0 mApnSetting={null} mReason=nwTypeChanged mDataEnabled=false mDependencyMet=true}

06-01 10:53:56.645  2812  2812 D GSMPhone: getDataConnectionState: Data is Out of Service. ret = DISCONNECTED

06-01 10:53:56.645  2812  2812 D SubscriptionController: [getSubId]- sSlotIdxToSubId.size == 0, return DummySubIds slotIdx=0

06-01 10:53:56.645  2812  2812 D DCT     : [0]isDataAllowed: not allowed due to - Attached= false - SIM not loaded - SIM not loaded and not NV subscription - defaultDataSelected= false

06-01 10:53:56.645  2812  2812 D SubscriptionController: [getPhoneId]- invalid subId return=-1

06-01 10:53:56.650  2812  2812 D DCT     : [0]setupDataForSinglePdn: reason = nwTypeChanged isDisconnected = true

06-01 10:53:56.650  2812  2812 D DCT     : [0]isOnlySingleDcAllowed(9): false

06-01 10:53:56.650  2812  2812 D DCT     : [0]cleanUpConnection: X tearDown=false reason=nwTypeChanged apnContext={mApnType=hipri mState=IDLE mWaitingApns={null} mWaitingApnsPermanentFailureCountDown=0 mApnSetting={null} mReason=nwTypeChanged mDataEnabled=false mDependencyMet=true} dcac=null

06-01 10:53:56.650  2812  2812 D DCT     : [0]stopNetStatPoll

06-01 10:53:56.650  2812  2812 D SubscriptionController: [getSubId]- sSlotIdxToSubId.size == 0, return DummySubIds slotIdx=0

06-01 10:53:56.650  2812  2812 D DCT     : [0]cleanUpConnection: mDisconnectPendingCount = 0

06-01 10:53:56.650  2812  2812 D DCT     : [0]setupDataOnConnectableApns: nwTypeChanged

06-01 10:53:56.650  2812  2812 D DCT     : [0]setupDataOnConnectableApns: apnContext {mApnType=dun mState=IDLE mWaitingApns={null} mWaitingApnsPermanentFailureCountDown=0 mApnSetting={null} mReason=nwTypeChanged mDataEnabled=false mDependencyMet=true}

06-01 10:53:56.650  2812  2812 D DCT     : [0]setupDataOnConnectableApns: apnContext {mApnType=hipri mState=IDLE mWaitingApns={null} mWaitingApnsPermanentFailureCountDown=0 mApnSetting={null} mReason=nwTypeChanged mDataEnabled=false mDependencyMet=true}

06-01 10:53:56.650  2812  2812 D DCT     : [0]setupDataOnConnectableApns: apnContext {mApnType=supl mState=IDLE mWaitingApns={null} mWaitingApnsPermanentFailureCountDown=0 mApnSetting={null} mReason=nwTypeChanged mDataEnabled=false mDependencyMet=true}

06-01 10:53:56.650  2812  2812 D DCT     : [0]setupDataOnConnectableApns: apnContext {mApnType=default mState=IDLE mWaitingApns={null} mWaitingApnsPermanentFailureCountDown=0 mApnSetting={null} mReason=nwTypeChanged mDataEnabled=false mDependencyMet=true}

06-01 10:53:56.650  2812  2812 D DCT     : [0]setupDataOnConnectableApns: apnContext {mApnType=mms mState=IDLE mWaitingApns={null} mWaitingApnsPermanentFailureCountDown=0 mApnSetting={null} mReason=nwTypeChanged mDataEnabled=false mDependencyMet=true}

06-01 10:53:56.650  2812  2812 D DctController: handleMessage msg={ when=-120ms what=107 target=com.android.internal.telephony.dataconnection.DctController }

06-01 10:53:56.650  2812  2812 D DctController: onSubInfoReady mPhoneNum=1

06-01 10:53:56.650  2812  2812 D SubscriptionController: [getSubId]- sSlotIdxToSubId.size == 0, return DummySubIds slotIdx=0

06-01 10:53:56.650  2812  2812 D DctController: onSubInfoReady handle pending requests subId=-2

06-01 10:53:56.650  2812  2812 D SubscriptionController: [getSubId]- sSlotIdxToSubId.size == 0, return DummySubIds slotIdx=0

06-01 10:53:56.650  2812  2812 D DctController: [TNF -2]evalPendingRequest, pending request size is 1

06-01 10:53:56.650  2812  2812 D SubscriptionController: [getSubId]- sSlotIdxToSubId.size == 0, return DummySubIds slotIdx=0

06-01 10:53:56.650  2812  2812 D DctController: [TNF -2]evalPendingRequest: request = NetworkRequest [ id=1, legacyType=-1, [ Capabilities: INTERNET&NOT_RESTRICTED&TRUSTED&NOT_VPN] ]

06-01 10:53:56.650  2812  2812 D SubscriptionController: [getSubId]- sSlotIdxToSubId.size == 0, return DummySubIds slotIdx=0

06-01 10:53:56.650  2812  2812 D DctController: [TNF -2]Cellular needs Network for NetworkRequest [ id=1, legacyType=-1, [ Capabilities: INTERNET&NOT_RESTRICTED&TRUSTED&NOT_VPN] ]

06-01 10:53:56.650  2812  2812 D SubscriptionController: [getSubId]- sSlotIdxToSubId.size == 0, return DummySubIds slotIdx=0

06-01 10:53:56.650  2812  2812 D SubscriptionController: [getSubId]- sSlotIdxToSubId.size == 0, return DummySubIds slotIdx=0

06-01 10:53:56.650  2812  2812 D DctController: [TNF -2]Request not useable, pending request.

06-01 10:53:56.650  2812  2812 D DctController: processRequests

06-01 10:53:56.650  2812  2812 D SubscriptionController: [getSubId]- sSlotIdxToSubId.size == 0, return DummySubIds slotIdx=0

06-01 10:53:56.655  2812  2812 D SubscriptionController: [getSubId]- sSlotIdxToSubId.size == 0, return DummySubIds slotIdx=0

06-01 10:53:56.655  2812  2812 D DCT     : [0]getDataOnRoamingEnabled: phoneSubId=-2 isDataRoamingEnabled=false

06-01 10:53:56.655  2812  2812 D SubscriptionController: [getSubId]- sSlotIdxToSubId.size == 0, return DummySubIds slotIdx=0

06-01 10:53:56.655  2812  2812 D DCT     : [0]getDataOnRoamingEnabled: phoneSubId=-2 isDataRoamingEnabled=false

06-01 10:53:56.655  2812  2812 D SubscriptionController: [getSubId]- sSlotIdxToSubId.size == 0, return DummySubIds slotIdx=0

06-01 10:53:56.655  2812  2812 D DCT     : [0]getDataOnRoamingEnabled: phoneSubId=-2 isDataRoamingEnabled=false

06-01 10:53:56.655  2812  2812 D SubscriptionController: [getSubId]- sSlotIdxToSubId.size == 0, return DummySubIds slotIdx=0

06-01 10:53:56.655  2812  2812 D DCT     : [0]getDataOnRoamingEnabled: phoneSubId=-2 isDataRoamingEnabled=false

06-01 10:53:56.655  2812  2812 D SubscriptionController: [getSubId]- sSlotIdxToSubId.size == 0, return DummySubIds slotIdx=0

06-01 10:53:56.655  2812  2812 D DCT     : [0]getDataOnRoamingEnabled: phoneSubId=-2 isDataRoamingEnabled=false

06-01 10:53:56.655  2812  2812 D DctController: handleMessage msg={ when=-3ms what=100 target=com.android.internal.telephony.dataconnection.DctController }

06-01 10:53:56.655  2812  2812 D DcSwitchAsyncChannel: [DcSwitchAsyncChannel-0]: rspIsIdle=true

06-01 10:53:56.655  2812  2812 D SubscriptionController: [getPhoneId]- invalid subId return=-1

06-01 10:53:56.655  2812  2812 D DcSwitchAsyncChannel: [DcSwitchAsyncChannel-0]: rspIsIdle=true

06-01 10:53:56.655  2812  2812 D DctController: onProcessRequest requestedPhoneId=-1, activePhoneId=-1

06-01 10:53:56.970  2812  2850 D SubscriptionController: [getSlotId]- subId invalid

06-01 10:53:56.975  2812  3063 D SubscriptionController: getSimStateForSlotIdx:  simState=PIN_REQUIRED ordinal=2

06-01 10:53:56.975  2457  3212 D SubscriptionManager: getSimStateForSubscriber: simState=2 slotIdx=0

06-01 10:53:56.975  2457  3212 D TelephonyManager: getSimState: default sim:-1, sim state for slotIdx=0 is 2, return state as unknown

06-01 10:53:57.060  2812  2846 D DCT     : [0]hasMatchedTetherApnSetting: APN=null

06-01 10:53:57.070  2812  2850 D SubscriptionController: [getSlotId]- subId invalid

06-01 10:53:57.070  2812  3063 D SubscriptionController: getSimStateForSlotIdx:  simState=PIN_REQUIRED ordinal=2

06-01 10:53:57.070  2457  3212 D SubscriptionManager: getSimStateForSubscriber: simState=2 slotIdx=0

06-01 10:53:57.070  2457  3212 D TelephonyManager: getSimState: default sim:-1, sim state for slotIdx=0 is 2, return state as unknown

06-01 10:53:57.080  2812  2846 D DCT     : [0]hasMatchedTetherApnSetting: APN=null

06-01 10:53:58.070  2812  3063 D SubscriptionController: [getActiveSubInfoList]+

06-01 10:53:58.070  2812  3063 D SubscriptionController: selection:sim_id>=0 null

06-01 10:53:58.075  2812  3063 D SubscriptionController: [getActiveSubInfoList]- no info return

06-01 10:53:58.080  2812  2846 D SubscriptionController: [getSubId]- sSlotIdxToSubId.size == 0, return DummySubIds slotIdx=0

06-01 10:53:58.260  2812  3017 D SubscriptionController: [getSlotId]- subId invalid

06-01 10:53:58.260  2812  3063 D SubscriptionController: getSimStateForSlotIdx:  simState=PIN_REQUIRED ordinal=2

06-01 10:53:58.260  2457  2457 D SubscriptionManager: getSimStateForSubscriber: simState=2 slotIdx=0

06-01 10:53:58.260  2457  2457 D TelephonyManager: getSimState: default sim:-1, sim state for slotIdx=0 is 2, return state as unknown

06-01 10:53:58.265  2812  2846 D SubscriptionController: [getActiveSubInfoList]+

06-01 10:53:58.265  2812  2846 D SubscriptionController: selection:sim_id>=0 null

06-01 10:53:58.275  2812  2846 D SubscriptionController: [getActiveSubInfoList]- no info return

06-01 10:53:58.275  2812  2850 D SubscriptionController: [getSubId]- sSlotIdxToSubId.size == 0, return DummySubIds slotIdx=0

06-01 10:53:58.280  2812  3017 D SubscriptionController: [getActiveSubInfoList]+

06-01 10:53:58.280  2812  3017 D SubscriptionController: selection:sim_id>=0 null

06-01 10:53:58.285  2812  3017 D SubscriptionController: [getActiveSubInfoList]- no info return

06-01 10:53:58.285  2812  3063 D SubscriptionController: [getSubId]- sSlotIdxToSubId.size == 0, return DummySubIds slotIdx=0

06-01 10:53:58.305  2812  2846 D DCT     : [0]hasMatchedTetherApnSetting: APN=null

06-01 10:53:58.320  2812  2850 D DCT     : [0]hasMatchedTetherApnSetting: APN=null

06-01 10:53:58.325  2812  3017 D DCT     : [0]hasMatchedTetherApnSetting: APN=null

06-01 10:53:58.815  2812  3063 D SubscriptionController: [getActiveSubInfoList]+

06-01 10:53:58.815  2812  3063 D SubscriptionController: selection:sim_id>=0 null

06-01 10:53:58.820  2812  3063 D SubscriptionController: [getActiveSubInfoList]- no info return

06-01 10:53:58.825  2812  2846 D SubscriptionController: [getSubId]- sSlotIdxToSubId.size == 0, return DummySubIds slotIdx=0

06-01 10:53:59.155  2812  2850 D DCT     : [0]hasMatchedTetherApnSetting: APN=null

06-01 10:53:59.295  2812  2812 D SubscriptionController: [getPhoneId] asked for default subId=-1

06-01 10:53:59.295  2812  2812 D SubscriptionController: [getPhoneId]- invalid subId return=-1

06-01 10:53:59.565  2812  2846 D SubscriptionController: [getPhoneId] asked for default subId=-1

06-01 10:53:59.565  2812  2846 D SubscriptionController: [getPhoneId]- invalid subId return=-1

06-01 10:54:01.715  2812  2812 D CAT     : com.android.stk.BootCompletedReceiver: [ACTION_BOOT_COMPLETED]

06-01 10:54:01.720  2812  2812 D CAT     : com.android.stk.StkAppService: onCreate()+

06-01 10:54:01.720  2812  2812 D CAT     : com.android.stk.StkAppService: simCount: 1

06-01 10:54:01.720  2812  2812 D CAT     : com.android.stk.StkAppService: slotId: 0

06-01 10:54:01.725  2812  2812 D CAT     : com.android.stk.StkAppService: onStart sim id: 0, op: 5, *****

06-01 10:54:01.825  2812  3436 D CAT     : com.android.stk.StkAppService: handleMessage opcode[5], sim id[0]

06-01 10:54:01.825  2812  3436 D CAT     : com.android.stk.StkAppService:  OP_BOOT_COMPLETED

06-01 10:54:01.825  2812  3436 D CAT     : StkAppInstaller: [setAppState]+

06-01 10:54:01.825  2812  3436 D CAT     : StkAppInstaller: Need not change app state!!

06-01 10:54:01.825  2812  3436 D CAT     : StkAppInstaller: [setAppState]-

06-01 10:54:02.085  2812  3063 D SubscriptionController: [getActiveSubInfoList]+

06-01 10:54:02.095  2812  2850 D SubscriptionController: [getPhoneId] asked for default subId=-1

06-01 10:54:02.095  2812  2850 D SubscriptionController: [getPhoneId]- invalid subId return=-1

06-01 10:54:02.110  2812  3063 D SubscriptionController: selection:sim_id>=0 null

06-01 10:54:02.125  2812  2846 D SubscriptionController: [getActiveSubInfoList]+

06-01 10:54:02.135  2812  2846 D SubscriptionController: selection:sim_id>=0 null

06-01 10:54:02.145  2812  2846 D SubscriptionController: [getActiveSubInfoList]- no info return

06-01 10:54:02.145  2812  3063 D SubscriptionController: [getActiveSubInfoList]- no info return

06-01 10:54:02.145  2812  3461 D SubscriptionController: [getActiveSubInfoList]+

06-01 10:54:02.150  2812  3461 D SubscriptionController: selection:sim_id>=0 null

06-01 10:54:02.150  2812  3461 D SubscriptionController: [getActiveSubInfoList]- no info return

06-01 10:54:02.155  2812  3063 D SubscriptionController: [getActiveSubInfoList]+

06-01 10:54:02.160  2812  3063 D SubscriptionController: selection:sim_id>=0 null

06-01 10:54:02.160  2812  3063 D SubscriptionController: [getActiveSubInfoList]- no info return

06-01 10:54:02.320  2812  3063 D SubscriptionController: [getPhoneId] asked for default subId=-1

06-01 10:54:02.320  2812  3063 D SubscriptionController: [getPhoneId]- invalid subId return=-1

06-01 10:54:08.855  2812  2812 D DCT     : [0]onReceive: action=android.intent.action.SCREEN_ON

06-01 10:54:08.855  2812  2812 D DCT     : [0]stopNetStatPoll

06-01 10:54:08.855  2812  2812 D SubscriptionController: [getSubId]- sSlotIdxToSubId.size == 0, return DummySubIds slotIdx=0

06-01 10:54:08.855  2812  2812 D DCT     : [0]overall state is IDLE

06-01 10:54:08.855  2812  2812 D SubscriptionController: [getSubId]- sSlotIdxToSubId.size == 0, return DummySubIds slotIdx=0

06-01 10:54:08.865  2812  2812 D DCT     : [0]onReceive: action=android.intent.action.SCREEN_OFF

06-01 10:54:08.865  2812  2812 D DCT     : [0]stopNetStatPoll

06-01 10:54:08.865  2812  2812 D SubscriptionController: [getSubId]- sSlotIdxToSubId.size == 0, return DummySubIds slotIdx=0

06-01 10:54:08.865  2812  2812 D DCT     : [0]overall state is IDLE

06-01 10:54:08.865  2812  2812 D SubscriptionController: [getSubId]- sSlotIdxToSubId.size == 0, return DummySubIds slotIdx=0

06-01 10:54:24.560  2812  2812 D DCT     : [0]onReceive: action=android.intent.action.SCREEN_ON

06-01 10:54:24.560  2812  2812 D DCT     : [0]stopNetStatPoll

06-01 10:54:24.560  2812  2812 D SubscriptionController: [getSubId]- sSlotIdxToSubId.size == 0, return DummySubIds slotIdx=0

06-01 10:54:24.565  2812  2812 D DCT     : [0]overall state is IDLE

06-01 10:54:24.565  2812  2812 D SubscriptionController: [getSubId]- sSlotIdxToSubId.size == 0, return DummySubIds slotIdx=0

06-01 10:54:26.390  2812  2846 D DCT     : [0]hasMatchedTetherApnSetting: APN=null

