D RILD    : **RIL Daemon Started**
D RILD    : **RILd param count=1**
W RILD    : RIL_SAP_Init not defined or exported in /system/lib/libsamsung-ril.so: undefined symbol: RIL_SAP_Init
D RILD    : RIL_Init argc = 5 clientId = 0
D use-Rlog/RLOG-RIL: Created IPC FMT client
D use-Rlog/RLOG-RIL: Created IPC RFS client
D use-Rlog/RLOG-RIL: Created SRS client
D use-Rlog/RLOG-RIL-IPC: Starting i9300 modem boot
D use-Rlog/RLOG-RIL-IPC: Opened modem image device
D use-Rlog/RLOG-RIL-IPC: Mapped modem image data to memory
D use-Rlog/RLOG-RIL-IPC: Opened modem boot device
D use-Rlog/RLOG-RIL-IPC: Opened modem link device
D use-Rlog/RLOG-RIL-IPC: Turned the modem off
D use-Rlog/RLOG-RIL-IPC: Turned the modem on
D use-Rlog/RLOG-RIL-IPC: Waited for link connected
D use-Rlog/RLOG-RIL-IPC: Wrote ATAT in ASCII
D use-Rlog/RLOG-RIL-IPC: Read chip id (0x16)
D use-Rlog/RLOG-RIL-IPC: Wrote PSI header
D use-Rlog/RLOG-RIL-IPC: Wrote PSI, CRC is 0xc8
D use-Rlog/RLOG-RIL-IPC: Wrote PSI CRC (0xc8)
D use-Rlog/RLOG-RIL-IPC: Read PSI CRC ACK
D use-Rlog/RLOG-RIL-IPC: Read PSI ACK
D use-Rlog/RLOG-RIL-IPC: Sent XMM626 HSIC PSI
D use-Rlog/RLOG-RIL-IPC: Wrote EBL size
D use-Rlog/RLOG-RIL-IPC: Wrote EBL, CRC is 0xb5
D use-Rlog/RLOG-RIL-IPC: Wrote EBL CRC (0xb5)
D use-Rlog/RLOG-RIL-IPC: Sent XMM626 HSIC EBL
D use-Rlog/RLOG-RIL-IPC: Read port config
D use-Rlog/RLOG-RIL-IPC: Sent XMM626 HSIC port config
D use-Rlog/RLOG-RIL-IPC: Sent XMM626 HSIC SEC start
D use-Rlog/RLOG-RIL-IPC: Sent XMM626 HSIC firmware
D use-Rlog/RLOG-RIL-IPC: Checked nv_data path
D use-Rlog/RLOG-RIL-IPC: Checked nv_data md5 path
D use-Rlog/RLOG-RIL-IPC: Calculated nv_data md5: 302aea06dda5362c3a57a5929d595bd1
D use-Rlog/RLOG-RIL-IPC: Read nv_data md5: 302aea06dda5362c3a57a5929d595bd1
D use-Rlog/RLOG-RIL-IPC: Checked nv_data backup path
D use-Rlog/RLOG-RIL-IPC: Loaded nv_data
D use-Rlog/RLOG-RIL-IPC: Sent XMM626 HSIC nv_data
D use-Rlog/RLOG-RIL-IPC: Sent XMM626 HSIC SEC end
D use-Rlog/RLOG-RIL-IPC: Sent XMM626 HSIC HW reset
D use-Rlog/RLOG-RIL-IPC: Waiting for host wake failed
D use-Rlog/RLOG-RIL-IPC: Waited for host wake
D use-Rlog/RLOG-RIL-IPC: Waited for link connected
D use-Rlog/RLOG-RIL: Opened IPC FMT client
D use-Rlog/RLOG-RIL: Started IPC FMT client loop
D use-Rlog/RLOG-RIL: Opened IPC RFS client
D use-Rlog/RLOG-RIL: Started IPC RFS client loop
D use-Rlog/RLOG-RIL-SRS: Started SRS server loop
D use-Rlog/RLOG-RIL: Opened SRS client
D use-Rlog/RLOG-RIL: Started SRS client loop
D RILD    : RIL_Init rilInit completed
I RILC    : SIM_COUNT: 1
E RILC    : RIL_register: RIL version 11
I RILC    : s_registerCalled flag set, 1
I RILC    : Start to listen RIL_SOCKET_1
D use-Rlog/RLOG-RIL-IPC: 
D use-Rlog/RLOG-RIL-IPC: xmm626_sec_modem_fmt_recv: Received FMT message
D RILD    : RIL_Init RIL_register completed
D use-Rlog/RLOG-RIL-IPC: xmm626_sec_modem_fmt_recv: Message: aseq=0xff, command=IPC_PWR_PHONE_PWR_UP, type=IPC_TYPE_NOTI, size=0
D RILD    : RIL_register_socket completed
D RILD    : RIL_Init starting sleep loop
D use-Rlog/RLOG-RIL: Updating RIL radio state to 0
D use-Rlog/RLOG-RIL-IPC: 
D use-Rlog/RLOG-RIL-IPC: xmm626_sec_modem_fmt_recv: Received FMT message
D use-Rlog/RLOG-RIL-IPC: xmm626_sec_modem_fmt_recv: Message: aseq=0x00, command=IPC_MISC_ME_IMSI, type=IPC_TYPE_NOTI, size=16
D use-Rlog/RLOG-RIL-IPC: ================================= IPC FMT data =================================
D use-Rlog/RLOG-RIL-IPC: [0000]   0F 30 30 30 30 30 30 30  30 30 30 30 30 30 30 30   .0000000 00000000
D use-Rlog/RLOG-RIL-IPC: ================================================================================
D use-Rlog/RLOG-RIL-IPC: 
D use-Rlog/RLOG-RIL-IPC: xmm626_sec_modem_fmt_recv: Received FMT message
D use-Rlog/RLOG-RIL-IPC: xmm626_sec_modem_fmt_recv: Message: aseq=0xff, command=IPC_NET_REGIST, type=IPC_TYPE_NOTI, size=11
D use-Rlog/RLOG-RIL-IPC: ================================= IPC FMT data =================================
D use-Rlog/RLOG-RIL-IPC: [0000]   FF 02 01 00 00 00 00 00  00 00 00                  ........ ...
D use-Rlog/RLOG-RIL-IPC: ================================================================================
D use-Rlog/RLOG-RIL-IPC: 
D use-Rlog/RLOG-RIL-IPC: xmm626_sec_modem_fmt_recv: Received FMT message
D use-Rlog/RLOG-RIL-IPC: xmm626_sec_modem_fmt_recv: Message: aseq=0xff, command=IPC_NET_REGIST, type=IPC_TYPE_NOTI, size=11
D use-Rlog/RLOG-RIL-IPC: ================================= IPC FMT data =================================
D use-Rlog/RLOG-RIL-IPC: [0000]   FF 03 01 00 00 00 00 00  00 00 00                  ........ ...
D use-Rlog/RLOG-RIL-IPC: ================================================================================
D use-Rlog/RLOG-RIL-IPC: 
D use-Rlog/RLOG-RIL-IPC: xmm626_sec_modem_fmt_recv: Received FMT message
D use-Rlog/RLOG-RIL-IPC: xmm626_sec_modem_fmt_recv: Message: aseq=0x00, command=IPC_DISP_ICON_INFO, type=IPC_TYPE_NOTI, size=4
D use-Rlog/RLOG-RIL-IPC: ================================= IPC FMT data =================================
D use-Rlog/RLOG-RIL-IPC: [0000]   FF 00 00 00                                        ....
D use-Rlog/RLOG-RIL-IPC: ================================================================================
D use-Rlog/RLOG-RIL-IPC: Reading RFS data failed
E use-Rlog/RLOG-RIL-IPC: Receiving from IPC RFS client failed
E use-Rlog/RLOG-RIL: IPC RFS client loop failed
D use-Rlog/RLOG-RIL: Closed IPC RFS client
D use-Rlog/RLOG-RIL: Opened IPC RFS client
D TelephonyManager: /proc/cmdline=console=ttySAC2,115200 consoleblank=0 androidboot.hardware=smdk4x12 console=ram loglevel=4 sec_debug.level=0 sec_watchdog.sec_pet=5 androidboot.debug_level=0x4f4c sec_log=0x100000@0x46000000 s3cfb.bootloaderfb=0x5ec00000 lcdtype=96 consoleblank=0 lpcharge=0 lpj=3981312 vmalloc=144m oops=panic pmic_info=33 cordon=3d296f432f676dc6918124a693bb1d19 connie=GT-I9300_OPEN_EUR_dcbb2a7cb6725399f35a51e434742c83 androidboot.emmc_checksum=3 androidboot.odin_download=1 androidboot.bootloader=I9300XXUGNH4 androidboot.serialno=4df0ffa71f9b5f31 snd_soc_core.pmdown_time=1000
W SmsApplication: com.android.phone does not have OP_WRITE_SMS:  (fixing)
W SmsApplication: com.android.bluetooth does not have OP_WRITE_SMS:  (fixing)
W SmsApplication: com.android.mms.service does not have OP_WRITE_SMS:  (fixing)
W SmsApplication: com.android.providers.telephony does not have OP_WRITE_SMS:  (fixing)
W CarrierConfigManager: Error getting config for subId -1 ICarrierConfigLoader is null
D TelephonyRegistry: listen oscl: hasNotifySubscriptionInfoChangedOccurred==false no callback
D TelephonyRegistry: listen oscl: hasNotifySubscriptionInfoChangedOccurred==false no callback
D TelephonyRegistry: systemRunning register for intents
D SubscriptionManager: getSimStateForSubscriber: simState=0 slotIdx=0
D SubscriptionManager: getSimStateForSubscriber: simState=0 slotIdx=0
D TelephonyRegistry: notifyCellLocationForSubscriber: subId=0 cellLocation=Bundle[{}]
D SubscriptionManager: getSimStateForSubscriber: simState=0 slotIdx=0
D TelephonyManager: getSimState: default sim:-1, sim state for slotIdx=0 is 0, return state as unknown
D SubscriptionManager: getSimStateForSubscriber: simState=0 slotIdx=0
D TelephonyManager: getSimState: default sim:-1, sim state for slotIdx=0 is 0, return state as unknown
D SubscriptionManager: getSimStateForSubscriber: simState=0 slotIdx=0
D TelephonyManager: getSimState: default sim:-1, sim state for slotIdx=0 is 0, return state as unknown
D SubscriptionManager: getSimStateForSubscriber: simState=0 slotIdx=0
D TelephonyManager: getSimState: default sim:-1, sim state for slotIdx=0 is 0, return state as unknown
D SubscriptionManager: getSimStateForSubscriber: simState=0 slotIdx=0
D TelephonyManager: getSimState: default sim:-1, sim state for slotIdx=0 is 0, return state as unknown
D SubscriptionManager: getSimStateForSubscriber: simState=0 slotIdx=0
D TelephonyManager: getSimState: default sim:-1, sim state for slotIdx=0 is 0, return state as unknown
D TelephonyPluginDelegate: Extension = @/system/framework/
D TelephonyPluginDelegate: classLoader = dalvik.system.PathClassLoader[DexPathList[[directory "/system/framework"],nativeLibraryDirectories=[/vendor/lib, /system/lib]]]
D TelephonyPluginDelegate: No customized TelephonyPlugin available, fallback to default
D TelephonyPluginDelegate: cls = class com.android.internal.telephony.DefaultTelephonyPlugin
D TelephonyPluginDelegate: constructor method = public com.android.internal.telephony.DefaultTelephonyPlugin()
D TDC     : updateOrInsert: inserting: Modem { uuid=modem, state=0, rilModel=0, rat={}, maxActiveVoiceCall=1, maxActiveDataCall=1, maxStandby=1 }
D TDC     : updateOrInsert: inserting: Sim { uuid=sim, modemUuid=modem, state=0 }
D TelephonyManager: getLteOnCdmaMode=0 curVal=-1 product_type='' lteOnCdmaProductType=''
D CdmaSSM : subscriptionSource from settings: 0
I PhoneFactory: Cdma Subscription set to 0
I PhoneFactory: RILClassname is RIL
I PhoneFactory: Network Mode set to 0
D RILJ    : RIL(context, preferredNetworkType=0 cdmaSubscription=0)
D RILJ    : Starting RILReceiver0 [SUB0]
I RILJ    : (0) Connected to 'rild' socket
D RILJ    : [3648]> GET_HARDWARE_CONFIG [SUB0]
I PhoneFactory: Creating SubscriptionController
I RILC    : libril: new connection to RIL_SOCKET_1
D RILJ    : [UNSL]< UNSOL_RIL_CONNECTED {11} [SUB0]
D RILJ    : [3649]> RADIO_POWER off [SUB0]
D SubscriptionController: [SubscriptionController] init by Context
D RILJ    : [3650]> RIL_REQUEST_CDMA_SET_SUBSCRIPTION_SOURCE : 0 [SUB0]
D RILJ    : setCellInfoListRate: 2147483647 [SUB0]
D RILJ    : [3651]> RIL_REQUEST_SET_CELL_INFO_LIST_RATE [SUB0]
I RILC    : RIL Daemon version: Samsung-RIL
D RILJ    : [UNSL]< UNSOL_RESPONSE_RADIO_STATE_CHANGED RADIO_OFF [SUB0]
D RILJ    : [3652]> SCREEN_STATE: true [SUB0]
D use-Rlog/RLOG-RIL: 1 RIL request in the queue (1 pending, 0 handled, 0 unhandled)
D use-Rlog/RLOG-RIL: 2 RIL requests in the queue (2 pending, 0 handled, 0 unhandled)
D use-Rlog/RLOG-RIL: 3 RIL requests in the queue (3 pending, 0 handled, 0 unhandled)
D use-Rlog/RLOG-RIL: 4 RIL requests in the queue (4 pending, 0 handled, 0 unhandled)
D use-Rlog/RLOG-RIL: Unhandled RIL request: 124
D use-Rlog/RLOG-RIL: 3 RIL requests in the queue (3 pending, 0 handled, 0 unhandled)
D use-Rlog/RLOG-RIL: Requesting low power mode power state
D use-Rlog/RLOG-RIL-IPC: 
D use-Rlog/RLOG-RIL-IPC: xmm626_sec_modem_fmt_send: Sent FMT message
D use-Rlog/RLOG-RIL-IPC: xmm626_sec_modem_fmt_send: Message: mseq=0x01, command=IPC_PWR_PHONE_STATE, type=IPC_TYPE_EXEC, size=2
D use-Rlog/RLOG-RIL-IPC: ================================= IPC FMT data =================================
D use-Rlog/RLOG-RIL-IPC: [0000]   01 00                                              ..
D use-Rlog/RLOG-RIL-IPC: ================================================================================
D use-Rlog/RLOG-RIL: Unhandled RIL request: 77
D use-Rlog/RLOG-RIL: 2 RIL requests in the queue (1 pending, 1 handled, 0 unhandled)
D use-Rlog/RLOG-RIL: Unhandled RIL request: 110
D use-Rlog/RLOG-RIL: 1 RIL request in the queue (0 pending, 1 handled, 0 unhandled)
D use-Rlog/RLOG-RIL: 2 RIL requests in the queue (1 pending, 1 handled, 0 unhandled)
D RilRequest: [3648]< GET_HARDWARE_CONFIG error: com.android.internal.telephony.CommandException: REQUEST_NOT_SUPPORTED ret=
D RilRequest: [3650]< RIL_REQUEST_CDMA_SET_SUBSCRIPTION_SOURCE error: com.android.internal.telephony.CommandException: REQUEST_NOT_SUPPORTED ret=
D RilRequest: [3651]< RIL_REQUEST_SET_CELL_INFO_LIST_RATE error: com.android.internal.telephony.CommandException: REQUEST_NOT_SUPPORTED ret=
D UiccController: Creating UiccController
D TelephonyTester: register for intent action=com.android.internal.telephony.gsm.action_detached
D TelephonyTester: register for intent action=com.android.internal.telephony.gsm.action_attached
D PhoneBase: mDoesRilSendMultipleCallRing=false
D PhoneBase: mCallRingDelay=3000
D RILJ    : [3653]> RIL_REQUEST_START_LCE [SUB0]
D PhoneBase: mOosIsDisconnect=true
D RILJ    : setPhoneType=1 old value=0 [SUB0]
D use-Rlog/RLOG-RIL: 3 RIL requests in the queue (1 pending, 1 handled, 1 unhandled)
D use-Rlog/RLOG-RIL: Unhandled RIL request: 132
D use-Rlog/RLOG-RIL: 2 RIL requests in the queue (0 pending, 1 handled, 1 unhandled)
D RilRequest: [3653]< RIL_REQUEST_START_LCE error: com.android.internal.telephony.CommandException: REQUEST_NOT_SUPPORTED ret=
D TelephonyRegistry: listen oscl: hasNotifySubscriptionInfoChangedOccurred==false no callback
D TelephonyManager: setTelephonyProperty: success phoneId=0 property=gsm.network.type value: Unknown propVal=Unknown
D RILJ    : [3654]> SIGNAL_STRENGTH [SUB0]
D use-Rlog/RLOG-RIL: 3 RIL requests in the queue (1 pending, 1 handled, 1 unhandled)
D         : [0]DCT.constructor
D SubscriptionController: [getSubId]- sSlotIdxToSubId.size == 0, return DummySubIds slotIdx=0
D         : [0]getDataEnabled: getIntWithSubId retVal=false
D TelephonyRegistry: listen oscl: hasNotifySubscriptionInfoChangedOccurred==false no callback
D Dcc     : E ctor
D Dcc     : X ctor
D SubscriptionController: [getPhoneId] asked for default subId=-1
D SubscriptionController: [getPhoneId]- invalid subId return=-1
D DcTesterDeacativeAll: register for intent action=com.android.internal.telephony.dataconnection.action_deactivate_all
D DcTesterDeacativeAll: register for intent action=com.android.internal.telephony.gsm.action_detached
D Dcc     : DccDefaultState: msg.what=EVENT_RIL_CONNECTED mRilVersion=11
D DcTesterFailBrinupAll: register for intent action=com.android.internal.telephony.dataconnection.action_fail_bringup
D DcTesterFailBrinupAll: register for intent action=com.android.internal.telephony.gsm.action_detached
D DcTesterFailBrinupAll: register for intent action=com.android.internal.telephony.gsm.action_attached
D DCT     : [0]GsmDCT.constructor
D GsmSST  : [GsmSST] notifyDataRegStateRilRadioTechnologyChanged: drs=1 rat=0
D TelephonyManager: setTelephonyProperty: success phoneId=0 property=gsm.network.type value: Unknown propVal=Unknown
D SubscriptionController: [getSubId]- sSlotIdxToSubId.size == 0, return DummySubIds slotIdx=0
D DCT     : [0]update sub = -2
D DCT     : [0]update(): Active DDS, register for all events now!
D DCT     : [0]onUpdateIcc: newIccRecords null
D DCT     : [0]getDataEnabled: getIntWithSubId retVal=false
D SubscriptionController: [getSubId]- sSlotIdxToSubId.size == 0, return DummySubIds slotIdx=0
D GSMPhone: [GSMPhone] updateCurrentCarrierInProvider: mSubId = -2 currentDds = -1 operatorNumeric = null
D DCT     : [0]initApnContexts: E
D DCT     : [0]initApnContexts: skipping unknown type=1
D DCT     : [0]initApnContexts: apnContext={mApnType=default mState=IDLE mWaitingApns={null} mWaitingApnsPermanentFailureCountDown=0 mApnSetting={null} mReason=dataEnabled mDataEnabled=false mDependencyMet=true}
D DCT     : [0]initApnContexts: apnContext={mApnType=mms mState=IDLE mWaitingApns={null} mWaitingApnsPermanentFailureCountDown=0 mApnSetting={null} mReason=dataEnabled mDataEnabled=false mDependencyMet=true}
D DCT     : [0]initApnContexts: apnContext={mApnType=supl mState=IDLE mWaitingApns={null} mWaitingApnsPermanentFailureCountDown=0 mApnSetting={null} mReason=dataEnabled mDataEnabled=false mDependencyMet=true}
D DCT     : [0]initApnContexts: apnContext={mApnType=dun mState=IDLE mWaitingApns={null} mWaitingApnsPermanentFailureCountDown=0 mApnSetting={null} mReason=dataEnabled mDataEnabled=false mDependencyMet=true}
D DCT     : [0]initApnContexts: apnContext={mApnType=hipri mState=IDLE mWaitingApns={null} mWaitingApnsPermanentFailureCountDown=0 mApnSetting={null} mReason=dataEnabled mDataEnabled=false mDependencyMet=true}
D DCT     : [0]initApnContexts: skipping unknown type=7
D DCT     : [0]initApnContexts: skipping unknown type=13
D DCT     : [0]initApnContexts: X mApnContexts={default={mApnType=default mState=IDLE mWaitingApns={null} mWaitingApnsPermanentFailureCountDown=0 mApnSetting={null} mReason=dataEnabled mDataEnabled=false mDependencyMet=true}, mms={mApnType=mms mState=IDLE mWaitingApns={null} mWaitingApnsPermanentFailureCountDown=0 mApnSetting={null} mReason=dataEnabled mDataEnabled=false mDependencyMet=true}, supl={mApnType=supl mState=IDLE mWaitingApns={null} mWaitingApnsPermanentFailureCountDown=0 mApnSetting={null} mReason=dataEnabled mDataEnabled=false mDependencyMet=true}, dun={mApnType=dun mState=IDLE mWaitingApns={null} mWaitingApnsPermanentFailureCountDown=0 mApnSetting={null} mReason=dataEnabled mDataEnabled=false mDependencyMet=true}, hipri={mApnType=hipri mState=IDLE mWaitingApns={null} mWaitingApnsPermanentFailureCountDown=0 mApnSetting={null} mReason=dataEnabled mDataEnabled=false mDependencyMet=true}}
D TelephonyManager: setTelephonyProperty: success phoneId=0 property=gsm.current.phone-type value: 1 propVal=1
D GSMPhone: [GSMPhone] GSMPhone: constructor: sub = 0
D TelephonyManager: setTelephonyProperty: success phoneId=0 property=gsm.current.phone-type value: 1 propVal=1
D SubscriptionController: [getSubId]- sSlotIdxToSubId.size == 0, return DummySubIds slotIdx=0
I PhoneFactory: Creating Phone with type = 1 sub = 0
E RIL_ImsSms: getFormat should never be called from here!
D SMSDispatcher: SMSDispatcher: ctor mSmsCapable=true format=unknown mSmsSendDisabled=false
D RIL_ImsSms: ImsSMSDispatcher created
D SMSDispatcher: SMSDispatcher: ctor mSmsCapable=true format=3gpp2 mSmsSendDisabled=false
D CdmaSMSDispatcher: CdmaSMSDispatcher created
D GsmInboundSmsHandler: created InboundSmsHandler
D CdmaInboundSmsHandler: created InboundSmsHandler
D SMSDispatcher: SMSDispatcher: ctor mSmsCapable=true format=3gpp mSmsSendDisabled=false
D GsmSMSDispatcher: GsmSMSDispatcher created
D SmsBroadcastUndelivered: scanning raw table for undelivered messages
D IccCardProxy: ctor: ci=com.android.internal.telephony.RIL@9e3084c phoneId=0
D CdmaSSM : subscriptionSource from settings: 0
D CdmaSSM : cdmaSSM constructor: 0
D IccCardProxy: update icc_operator_numeric=
D TelephonyManager: setTelephonyProperty: success phoneId=0 property=gsm.sim.operator.numeric value:  propVal=
D TelephonyManager: setTelephonyProperty: success phoneId=0 property=gsm.sim.operator.iso-country value:  propVal=
D TelephonyManager: setTelephonyProperty: success phoneId=0 property=gsm.sim.operator.alpha value:  propVal=
E IccCardProxy: setExternalState: set mPhoneId=0 mExternalState=NOT_READY
D TelephonyManager: setTelephonyProperty: success phoneId=0 property=gsm.sim.state value: NOT_READY propVal=NOT_READY
D SubscriptionController: [getSubId]- sSlotIdxToSubId.size == 0, return DummySubIds slotIdx=0
D IccCardProxy: broadcastIccStateChangedIntent intent ACTION_SIM_STATE_CHANGED value=NOT_READY reason=null for mPhoneId=0
D IccCardProxy: Setting radio tech UMTS
D IccCardProxy: updateQuietMode: 3GPP subscription -> newQuietMode=false
D IccCardProxy: updateQuietMode: no changes don't setExternalState
D IccCardProxy: updateQuietMode: QuietMode is false (app_type=1 cdmaSource=-1)
D ProxyController: Constructor - Enter
D DctController: makeDctController: new DctController phones.length=1
D SubscriptionController: [getActiveSubInfoList]+
D SubscriptionController: [getActiveSubInfoList] Sub Controller not ready
D DctController: DctController(): phones.length=1
D DcSwitchSM: [DcSwitchStateMachine-0] DcSwitchState constructor E
D DcSwitchSM: [DcSwitchStateMachine-0] DcSwitchState constructor X
D DcSwitchSM: [DcSwitchStateMachine-0] IdleState: enter
D DctController: DctController(phones): Connect success: 0
D DctController: updatePhoneBaseForIndex for phone index=0
D DctController: unregister TelephonyNetworkFactory for phone index=0
D SubscriptionController: [getSubId]- sSlotIdxToSubId.size == 0, return DummySubIds slotIdx=0
D DctController: [TNF -2]NetworkCapabilities: [ Transports: CELLULAR Capabilities: MMS&SUPL&DUN&FOTA&IMS&CBS&IA&RCS&XCAP&EIMS&INTERNET&NOT_RESTRICTED&TRUSTED&NOT_VPN]
D TelephonyRegistry: listen oscl: hasNotifySubscriptionInfoChangedOccurred==false no callback
D DctController: makeDctController: X sDctController=Handler (com.android.internal.telephony.dataconnection.DctController) {6d39b50}
D ProxyController: clearTransaction
D ProxyController: clearTransaction: phoneId=0 status=IDLE
D ProxyController: Constructor - Exit
I PhoneFactory: defaultSmsApplication: com.android.messaging
I PhoneFactory: Creating SubInfoRecordUpdater 
D SubscriptionInfoUpdater: Constructor invoked
D SubscriptionController: [getSubId]- sSlotIdxToSubId.size == 0, return DummySubIds slotIdx=0
D SubscriptionController: [getActiveSubInfoList]+
D SubscriptionController: selection:sim_id>=0 null
D SubscriptionController: [getActiveSubInfoList]- no info return
D SubscriptionController: [getActiveSubInfoForSubscriber]- subId=-2 subList=null subInfo=null
E SubscriptionController: getUserNwMode: invalid subId = -2
D SubscriptionController: getSimStateForSlotIdx:  simState=NOT_READY ordinal=6
D SubscriptionManager: getSimStateForSubscriber: simState=6 slotIdx=0
D SubscriptionController: getSimStateForSlotIdx:  simState=NOT_READY ordinal=6
D SubscriptionManager: getSimStateForSubscriber: simState=6 slotIdx=0
D CallManager: registerPhone(GSM Handler (com.android.internal.telephony.PhoneProxy) {3ba5b8b})
D RILJ    : [3655]> SET_SUPP_SVC_NOTIFICATION [SUB0]
D use-Rlog/RLOG-RIL: 4 RIL requests in the queue (1 pending, 1 handled, 2 unhandled)
D use-Rlog/RLOG-RIL: Unhandled RIL request: 62
D use-Rlog/RLOG-RIL: 3 RIL requests in the queue (0 pending, 1 handled, 2 unhandled)
D RilRequest: [3655]< SET_SUPP_SVC_NOTIFICATION error: com.android.internal.telephony.CommandException: REQUEST_NOT_SUPPORTED ret=
D TelephonyRegistry: listen oscl: hasNotifySubscriptionInfoChangedOccurred==false no callback
D RILJ    : [3656]> RIL_REQUEST_SET_TTY_MODE : 0 [SUB0]
D use-Rlog/RLOG-RIL: 4 RIL requests in the queue (1 pending, 1 handled, 2 unhandled)
D use-Rlog/RLOG-RIL: Unhandled RIL request: 80
D use-Rlog/RLOG-RIL: 3 RIL requests in the queue (0 pending, 1 handled, 2 unhandled)
D RilRequest: [3656]< RIL_REQUEST_SET_TTY_MODE error: com.android.internal.telephony.CommandException: REQUEST_NOT_SUPPORTED ret=
D TelephonyRegistry: listen oscl: hasNotifySubscriptionInfoChangedOccurred==false no callback
D SubscriptionController: [getPhoneId] asked for default subId=-1
D SubscriptionController: [getPhoneId]- invalid subId return=-1
D SubscriptionController: [getPhoneId] asked for default subId=-1
D SubscriptionController: [getPhoneId]- invalid subId return=-1
D PhoneBase: config LCE service failed: com.android.internal.telephony.CommandException: REQUEST_NOT_SUPPORTED
D GsmSST  : [GsmSST] mDeviceShuttingDown = false
D GsmSST  : [GsmSST] mDesiredPowerState = true
D GsmSST  : [GsmSST] getRadioState = RADIO_OFF
D GsmSST  : [GsmSST] mPowerOffDelayNeed = true
D GsmSST  : [GsmSST] mAlarmSwitch = false
D RILJ    : [3657]> RADIO_POWER on [SUB0]
D use-Rlog/RLOG-RIL: 4 RIL requests in the queue (1 pending, 1 handled, 2 unhandled)
D PHONE   : [ServiceState] setNullState=3
D GsmSST  : [GsmSST] set service state as POWER_OFF
D PHONE   : [ServiceState] setNullState=3
D GsmSST  : [GsmSST] Poll ServiceState done:  oldSS=[1 1 voice home data home null null null null null null  Unknown Unknown CSS not supported 0 0 RoamInd=0 DefRoamInd=0 EmergOnly=false IsDataRoamingFromRegistration=false] newSS=[3 3 voice home data home null null null null null null  Unknown Unknown CSS not supported -1 -1 RoamInd=-1 DefRoamInd=-1 EmergOnly=false IsDataRoamingFromRegistration=false] oldMaxDataCalls=1 mNewMaxDataCalls=1 oldReasonDataDenied=-1 mNewReasonDataDenied=-1
D PHONE   : [ServiceState] setNullState=1
D GsmSST  : [GsmSST] updateSpnDisplay: radio is off w/ showPlmn=true plmn=No service.
D SubscriptionController: [getSubId]- sSlotIdxToSubId.size == 0, return DummySubIds slotIdx=0
D GsmSST  : [GsmSST] updateSpnDisplay: changed sending intent rule=0 showPlmn='true' plmn='No service.' showSpn='false' spn='null' dataSpn='' subId='-2'
D SubscriptionController: [getSubId]- sSlotIdxToSubId.size == 0, return DummySubIds slotIdx=0
D SubscriptionController: [getSubId]- sSlotIdxToSubId.size == 0, return DummySubIds slotIdx=0
D SubscriptionController: [setPlmnSpn] No valid subscription to store info
D SubscriptionController: notifySubscriptionInfoChanged:
D TelephonyRegistry: notifySubscriptionInfoChanged: first invocation mRecords.size=14
D SubscriptionController: [getActiveSubInfoList]+
D SubscriptionController: [getActiveSubInfoList]+
D SubscriptionController: selection:sim_id>=0 null
D TelephonyManager: setTelephonyProperty: success phoneId=0 property=gsm.operator.alpha value:  propVal=
D TelephonyManager: setTelephonyProperty: success phoneId=0 property=gsm.operator.numeric value:  propVal=
D GsmSST  : [GsmSST] operatorNumeric is null
D SubscriptionController: selection:sim_id>=0 null
D TelephonyManager: setTelephonyProperty: success phoneId=0 property=gsm.operator.iso-country value:  propVal=
D TelephonyManager: setTelephonyProperty: success phoneId=0 property=gsm.operator.isroaming value: false propVal=false
D GsmSST  : [GsmSST] Broadcasting ServiceState : 3 3 voice home data home null null null null null null  Unknown Unknown CSS not supported -1 -1 RoamInd=-1 DefRoamInd=-1 EmergOnly=false IsDataRoamingFromRegistration=false
D SubscriptionController: [getSubId]- sSlotIdxToSubId.size == 0, return DummySubIds slotIdx=0
D DefaultPhoneNotifier: nofityServiceState: mRegistry=com.android.internal.telephony.ITelephonyRegistry$Stub$Proxy@5667eb9 ss=3 3 voice home data home null null null null null null  Unknown Unknown CSS not supported -1 -1 RoamInd=-1 DefRoamInd=-1 EmergOnly=false IsDataRoamingFromRegistration=false sender=Handler (com.android.internal.telephony.gsm.GSMPhone) {6bf8468} phondId=0 subId=-2
D SubscriptionController: [getActiveSubInfoList]- no info return
D SmsBroadcastUndelivered: finished scanning raw table in 227 ms
D CdmaInboundSmsHandler: StartupState.processMessage:6
D CdmaInboundSmsHandler: entering Idle state
D CdmaInboundSmsHandler: IdleState.processMessage:5
D SubscriptionController: [getSubId]- sSlotIdxToSubId.size == 0, return DummySubIds slotIdx=0
D CdmaInboundSmsHandler: Idle state processing message type 5
D GsmInboundSmsHandler: StartupState.processMessage:6
D GsmInboundSmsHandler: entering Idle state
D GsmInboundSmsHandler: IdleState.processMessage:5
D GsmInboundSmsHandler: Idle state processing message type 5
D CdmaInboundSmsHandler: mWakeLock released wakelockcount = 0
D GsmInboundSmsHandler: mWakeLock released wakelockcount = 0
D SubscriptionController: [getSlotId]- subId invalid
D SubscriptionController: getSimStateForSlotIdx:  simState=NOT_READY ordinal=6
D SubscriptionManager: getSimStateForSubscriber: simState=6 slotIdx=0
D TelephonyManager: getSimState: default sim:-1, sim state for slotIdx=0 is 6, return state as unknown
D GsmSST  : [GsmSST] notifyDataRegStateRilRadioTechnologyChanged: drs=3 rat=0
D TelephonyManager: setTelephonyProperty: success phoneId=0 property=gsm.network.type value: Unknown propVal=Unknown
D DCT     : [0]get all active apn types
D RILJ    : [3658]> OPERATOR [SUB0]
D RILJ    : [3659]> DATA_REGISTRATION_STATE [SUB0]
D use-Rlog/RLOG-RIL: 5 RIL requests in the queue (1 pending, 1 handled, 3 unhandled)
D RILJ    : [3660]> VOICE_REGISTRATION_STATE [SUB0]
D use-Rlog/RLOG-RIL: 6 RIL requests in the queue (1 pending, 1 handled, 4 unhandled)
D RILJ    : [3661]> QUERY_NETWORK_SELECTION_MODE [SUB0]
D use-Rlog/RLOG-RIL: 7 RIL requests in the queue (1 pending, 1 handled, 5 unhandled)
D DCT     : [0]handleMessage msg={ when=-356ms what=270369 obj=android.os.AsyncResult@35682fe target=com.android.internal.telephony.dataconnection.DcTracker }
D DCT     : [0]onUpdateIcc: newIccRecords null
D use-Rlog/RLOG-RIL: 8 RIL requests in the queue (1 pending, 1 handled, 6 unhandled)
D DCT     : [0]handleMessage msg={ when=-339ms what=270337 obj=android.os.AsyncResult@6335a5f target=com.android.internal.telephony.dataconnection.DcTracker }
D DCT     : [0]onRadioAvailable
D DCT     : [0]overall state is IDLE
D DCT     : [0]handleMessage msg={ when=-339ms what=270342 obj=android.os.AsyncResult@de09cac target=com.android.internal.telephony.dataconnection.DcTracker }
D DCT     : [0]onRadioOffOrNotAvailable: is off and clean up all connections
D DCT     : [0]cleanUpAllConnections: tearDown=false reason=radioTurnedOff
D DCT     : [0]cleanUpConnection: tearDown=false reason=radioTurnedOff apnContext={mApnType=default mState=IDLE mWaitingApns={null} mWaitingApnsPermanentFailureCountDown=0 mApnSetting={null} mReason=radioTurnedOff mDataEnabled=false mDependencyMet=true}
D GSMPhone: getDataConnectionState: Data is Out of Service. ret = DISCONNECTED
D SubscriptionController: [getSubId]- sSlotIdxToSubId.size == 0, return DummySubIds slotIdx=0
D SubscriptionController: [getActiveSubInfoList]- no info return
D DCT     : [0]isDataAllowed: not allowed due to - Attached= false - SIM not loaded - SIM not loaded and not NV subscription - defaultDataSelected= false
D SubscriptionController: [getPhoneId]- invalid subId return=-1
D DCT     : [0]setupDataForSinglePdn: reason = radioTurnedOff isDisconnected = true
D DCT     : [0]isOnlySingleDcAllowed(0): false
D DCT     : [0]cleanUpConnection: X tearDown=false reason=radioTurnedOff apnContext={mApnType=default mState=IDLE mWaitingApns={null} mWaitingApnsPermanentFailureCountDown=0 mApnSetting={null} mReason=radioTurnedOff mDataEnabled=false mDependencyMet=true} dcac=null
D DCT     : [0]cleanUpConnection: tearDown=false reason=radioTurnedOff apnContext={mApnType=mms mState=IDLE mWaitingApns={null} mWaitingApnsPermanentFailureCountDown=0 mApnSetting={null} mReason=radioTurnedOff mDataEnabled=false mDependencyMet=true}
D SubscriptionController: getSimStateForSlotIdx:  simState=NOT_READY ordinal=6
D GSMPhone: getDataConnectionState: Data is Out of Service. ret = DISCONNECTED
D SubscriptionController: [getSubId]- sSlotIdxToSubId.size == 0, return DummySubIds slotIdx=0
D SubscriptionManager: getSimStateForSubscriber: simState=6 slotIdx=0
D DCT     : [0]isDataAllowed: not allowed due to - Attached= false - SIM not loaded - SIM not loaded and not NV subscription - defaultDataSelected= false
D SubscriptionController: [getPhoneId]- invalid subId return=-1
D DCT     : [0]setupDataForSinglePdn: reason = radioTurnedOff isDisconnected = true
D DCT     : [0]isOnlySingleDcAllowed(0): false
D DCT     : [0]cleanUpConnection: X tearDown=false reason=radioTurnedOff apnContext={mApnType=mms mState=IDLE mWaitingApns={null} mWaitingApnsPermanentFailureCountDown=0 mApnSetting={null} mReason=radioTurnedOff mDataEnabled=false mDependencyMet=true} dcac=null
D DCT     : [0]cleanUpConnection: tearDown=false reason=radioTurnedOff apnContext={mApnType=supl mState=IDLE mWaitingApns={null} mWaitingApnsPermanentFailureCountDown=0 mApnSetting={null} mReason=radioTurnedOff mDataEnabled=false mDependencyMet=true}
D GSMPhone: getDataConnectionState: Data is Out of Service. ret = DISCONNECTED
D SubscriptionController: [getSubId]- sSlotIdxToSubId.size == 0, return DummySubIds slotIdx=0
D SubscriptionController: getSimStateForSlotIdx:  simState=NOT_READY ordinal=6
D SubscriptionManager: getSimStateForSubscriber: simState=6 slotIdx=0
D DCT     : [0]isDataAllowed: not allowed due to - Attached= false - SIM not loaded - SIM not loaded and not NV subscription - defaultDataSelected= false
D SubscriptionController: [getPhoneId]- invalid subId return=-1
D DCT     : [0]setupDataForSinglePdn: reason = radioTurnedOff isDisconnected = true
D DCT     : [0]isOnlySingleDcAllowed(0): false
D DCT     : [0]cleanUpConnection: X tearDown=false reason=radioTurnedOff apnContext={mApnType=supl mState=IDLE mWaitingApns={null} mWaitingApnsPermanentFailureCountDown=0 mApnSetting={null} mReason=radioTurnedOff mDataEnabled=false mDependencyMet=true} dcac=null
D DCT     : [0]cleanUpConnection: tearDown=false reason=radioTurnedOff apnContext={mApnType=dun mState=IDLE mWaitingApns={null} mWaitingApnsPermanentFailureCountDown=0 mApnSetting={null} mReason=radioTurnedOff mDataEnabled=false mDependencyMet=true}
D GSMPhone: getDataConnectionState: Data is Out of Service. ret = DISCONNECTED
D SubscriptionController: [getSubId]- sSlotIdxToSubId.size == 0, return DummySubIds slotIdx=0
D DCT     : [0]isDataAllowed: not allowed due to - Attached= false - SIM not loaded - SIM not loaded and not NV subscription - defaultDataSelected= false
D SubscriptionController: [getPhoneId]- invalid subId return=-1
D DCT     : [0]setupDataForSinglePdn: reason = radioTurnedOff isDisconnected = true
D DCT     : [0]isOnlySingleDcAllowed(0): false
D DCT     : [0]cleanUpConnection: X tearDown=false reason=radioTurnedOff apnContext={mApnType=dun mState=IDLE mWaitingApns={null} mWaitingApnsPermanentFailureCountDown=0 mApnSetting={null} mReason=radioTurnedOff mDataEnabled=false mDependencyMet=true} dcac=null
D DCT     : [0]cleanUpConnection: tearDown=false reason=radioTurnedOff apnContext={mApnType=hipri mState=IDLE mWaitingApns={null} mWaitingApnsPermanentFailureCountDown=0 mApnSetting={null} mReason=radioTurnedOff mDataEnabled=false mDependencyMet=true}
D GSMPhone: getDataConnectionState: Data is Out of Service. ret = DISCONNECTED
D SubscriptionController: [getSubId]- sSlotIdxToSubId.size == 0, return DummySubIds slotIdx=0
D SubscriptionController: getSimStateForSlotIdx:  simState=NOT_READY ordinal=6
D SubscriptionManager: getSimStateForSubscriber: simState=6 slotIdx=0
D DCT     : [0]isDataAllowed: not allowed due to - Attached= false - SIM not loaded - SIM not loaded and not NV subscription - defaultDataSelected= false
D SubscriptionController: getSimStateForSlotIdx:  simState=NOT_READY ordinal=6
D SubscriptionManager: getSimStateForSubscriber: simState=6 slotIdx=0
D SubscriptionController: [getPhoneId]- invalid subId return=-1
D DCT     : [0]setupDataForSinglePdn: reason = radioTurnedOff isDisconnected = true
D DCT     : [0]isOnlySingleDcAllowed(0): false
D DCT     : [0]cleanUpConnection: X tearDown=false reason=radioTurnedOff apnContext={mApnType=hipri mState=IDLE mWaitingApns={null} mWaitingApnsPermanentFailureCountDown=0 mApnSetting={null} mReason=radioTurnedOff mDataEnabled=false mDependencyMet=true} dcac=null
D DCT     : [0]stopNetStatPoll
D SubscriptionController: [getSubId]- sSlotIdxToSubId.size == 0, return DummySubIds slotIdx=0
D DCT     : [0]cleanUpConnection: mDisconnectPendingCount = 0
D SubscriptionController: [getSubId]- sSlotIdxToSubId.size == 0, return DummySubIds slotIdx=0
D SubscriptionController: getSimStateForSlotIdx:  simState=NOT_READY ordinal=6
D SubscriptionManager: getSimStateForSubscriber: simState=6 slotIdx=0
D DCT     : [0]isDataAllowed: not allowed due to - Attached= false - SIM not loaded - SIM not loaded and not NV subscription - defaultDataSelected= false
D SubscriptionController: [getPhoneId]- invalid subId return=-1
D SubscriptionController: [getSubId]- sSlotIdxToSubId.size == 0, return DummySubIds slotIdx=0
D SubscriptionController: getSimStateForSlotIdx:  simState=NOT_READY ordinal=6
D SubscriptionManager: getSimStateForSubscriber: simState=6 slotIdx=0
D DCT     : [0]isDataAllowed: not allowed due to - Attached= false - SIM not loaded - SIM not loaded and not NV subscription - defaultDataSelected= false
D SubscriptionController: [getPhoneId]- invalid subId return=-1
D SubscriptionController: [getSubId]- sSlotIdxToSubId.size == 0, return DummySubIds slotIdx=0
D SubscriptionController: getSimStateForSlotIdx:  simState=NOT_READY ordinal=6
D SubscriptionManager: getSimStateForSubscriber: simState=6 slotIdx=0
D DCT     : [0]isDataAllowed: not allowed due to - Attached= false - SIM not loaded - SIM not loaded and not NV subscription - defaultDataSelected= false
D SubscriptionController: [getPhoneId]- invalid subId return=-1
D SubscriptionController: [getSubId]- sSlotIdxToSubId.size == 0, return DummySubIds slotIdx=0
D DCT     : [0]isDataAllowed: not allowed due to - Attached= false - SIM not loaded - SIM not loaded and not NV subscription - defaultDataSelected= false
D SubscriptionController: getSimStateForSlotIdx:  simState=NOT_READY ordinal=6
D SubscriptionManager: getSimStateForSubscriber: simState=6 slotIdx=0
D SubscriptionController: [getPhoneId]- invalid subId return=-1
D SubscriptionController: [getSubId]- sSlotIdxToSubId.size == 0, return DummySubIds slotIdx=0
D SubscriptionController: getSimStateForSlotIdx:  simState=NOT_READY ordinal=6
D SubscriptionManager: getSimStateForSubscriber: simState=6 slotIdx=0
D DCT     : [0]isDataAllowed: not allowed due to - Attached= false - SIM not loaded - SIM not loaded and not NV subscription - defaultDataSelected= false
D SubscriptionController: [getPhoneId]- invalid subId return=-1
D DCT     : [0]handleMessage msg={ when=-381ms what=270345 obj=android.os.AsyncResult@1674d75 target=com.android.internal.telephony.dataconnection.DcTracker }
D DCT     : [0]onDataConnectionDetached: stop polling and notify detached
D DCT     : [0]stopNetStatPoll
D SubscriptionController: [getSubId]- sSlotIdxToSubId.size == 0, return DummySubIds slotIdx=0
D SubscriptionController: getSimStateForSlotIdx:  simState=NOT_READY ordinal=6
D SubscriptionManager: getSimStateForSubscriber: simState=6 slotIdx=0
D DCT     : [0]notifyDataConnection: reason=dataDetached
D SubscriptionController: [getSubId]- sSlotIdxToSubId.size == 0, return DummySubIds slotIdx=0
D DCT     : [0]isDataAllowed: not allowed due to - Attached= false - SIM not loaded - SIM not loaded and not NV subscription - defaultDataSelected= false
D SubscriptionController: [getPhoneId]- invalid subId return=-1
D SubscriptionController: [getSubId]- sSlotIdxToSubId.size == 0, return DummySubIds slotIdx=0
D DCT     : [0]isDataAllowed: not allowed due to - Attached= false - SIM not loaded - SIM not loaded and not NV subscription - defaultDataSelected= false
D SubscriptionController: getSimStateForSlotIdx:  simState=NOT_READY ordinal=6
D SubscriptionController: [getPhoneId]- invalid subId return=-1
D SubscriptionManager: getSimStateForSubscriber: simState=6 slotIdx=0
D SubscriptionController: [getSubId]- sSlotIdxToSubId.size == 0, return DummySubIds slotIdx=0
D DCT     : [0]isDataAllowed: not allowed due to - Attached= false - SIM not loaded - SIM not loaded and not NV subscription - defaultDataSelected= false
D SubscriptionController: getSimStateForSlotIdx:  simState=NOT_READY ordinal=6
D SubscriptionManager: getSimStateForSubscriber: simState=6 slotIdx=0
D SubscriptionController: [getPhoneId]- invalid subId return=-1
D SubscriptionController: [getSubId]- sSlotIdxToSubId.size == 0, return DummySubIds slotIdx=0
D SubscriptionController: getSimStateForSlotIdx:  simState=NOT_READY ordinal=6
D SubscriptionManager: getSimStateForSubscriber: simState=6 slotIdx=0
D DCT     : [0]isDataAllowed: not allowed due to - Attached= false - SIM not loaded - SIM not loaded and not NV subscription - defaultDataSelected= false
D SubscriptionController: [getPhoneId]- invalid subId return=-1
D SubscriptionController: [getSubId]- sSlotIdxToSubId.size == 0, return DummySubIds slotIdx=0
D SubscriptionController: getSimStateForSlotIdx:  simState=NOT_READY ordinal=6
D SubscriptionManager: getSimStateForSubscriber: simState=6 slotIdx=0
D DCT     : [0]isDataAllowed: not allowed due to - Attached= false - SIM not loaded - SIM not loaded and not NV subscription - defaultDataSelected= false
D SubscriptionController: [getPhoneId]- invalid subId return=-1
D DCT     : [0]handleMessage msg={ when=-398ms what=270348 obj=android.os.AsyncResult@13d10a target=com.android.internal.telephony.dataconnection.DcTracker }
D DCT     : [0]onRoamingOff
D DCT     : [0]handleMessage msg={ when=-397ms what=270377 obj=android.os.AsyncResult@9dd3d7b target=com.android.internal.telephony.dataconnection.DcTracker }
D DCT     : [0]onUpdateIcc: newIccRecords null
D SubscriptionController: getSimStateForSlotIdx:  simState=NOT_READY ordinal=6
D SubscriptionManager: getSimStateForSubscriber: simState=6 slotIdx=0
D DCT     : [0]setupDataOnConnectableApns: nwTypeChanged
D DCT     : [0]setupDataOnConnectableApns: apnContext {mApnType=dun mState=IDLE mWaitingApns={null} mWaitingApnsPermanentFailureCountDown=0 mApnSetting={null} mReason=radioTurnedOff mDataEnabled=false mDependencyMet=true}
D DCT     : [0]setupDataOnConnectableApns: apnContext {mApnType=hipri mState=IDLE mWaitingApns={null} mWaitingApnsPermanentFailureCountDown=0 mApnSetting={null} mReason=radioTurnedOff mDataEnabled=false mDependencyMet=true}
D DCT     : [0]setupDataOnConnectableApns: apnContext {mApnType=supl mState=IDLE mWaitingApns={null} mWaitingApnsPermanentFailureCountDown=0 mApnSetting={null} mReason=radioTurnedOff mDataEnabled=false mDependencyMet=true}
D DCT     : [0]setupDataOnConnectableApns: apnContext {mApnType=default mState=IDLE mWaitingApns={null} mWaitingApnsPermanentFailureCountDown=0 mApnSetting={null} mReason=radioTurnedOff mDataEnabled=false mDependencyMet=true}
D DCT     : [0]setupDataOnConnectableApns: apnContext {mApnType=mms mState=IDLE mWaitingApns={null} mWaitingApnsPermanentFailureCountDown=0 mApnSetting={null} mReason=radioTurnedOff mDataEnabled=false mDependencyMet=true}
D RILJ    : [3662]> BASEBAND_VERSION [SUB0]
D use-Rlog/RLOG-RIL: 9 RIL requests in the queue (1 pending, 1 handled, 7 unhandled)
D RILJ    : [3663]> GET_IMEI [SUB0]
D use-Rlog/RLOG-RIL: 10 RIL requests in the queue (1 pending, 1 handled, 8 unhandled)
D RILJ    : [3664]> GET_IMEISV [SUB0]
D use-Rlog/RLOG-RIL: 11 RIL requests in the queue (1 pending, 1 handled, 9 unhandled)
D RILJ    : [3665]> RIL_REQUEST_GET_RADIO_CAPABILITY [SUB0]
D use-Rlog/RLOG-RIL: 12 RIL requests in the queue (1 pending, 1 handled, 10 unhandled)
D use-Rlog/RLOG-RIL: Unhandled RIL request: 130
D use-Rlog/RLOG-RIL: 11 RIL requests in the queue (0 pending, 1 handled, 10 unhandled)
D RILJ    : Faking RIL_REQUEST_GET_RADIO_CAPABILITY response using 36366 [SUB0]
D RILJ    : [3665]< RIL_REQUEST_GET_RADIO_CAPABILITY {mPhoneId = 0 mVersion=1 mSession=0 mPhase=0 mRadioAccessFamily=36366 mLogicModemId= mStatus=1} [SUB0]
D RILJ    : [3666]> RIL_REQUEST_START_LCE [SUB0]
D use-Rlog/RLOG-RIL: 12 RIL requests in the queue (1 pending, 1 handled, 10 unhandled)
D use-Rlog/RLOG-RIL: Unhandled RIL request: 132
D use-Rlog/RLOG-RIL: 11 RIL requests in the queue (0 pending, 1 handled, 10 unhandled)
D RilRequest: [3666]< RIL_REQUEST_START_LCE error: com.android.internal.telephony.CommandException: REQUEST_NOT_SUPPORTED ret=
D RILJ    : [3667]> RIL_REQUEST_VOICE_RADIO_TECH [SUB0]
D RILC    : decodeVoiceRadioTechnology: Invoked with incorrect RadioState
E RILC    : RIL_onRequestComplete: invalid RIL_Token
D RilRequest: [3667]< RIL_REQUEST_VOICE_RADIO_TECH error: com.android.internal.telephony.CommandException: RADIO_NOT_AVAILABLE ret=
D SubscriptionController: [getSubId]- sSlotIdxToSubId.size == 0, return DummySubIds slotIdx=0
D GsmSMSDispatcher: GsmSMSDispatcher: subId = -2 slotId = 0
E IccCardProxy: setExternalState: !override and newstate unchanged from NOT_READY
E IccCardProxy: setExternalState: !override and newstate unchanged from NOT_READY
D DctController: EVENT_PHONE1_DATA_DETACH.
D DcSwitchSM: [DcSwitchStateMachine-0] DefaultState: shouldn't happen but ignore msg.what=0x44008
D SubscriptionController: [getSubId]- sSlotIdxToSubId.size == 0, return DummySubIds slotIdx=0
D DctController: [TNF -2]got request NetworkRequest [ id=1, legacyType=-1, [ Capabilities: INTERNET&NOT_RESTRICTED&TRUSTED&NOT_VPN] ] with score 0
D SubscriptionController: [getSubId]- sSlotIdxToSubId.size == 0, return DummySubIds slotIdx=0
D DctController: [TNF -2]Cellular needs Network for NetworkRequest [ id=1, legacyType=-1, [ Capabilities: INTERNET&NOT_RESTRICTED&TRUSTED&NOT_VPN] ]
D SubscriptionController: [getSubId]- sSlotIdxToSubId.size == 0, return DummySubIds slotIdx=0
D SubscriptionController: [getSubId]- sSlotIdxToSubId.size == 0, return DummySubIds slotIdx=0
D DctController: [TNF -2]Request not useable, pending request.
D SubscriptionInfoUpdater: [Receiver]+
D SubscriptionInfoUpdater: Action: android.intent.action.SIM_STATE_CHANGED
D SubscriptionInfoUpdater: slotId: 0
D SubscriptionInfoUpdater: simStatus: NOT_READY
D SubscriptionInfoUpdater: Ignoring simStatus: NOT_READY
D SubscriptionInfoUpdater: Wait for SIM1 IccId
D SubscriptionInfoUpdater: [Receiver]-
D DebugService: DebugService DebugService:
D SipService: SipService: started!
D SipService: start:
D RILJ    : [3668]> RIL_REQUEST_QUERY_TTY_MODE [SUB0]
D use-Rlog/RLOG-RIL: 12 RIL requests in the queue (1 pending, 1 handled, 10 unhandled)
D use-Rlog/RLOG-RIL: Unhandled RIL request: 81
D use-Rlog/RLOG-RIL: 11 RIL requests in the queue (0 pending, 1 handled, 10 unhandled)
D RilRequest: [3668]< RIL_REQUEST_QUERY_TTY_MODE error: com.android.internal.telephony.CommandException: REQUEST_NOT_SUPPORTED ret=
D GsmSST  : [GsmSST] SubscriptionListener.onSubscriptionInfoChanged
D SubscriptionController: [getSubId]- sSlotIdxToSubId.size == 0, return DummySubIds slotIdx=0
D DCT     : [0]SubscriptionListener.onSubscriptionInfoChanged
D SubscriptionController: [getSubId]- sSlotIdxToSubId.size == 0, return DummySubIds slotIdx=0
D SubscriptionController: [getActiveSubInfoList]+
D SubscriptionController: selection:sim_id>=0 null
D SubscriptionController: [getPhoneId] asked for default subId=-1
D SubscriptionController: [getPhoneId]- invalid subId return=-1
D SubscriptionController: [getActiveSubInfoList]- no info return
D SubscriptionController: [getSubId]- sSlotIdxToSubId.size == 0, return DummySubIds slotIdx=0
D SubscriptionController: [getSubId]- sSlotIdxToSubId.size == 0, return DummySubIds slotIdx=0
D SubscriptionController: [getPhoneId]- invalid subId return=-1
D SubscriptionController: [getSubId]- sSlotIdxToSubId.size == 0, return DummySubIds slotIdx=0
D SubscriptionController: [getSubId]- sSlotIdxToSubId.size == 0, return DummySubIds slotIdx=0
D SubscriptionController: [getSubId]- sSlotIdxToSubId.size == 0, return DummySubIds slotIdx=0
E PhoneBase: Error! registerForCallWaiting() in PhoneBase should not be called, CDMAPhone inactive.
D SubscriptionController: [getSubId]- sSlotIdxToSubId.size == 0, return DummySubIds slotIdx=0
D DCT     : [0]handleMessage msg={ when=-203ms what=270377 obj=android.os.AsyncResult@c31eb2f target=com.android.internal.telephony.dataconnection.DcTracker }
D DCT     : [0]onUpdateIcc: newIccRecords null
D DCT     : [0]setupDataOnConnectableApns: nwTypeChanged
D DCT     : [0]setupDataOnConnectableApns: apnContext {mApnType=dun mState=IDLE mWaitingApns={null} mWaitingApnsPermanentFailureCountDown=0 mApnSetting={null} mReason=radioTurnedOff mDataEnabled=false mDependencyMet=true}
D DCT     : [0]setupDataOnConnectableApns: apnContext {mApnType=hipri mState=IDLE mWaitingApns={null} mWaitingApnsPermanentFailureCountDown=0 mApnSetting={null} mReason=radioTurnedOff mDataEnabled=false mDependencyMet=true}
D DCT     : [0]setupDataOnConnectableApns: apnContext {mApnType=supl mState=IDLE mWaitingApns={null} mWaitingApnsPermanentFailureCountDown=0 mApnSetting={null} mReason=radioTurnedOff mDataEnabled=false mDependencyMet=true}
D DCT     : [0]setupDataOnConnectableApns: apnContext {mApnType=default mState=IDLE mWaitingApns={null} mWaitingApnsPermanentFailureCountDown=0 mApnSetting={null} mReason=radioTurnedOff mDataEnabled=false mDependencyMet=true}
D DCT     : [0]setupDataOnConnectableApns: apnContext {mApnType=mms mState=IDLE mWaitingApns={null} mWaitingApnsPermanentFailureCountDown=0 mApnSetting={null} mReason=radioTurnedOff mDataEnabled=false mDependencyMet=true}
D SubscriptionController: [getSubId]- sSlotIdxToSubId.size == 0, return DummySubIds slotIdx=0
D DCT     : [0]getDataOnRoamingEnabled: phoneSubId=-2 isDataRoamingEnabled=false
D SubscriptionController: [getSubId]- sSlotIdxToSubId.size == 0, return DummySubIds slotIdx=0
D DCT     : [0]getDataOnRoamingEnabled: phoneSubId=-2 isDataRoamingEnabled=false
D SubscriptionController: [getSubId]- sSlotIdxToSubId.size == 0, return DummySubIds slotIdx=0
D DCT     : [0]getDataOnRoamingEnabled: phoneSubId=-2 isDataRoamingEnabled=false
D SubscriptionController: [getSubId]- sSlotIdxToSubId.size == 0, return DummySubIds slotIdx=0
D DCT     : [0]getDataOnRoamingEnabled: phoneSubId=-2 isDataRoamingEnabled=false
D SubscriptionController: [getSubId]- sSlotIdxToSubId.size == 0, return DummySubIds slotIdx=0
D DCT     : [0]getDataOnRoamingEnabled: phoneSubId=-2 isDataRoamingEnabled=false
D SubscriptionController: [getSubId]- sSlotIdxToSubId.size == 0, return DummySubIds slotIdx=0
D DCT     : [0]getDataOnRoamingEnabled: phoneSubId=-2 isDataRoamingEnabled=false
D SubscriptionController: [getSubId]- sSlotIdxToSubId.size == 0, return DummySubIds slotIdx=0
D DCT     : [0]getDataOnRoamingEnabled: phoneSubId=-2 isDataRoamingEnabled=false
D SubscriptionController: [getSubId]- sSlotIdxToSubId.size == 0, return DummySubIds slotIdx=0
D DCT     : [0]getDataOnRoamingEnabled: phoneSubId=-2 isDataRoamingEnabled=false
D SubscriptionController: [getSubId]- sSlotIdxToSubId.size == 0, return DummySubIds slotIdx=0
D DCT     : [0]getDataOnRoamingEnabled: phoneSubId=-2 isDataRoamingEnabled=false
D SubscriptionController: [getSubId]- sSlotIdxToSubId.size == 0, return DummySubIds slotIdx=0
D DCT     : [0]getDataOnRoamingEnabled: phoneSubId=-2 isDataRoamingEnabled=false
D SubscriptionController: [getSubId]- sSlotIdxToSubId.size == 0, return DummySubIds slotIdx=0
D DCT     : [0]getDataOnRoamingEnabled: phoneSubId=-2 isDataRoamingEnabled=false
D SubscriptionController: [getSubId]- sSlotIdxToSubId.size == 0, return DummySubIds slotIdx=0
D DCT     : [0]getDataOnRoamingEnabled: phoneSubId=-2 isDataRoamingEnabled=false
D SubscriptionController: [getSubId]- sSlotIdxToSubId.size == 0, return DummySubIds slotIdx=0
D DCT     : [0]getDataOnRoamingEnabled: phoneSubId=-2 isDataRoamingEnabled=false
D SubscriptionController: [getSubId]- sSlotIdxToSubId.size == 0, return DummySubIds slotIdx=0
D DCT     : [0]getDataOnRoamingEnabled: phoneSubId=-2 isDataRoamingEnabled=false
D SubscriptionController: [getSubId]- sSlotIdxToSubId.size == 0, return DummySubIds slotIdx=0
D DCT     : [0]getDataOnRoamingEnabled: phoneSubId=-2 isDataRoamingEnabled=false
D SubscriptionController: [getSubId]- sSlotIdxToSubId.size == 0, return DummySubIds slotIdx=0
D PhoneBase: EVENT_GET_RADIO_CAPABILITY :phone rc : {mPhoneId = 0 mVersion=1 mSession=0 mPhase=0 mRadioAccessFamily=36366 mLogicModemId= mStatus=1}
D PhoneBase: config LCE service failed: com.android.internal.telephony.CommandException: REQUEST_NOT_SUPPORTED
E PhoneProxy: [PhoneProxy] EVENT_REQUEST_VOICE_RADIO_TECH_DONE: exception=com.android.internal.telephony.CommandException: RADIO_NOT_AVAILABLE
D DctController: handleMessage msg={ when=-101ms what=107 target=com.android.internal.telephony.dataconnection.DctController }
D DctController: onSubInfoReady mPhoneNum=1
D SubscriptionController: [getSubId]- sSlotIdxToSubId.size == 0, return DummySubIds slotIdx=0
D DctController: onSubInfoReady handle pending requests subId=-2
D DctController: onSubInfoReady: SIM card absent on phoneId = 0
D SubscriptionController: [getSubId]- sSlotIdxToSubId.size == 0, return DummySubIds slotIdx=0
D DctController: [TNF -2]evalPendingRequest, pending request size is 1
D SubscriptionController: [getSubId]- sSlotIdxToSubId.size == 0, return DummySubIds slotIdx=0
D DctController: [TNF -2]evalPendingRequest: request = NetworkRequest [ id=1, legacyType=-1, [ Capabilities: INTERNET&NOT_RESTRICTED&TRUSTED&NOT_VPN] ]
D SubscriptionController: [getSubId]- sSlotIdxToSubId.size == 0, return DummySubIds slotIdx=0
D DctController: [TNF -2]Cellular needs Network for NetworkRequest [ id=1, legacyType=-1, [ Capabilities: INTERNET&NOT_RESTRICTED&TRUSTED&NOT_VPN] ]
D SubscriptionController: [getSubId]- sSlotIdxToSubId.size == 0, return DummySubIds slotIdx=0
D SubscriptionController: [getSubId]- sSlotIdxToSubId.size == 0, return DummySubIds slotIdx=0
D DctController: [TNF -2]Request not useable, pending request.
D DctController: processRequests
D SubscriptionController: [getSubId]- sSlotIdxToSubId.size == 0, return DummySubIds slotIdx=0
D DctController: handleMessage msg={ when=-61ms what=100 target=com.android.internal.telephony.dataconnection.DctController }
D DcSwitchAsyncChannel: [DcSwitchAsyncChannel-0]: rspIsIdle=true
D SubscriptionController: [getPhoneId]- invalid subId return=-1
D DcSwitchAsyncChannel: [DcSwitchAsyncChannel-0]: rspIsIdle=true
D DctController: onProcessRequest requestedPhoneId=-1, activePhoneId=-1
E use-Rlog/RLOG-RIL-IPC: Polling IPC FMT client failed
D use-Rlog/RLOG-RIL: Updating RIL radio state to 1
D RILJ    : [UNSL]< UNSOL_RESPONSE_RADIO_STATE_CHANGED RADIO_UNAVAILABLE [SUB0]
D GsmSST  : [GsmSST] mDeviceShuttingDown = false
D GsmSST  : [GsmSST] mDesiredPowerState = true
D GsmSST  : [GsmSST] getRadioState = RADIO_UNAVAILABLE
D GsmSST  : [GsmSST] mPowerOffDelayNeed = true
D GsmSST  : [GsmSST] mAlarmSwitch = false
D PHONE   : [ServiceState] setNullState=1
D GsmSST  : [GsmSST] Poll ServiceState done:  oldSS=[3 3 voice home data home null null null null null null  Unknown Unknown CSS not supported -1 -1 RoamInd=-1 DefRoamInd=-1 EmergOnly=false IsDataRoamingFromRegistration=false] newSS=[1 1 voice home data home null null null null null null  Unknown Unknown CSS not supported -1 -1 RoamInd=-1 DefRoamInd=-1 EmergOnly=false IsDataRoamingFromRegistration=false] oldMaxDataCalls=1 mNewMaxDataCalls=1 oldReasonDataDenied=-1 mNewReasonDataDenied=-1
D PHONE   : [ServiceState] setNullState=1
D GsmSST  : [GsmSST] updateSpnDisplay: radio is on but out of service, set plmn='No service.'
D use-Rlog/RLOG-RIL: 10 RIL requests in the queue (0 pending, 0 handled, 10 unhandled)
D SubscriptionController: [getSubId]- sSlotIdxToSubId.size == 0, return DummySubIds slotIdx=0
D RilRequest: [3649]< RADIO_POWER error: com.android.internal.telephony.CommandException: RADIO_NOT_AVAILABLE ret=
D use-Rlog/RLOG-RIL: 9 RIL requests in the queue (0 pending, 0 handled, 9 unhandled)
D RilRequest: [3652]< SCREEN_STATE error: com.android.internal.telephony.CommandException: RADIO_NOT_AVAILABLE ret=
D use-Rlog/RLOG-RIL: 8 RIL requests in the queue (0 pending, 0 handled, 8 unhandled)
D RilRequest: [3654]< SIGNAL_STRENGTH error: com.android.internal.telephony.CommandException: RADIO_NOT_AVAILABLE ret=
D use-Rlog/RLOG-RIL: 7 RIL requests in the queue (0 pending, 0 handled, 7 unhandled)
D RilRequest: [3657]< RADIO_POWER error: com.android.internal.telephony.CommandException: RADIO_NOT_AVAILABLE ret=
D use-Rlog/RLOG-RIL: 6 RIL requests in the queue (0 pending, 0 handled, 6 unhandled)
D RilRequest: [3658]< OPERATOR error: com.android.internal.telephony.CommandException: RADIO_NOT_AVAILABLE ret=
D use-Rlog/RLOG-RIL: 5 RIL requests in the queue (0 pending, 0 handled, 5 unhandled)
D RilRequest: [3659]< DATA_REGISTRATION_STATE error: com.android.internal.telephony.CommandException: RADIO_NOT_AVAILABLE ret=
D use-Rlog/RLOG-RIL: 4 RIL requests in the queue (0 pending, 0 handled, 4 unhandled)
D RilRequest: [3660]< VOICE_REGISTRATION_STATE error: com.android.internal.telephony.CommandException: RADIO_NOT_AVAILABLE ret=
D use-Rlog/RLOG-RIL: 3 RIL requests in the queue (0 pending, 0 handled, 3 unhandled)
D RilRequest: [3661]< QUERY_NETWORK_SELECTION_MODE error: com.android.internal.telephony.CommandException: RADIO_NOT_AVAILABLE ret=
D use-Rlog/RLOG-RIL: 2 RIL requests in the queue (0 pending, 0 handled, 2 unhandled)
D RilRequest: [3662]< BASEBAND_VERSION error: com.android.internal.telephony.CommandException: RADIO_NOT_AVAILABLE ret=
D use-Rlog/RLOG-RIL: 1 RIL request in the queue (0 pending, 0 handled, 1 unhandled)
D RilRequest: [3663]< GET_IMEI error: com.android.internal.telephony.CommandException: RADIO_NOT_AVAILABLE ret=
D use-Rlog/RLOG-RIL: 0 RIL request in the queue (0 pending, 0 handled, 0 unhandled)
D use-Rlog/RLOG-RIL: 0 RIL request in the queue (0 pending, 0 handled, 0 unhandled)
D RilRequest: [3664]< GET_IMEISV error: com.android.internal.telephony.CommandException: RADIO_NOT_AVAILABLE ret=
E use-Rlog/RLOG-RIL: IPC FMT client loop failed
D RILJ    : [UNSL]< UNSOL_RESPONSE_CALL_STATE_CHANGED [SUB0]
D RILJ    : [UNSL]< UNSOL_RESPONSE_VOICE_NETWORK_STATE_CHANGED [SUB0]
D RILJ    : responseDataCallList ver=6 num=0 [SUB0]
D RILJ    : [UNSL]< UNSOL_DATA_CALL_LIST_CHANGED [] [SUB0]
D RILJ    : [UNSL]< UNSOL_RESPONSE_SIM_STATUS_CHANGED [SUB0]
D Dcc     : onDataStateChanged: dcsList=[] mDcListActiveByCid={}
D Dcc     : onDataStateChanged: dcsToRetry=[]
D Dcc     : onDataStateChanged: Data Activity updated to NONE. isAnyDataCallActive = false isAnyDataCallDormant = false
D Dcc     : onDataStateChanged: dcsToRetry=[] apnsToCleanup=[]
D Dcc     : onDataStateChanged: X
D GsmSST  : [GsmSST] updateSpnDisplay: changed sending intent rule=0 showPlmn='true' plmn='No service.' showSpn='false' spn='' dataSpn='' subId='-2'
D SubscriptionController: [getSubId]- sSlotIdxToSubId.size == 0, return DummySubIds slotIdx=0
D SubscriptionController: [getSubId]- sSlotIdxToSubId.size == 0, return DummySubIds slotIdx=0
D SubscriptionController: [setPlmnSpn] No valid subscription to store info
D SubscriptionController: notifySubscriptionInfoChanged:
D SubscriptionController: [getActiveSubInfoList]+
D SubscriptionController: [getActiveSubInfoList]+
D SubscriptionController: selection:sim_id>=0 null
D TelephonyManager: setTelephonyProperty: success phoneId=0 property=gsm.operator.alpha value:  propVal=
D SubscriptionController: selection:sim_id>=0 null
D TelephonyManager: setTelephonyProperty: success phoneId=0 property=gsm.operator.numeric value:  propVal=
D GsmSST  : [GsmSST] operatorNumeric is null
D TelephonyManager: setTelephonyProperty: success phoneId=0 property=gsm.operator.iso-country value:  propVal=
D TelephonyManager: setTelephonyProperty: success phoneId=0 property=gsm.operator.isroaming value: false propVal=false
D GsmSST  : [GsmSST] Broadcasting ServiceState : 1 1 voice home data home null null null null null null  Unknown Unknown CSS not supported -1 -1 RoamInd=-1 DefRoamInd=-1 EmergOnly=false IsDataRoamingFromRegistration=false
D SubscriptionController: [getSubId]- sSlotIdxToSubId.size == 0, return DummySubIds slotIdx=0
D DefaultPhoneNotifier: nofityServiceState: mRegistry=com.android.internal.telephony.ITelephonyRegistry$Stub$Proxy@5667eb9 ss=1 1 voice home data home null null null null null null  Unknown Unknown CSS not supported -1 -1 RoamInd=-1 DefRoamInd=-1 EmergOnly=false IsDataRoamingFromRegistration=false sender=Handler (com.android.internal.telephony.gsm.GSMPhone) {6bf8468} phondId=0 subId=-2
D SubscriptionController: [getActiveSubInfoList]- no info return
D SubscriptionController: [getSlotId]- subId invalid
D SubscriptionController: [getSubId]- sSlotIdxToSubId.size == 0, return DummySubIds slotIdx=0
D SubscriptionController: getSimStateForSlotIdx:  simState=NOT_READY ordinal=6
D SubscriptionManager: getSimStateForSubscriber: simState=6 slotIdx=0
D TelephonyManager: getSimState: default sim:-1, sim state for slotIdx=0 is 6, return state as unknown
D GsmSST  : [GsmSST] notifyDataRegStateRilRadioTechnologyChanged: drs=1 rat=0
D TelephonyManager: setTelephonyProperty: success phoneId=0 property=gsm.network.type value: Unknown propVal=Unknown
D DCT     : [0]get all active apn types
D UiccController: EVENT_RADIO_UNAVAILABLE, dispose card
D RILJ    : [3669]> GET_CURRENT_CALLS [SUB0]
E PhoneProxy: [PhoneProxy] Error! This handler was not registered for this message type. Message: 9
D RILJ    : [3670]> GET_CURRENT_CALLS [SUB0]
D use-Rlog/RLOG-RIL: 1 RIL request in the queue (1 pending, 0 handled, 0 unhandled)
D PHONE   : [ServiceState] setNullState=1
D GsmSST  : [GsmSST] Poll ServiceState done:  oldSS=[1 1 voice home data home null null null null null null  Unknown Unknown CSS not supported -1 -1 RoamInd=-1 DefRoamInd=-1 EmergOnly=false IsDataRoamingFromRegistration=false] newSS=[1 1 voice home data home null null null null null null  Unknown Unknown CSS not supported -1 -1 RoamInd=-1 DefRoamInd=-1 EmergOnly=false IsDataRoamingFromRegistration=false] oldMaxDataCalls=1 mNewMaxDataCalls=1 oldReasonDataDenied=-1 mNewReasonDataDenied=-1
D use-Rlog/RLOG-RIL: 2 RIL requests in the queue (2 pending, 0 handled, 0 unhandled)
D PHONE   : [ServiceState] setNullState=1
D DCT     : [0]handleMessage msg={ when=-26ms what=270340 obj=android.os.AsyncResult@c43a53c target=com.android.internal.telephony.dataconnection.DcTracker }
E DATA    : Unidentified event msg={ when=-26ms what=270340 obj=android.os.AsyncResult@c43a53c target=com.android.internal.telephony.dataconnection.DcTracker }
D UiccController: Received EVENT_ICC_STATUS_CHANGED, calling getIccCardStatus
D RILJ    : [3671]> GET_SIM_STATUS [SUB0]
D GsmSST  : [GsmSST] SubscriptionListener.onSubscriptionInfoChanged
D SubscriptionController: [getSubId]- sSlotIdxToSubId.size == 0, return DummySubIds slotIdx=0
D DCT     : [0]SubscriptionListener.onSubscriptionInfoChanged
D SubscriptionController: [getSubId]- sSlotIdxToSubId.size == 0, return DummySubIds slotIdx=0
D SubscriptionController: [getActiveSubInfoList]+
D use-Rlog/RLOG-RIL: 3 RIL requests in the queue (3 pending, 0 handled, 0 unhandled)
D SubscriptionController: selection:sim_id>=0 null
D SubscriptionController: [getActiveSubInfoList]- no info return
D SubscriptionController: [getActiveSubInfoList]- no info return
E PhoneBase: Error! unregisterForCallWaiting() in PhoneBase should not be called, CDMAPhone inactive.
D SubscriptionController: [getSubId]- sSlotIdxToSubId.size == 0, return DummySubIds slotIdx=0
D SubscriptionController: [getSubId]- sSlotIdxToSubId.size == 0, return DummySubIds slotIdx=0
D SubscriptionController: [getPhoneId]- invalid subId return=-1
D SubscriptionController: [getSubId]- sSlotIdxToSubId.size == 0, return DummySubIds slotIdx=0
D SubscriptionController: [getSubId]- sSlotIdxToSubId.size == 0, return DummySubIds slotIdx=0
D SubscriptionController: [getSubId]- sSlotIdxToSubId.size == 0, return DummySubIds slotIdx=0
D use-Rlog/RLOG-RIL: Closed IPC FMT client
E PhoneBase: Error! registerForCallWaiting() in PhoneBase should not be called, CDMAPhone inactive.
E use-Rlog/RLOG-RIL-IPC: Opening IPC FMT client failed
E use-Rlog/RLOG-RIL: Opening IPC FMT client failed
D DCT     : [0]handleMessage msg={ when=-48ms what=270377 obj=android.os.AsyncResult@d43d928 target=com.android.internal.telephony.dataconnection.DcTracker }
D DCT     : [0]onUpdateIcc: newIccRecords null
D DCT     : [0]setupDataOnConnectableApns: nwTypeChanged
D DCT     : [0]setupDataOnConnectableApns: apnContext {mApnType=dun mState=IDLE mWaitingApns={null} mWaitingApnsPermanentFailureCountDown=0 mApnSetting={null} mReason=radioTurnedOff mDataEnabled=false mDependencyMet=true}
D DCT     : [0]setupDataOnConnectableApns: apnContext {mApnType=hipri mState=IDLE mWaitingApns={null} mWaitingApnsPermanentFailureCountDown=0 mApnSetting={null} mReason=radioTurnedOff mDataEnabled=false mDependencyMet=true}
D DCT     : [0]setupDataOnConnectableApns: apnContext {mApnType=supl mState=IDLE mWaitingApns={null} mWaitingApnsPermanentFailureCountDown=0 mApnSetting={null} mReason=radioTurnedOff mDataEnabled=false mDependencyMet=true}
D DCT     : [0]setupDataOnConnectableApns: apnContext {mApnType=default mState=IDLE mWaitingApns={null} mWaitingApnsPermanentFailureCountDown=0 mApnSetting={null} mReason=radioTurnedOff mDataEnabled=false mDependencyMet=true}
D DCT     : [0]setupDataOnConnectableApns: apnContext {mApnType=mms mState=IDLE mWaitingApns={null} mWaitingApnsPermanentFailureCountDown=0 mApnSetting={null} mReason=radioTurnedOff mDataEnabled=false mDependencyMet=true}
D SubscriptionController: [getSubId]- sSlotIdxToSubId.size == 0, return DummySubIds slotIdx=0
D DCT     : [0]handleMessage msg={ when=-48ms what=270369 obj=android.os.AsyncResult@efdd641 target=com.android.internal.telephony.dataconnection.DcTracker }
D DCT     : [0]onUpdateIcc: newIccRecords null
D SubscriptionController: [getSubId]- sSlotIdxToSubId.size == 0, return DummySubIds slotIdx=0
D GsmSMSDispatcher: GsmSMSDispatcher: subId = -2 slotId = 0
E IccCardProxy: setExternalState: !override and newstate unchanged from NOT_READY
D DctController: handleMessage msg={ when=-45ms what=107 target=com.android.internal.telephony.dataconnection.DctController }
D DctController: onSubInfoReady mPhoneNum=1
D SubscriptionController: [getSubId]- sSlotIdxToSubId.size == 0, return DummySubIds slotIdx=0
D DctController: onSubInfoReady handle pending requests subId=-2
D DctController: onSubInfoReady: SIM card absent on phoneId = 0
D SubscriptionController: [getSubId]- sSlotIdxToSubId.size == 0, return DummySubIds slotIdx=0
D DctController: [TNF -2]evalPendingRequest, pending request size is 1
D SubscriptionController: [getSubId]- sSlotIdxToSubId.size == 0, return DummySubIds slotIdx=0
D DctController: [TNF -2]evalPendingRequest: request = NetworkRequest [ id=1, legacyType=-1, [ Capabilities: INTERNET&NOT_RESTRICTED&TRUSTED&NOT_VPN] ]
D SubscriptionController: [getSubId]- sSlotIdxToSubId.size == 0, return DummySubIds slotIdx=0
D DctController: [TNF -2]Cellular needs Network for NetworkRequest [ id=1, legacyType=-1, [ Capabilities: INTERNET&NOT_RESTRICTED&TRUSTED&NOT_VPN] ]
D SubscriptionController: [getSubId]- sSlotIdxToSubId.size == 0, return DummySubIds slotIdx=0
D SubscriptionController: [getSubId]- sSlotIdxToSubId.size == 0, return DummySubIds slotIdx=0
D DctController: [TNF -2]Request not useable, pending request.
D DctController: processRequests
D SubscriptionController: [getSubId]- sSlotIdxToSubId.size == 0, return DummySubIds slotIdx=0
D DctController: handleMessage msg={ when=-1ms what=100 target=com.android.internal.telephony.dataconnection.DctController }
D DcSwitchAsyncChannel: [DcSwitchAsyncChannel-0]: rspIsIdle=true
D SubscriptionController: [getPhoneId]- invalid subId return=-1
D DcSwitchAsyncChannel: [DcSwitchAsyncChannel-0]: rspIsIdle=true
D DctController: onProcessRequest requestedPhoneId=-1, activePhoneId=-1
D use-Rlog/RLOG-RIL: Closed IPC FMT client
D use-Rlog/RLOG-RIL-IPC: Starting i9300 modem boot
D use-Rlog/RLOG-RIL-IPC: Opened modem image device
D use-Rlog/RLOG-RIL-IPC: Mapped modem image data to memory
D use-Rlog/RLOG-RIL-IPC: Opened modem boot device
D use-Rlog/RLOG-RIL-IPC: Opened modem link device
D use-Rlog/RLOG-RIL-IPC: Turned the modem off
D CAT     : com.android.stk.BootCompletedReceiver: [ACTION_BOOT_COMPLETED]
D CAT     : com.android.stk.StkAppService: onCreate()+
D CAT     : com.android.stk.StkAppService: simCount: 1
D CAT     : com.android.stk.StkAppService: slotId: 0
D CAT     : com.android.stk.StkAppService: onStart sim id: 0, op: 5, *****
D CAT     : com.android.stk.StkAppService: mStkService is: -1
D CAT     : StkAppInstaller: [setAppState]+
D CAT     : StkAppInstaller: Change app state[false]
D CAT     : StkAppInstaller: [setAppState]-
D CAT     : com.android.stk.StkAppService: onDestroy()
D use-Rlog/RLOG-RIL-IPC: Turned the modem on
D use-Rlog/RLOG-RIL-IPC: Waited for link connected
D use-Rlog/RLOG-RIL-IPC: Wrote ATAT in ASCII
D use-Rlog/RLOG-RIL-IPC: Reading boot ACK failed
D use-Rlog/RLOG-RIL-IPC: Sending XMM626 HSIC PSI failed
E use-Rlog/RLOG-RIL-IPC: Booting IPC FMT client failed
E use-Rlog/RLOG-RIL: Opening IPC FMT client failed
D use-Rlog/RLOG-RIL: Closed IPC FMT client
D use-Rlog/RLOG-RIL-IPC: Starting i9300 modem boot
D use-Rlog/RLOG-RIL-IPC: Opened modem image device
D use-Rlog/RLOG-RIL-IPC: Mapped modem image data to memory
D use-Rlog/RLOG-RIL-IPC: Opened modem boot device
D use-Rlog/RLOG-RIL-IPC: Opened modem link device
D GsmCellBroadcastHandler: mWakeLock released
D CellBroadcastHandler: mWakeLock released
D CdmaServiceCategoryProgramHandler: mWakeLock released
D use-Rlog/RLOG-RIL-IPC: Turned the modem off
D SubscriptionController: [getSlotId]- subId invalid
D SubscriptionController: getSimStateForSlotIdx:  simState=NOT_READY ordinal=6
D SubscriptionManager: getSimStateForSubscriber: simState=6 slotIdx=0
D TelephonyManager: getSimState: default sim:-1, sim state for slotIdx=0 is 6, return state as unknown
D SubscriptionController: [getActiveSubInfoList]+
D SubscriptionController: selection:sim_id>=0 null
D SubscriptionController: [getActiveSubInfoList]- no info return
D SubscriptionController: [getActiveSubInfoList]+
D SubscriptionController: selection:sim_id>=0 null
D SubscriptionController: [getActiveSubInfoList]- no info return
D SubscriptionController: [getPhoneId] asked for default subId=-1
D SubscriptionController: [getPhoneId]- invalid subId return=-1
D SubscriptionController: [getActiveSubInfoList]+
D SubscriptionController: selection:sim_id>=0 null
D SubscriptionController: [getActiveSubInfoList]- no info return
D SubscriptionController: [getActiveSubInfoList]+
D SubscriptionController: selection:sim_id>=0 null
D SubscriptionController: [getActiveSubInfoList]- no info return
D SubscriptionController: [getPhoneId]- invalid subId return=-1
D SubscriptionController: [getSubId]- sSlotIdxToSubId.size == 0, return DummySubIds slotIdx=0
D SubscriptionController: [getActiveSubInfoList]+
D SubscriptionController: selection:sim_id>=0 null
D SubscriptionController: [getActiveSubInfoList]- no info return
D SubscriptionController: [getActiveSubInfoList]+
D SubscriptionController: selection:sim_id>=0 null
D SubscriptionController: [getActiveSubInfoList]- no info return
D use-Rlog/RLOG-RIL-IPC: Turned the modem on
D SubscriptionController: [getPhoneId] asked for default subId=-1
D SubscriptionController: [getPhoneId]- invalid subId return=-1
D use-Rlog/RLOG-RIL-IPC: Waited for link connected
D use-Rlog/RLOG-RIL-IPC: Wrote ATAT in ASCII
D use-Rlog/RLOG-RIL-IPC: Read chip id (0x16)
D use-Rlog/RLOG-RIL-IPC: Wrote PSI header
D use-Rlog/RLOG-RIL-IPC: Wrote PSI, CRC is 0xc8
D use-Rlog/RLOG-RIL-IPC: Wrote PSI CRC (0xc8)
D use-Rlog/RLOG-RIL-IPC: Read PSI CRC ACK
D use-Rlog/RLOG-RIL-IPC: Read PSI ACK
D use-Rlog/RLOG-RIL-IPC: Sent XMM626 HSIC PSI
D use-Rlog/RLOG-RIL-IPC: Wrote EBL size
D use-Rlog/RLOG-RIL-IPC: Wrote EBL, CRC is 0xb5
D use-Rlog/RLOG-RIL-IPC: Wrote EBL CRC (0xb5)
D use-Rlog/RLOG-RIL-IPC: Sent XMM626 HSIC EBL
D use-Rlog/RLOG-RIL-IPC: Read port config
D use-Rlog/RLOG-RIL-IPC: Sent XMM626 HSIC port config
D use-Rlog/RLOG-RIL-IPC: Sent XMM626 HSIC SEC start
D use-Rlog/RLOG-RIL-IPC: Sent XMM626 HSIC firmware
D use-Rlog/RLOG-RIL-IPC: Checked nv_data path
D use-Rlog/RLOG-RIL-IPC: Checked nv_data md5 path
D use-Rlog/RLOG-RIL-IPC: Calculated nv_data md5: 302aea06dda5362c3a57a5929d595bd1
D use-Rlog/RLOG-RIL-IPC: Read nv_data md5: 302aea06dda5362c3a57a5929d595bd1
D use-Rlog/RLOG-RIL-IPC: Checked nv_data backup path
D use-Rlog/RLOG-RIL-IPC: Loaded nv_data
D use-Rlog/RLOG-RIL-IPC: Sent XMM626 HSIC nv_data
D use-Rlog/RLOG-RIL-IPC: Sent XMM626 HSIC SEC end
D use-Rlog/RLOG-RIL-IPC: Sent XMM626 HSIC HW reset
D use-Rlog/RLOG-RIL-IPC: Waiting for host wake failed
D use-Rlog/RLOG-RIL-IPC: Waited for host wake
D use-Rlog/RLOG-RIL-IPC: Waited for link connected
D use-Rlog/RLOG-RIL: Opened IPC FMT client
D use-Rlog/RLOG-RIL-IPC: 
D use-Rlog/RLOG-RIL-IPC: xmm626_sec_modem_fmt_recv: Received FMT message
D use-Rlog/RLOG-RIL-IPC: xmm626_sec_modem_fmt_recv: Message: aseq=0xff, command=IPC_PWR_PHONE_PWR_UP, type=IPC_TYPE_NOTI, size=0
D use-Rlog/RLOG-RIL: Updating RIL radio state to 0
D use-Rlog/RLOG-RIL-IPC: 
D use-Rlog/RLOG-RIL-IPC: xmm626_sec_modem_fmt_recv: Received FMT message
D use-Rlog/RLOG-RIL-IPC: xmm626_sec_modem_fmt_recv: Message: aseq=0x00, command=IPC_MISC_ME_IMSI, type=IPC_TYPE_NOTI, size=16
D use-Rlog/RLOG-RIL-IPC: ================================= IPC FMT data =================================
D use-Rlog/RLOG-RIL-IPC: [0000]   0F 30 30 30 30 30 30 30  30 30 30 30 30 30 30 30   .0000000 00000000
D use-Rlog/RLOG-RIL-IPC: ================================================================================
D RILJ    : [UNSL]< UNSOL_RESPONSE_RADIO_STATE_CHANGED RADIO_OFF [SUB0]
D RILJ    : [UNSL]< UNSOL_RESPONSE_CALL_STATE_CHANGED [SUB0]
D GsmSST  : [GsmSST] mDeviceShuttingDown = false
D RILJ    : [UNSL]< UNSOL_RESPONSE_VOICE_NETWORK_STATE_CHANGED [SUB0]
D GsmSST  : [GsmSST] mDesiredPowerState = true
D GsmSST  : [GsmSST] getRadioState = RADIO_OFF
D GsmSST  : [GsmSST] mPowerOffDelayNeed = true
D GsmSST  : [GsmSST] mAlarmSwitch = false
D RILJ    : responseDataCallList ver=6 num=0 [SUB0]
D RILJ    : [3672]> RADIO_POWER on [SUB0]
D RILJ    : [UNSL]< UNSOL_DATA_CALL_LIST_CHANGED [] [SUB0]
D RILJ    : [UNSL]< UNSOL_RESPONSE_SIM_STATUS_CHANGED [SUB0]
D Dcc     : onDataStateChanged: dcsList=[] mDcListActiveByCid={}
D Dcc     : onDataStateChanged: dcsToRetry=[]
D Dcc     : onDataStateChanged: Data Activity updated to NONE. isAnyDataCallActive = false isAnyDataCallDormant = false
D Dcc     : onDataStateChanged: dcsToRetry=[] apnsToCleanup=[]
D Dcc     : onDataStateChanged: X
D PHONE   : [ServiceState] setNullState=3
D GsmSST  : [GsmSST] set service state as POWER_OFF
D PHONE   : [ServiceState] setNullState=3
D GsmSST  : [GsmSST] Poll ServiceState done:  oldSS=[1 1 voice home data home null null null null null null  Unknown Unknown CSS not supported -1 -1 RoamInd=-1 DefRoamInd=-1 EmergOnly=false IsDataRoamingFromRegistration=false] newSS=[3 3 voice home data home null null null null null null  Unknown Unknown CSS not supported -1 -1 RoamInd=-1 DefRoamInd=-1 EmergOnly=false IsDataRoamingFromRegistration=false] oldMaxDataCalls=1 mNewMaxDataCalls=1 oldReasonDataDenied=-1 mNewReasonDataDenied=-1
D PHONE   : [ServiceState] setNullState=1
D GsmSST  : [GsmSST] updateSpnDisplay: radio is off w/ showPlmn=true plmn=No service.
D SubscriptionController: [getSubId]- sSlotIdxToSubId.size == 0, return DummySubIds slotIdx=0
D use-Rlog/RLOG-RIL: 4 RIL requests in the queue (4 pending, 0 handled, 0 unhandled)
D GsmSST  : [GsmSST] updateSpnDisplay: changed sending intent rule=0 showPlmn='true' plmn='No service.' showSpn='false' spn='null' dataSpn='' subId='-2'
D use-Rlog/RLOG-RIL: 3 RIL requests in the queue (3 pending, 0 handled, 0 unhandled)
D use-Rlog/RLOG-RIL: 2 RIL requests in the queue (2 pending, 0 handled, 0 unhandled)
D use-Rlog/RLOG-RIL: Requesting normal power state
D use-Rlog/RLOG-RIL-IPC: 
D use-Rlog/RLOG-RIL-IPC: xmm626_sec_modem_fmt_send: Sent FMT message
D use-Rlog/RLOG-RIL-IPC: xmm626_sec_modem_fmt_send: Message: mseq=0x01, command=IPC_PWR_PHONE_STATE, type=IPC_TYPE_EXEC, size=2
D use-Rlog/RLOG-RIL-IPC: ================================= IPC FMT data =================================
D use-Rlog/RLOG-RIL-IPC: [0000]   02 02                                              ..
D use-Rlog/RLOG-RIL-IPC: ================================================================================
D RILJ    : [3669]< GET_CURRENT_CALLS {} [SUB0]
D SubscriptionController: [getSubId]- sSlotIdxToSubId.size == 0, return DummySubIds slotIdx=0
D RILJ    : [3670]< GET_CURRENT_CALLS {} [SUB0]
D SubscriptionController: [getSubId]- sSlotIdxToSubId.size == 0, return DummySubIds slotIdx=0
D SubscriptionController: [setPlmnSpn] No valid subscription to store info
D SubscriptionController: notifySubscriptionInfoChanged:
D SubscriptionController: [getActiveSubInfoList]+
D SubscriptionController: selection:sim_id>=0 null
D TelephonyManager: setTelephonyProperty: success phoneId=0 property=gsm.operator.alpha value:  propVal=
D TelephonyManager: setTelephonyProperty: success phoneId=0 property=gsm.operator.numeric value:  propVal=
D GsmSST  : [GsmSST] operatorNumeric is null
D TelephonyManager: setTelephonyProperty: success phoneId=0 property=gsm.operator.iso-country value:  propVal=
D TelephonyManager: setTelephonyProperty: success phoneId=0 property=gsm.operator.isroaming value: false propVal=false
D GsmSST  : [GsmSST] Broadcasting ServiceState : 3 3 voice home data home null null null null null null  Unknown Unknown CSS not supported -1 -1 RoamInd=-1 DefRoamInd=-1 EmergOnly=false IsDataRoamingFromRegistration=false
D SubscriptionController: [getSubId]- sSlotIdxToSubId.size == 0, return DummySubIds slotIdx=0
D DefaultPhoneNotifier: nofityServiceState: mRegistry=com.android.internal.telephony.ITelephonyRegistry$Stub$Proxy@5667eb9 ss=3 3 voice home data home null null null null null null  Unknown Unknown CSS not supported -1 -1 RoamInd=-1 DefRoamInd=-1 EmergOnly=false IsDataRoamingFromRegistration=false sender=Handler (com.android.internal.telephony.gsm.GSMPhone) {6bf8468} phondId=0 subId=-2
D SubscriptionController: [getActiveSubInfoList]+
D SubscriptionController: selection:sim_id>=0 null
D SubscriptionController: [getSlotId]- subId invalid
D SubscriptionController: [getActiveSubInfoList]- no info return
D SubscriptionController: [getSubId]- sSlotIdxToSubId.size == 0, return DummySubIds slotIdx=0
D SubscriptionController: [getActiveSubInfoList]+
D SubscriptionController: getSimStateForSlotIdx:  simState=NOT_READY ordinal=6
D SubscriptionManager: getSimStateForSubscriber: simState=6 slotIdx=0
D TelephonyManager: getSimState: default sim:-1, sim state for slotIdx=0 is 6, return state as unknown
D SubscriptionController: [getActiveSubInfoList]+
D GsmSST  : [GsmSST] notifyDataRegStateRilRadioTechnologyChanged: drs=3 rat=0
D TelephonyManager: setTelephonyProperty: success phoneId=0 property=gsm.network.type value: Unknown propVal=Unknown
D SubscriptionController: selection:sim_id>=0 null
D DCT     : [0]get all active apn types
D RILJ    : [3673]> OPERATOR [SUB0]
D RILJ    : [3674]> DATA_REGISTRATION_STATE [SUB0]
D RILJ    : [3675]> VOICE_REGISTRATION_STATE [SUB0]
D use-Rlog/RLOG-RIL: 3 RIL requests in the queue (1 pending, 1 handled, 1 unhandled)
D use-Rlog/RLOG-RIL: 4 RIL requests in the queue (1 pending, 1 handled, 2 unhandled)
D RILJ    : [3676]> QUERY_NETWORK_SELECTION_MODE [SUB0]
D use-Rlog/RLOG-RIL: 5 RIL requests in the queue (1 pending, 1 handled, 3 unhandled)
D DCT     : [0]handleMessage msg={ when=-35ms what=270337 obj=android.os.AsyncResult@db098c3 target=com.android.internal.telephony.dataconnection.DcTracker }
D DCT     : [0]onRadioAvailable
D DCT     : [0]overall state is IDLE
D RILJ    : [3677]> BASEBAND_VERSION [SUB0]
D SubscriptionController: selection:sim_id>=0 null
D use-Rlog/RLOG-RIL: 6 RIL requests in the queue (1 pending, 1 handled, 4 unhandled)
D RILJ    : [3678]> GET_IMEI [SUB0]
D use-Rlog/RLOG-RIL: 7 RIL requests in the queue (1 pending, 1 handled, 5 unhandled)
D SubscriptionController: [getActiveSubInfoList]- no info return
D RILJ    : [3679]> GET_IMEISV [SUB0]
D use-Rlog/RLOG-RIL: 8 RIL requests in the queue (1 pending, 1 handled, 6 unhandled)
D RILJ    : [3680]> RIL_REQUEST_GET_RADIO_CAPABILITY [SUB0]
D use-Rlog/RLOG-RIL: 9 RIL requests in the queue (1 pending, 1 handled, 7 unhandled)
D RILJ    : [3681]> RIL_REQUEST_START_LCE [SUB0]
D use-Rlog/RLOG-RIL: 10 RIL requests in the queue (1 pending, 1 handled, 8 unhandled)
D use-Rlog/RLOG-RIL: Unhandled RIL request: 130
D use-Rlog/RLOG-RIL: 9 RIL requests in the queue (0 pending, 1 handled, 8 unhandled)
D RILJ    : [3682]> RIL_REQUEST_VOICE_RADIO_TECH [SUB0]
D RILJ    : [3683]> GET_CURRENT_CALLS [SUB0]
D RILJ    : Faking RIL_REQUEST_GET_RADIO_CAPABILITY response using 36366 [SUB0]
D RILJ    : [3680]< RIL_REQUEST_GET_RADIO_CAPABILITY {mPhoneId = 0 mVersion=1 mSession=0 mPhase=0 mRadioAccessFamily=36366 mLogicModemId= mStatus=1} [SUB0]
D PHONE   : [ServiceState] setNullState=3
D SubscriptionController: [getActiveSubInfoList]- no info return
D GsmSST  : [GsmSST] set service state as POWER_OFF
D PHONE   : [ServiceState] setNullState=3
D GsmSST  : [GsmSST] Poll ServiceState done:  oldSS=[3 3 voice home data home null null null null null null  Unknown Unknown CSS not supported -1 -1 RoamInd=-1 DefRoamInd=-1 EmergOnly=false IsDataRoamingFromRegistration=false] newSS=[3 3 voice home data home null null null null null null  Unknown Unknown CSS not supported -1 -1 RoamInd=-1 DefRoamInd=-1 EmergOnly=false IsDataRoamingFromRegistration=false] oldMaxDataCalls=1 mNewMaxDataCalls=1 oldReasonDataDenied=-1 mNewReasonDataDenied=-1
D PHONE   : [ServiceState] setNullState=1
D RILJ    : [3684]> OPERATOR [SUB0]
D use-Rlog/RLOG-RIL: 10 RIL requests in the queue (1 pending, 1 handled, 8 unhandled)
D RILC    : decodeVoiceRadioTechnology: Invoked with incorrect RadioState
E RILC    : RIL_onRequestComplete: invalid RIL_Token
D use-Rlog/RLOG-RIL: 11 RIL requests in the queue (2 pending, 1 handled, 8 unhandled)
D RILJ    : [3685]> DATA_REGISTRATION_STATE [SUB0]
D RilRequest: [3682]< RIL_REQUEST_VOICE_RADIO_TECH error: com.android.internal.telephony.CommandException: RADIO_NOT_AVAILABLE ret=
D use-Rlog/RLOG-RIL: Unhandled RIL request: 132
D use-Rlog/RLOG-RIL: 10 RIL requests in the queue (1 pending, 1 handled, 8 unhandled)
D use-Rlog/RLOG-RIL: 9 RIL requests in the queue (0 pending, 1 handled, 8 unhandled)
D use-Rlog/RLOG-RIL: 10 RIL requests in the queue (1 pending, 1 handled, 8 unhandled)
D RILJ    : [3686]> VOICE_REGISTRATION_STATE [SUB0]
D RilRequest: [3681]< RIL_REQUEST_START_LCE error: com.android.internal.telephony.CommandException: REQUEST_NOT_SUPPORTED ret=
D use-Rlog/RLOG-RIL: 11 RIL requests in the queue (2 pending, 1 handled, 8 unhandled)
D SubscriptionController: [getActiveSubInfoList]- no info return
D RILJ    : [3687]> QUERY_NETWORK_SELECTION_MODE [SUB0]
D RILJ    : [3683]< GET_CURRENT_CALLS {} [SUB0]
D DCT     : [0]handleMessage msg={ when=-48ms what=270340 obj=android.os.AsyncResult@c8ea540 target=com.android.internal.telephony.dataconnection.DcTracker }
E DATA    : Unidentified event msg={ when=-48ms what=270340 obj=android.os.AsyncResult@c8ea540 target=com.android.internal.telephony.dataconnection.DcTracker }
D UiccController: Received EVENT_ICC_STATUS_CHANGED, calling getIccCardStatus
D RILJ    : [3688]> GET_SIM_STATUS [SUB0]
D use-Rlog/RLOG-RIL: 12 RIL requests in the queue (1 pending, 1 handled, 10 unhandled)
D use-Rlog/RLOG-RIL: 13 RIL requests in the queue (1 pending, 1 handled, 11 unhandled)
D GsmSST  : [GsmSST] SubscriptionListener.onSubscriptionInfoChanged
D SubscriptionController: [getSubId]- sSlotIdxToSubId.size == 0, return DummySubIds slotIdx=0
D DCT     : [0]SubscriptionListener.onSubscriptionInfoChanged
D SubscriptionController: [getSubId]- sSlotIdxToSubId.size == 0, return DummySubIds slotIdx=0
D use-Rlog/RLOG-RIL: 14 RIL requests in the queue (1 pending, 1 handled, 12 unhandled)
D SubscriptionController: [getActiveSubInfoList]+
D SubscriptionController: selection:sim_id>=0 null
D SubscriptionController: [getActiveSubInfoList]- no info return
E PhoneBase: Error! unregisterForCallWaiting() in PhoneBase should not be called, CDMAPhone inactive.
D SubscriptionController: [getSubId]- sSlotIdxToSubId.size == 0, return DummySubIds slotIdx=0
D SubscriptionController: [getSubId]- sSlotIdxToSubId.size == 0, return DummySubIds slotIdx=0
D SubscriptionController: [getPhoneId]- invalid subId return=-1
D SubscriptionController: [getSubId]- sSlotIdxToSubId.size == 0, return DummySubIds slotIdx=0
D SubscriptionController: [getSubId]- sSlotIdxToSubId.size == 0, return DummySubIds slotIdx=0
D SubscriptionController: [getSubId]- sSlotIdxToSubId.size == 0, return DummySubIds slotIdx=0
E PhoneBase: Error! registerForCallWaiting() in PhoneBase should not be called, CDMAPhone inactive.
D DCT     : [0]handleMessage msg={ when=-83ms what=270377 obj=android.os.AsyncResult@979fe1f target=com.android.internal.telephony.dataconnection.DcTracker }
D DCT     : [0]onUpdateIcc: newIccRecords null
D DCT     : [0]setupDataOnConnectableApns: nwTypeChanged
D DCT     : [0]setupDataOnConnectableApns: apnContext {mApnType=dun mState=IDLE mWaitingApns={null} mWaitingApnsPermanentFailureCountDown=0 mApnSetting={null} mReason=radioTurnedOff mDataEnabled=false mDependencyMet=true}
D DCT     : [0]setupDataOnConnectableApns: apnContext {mApnType=hipri mState=IDLE mWaitingApns={null} mWaitingApnsPermanentFailureCountDown=0 mApnSetting={null} mReason=radioTurnedOff mDataEnabled=false mDependencyMet=true}
D DCT     : [0]setupDataOnConnectableApns: apnContext {mApnType=supl mState=IDLE mWaitingApns={null} mWaitingApnsPermanentFailureCountDown=0 mApnSetting={null} mReason=radioTurnedOff mDataEnabled=false mDependencyMet=true}
D DCT     : [0]setupDataOnConnectableApns: apnContext {mApnType=default mState=IDLE mWaitingApns={null} mWaitingApnsPermanentFailureCountDown=0 mApnSetting={null} mReason=radioTurnedOff mDataEnabled=false mDependencyMet=true}
D DCT     : [0]setupDataOnConnectableApns: apnContext {mApnType=mms mState=IDLE mWaitingApns={null} mWaitingApnsPermanentFailureCountDown=0 mApnSetting={null} mReason=radioTurnedOff mDataEnabled=false mDependencyMet=true}
D SubscriptionController: [getSubId]- sSlotIdxToSubId.size == 0, return DummySubIds slotIdx=0
D SubscriptionController: [getSubId]- sSlotIdxToSubId.size == 0, return DummySubIds slotIdx=0
D PhoneBase: EVENT_GET_RADIO_CAPABILITY :phone rc : {mPhoneId = 0 mVersion=1 mSession=0 mPhase=0 mRadioAccessFamily=36366 mLogicModemId= mStatus=1}
E PhoneProxy: [PhoneProxy] EVENT_REQUEST_VOICE_RADIO_TECH_DONE: exception=com.android.internal.telephony.CommandException: RADIO_NOT_AVAILABLE
D PhoneBase: config LCE service failed: com.android.internal.telephony.CommandException: REQUEST_NOT_SUPPORTED
D DctController: handleMessage msg={ when=-67ms what=107 target=com.android.internal.telephony.dataconnection.DctController }
D DctController: onSubInfoReady mPhoneNum=1
D SubscriptionController: [getSubId]- sSlotIdxToSubId.size == 0, return DummySubIds slotIdx=0
D DctController: onSubInfoReady handle pending requests subId=-2
D DctController: onSubInfoReady: SIM card absent on phoneId = 0
D SubscriptionController: [getSubId]- sSlotIdxToSubId.size == 0, return DummySubIds slotIdx=0
D DctController: [TNF -2]evalPendingRequest, pending request size is 1
D SubscriptionController: [getSubId]- sSlotIdxToSubId.size == 0, return DummySubIds slotIdx=0
D DctController: [TNF -2]evalPendingRequest: request = NetworkRequest [ id=1, legacyType=-1, [ Capabilities: INTERNET&NOT_RESTRICTED&TRUSTED&NOT_VPN] ]
D SubscriptionController: [getSubId]- sSlotIdxToSubId.size == 0, return DummySubIds slotIdx=0
D DctController: [TNF -2]Cellular needs Network for NetworkRequest [ id=1, legacyType=-1, [ Capabilities: INTERNET&NOT_RESTRICTED&TRUSTED&NOT_VPN] ]
D SubscriptionController: [getSubId]- sSlotIdxToSubId.size == 0, return DummySubIds slotIdx=0
D SubscriptionController: [getSubId]- sSlotIdxToSubId.size == 0, return DummySubIds slotIdx=0
D DctController: [TNF -2]Request not useable, pending request.
D DctController: processRequests
D SubscriptionController: [getSubId]- sSlotIdxToSubId.size == 0, return DummySubIds slotIdx=0
D DctController: handleMessage msg={ when=-1ms what=100 target=com.android.internal.telephony.dataconnection.DctController }
D DcSwitchAsyncChannel: [DcSwitchAsyncChannel-0]: rspIsIdle=true
D SubscriptionController: [getPhoneId]- invalid subId return=-1
D DcSwitchAsyncChannel: [DcSwitchAsyncChannel-0]: rspIsIdle=true
D DctController: onProcessRequest requestedPhoneId=-1, activePhoneId=-1
D use-Rlog/RLOG-RIL-IPC: 
D use-Rlog/RLOG-RIL-IPC: xmm626_sec_modem_fmt_recv: Received FMT message
D use-Rlog/RLOG-RIL-IPC: xmm626_sec_modem_fmt_recv: Message: aseq=0xff, command=IPC_NET_REGIST, type=IPC_TYPE_NOTI, size=11
D use-Rlog/RLOG-RIL-IPC: ================================= IPC FMT data =================================
D use-Rlog/RLOG-RIL-IPC: [0000]   FF 02 01 00 00 00 00 00  00 00 00                  ........ ...
D use-Rlog/RLOG-RIL-IPC: ================================================================================
D use-Rlog/RLOG-RIL-IPC: 
D use-Rlog/RLOG-RIL-IPC: xmm626_sec_modem_fmt_recv: Received FMT message
D use-Rlog/RLOG-RIL-IPC: xmm626_sec_modem_fmt_recv: Message: aseq=0xff, command=IPC_NET_REGIST, type=IPC_TYPE_NOTI, size=11
D use-Rlog/RLOG-RIL-IPC: ================================= IPC FMT data =================================
D use-Rlog/RLOG-RIL-IPC: [0000]   FF 03 01 00 00 00 00 00  00 00 00                  ........ ...
D use-Rlog/RLOG-RIL-IPC: ================================================================================
D use-Rlog/RLOG-RIL-IPC: 
D use-Rlog/RLOG-RIL-IPC: xmm626_sec_modem_fmt_recv: Received FMT message
D use-Rlog/RLOG-RIL-IPC: xmm626_sec_modem_fmt_recv: Message: aseq=0x00, command=IPC_DISP_ICON_INFO, type=IPC_TYPE_NOTI, size=4
D use-Rlog/RLOG-RIL-IPC: ================================= IPC FMT data =================================
D use-Rlog/RLOG-RIL-IPC: [0000]   FF 00 00 00                                        ....
D use-Rlog/RLOG-RIL-IPC: ================================================================================
D use-Rlog/RLOG-RIL-IPC: 
D use-Rlog/RLOG-RIL-IPC: xmm626_sec_modem_fmt_recv: Received FMT message
D use-Rlog/RLOG-RIL-IPC: xmm626_sec_modem_fmt_recv: Message: aseq=0x01, command=IPC_GEN_PHONE_RES, type=IPC_TYPE_RESP, size=5
D use-Rlog/RLOG-RIL-IPC: ================================= IPC FMT data =================================
D use-Rlog/RLOG-RIL-IPC: [0000]   01 07 01 00 80                                     .....
D use-Rlog/RLOG-RIL-IPC: ================================================================================
D use-Rlog/RLOG-RIL: Generic response was expected
D use-Rlog/RLOG-RIL-IPC: 
D use-Rlog/RLOG-RIL-IPC: xmm626_sec_modem_fmt_recv: Received FMT message
D use-Rlog/RLOG-RIL-IPC: xmm626_sec_modem_fmt_recv: Message: aseq=0x01, command=IPC_PWR_PHONE_STATE, type=IPC_TYPE_NOTI, size=1
D use-Rlog/RLOG-RIL-IPC: ================================= IPC FMT data =================================
D use-Rlog/RLOG-RIL-IPC: [0000]   02                                                 .
D use-Rlog/RLOG-RIL-IPC: ================================================================================
D use-Rlog/RLOG-RIL: Power state is normal
D use-Rlog/RLOG-RIL: 13 RIL requests in the queue (0 pending, 0 handled, 13 unhandled)
D use-Rlog/RLOG-RIL: Updating RIL radio state to 2
D use-Rlog/RLOG-RIL-IPC: 
D use-Rlog/RLOG-RIL-IPC: xmm626_sec_modem_fmt_send: Sent FMT message
D use-Rlog/RLOG-RIL-IPC: xmm626_sec_modem_fmt_send: Message: mseq=0x02, command=IPC_SEC_PIN_STATUS, type=IPC_TYPE_GET, size=0
D use-Rlog/RLOG-RIL-IPC: 
D use-Rlog/RLOG-RIL-IPC: xmm626_sec_modem_fmt_send: Sent FMT message
D use-Rlog/RLOG-RIL-IPC: xmm626_sec_modem_fmt_send: Message: mseq=0x03, command=IPC_NET_SERVING_NETWORK, type=IPC_TYPE_GET, size=0
D use-Rlog/RLOG-RIL-IPC: 
D use-Rlog/RLOG-RIL-IPC: xmm626_sec_modem_fmt_send: Sent FMT message
D use-Rlog/RLOG-RIL-IPC: xmm626_sec_modem_fmt_send: Message: mseq=0x04, command=IPC_NET_REGIST, type=IPC_TYPE_GET, size=2
D RILJ    : [3672]< RADIO_POWER  [SUB0]
D use-Rlog/RLOG-RIL-IPC: ================================= IPC FMT data =================================
D use-Rlog/RLOG-RIL-IPC: [0000]   FF 03                                              ..
D use-Rlog/RLOG-RIL-IPC: ================================================================================
D use-Rlog/RLOG-RIL-IPC: 
D use-Rlog/RLOG-RIL-IPC: xmm626_sec_modem_fmt_send: Sent FMT message
D use-Rlog/RLOG-RIL-IPC: xmm626_sec_modem_fmt_send: Message: mseq=0x05, command=IPC_NET_REGIST, type=IPC_TYPE_GET, size=2
D use-Rlog/RLOG-RIL-IPC: ================================= IPC FMT data =================================
D RILJ    : [UNSL]< UNSOL_VOICE_RADIO_TECH_CHANGED {3} [SUB0]
D use-Rlog/RLOG-RIL-IPC: [0000]   FF 02                                              ..
D use-Rlog/RLOG-RIL-IPC: ================================================================================
D use-Rlog/RLOG-RIL-IPC: 
D use-Rlog/RLOG-RIL-IPC: xmm626_sec_modem_fmt_send: Sent FMT message
D use-Rlog/RLOG-RIL-IPC: xmm626_sec_modem_fmt_send: Message: mseq=0x06, command=IPC_NET_PLMN_SEL, type=IPC_TYPE_GET, size=0
D use-Rlog/RLOG-RIL-IPC: 
D use-Rlog/RLOG-RIL-IPC: xmm626_sec_modem_fmt_send: Sent FMT message
D RILJ    : [UNSL]< UNSOL_RESPONSE_RADIO_STATE_CHANGED RADIO_ON [SUB0]
D use-Rlog/RLOG-RIL-IPC: xmm626_sec_modem_fmt_send: Message: mseq=0x07, command=IPC_MISC_ME_VERSION, type=IPC_TYPE_GET, size=1
D use-Rlog/RLOG-RIL-IPC: ================================= IPC FMT data =================================
D use-Rlog/RLOG-RIL-IPC: [0000]   FF                                                 .
D use-Rlog/RLOG-RIL-IPC: ================================================================================
D PhoneProxy: [PhoneProxy] EVENT_VOICE_RADIO_TECH_CHANGED: newVoiceTech=3
D PhoneProxy: [PhoneProxy] phoneObjectUpdater: newVoiceRadioTech=3
D use-Rlog/RLOG-RIL-IPC: 
D use-Rlog/RLOG-RIL-IPC: xmm626_sec_modem_fmt_send: Sent FMT message
D use-Rlog/RLOG-RIL-IPC: xmm626_sec_modem_fmt_send: Message: mseq=0x08, command=IPC_MISC_ME_SN, type=IPC_TYPE_GET, size=1
D PhoneProxy: [PhoneProxy] phoneObjectUpdater: No change ignore, newVoiceRadioTech=3 mActivePhone=GSM
D use-Rlog/RLOG-RIL-IPC: ================================= IPC FMT data =================================
D use-Rlog/RLOG-RIL-IPC: [0000]   01                                                 .
D use-Rlog/RLOG-RIL-IPC: ================================================================================
D GsmSST  : [GsmSST] mDeviceShuttingDown = false
D GsmSST  : [GsmSST] mDesiredPowerState = true
D GsmSST  : [GsmSST] getRadioState = RADIO_ON
D use-Rlog/RLOG-RIL-IPC: 
D GsmSST  : [GsmSST] mPowerOffDelayNeed = true
D use-Rlog/RLOG-RIL-IPC: xmm626_sec_modem_fmt_send: Sent FMT message
D GsmSST  : [GsmSST] mAlarmSwitch = false
D use-Rlog/RLOG-RIL-IPC: xmm626_sec_modem_fmt_send: Message: mseq=0x09, command=IPC_NET_PLMN_SEL, type=IPC_TYPE_GET, size=0
D RILJ    : [3689]> OPERATOR [SUB0]
D use-Rlog/RLOG-RIL-IPC: 
D use-Rlog/RLOG-RIL-IPC: xmm626_sec_modem_fmt_recv: Received FMT message
D use-Rlog/RLOG-RIL-IPC: xmm626_sec_modem_fmt_recv: Message: aseq=0xff, command=IPC_NET_REGIST, type=IPC_TYPE_NOTI, size=11
D use-Rlog/RLOG-RIL-IPC: ================================= IPC FMT data =================================
D use-Rlog/RLOG-RIL-IPC: [0000]   FF 02 01 00 00 00 00 00  00 00 00                  ........ ...
D use-Rlog/RLOG-RIL-IPC: ================================================================================
D RILJ    : [3690]> DATA_REGISTRATION_STATE [SUB0]
D use-Rlog/RLOG-RIL-IPC: 
D RILJ    : [UNSL]< UNSOL_RESPONSE_VOICE_NETWORK_STATE_CHANGED [SUB0]
D use-Rlog/RLOG-RIL-IPC: xmm626_sec_modem_fmt_recv: Received FMT message
D use-Rlog/RLOG-RIL-IPC: xmm626_sec_modem_fmt_recv: Message: aseq=0xff, command=IPC_NET_REGIST, type=IPC_TYPE_NOTI, size=11
D use-Rlog/RLOG-RIL-IPC: ================================= IPC FMT data =================================
D use-Rlog/RLOG-RIL-IPC: [0000]   FF 03 01 00 00 00 00 00  00 00 00                  ........ ...
D use-Rlog/RLOG-RIL-IPC: ================================================================================
D RILJ    : [3691]> VOICE_REGISTRATION_STATE [SUB0]
D use-Rlog/RLOG-RIL: 14 RIL requests in the queue (1 pending, 9 handled, 4 unhandled)
D use-Rlog/RLOG-RIL: 2 RIL requests data in the queue
D use-Rlog/RLOG-RIL-IPC: 
D use-Rlog/RLOG-RIL-IPC: xmm626_sec_modem_fmt_recv: Received FMT message
D use-Rlog/RLOG-RIL-IPC: xmm626_sec_modem_fmt_recv: Message: aseq=0x00, command=IPC_DISP_ICON_INFO, type=IPC_TYPE_NOTI, size=4
D use-Rlog/RLOG-RIL-IPC: ================================= IPC FMT data =================================
D use-Rlog/RLOG-RIL-IPC: [0000]   FF 00 00 00                                        ....
D use-Rlog/RLOG-RIL-IPC: ================================================================================
D use-Rlog/RLOG-RIL: Signal strength is 1
D use-Rlog/RLOG-RIL: 15 RIL requests in the queue (2 pending, 9 handled, 4 unhandled)
D RILJ    : [3692]> QUERY_NETWORK_SELECTION_MODE [SUB0]
D use-Rlog/RLOG-RIL: 2 RIL requests data in the queue
D RILJ    : [UNSL]< UNSOL_RESPONSE_VOICE_NETWORK_STATE_CHANGED [SUB0]
D use-Rlog/RLOG-RIL: 16 RIL requests in the queue (1 pending, 9 handled, 6 unhandled)
D use-Rlog/RLOG-RIL: 2 RIL requests data in the queue
D UiccController: Received EVENT_ICC_STATUS_CHANGED, calling getIccCardStatus
D RILJ    : [3693]> GET_SIM_STATUS [SUB0]
D use-Rlog/RLOG-RIL-IPC: 
D use-Rlog/RLOG-RIL-IPC: xmm626_sec_modem_fmt_recv: Received FMT message
D use-Rlog/RLOG-RIL-IPC: xmm626_sec_modem_fmt_recv: Message: aseq=0x02, command=IPC_GEN_PHONE_RES, type=IPC_TYPE_RESP, size=5
D use-Rlog/RLOG-RIL-IPC: ================================= IPC FMT data =================================
D use-Rlog/RLOG-RIL-IPC: [0000]   05 01 02 0E 00                                     .....
D use-Rlog/RLOG-RIL-IPC: ================================================================================
D RILJ    : [3694]> GET_CURRENT_CALLS [SUB0]
D use-Rlog/RLOG-RIL: Ignoring generic response for command IPC_SEC_PIN_STATUS
D use-Rlog/RLOG-RIL: 17 RIL requests in the queue (1 pending, 9 handled, 7 unhandled)
D use-Rlog/RLOG-RIL: 2 RIL requests data in the queue
D use-Rlog/RLOG-RIL: 18 RIL requests in the queue (2 pending, 9 handled, 7 unhandled)
D use-Rlog/RLOG-RIL: 2 RIL requests data in the queue
D use-Rlog/RLOG-RIL-IPC: 
D use-Rlog/RLOG-RIL-IPC: xmm626_sec_modem_fmt_recv: Received FMT message
D use-Rlog/RLOG-RIL-IPC: xmm626_sec_modem_fmt_recv: Message: aseq=0x03, command=IPC_NET_SERVING_NETWORK, type=IPC_TYPE_RESP, size=11
D use-Rlog/RLOG-RIL-IPC: ================================= IPC FMT data =================================
D use-Rlog/RLOG-RIL-IPC: [0000]   02 05 FF 30 30 30 30 30  23 00 00                  ...00000 #..
D use-Rlog/RLOG-RIL-IPC: ================================================================================
D SubscriptionController: [getSubId]- sSlotIdxToSubId.size == 0, return DummySubIds slotIdx=0
D RILJ    : [3695]> RIL_REQUEST_VOICE_RADIO_TECH [SUB0]
D use-Rlog/RLOG-RIL: 17 RIL requests in the queue (2 pending, 8 handled, 7 unhandled)
D use-Rlog/RLOG-RIL: 2 RIL requests data in the queue
D RILJ    : [3696]> RIL_REQUEST_IMS_REGISTRATION_STATE [SUB0]
D RILJ    : [3673]< OPERATOR {null, null, 00000} [SUB0]
D use-Rlog/RLOG-RIL-IPC: 
D use-Rlog/RLOG-RIL-IPC: xmm626_sec_modem_fmt_send: Sent FMT message
D use-Rlog/RLOG-RIL-IPC: xmm626_sec_modem_fmt_send: Message: mseq=0x0a, command=IPC_NET_SERVING_NETWORK, type=IPC_TYPE_GET, size=0
D use-Rlog/RLOG-RIL-IPC: 
D use-Rlog/RLOG-RIL-IPC: xmm626_sec_modem_fmt_send: Sent FMT message
D use-Rlog/RLOG-RIL-IPC: xmm626_sec_modem_fmt_send: Message: mseq=0x0b, command=IPC_NET_PLMN_SEL, type=IPC_TYPE_GET, size=0
D use-Rlog/RLOG-RIL-IPC: 
D use-Rlog/RLOG-RIL-IPC: xmm626_sec_modem_fmt_recv: Received FMT message
D use-Rlog/RLOG-RIL-IPC: xmm626_sec_modem_fmt_recv: Message: aseq=0x04, command=IPC_NET_REGIST, type=IPC_TYPE_RESP, size=11
D use-Rlog/RLOG-RIL-IPC: ================================= IPC FMT data =================================
D use-Rlog/RLOG-RIL-IPC: [0000]   FF 03 01 00 00 00 00 00  00 00 00                  ........ ...
D use-Rlog/RLOG-RIL-IPC: ================================================================================
D use-Rlog/RLOG-RIL: 16 RIL requests in the queue (0 pending, 9 handled, 7 unhandled)
D use-Rlog/RLOG-RIL: 2 RIL requests data in the queue
D use-Rlog/RLOG-RIL: 17 RIL requests in the queue (1 pending, 9 handled, 7 unhandled)
D use-Rlog/RLOG-RIL: 2 RIL requests data in the queue
D RILJ    : [3697]> RIL_REQUEST_CDMA_GET_SUBSCRIPTION_SOURCE [SUB0]
D RILJ    : [3674]< DATA_REGISTRATION_STATE {0, 0, 0, 0, 3} [SUB0]
D use-Rlog/RLOG-RIL: 16 RIL requests in the queue (7 pending, 9 handled, 0 unhandled)
D use-Rlog/RLOG-RIL: 1 RIL request data in the queue
D use-Rlog/RLOG-RIL-IPC: 
D use-Rlog/RLOG-RIL-IPC: xmm626_sec_modem_fmt_send: Sent FMT message
D use-Rlog/RLOG-RIL-IPC: xmm626_sec_modem_fmt_send: Message: mseq=0x0c, command=IPC_NET_REGIST, type=IPC_TYPE_GET, size=2
D RILJ    : [3698]> OPERATOR [SUB0]
D use-Rlog/RLOG-RIL-IPC: ================================= IPC FMT data =================================
D use-Rlog/RLOG-RIL-IPC: [0000]   FF 03                                              ..
D use-Rlog/RLOG-RIL-IPC: ================================================================================
D use-Rlog/RLOG-RIL-IPC: 
D use-Rlog/RLOG-RIL-IPC: xmm626_sec_modem_fmt_send: Sent FMT message
D use-Rlog/RLOG-RIL-IPC: xmm626_sec_modem_fmt_send: Message: mseq=0x0d, command=IPC_CALL_LIST, type=IPC_TYPE_GET, size=0
D use-Rlog/RLOG-RIL-IPC: 
D use-Rlog/RLOG-RIL-IPC: xmm626_sec_modem_fmt_recv: Received FMT message
D use-Rlog/RLOG-RIL-IPC: xmm626_sec_modem_fmt_recv: Message: aseq=0x05, command=IPC_NET_REGIST, type=IPC_TYPE_RESP, size=11
D use-Rlog/RLOG-RIL-IPC: ================================= IPC FMT data =================================
D use-Rlog/RLOG-RIL-IPC: [0000]   FF 02 01 00 00 00 00 00  00 00 00                  ........ ...
D use-Rlog/RLOG-RIL-IPC: ================================================================================
D RILJ    : [3699]> DATA_REGISTRATION_STATE [SUB0]
D use-Rlog/RLOG-RIL: 15 RIL requests in the queue (0 pending, 10 handled, 5 unhandled)
D use-Rlog/RLOG-RIL: 1 RIL request data in the queue
D use-Rlog/RLOG-RIL: 16 RIL requests in the queue (1 pending, 10 handled, 5 unhandled)
D use-Rlog/RLOG-RIL: 1 RIL request data in the queue
D use-Rlog/RLOG-RIL: 15 RIL requests in the queue (5 pending, 10 handled, 0 unhandled)
D RILJ    : [3700]> VOICE_REGISTRATION_STATE [SUB0]
D use-Rlog/RLOG-RIL-IPC: 
D use-Rlog/RLOG-RIL-IPC: xmm626_sec_modem_fmt_send: Sent FMT message
D use-Rlog/RLOG-RIL-IPC: xmm626_sec_modem_fmt_send: Message: mseq=0x0e, command=IPC_NET_REGIST, type=IPC_TYPE_GET, size=2
D use-Rlog/RLOG-RIL-IPC: ================================= IPC FMT data =================================
D use-Rlog/RLOG-RIL-IPC: [0000]   FF 02                                              ..
D use-Rlog/RLOG-RIL-IPC: ================================================================================
D use-Rlog/RLOG-RIL: Unhandled RIL request: 112
D use-Rlog/RLOG-RIL: 14 RIL requests in the queue (0 pending, 11 handled, 3 unhandled)
D RILJ    : [3701]> QUERY_NETWORK_SELECTION_MODE [SUB0]
D use-Rlog/RLOG-RIL-IPC: 
D use-Rlog/RLOG-RIL-IPC: xmm626_sec_modem_fmt_recv: Received FMT message
D use-Rlog/RLOG-RIL-IPC: xmm626_sec_modem_fmt_recv: Message: aseq=0x06, command=IPC_NET_PLMN_SEL, type=IPC_TYPE_RESP, size=1
D use-Rlog/RLOG-RIL-IPC: ================================= IPC FMT data =================================
D use-Rlog/RLOG-RIL-IPC: [0000]   02                                                 .
D use-Rlog/RLOG-RIL-IPC: ================================================================================
D use-Rlog/RLOG-RIL: 13 RIL requests in the queue (0 pending, 10 handled, 3 unhandled)
D use-Rlog/RLOG-RIL: 14 RIL requests in the queue (1 pending, 10 handled, 3 unhandled)
D use-Rlog/RLOG-RIL: 15 RIL requests in the queue (2 pending, 10 handled, 3 unhandled)
D use-Rlog/RLOG-RIL: 16 RIL requests in the queue (3 pending, 10 handled, 3 unhandled)
D RILJ    : [3702]> OPERATOR [SUB0]
D use-Rlog/RLOG-RIL: 17 RIL requests in the queue (1 pending, 10 handled, 6 unhandled)
D use-Rlog/RLOG-RIL-IPC: 
D use-Rlog/RLOG-RIL-IPC: xmm626_sec_modem_fmt_send: Sent FMT message
D use-Rlog/RLOG-RIL-IPC: xmm626_sec_modem_fmt_send: Message: mseq=0x0f, command=IPC_NET_PLMN_SEL, type=IPC_TYPE_GET, size=0
D RILJ    : [3695]< RIL_REQUEST_VOICE_RADIO_TECH {3} [SUB0]
D use-Rlog/RLOG-RIL-IPC: 
D use-Rlog/RLOG-RIL-IPC: xmm626_sec_modem_fmt_recv: Received FMT message
D use-Rlog/RLOG-RIL-IPC: xmm626_sec_modem_fmt_recv: Message: aseq=0x07, command=IPC_MISC_ME_VERSION, type=IPC_TYPE_RESP, size=148
D use-Rlog/RLOG-RIL-IPC: ================================= IPC FMT data =================================
D use-Rlog/RLOG-RIL-IPC: [0000]   1F 49 39 33 30 30 42 55  55 47 4E 46 31 00 00 00   .I9300BU UGNF1...
D use-Rlog/RLOG-RIL-IPC: [0010]   00 00 00 00 00 00 00 00  00 00 00 00 00 00 00 00   ........ ........
D RILJ    : [3685]< DATA_REGISTRATION_STATE {0, 0, 0, 0, 3} [SUB0]
D use-Rlog/RLOG-RIL-IPC: [0020]   00 4D 50 20 31 2E 31 30  30 00 00 00 00 00 00 00   .MP 1.10 0.......
D use-Rlog/RLOG-RIL-IPC: [0030]   00 00 00 00 00 00 00 00  00 00 00 00 00 00 00 00   ........ ........
D use-Rlog/RLOG-RIL-IPC: [0040]   00 32 30 31 32 2E 35 2E  32 39 00 00 00 00 00 00   .2012.5. 29......
D use-Rlog/RLOG-RIL-IPC: [0050]   00 00 00 00 00 00 00 00  00 00 00 00 00 00 00 00   ........ ........
D RILJ    : [3675]< VOICE_REGISTRATION_STATE {0, 0, 0, 0, null, null, null, null, null, null, null, null, null, null, null} [SUB0]
D use-Rlog/RLOG-RIL-IPC: [0060]   00 47 54 2D 49 39 33 30  30 52 57 41 56 44 32 00   .GT-I930 0RWAVD2.
D use-Rlog/RLOG-RIL-IPC: [0070]   00 00 00 00 00 00 00 00  00 00 00 00 00 00 00 00   ........ ........
D RILJ    : [3697]< RIL_REQUEST_CDMA_GET_SUBSCRIPTION_SOURCE {0} [SUB0]
D use-Rlog/RLOG-RIL-IPC: [0080]   00 49 39 33 30 30 00 00  00 00 00 00 00 00 00 00   .I9300.. ........
D use-Rlog/RLOG-RIL-IPC: [0090]   00 00 00 00                                        ....
D use-Rlog/RLOG-RIL-IPC: ================================================================================
D use-Rlog/RLOG-RIL: 16 RIL requests in the queue (0 pending, 10 handled, 6 unhandled)
D RILJ    : [3686]< VOICE_REGISTRATION_STATE {0, 0, 0, 0, null, null, null, null, null, null, null, null, null, null, null} [SUB0]
D use-Rlog/RLOG-RIL-IPC: 
D use-Rlog/RLOG-RIL-IPC: xmm626_sec_modem_fmt_recv: Received FMT message
D use-Rlog/RLOG-RIL-IPC: xmm626_sec_modem_fmt_recv: Message: aseq=0x08, command=IPC_MISC_ME_SN, type=IPC_TYPE_RESP, size=34
D use-Rlog/RLOG-RIL-IPC: ================================= IPC FMT data =================================
D RilRequest: [3696]< RIL_REQUEST_IMS_REGISTRATION_STATE error: com.android.internal.telephony.CommandException: REQUEST_NOT_SUPPORTED ret=
D use-Rlog/RLOG-RIL-IPC: [0000]   01 11 33 35 33 31 36 34  30 35 30 35 32 38 32 38   ..353164 05052828
D use-Rlog/RLOG-RIL-IPC: [0010]   37 31 35 00 00 00 00 00  00 00 00 00 00 00 00 00   715..... ........
D use-Rlog/RLOG-RIL-IPC: [0020]   00 4D                                              .M
D RILJ    : [3676]< QUERY_NETWORK_SELECTION_MODE {0} [SUB0]
D use-Rlog/RLOG-RIL-IPC: ================================================================================
D use-Rlog/RLOG-RIL: 15 RIL requests in the queue (0 pending, 9 handled, 6 unhandled)
D use-Rlog/RLOG-RIL: 14 RIL requests in the queue (0 pending, 8 handled, 6 unhandled)
D RILJ    : [3677]< BASEBAND_VERSION I9300BUUGNF1 [SUB0]
D RILJ    : [3678]< GET_IMEI  [SUB0]
D use-Rlog/RLOG-RIL-IPC: 
D use-Rlog/RLOG-RIL-IPC: xmm626_sec_modem_fmt_recv: Received FMT message
D use-Rlog/RLOG-RIL-IPC: xmm626_sec_modem_fmt_recv: Message: aseq=0x09, command=IPC_NET_PLMN_SEL, type=IPC_TYPE_RESP, size=1
D use-Rlog/RLOG-RIL-IPC: ================================= IPC FMT data =================================
D RILJ    : [3679]< GET_IMEISV  [SUB0]
D use-Rlog/RLOG-RIL-IPC: [0000]   02                                                 .
D use-Rlog/RLOG-RIL-IPC: ================================================================================
D use-Rlog/RLOG-RIL: 13 RIL requests in the queue (0 pending, 7 handled, 6 unhandled)
D use-Rlog/RLOG-RIL-IPC: 
D use-Rlog/RLOG-RIL-IPC: xmm626_sec_modem_fmt_recv: Received FMT message
D use-Rlog/RLOG-RIL-IPC: xmm626_sec_modem_fmt_recv: Message: aseq=0x0a, command=IPC_NET_SERVING_NETWORK, type=IPC_TYPE_RESP, size=11
D use-Rlog/RLOG-RIL-IPC: ================================= IPC FMT data =================================
D use-Rlog/RLOG-RIL-IPC: [0000]   02 05 FF 30 30 30 30 30  23 00 00                  ...00000 #..
D use-Rlog/RLOG-RIL-IPC: ================================================================================
D RILJ    : [3703]> DATA_REGISTRATION_STATE [SUB0]
D use-Rlog/RLOG-RIL: 12 RIL requests in the queue (0 pending, 6 handled, 6 unhandled)
D use-Rlog/RLOG-RIL-IPC: 
D use-Rlog/RLOG-RIL-IPC: xmm626_sec_modem_fmt_recv: Received FMT message
D use-Rlog/RLOG-RIL-IPC: xmm626_sec_modem_fmt_recv: Message: aseq=0x0b, command=IPC_NET_PLMN_SEL, type=IPC_TYPE_RESP, size=1
D use-Rlog/RLOG-RIL-IPC: ================================= IPC FMT data =================================
D use-Rlog/RLOG-RIL-IPC: [0000]   02                                                 .
D use-Rlog/RLOG-RIL-IPC: ================================================================================
D use-Rlog/RLOG-RIL: 11 RIL requests in the queue (0 pending, 5 handled, 6 unhandled)
D use-Rlog/RLOG-RIL-IPC: 
D use-Rlog/RLOG-RIL-IPC: xmm626_sec_modem_fmt_recv: Received FMT message
D use-Rlog/RLOG-RIL-IPC: xmm626_sec_modem_fmt_recv: Message: aseq=0x0c, command=IPC_NET_REGIST, type=IPC_TYPE_RESP, size=11
D use-Rlog/RLOG-RIL-IPC: ================================= IPC FMT data =================================
D use-Rlog/RLOG-RIL-IPC: [0000]   FF 03 01 00 00 00 00 00  00 00 00                  ........ ...
D use-Rlog/RLOG-RIL-IPC: ================================================================================
D use-Rlog/RLOG-RIL: 10 RIL requests in the queue (0 pending, 4 handled, 6 unhandled)
D use-Rlog/RLOG-RIL-IPC: 
D use-Rlog/RLOG-RIL-IPC: xmm626_sec_modem_fmt_recv: Received FMT message
D use-Rlog/RLOG-RIL-IPC: xmm626_sec_modem_fmt_recv: Message: aseq=0x0d, command=IPC_CALL_LIST, type=IPC_TYPE_RESP, size=1
D use-Rlog/RLOG-RIL-IPC: ================================= IPC FMT data =================================
D use-Rlog/RLOG-RIL-IPC: [0000]   00                                                 .
D use-Rlog/RLOG-RIL-IPC: ================================================================================
D use-Rlog/RLOG-RIL: 9 RIL requests in the queue (0 pending, 3 handled, 6 unhandled)
D use-Rlog/RLOG-RIL-IPC: 
D use-Rlog/RLOG-RIL-IPC: xmm626_sec_modem_fmt_send: Sent FMT message
D use-Rlog/RLOG-RIL-IPC: xmm626_sec_modem_fmt_send: Message: mseq=0x10, command=IPC_NET_SERVING_NETWORK, type=IPC_TYPE_GET, size=0
D RILJ    : [3704]> VOICE_REGISTRATION_STATE [SUB0]
D use-Rlog/RLOG-RIL-IPC: 
D RILJ    : [3687]< QUERY_NETWORK_SELECTION_MODE {0} [SUB0]
D use-Rlog/RLOG-RIL-IPC: xmm626_sec_modem_fmt_send: Sent FMT message
D use-Rlog/RLOG-RIL-IPC: xmm626_sec_modem_fmt_send: Message: mseq=0x11, command=IPC_NET_REGIST, type=IPC_TYPE_GET, size=2
D use-Rlog/RLOG-RIL-IPC: ================================= IPC FMT data =================================
D use-Rlog/RLOG-RIL-IPC: [0000]   FF 03                                              ..
D use-Rlog/RLOG-RIL-IPC: ================================================================================
D use-Rlog/RLOG-RIL: 10 RIL requests in the queue (1 pending, 5 handled, 4 unhandled)
D use-Rlog/RLOG-RIL: 11 RIL requests in the queue (2 pending, 5 handled, 4 unhandled)
D use-Rlog/RLOG-RIL-IPC: 
D use-Rlog/RLOG-RIL-IPC: xmm626_sec_modem_fmt_recv: Received FMT message
D use-Rlog/RLOG-RIL-IPC: xmm626_sec_modem_fmt_recv: Message: aseq=0x0e, command=IPC_NET_REGIST, type=IPC_TYPE_RESP, size=11
D use-Rlog/RLOG-RIL-IPC: ================================= IPC FMT data =================================
D use-Rlog/RLOG-RIL-IPC: [0000]   FF 02 01 00 00 00 00 00  00 00 00                  ........ ...
D use-Rlog/RLOG-RIL-IPC: ================================================================================
D use-Rlog/RLOG-RIL: 10 RIL requests in the queue (0 pending, 4 handled, 6 unhandled)
D use-Rlog/RLOG-RIL-IPC: 
D use-Rlog/RLOG-RIL-IPC: xmm626_sec_modem_fmt_send: Sent FMT message
D use-Rlog/RLOG-RIL-IPC: xmm626_sec_modem_fmt_send: Message: mseq=0x12, command=IPC_NET_REGIST, type=IPC_TYPE_GET, size=2
D use-Rlog/RLOG-RIL-IPC: ================================= IPC FMT data =================================
D use-Rlog/RLOG-RIL-IPC: [0000]   FF 02                                              ..
D use-Rlog/RLOG-RIL-IPC: ================================================================================
D use-Rlog/RLOG-RIL-IPC: 
D use-Rlog/RLOG-RIL-IPC: xmm626_sec_modem_fmt_recv: Received FMT message
D use-Rlog/RLOG-RIL-IPC: xmm626_sec_modem_fmt_recv: Message: aseq=0x0f, command=IPC_NET_PLMN_SEL, type=IPC_TYPE_RESP, size=1
D use-Rlog/RLOG-RIL-IPC: ================================= IPC FMT data =================================
D use-Rlog/RLOG-RIL-IPC: [0000]   02                                                 .
D RILJ    : [3705]> QUERY_NETWORK_SELECTION_MODE [SUB0]
D use-Rlog/RLOG-RIL-IPC: ================================================================================
D RILJ    : [3684]< OPERATOR {null, null, 00000} [SUB0]
D use-Rlog/RLOG-RIL: 9 RIL requests in the queue (0 pending, 4 handled, 5 unhandled)
D use-Rlog/RLOG-RIL: 10 RIL requests in the queue (1 pending, 4 handled, 5 unhandled)
D use-Rlog/RLOG-RIL-IPC: 
D use-Rlog/RLOG-RIL-IPC: xmm626_sec_modem_fmt_recv: Received FMT message
D use-Rlog/RLOG-RIL-IPC: xmm626_sec_modem_fmt_recv: Message: aseq=0x10, command=IPC_NET_SERVING_NETWORK, type=IPC_TYPE_RESP, size=11
D use-Rlog/RLOG-RIL-IPC: ================================= IPC FMT data =================================
D use-Rlog/RLOG-RIL-IPC: [0000]   02 05 FF 30 30 30 30 30  23 00 00                  ...00000 #..
D use-Rlog/RLOG-RIL-IPC: ================================================================================
D use-Rlog/RLOG-RIL: 9 RIL requests in the queue (0 pending, 3 handled, 6 unhandled)
D use-Rlog/RLOG-RIL-IPC: 
D use-Rlog/RLOG-RIL-IPC: xmm626_sec_modem_fmt_recv: Received FMT message
D use-Rlog/RLOG-RIL-IPC: xmm626_sec_modem_fmt_recv: Message: aseq=0x11, command=IPC_NET_REGIST, type=IPC_TYPE_RESP, size=11
D use-Rlog/RLOG-RIL-IPC: ================================= IPC FMT data =================================
D use-Rlog/RLOG-RIL-IPC: [0000]   FF 03 01 00 00 00 00 00  00 00 00                  ........ ...
D use-Rlog/RLOG-RIL-IPC: ================================================================================
D use-Rlog/RLOG-RIL: 8 RIL requests in the queue (0 pending, 2 handled, 6 unhandled)
D use-Rlog/RLOG-RIL-IPC: 
D use-Rlog/RLOG-RIL-IPC: xmm626_sec_modem_fmt_recv: Received FMT message
D use-Rlog/RLOG-RIL-IPC: xmm626_sec_modem_fmt_recv: Message: aseq=0x12, command=IPC_NET_REGIST, type=IPC_TYPE_RESP, size=11
D use-Rlog/RLOG-RIL-IPC: ================================= IPC FMT data =================================
D use-Rlog/RLOG-RIL-IPC: [0000]   FF 02 01 00 00 00 00 00  00 00 00                  ........ ...
D RILJ    : [3692]< QUERY_NETWORK_SELECTION_MODE {0} [SUB0]
D use-Rlog/RLOG-RIL-IPC: ================================================================================
D use-Rlog/RLOG-RIL: 7 RIL requests in the queue (0 pending, 1 handled, 6 unhandled)
D use-Rlog/RLOG-RIL-IPC: 
D use-Rlog/RLOG-RIL-IPC: xmm626_sec_modem_fmt_send: Sent FMT message
D RILJ    : [3690]< DATA_REGISTRATION_STATE {0, 0, 0, 0, 3} [SUB0]
D use-Rlog/RLOG-RIL-IPC: xmm626_sec_modem_fmt_send: Message: mseq=0x13, command=IPC_NET_SERVING_NETWORK, type=IPC_TYPE_GET, size=0
D use-Rlog/RLOG-RIL-IPC: 
D use-Rlog/RLOG-RIL-IPC: xmm626_sec_modem_fmt_send: Sent FMT message
D use-Rlog/RLOG-RIL-IPC: xmm626_sec_modem_fmt_send: Message: mseq=0x14, command=IPC_NET_REGIST, type=IPC_TYPE_GET, size=2
D use-Rlog/RLOG-RIL-IPC: ================================= IPC FMT data =================================
D SubscriptionController: [getSubId]- sSlotIdxToSubId.size == 0, return DummySubIds slotIdx=0
D use-Rlog/RLOG-RIL-IPC: [0000]   FF 03                                              ..
D RILJ    : [3694]< GET_CURRENT_CALLS {} [SUB0]
D use-Rlog/RLOG-RIL-IPC: ================================================================================
D use-Rlog/RLOG-RIL-IPC: 
D use-Rlog/RLOG-RIL-IPC: xmm626_sec_modem_fmt_send: Sent FMT message
D use-Rlog/RLOG-RIL-IPC: xmm626_sec_modem_fmt_send: Message: mseq=0x15, command=IPC_NET_REGIST, type=IPC_TYPE_GET, size=2
D use-Rlog/RLOG-RIL-IPC: ================================= IPC FMT data =================================
D use-Rlog/RLOG-RIL-IPC: [0000]   FF 02                                              ..
D DefaultPhoneNotifier: notifySignalStrength: mRegistry=com.android.internal.telephony.ITelephonyRegistry$Stub$Proxy@5667eb9 ss=SignalStrength: 1 99 -120 -160 -120 -1 -1 99 2147483647 2147483647 2147483647 -1 2147483647 gsm|lte sender=Handler (com.android.internal.telephony.gsm.GSMPhone) {6bf8468}
D use-Rlog/RLOG-RIL-IPC: ================================================================================
D RILJ    : [3691]< VOICE_REGISTRATION_STATE {0, 0, 0, 0, null, null, null, null, null, null, null, null, null, null, null} [SUB0]
D use-Rlog/RLOG-RIL: 8 RIL requests in the queue (1 pending, 4 handled, 3 unhandled)
D use-Rlog/RLOG-RIL-IPC: 
D use-Rlog/RLOG-RIL-IPC: xmm626_sec_modem_fmt_send: Sent FMT message
D use-Rlog/RLOG-RIL-IPC: xmm626_sec_modem_fmt_send: Message: mseq=0x16, command=IPC_NET_PLMN_SEL, type=IPC_TYPE_GET, size=0
D RILJ    : [3701]< QUERY_NETWORK_SELECTION_MODE {0} [SUB0]
D RILJ    : [3689]< OPERATOR {null, null, 00000} [SUB0]
D use-Rlog/RLOG-RIL-IPC: 
D use-Rlog/RLOG-RIL-IPC: xmm626_sec_modem_fmt_recv: Received FMT message
D use-Rlog/RLOG-RIL-IPC: xmm626_sec_modem_fmt_recv: Message: aseq=0x13, command=IPC_NET_SERVING_NETWORK, type=IPC_TYPE_RESP, size=11
D use-Rlog/RLOG-RIL-IPC: ================================= IPC FMT data =================================
D RILJ    : [3699]< DATA_REGISTRATION_STATE {0, 0, 0, 0, 3} [SUB0]
D use-Rlog/RLOG-RIL-IPC: [0000]   02 05 FF 30 30 30 30 30  23 00 00                  ...00000 #..
D use-Rlog/RLOG-RIL-IPC: ================================================================================
D use-Rlog/RLOG-RIL: 7 RIL requests in the queue (0 pending, 4 handled, 3 unhandled)
D RILJ    : [3700]< VOICE_REGISTRATION_STATE {0, 0, 0, 0, null, null, null, null, null, null, null, null, null, null, null} [SUB0]
D use-Rlog/RLOG-RIL-IPC: 
D use-Rlog/RLOG-RIL-IPC: xmm626_sec_modem_fmt_send: Sent FMT message
D use-Rlog/RLOG-RIL-IPC: xmm626_sec_modem_fmt_send: Message: mseq=0x17, command=IPC_NET_SERVING_NETWORK, type=IPC_TYPE_GET, size=0
D use-Rlog/RLOG-RIL-IPC: 
D use-Rlog/RLOG-RIL-IPC: xmm626_sec_modem_fmt_recv: Received FMT message
D use-Rlog/RLOG-RIL-IPC: xmm626_sec_modem_fmt_recv: Message: aseq=0x14, command=IPC_NET_REGIST, type=IPC_TYPE_RESP, size=11
D use-Rlog/RLOG-RIL-IPC: ================================= IPC FMT data =================================
D RILJ    : [3698]< OPERATOR {null, null, 00000} [SUB0]
D use-Rlog/RLOG-RIL-IPC: [0000]   FF 03 01 00 00 00 00 00  00 00 00                  ........ ...
D use-Rlog/RLOG-RIL-IPC: ================================================================================
D use-Rlog/RLOG-RIL: 6 RIL requests in the queue (0 pending, 4 handled, 2 unhandled)
D TelephonyRegistry: notifySignalStrengthForSubscriber: invalid phoneId=-1
D PhoneProxy: [PhoneProxy] EVENT_REQUEST_VOICE_RADIO_TECH_DONE: newVoiceTech=3
D PhoneProxy: [PhoneProxy] phoneObjectUpdater: newVoiceRadioTech=3
D PhoneProxy: [PhoneProxy] phoneObjectUpdater: No change ignore, newVoiceRadioTech=3 mActivePhone=GSM
D CdmaSSM : CDMA_SUBSCRIPTION_SOURCE event = 2
D use-Rlog/RLOG-RIL-IPC: 
E RIL_ImsSms: IMS State query failed with exp com.android.internal.telephony.CommandException: REQUEST_NOT_SUPPORTED
D use-Rlog/RLOG-RIL-IPC: xmm626_sec_modem_fmt_recv: Received FMT message
D use-Rlog/RLOG-RIL-IPC: xmm626_sec_modem_fmt_recv: Message: aseq=0x15, command=IPC_NET_REGIST, type=IPC_TYPE_RESP, size=11
D GSMPhone: Baseband version: I9300BUUGNF1
D use-Rlog/RLOG-RIL-IPC: ================================= IPC FMT data =================================
D use-Rlog/RLOG-RIL-IPC: [0000]   FF 02 01 00 00 00 00 00  00 00 00                  ........ ...
D use-Rlog/RLOG-RIL-IPC: ================================================================================
D use-Rlog/RLOG-RIL: 5 RIL requests in the queue (0 pending, 3 handled, 2 unhandled)
D use-Rlog/RLOG-RIL-IPC: 
D use-Rlog/RLOG-RIL-IPC: xmm626_sec_modem_fmt_recv: Received FMT message
D use-Rlog/RLOG-RIL-IPC: xmm626_sec_modem_fmt_recv: Message: aseq=0x16, command=IPC_NET_PLMN_SEL, type=IPC_TYPE_RESP, size=1
D use-Rlog/RLOG-RIL-IPC: ================================= IPC FMT data =================================
D use-Rlog/RLOG-RIL-IPC: [0000]   02                                                 .
D use-Rlog/RLOG-RIL-IPC: ================================================================================
D use-Rlog/RLOG-RIL: 4 RIL requests in the queue (0 pending, 2 handled, 2 unhandled)
D use-Rlog/RLOG-RIL-IPC: 
D use-Rlog/RLOG-RIL-IPC: xmm626_sec_modem_fmt_recv: Received FMT message
D use-Rlog/RLOG-RIL-IPC: xmm626_sec_modem_fmt_recv: Message: aseq=0x17, command=IPC_NET_SERVING_NETWORK, type=IPC_TYPE_RESP, size=11
D use-Rlog/RLOG-RIL-IPC: ================================= IPC FMT data =================================
D use-Rlog/RLOG-RIL-IPC: [0000]   02 05 FF 30 30 30 30 30  23 00 00                  ...00000 #..
D use-Rlog/RLOG-RIL-IPC: ================================================================================
D use-Rlog/RLOG-RIL: 3 RIL requests in the queue (0 pending, 1 handled, 2 unhandled)
D RILJ    : [3703]< DATA_REGISTRATION_STATE {0, 0, 0, 0, 3} [SUB0]
D PHONE   : [ServiceState] setDataRegState=1
D RILJ    : [3704]< VOICE_REGISTRATION_STATE {0, 0, 0, 0, null, null, null, null, null, null, null, null, null, null, null} [SUB0]
D PHONE   : [ServiceState] setDataRadioTechnology=0
D GsmSST  : [GsmSST] handlPollStateResultMessage: GsmSST setDataRegState=1 regState=0 dataRadioTechnology=0
D PHONE   : [ServiceState] setVoiceRegState=1
E PHONE   : [ServiceState] setState deprecated use setVoiceRegState()
D RILJ    : [3705]< QUERY_NETWORK_SELECTION_MODE {0} [SUB0]
D RILJ    : [3702]< OPERATOR {null, null, 00000} [SUB0]
D SubscriptionController: [getSubId]- sSlotIdxToSubId.size == 0, return DummySubIds slotIdx=0
D GsmSST  : [GsmSST] Poll ServiceState done:  oldSS=[3 3 voice home data home null null null null null null  Unknown Unknown CSS not supported -1 -1 RoamInd=-1 DefRoamInd=-1 EmergOnly=false IsDataRoamingFromRegistration=false] newSS=[1 1 voice home data home null null 00000 null null 00000  Unknown Unknown CSS not supported -1 -1 RoamInd=-1 DefRoamInd=-1 EmergOnly=false IsDataRoamingFromRegistration=false] oldMaxDataCalls=1 mNewMaxDataCalls=1 oldReasonDataDenied=-1 mNewReasonDataDenied=-1
D PHONE   : [ServiceState] setNullState=1
D GsmSST  : [GsmSST] updateSpnDisplay: radio is on but out of service, set plmn='No service.'
D SubscriptionController: [getSubId]- sSlotIdxToSubId.size == 0, return DummySubIds slotIdx=0
D GsmSST  : [GsmSST] updateSpnDisplay: changed sending intent rule=0 showPlmn='true' plmn='No service.' showSpn='false' spn='' dataSpn='' subId='-2'
D SubscriptionController: [getSubId]- sSlotIdxToSubId.size == 0, return DummySubIds slotIdx=0
D SubscriptionController: [getSubId]- sSlotIdxToSubId.size == 0, return DummySubIds slotIdx=0
D SubscriptionController: [setPlmnSpn] No valid subscription to store info
D SubscriptionController: notifySubscriptionInfoChanged:
D SubscriptionController: [getActiveSubInfoList]+
D SubscriptionController: selection:sim_id>=0 null
D TelephonyManager: setTelephonyProperty: success phoneId=0 property=gsm.operator.alpha value: null propVal=null
D TelephonyManager: setTelephonyProperty: success phoneId=0 property=gsm.operator.numeric value: 00000 propVal=00000
D GsmSST  : [GsmSST] update mccmnc=00000 fromServiceState=true
D SubscriptionController: [getActiveSubInfoList]+
D SubscriptionController: [getActiveSubInfoList]+
D SubscriptionController: [getActiveSubInfoList]+
D SubscriptionController: selection:sim_id>=0 null
D SubscriptionController: selection:sim_id>=0 null
D SubscriptionController: selection:sim_id>=0 null
D SubscriptionController: [getActiveSubInfoList]- no info return
D SubscriptionController: [getSubId]- sSlotIdxToSubId.size == 0, return DummySubIds slotIdx=0
D SubscriptionController: [getActiveSubInfoList]- no info return
D SubscriptionController: [getActiveSubInfoList]- no info return
D SubscriptionController: [getActiveSubInfoList]- no info return
D TelephonyManager: setTelephonyProperty: success phoneId=0 property=gsm.operator.iso-country value:  propVal=
D GsmSST  : [GsmSST] shouldFixTimeZoneNow: retVal=false iccCardExist=false operatorNumeric=00000 mcc=0 prevOperatorNumeric= prevMcc=1 needToFixTimeZone=false ltod=10-08 13:22:00.137
D TelephonyManager: setTelephonyProperty: success phoneId=0 property=gsm.operator.isroaming value: false propVal=false
D GsmSST  : [GsmSST] Broadcasting ServiceState : 1 1 voice home data home null null 00000 null null 00000  Unknown Unknown CSS not supported -1 -1 RoamInd=-1 DefRoamInd=-1 EmergOnly=false IsDataRoamingFromRegistration=false
D SubscriptionController: [getSubId]- sSlotIdxToSubId.size == 0, return DummySubIds slotIdx=0
D DefaultPhoneNotifier: nofityServiceState: mRegistry=com.android.internal.telephony.ITelephonyRegistry$Stub$Proxy@5667eb9 ss=1 1 voice home data home null null 00000 null null 00000  Unknown Unknown CSS not supported -1 -1 RoamInd=-1 DefRoamInd=-1 EmergOnly=false IsDataRoamingFromRegistration=false sender=Handler (com.android.internal.telephony.gsm.GSMPhone) {6bf8468} phondId=0 subId=-2
D SubscriptionController: [getSlotId]- subId invalid
D SubscriptionController: getSimStateForSlotIdx:  simState=NOT_READY ordinal=6
D use-Rlog/RLOG-RIL-IPC: Reading RFS data failed
E use-Rlog/RLOG-RIL-IPC: Receiving from IPC RFS client failed
E use-Rlog/RLOG-RIL: IPC RFS client loop failed
D SubscriptionManager: getSimStateForSubscriber: simState=6 slotIdx=0
D TelephonyManager: getSimState: default sim:-1, sim state for slotIdx=0 is 6, return state as unknown
D GsmSST  : [GsmSST] notifyDataRegStateRilRadioTechnologyChanged: drs=1 rat=0
D TelephonyManager: setTelephonyProperty: success phoneId=0 property=gsm.network.type value: Unknown propVal=Unknown
D DCT     : [0]get all active apn types
D SubscriptionController: [getSubId]- sSlotIdxToSubId.size == 0, return DummySubIds slotIdx=0
D GsmSST  : [GsmSST] getCellLocation(): X good mCellLoc=[0,0,-1]
D TelephonyRegistry: notifyCellLocationForSubscriber: subId=-2 cellLocation=Bundle[mParcelledData.dataSize=64]
D GsmSST  : [GsmSST] SubscriptionListener.onSubscriptionInfoChanged
D SubscriptionController: [getSubId]- sSlotIdxToSubId.size == 0, return DummySubIds slotIdx=0
D DCT     : [0]SubscriptionListener.onSubscriptionInfoChanged
D SubscriptionController: [getSubId]- sSlotIdxToSubId.size == 0, return DummySubIds slotIdx=0
D SubscriptionController: [getActiveSubInfoList]+
D SubscriptionController: selection:sim_id>=0 null
D SubscriptionController: [getActiveSubInfoList]- no info return
E PhoneBase: Error! unregisterForCallWaiting() in PhoneBase should not be called, CDMAPhone inactive.
D SubscriptionController: [getSubId]- sSlotIdxToSubId.size == 0, return DummySubIds slotIdx=0
D SubscriptionController: [getSubId]- sSlotIdxToSubId.size == 0, return DummySubIds slotIdx=0
D SubscriptionController: [getPhoneId]- invalid subId return=-1
D SubscriptionController: [getSubId]- sSlotIdxToSubId.size == 0, return DummySubIds slotIdx=0
D SubscriptionController: [getSubId]- sSlotIdxToSubId.size == 0, return DummySubIds slotIdx=0
D SubscriptionController: [getSubId]- sSlotIdxToSubId.size == 0, return DummySubIds slotIdx=0
E PhoneBase: Error! registerForCallWaiting() in PhoneBase should not be called, CDMAPhone inactive.
D SubscriptionController: [getSubId]- sSlotIdxToSubId.size == 0, return DummySubIds slotIdx=0
D DCT     : [0]handleMessage msg={ when=-54ms what=270377 obj=android.os.AsyncResult@60697ca target=com.android.internal.telephony.dataconnection.DcTracker }
D DCT     : [0]onUpdateIcc: newIccRecords null
D DCT     : [0]setupDataOnConnectableApns: nwTypeChanged
D DCT     : [0]setupDataOnConnectableApns: apnContext {mApnType=dun mState=IDLE mWaitingApns={null} mWaitingApnsPermanentFailureCountDown=0 mApnSetting={null} mReason=radioTurnedOff mDataEnabled=false mDependencyMet=true}
D DCT     : [0]setupDataOnConnectableApns: apnContext {mApnType=hipri mState=IDLE mWaitingApns={null} mWaitingApnsPermanentFailureCountDown=0 mApnSetting={null} mReason=radioTurnedOff mDataEnabled=false mDependencyMet=true}
D DCT     : [0]setupDataOnConnectableApns: apnContext {mApnType=supl mState=IDLE mWaitingApns={null} mWaitingApnsPermanentFailureCountDown=0 mApnSetting={null} mReason=radioTurnedOff mDataEnabled=false mDependencyMet=true}
D DCT     : [0]setupDataOnConnectableApns: apnContext {mApnType=default mState=IDLE mWaitingApns={null} mWaitingApnsPermanentFailureCountDown=0 mApnSetting={null} mReason=radioTurnedOff mDataEnabled=false mDependencyMet=true}
D DCT     : [0]setupDataOnConnectableApns: apnContext {mApnType=mms mState=IDLE mWaitingApns={null} mWaitingApnsPermanentFailureCountDown=0 mApnSetting={null} mReason=radioTurnedOff mDataEnabled=false mDependencyMet=true}
D DctController: handleMessage msg={ when=-53ms what=107 target=com.android.internal.telephony.dataconnection.DctController }
D DctController: onSubInfoReady mPhoneNum=1
D SubscriptionController: [getSubId]- sSlotIdxToSubId.size == 0, return DummySubIds slotIdx=0
D DctController: onSubInfoReady handle pending requests subId=-2
D DctController: onSubInfoReady: SIM card absent on phoneId = 0
D SubscriptionController: [getSubId]- sSlotIdxToSubId.size == 0, return DummySubIds slotIdx=0
D DctController: [TNF -2]evalPendingRequest, pending request size is 1
D SubscriptionController: [getSubId]- sSlotIdxToSubId.size == 0, return DummySubIds slotIdx=0
D DctController: [TNF -2]evalPendingRequest: request = NetworkRequest [ id=1, legacyType=-1, [ Capabilities: INTERNET&NOT_RESTRICTED&TRUSTED&NOT_VPN] ]
D SubscriptionController: [getSubId]- sSlotIdxToSubId.size == 0, return DummySubIds slotIdx=0
D DctController: [TNF -2]Cellular needs Network for NetworkRequest [ id=1, legacyType=-1, [ Capabilities: INTERNET&NOT_RESTRICTED&TRUSTED&NOT_VPN] ]
D SubscriptionController: [getSubId]- sSlotIdxToSubId.size == 0, return DummySubIds slotIdx=0
D SubscriptionController: [getSubId]- sSlotIdxToSubId.size == 0, return DummySubIds slotIdx=0
D DctController: [TNF -2]Request not useable, pending request.
D DctController: processRequests
D SubscriptionController: [getSubId]- sSlotIdxToSubId.size == 0, return DummySubIds slotIdx=0
D DctController: handleMessage msg={ when=-2ms what=100 target=com.android.internal.telephony.dataconnection.DctController }
D DcSwitchAsyncChannel: [DcSwitchAsyncChannel-0]: rspIsIdle=true
D use-Rlog/RLOG-RIL: Closed IPC RFS client
D SubscriptionController: [getPhoneId]- invalid subId return=-1
D DcSwitchAsyncChannel: [DcSwitchAsyncChannel-0]: rspIsIdle=true
D DctController: onProcessRequest requestedPhoneId=-1, activePhoneId=-1
D use-Rlog/RLOG-RIL: Opened IPC RFS client
D DCT     : [0]hasMatchedTetherApnSetting: APN=null
D GsmSST  : [GsmSST] updateSpnDisplay: radio is on but out of service, set plmn='No service'
D SubscriptionController: [getSubId]- sSlotIdxToSubId.size == 0, return DummySubIds slotIdx=0
D GsmSST  : [GsmSST] updateSpnDisplay: changed sending intent rule=0 showPlmn='true' plmn='No service' showSpn='false' spn='' dataSpn='' subId='-2'
D SubscriptionController: [getSubId]- sSlotIdxToSubId.size == 0, return DummySubIds slotIdx=0
D SubscriptionController: [getSubId]- sSlotIdxToSubId.size == 0, return DummySubIds slotIdx=0
D SubscriptionController: [setPlmnSpn] No valid subscription to store info
D SubscriptionController: notifySubscriptionInfoChanged:
D SubscriptionController: [getActiveSubInfoList]+
D SubscriptionController: selection:sim_id>=0 null
D GsmSST  : [GsmSST] SubscriptionListener.onSubscriptionInfoChanged
D SubscriptionController: [getSubId]- sSlotIdxToSubId.size == 0, return DummySubIds slotIdx=0
D DCT     : [0]SubscriptionListener.onSubscriptionInfoChanged
D SubscriptionController: [getSubId]- sSlotIdxToSubId.size == 0, return DummySubIds slotIdx=0
D SubscriptionController: [getActiveSubInfoList]+
D SubscriptionController: selection:sim_id>=0 null
D SubscriptionController: [getActiveSubInfoList]- no info return
D SubscriptionController: [getActiveSubInfoList]- no info return
E PhoneBase: Error! unregisterForCallWaiting() in PhoneBase should not be called, CDMAPhone inactive.
D SubscriptionController: [getSubId]- sSlotIdxToSubId.size == 0, return DummySubIds slotIdx=0
D SubscriptionController: [getSubId]- sSlotIdxToSubId.size == 0, return DummySubIds slotIdx=0
D SubscriptionController: [getPhoneId]- invalid subId return=-1
D SubscriptionController: [getSubId]- sSlotIdxToSubId.size == 0, return DummySubIds slotIdx=0
D SubscriptionController: [getSubId]- sSlotIdxToSubId.size == 0, return DummySubIds slotIdx=0
D SubscriptionController: [getSubId]- sSlotIdxToSubId.size == 0, return DummySubIds slotIdx=0
E PhoneBase: Error! registerForCallWaiting() in PhoneBase should not be called, CDMAPhone inactive.
D DctController: handleMessage msg={ when=-161ms what=107 target=com.android.internal.telephony.dataconnection.DctController }
D DctController: onSubInfoReady mPhoneNum=1
D SubscriptionController: [getSubId]- sSlotIdxToSubId.size == 0, return DummySubIds slotIdx=0
D DctController: onSubInfoReady handle pending requests subId=-2
D DctController: onSubInfoReady: SIM card absent on phoneId = 0
D SubscriptionController: [getSubId]- sSlotIdxToSubId.size == 0, return DummySubIds slotIdx=0
D DctController: [TNF -2]evalPendingRequest, pending request size is 1
D SubscriptionController: [getSubId]- sSlotIdxToSubId.size == 0, return DummySubIds slotIdx=0
D DctController: [TNF -2]evalPendingRequest: request = NetworkRequest [ id=1, legacyType=-1, [ Capabilities: INTERNET&NOT_RESTRICTED&TRUSTED&NOT_VPN] ]
D SubscriptionController: [getSubId]- sSlotIdxToSubId.size == 0, return DummySubIds slotIdx=0
D DctController: [TNF -2]Cellular needs Network for NetworkRequest [ id=1, legacyType=-1, [ Capabilities: INTERNET&NOT_RESTRICTED&TRUSTED&NOT_VPN] ]
D SubscriptionController: [getSubId]- sSlotIdxToSubId.size == 0, return DummySubIds slotIdx=0
D SubscriptionController: [getSubId]- sSlotIdxToSubId.size == 0, return DummySubIds slotIdx=0
D DctController: [TNF -2]Request not useable, pending request.
D DctController: processRequests
D SubscriptionController: [getSubId]- sSlotIdxToSubId.size == 0, return DummySubIds slotIdx=0
D DctController: handleMessage msg={ when=-55ms what=100 target=com.android.internal.telephony.dataconnection.DctController }
D DcSwitchAsyncChannel: [DcSwitchAsyncChannel-0]: rspIsIdle=true
D SubscriptionController: [getPhoneId]- invalid subId return=-1
D DcSwitchAsyncChannel: [DcSwitchAsyncChannel-0]: rspIsIdle=true
D DctController: onProcessRequest requestedPhoneId=-1, activePhoneId=-1
D SubscriptionController: [getActiveSubInfoList]+
D SubscriptionController: selection:sim_id>=0 null
D SubscriptionController: [getActiveSubInfoList]- no info return
D SubscriptionController: [getSubId]- sSlotIdxToSubId.size == 0, return DummySubIds slotIdx=0
D SubscriptionController: getSimStateForSlotIdx:  simState=NOT_READY ordinal=6
D SubscriptionManager: getSimStateForSubscriber: simState=6 slotIdx=0
D SubscriptionController: getSimStateForSlotIdx:  simState=NOT_READY ordinal=6
D SubscriptionManager: getSimStateForSubscriber: simState=6 slotIdx=0
D SubscriptionController: getSimStateForSlotIdx:  simState=NOT_READY ordinal=6
D SubscriptionManager: getSimStateForSubscriber: simState=6 slotIdx=0
D SubscriptionController: [getActiveSubInfoList]+
D SubscriptionController: [getActiveSubInfoList]+
D SubscriptionController: selection:sim_id>=0 null
D SubscriptionController: selection:sim_id>=0 null
D SubscriptionController: [getActiveSubInfoList]- no info return
D SubscriptionController: [getActiveSubInfoList]- no info return
D CAT     : com.android.stk.StkAppService: onCreate()+
D CAT     : com.android.stk.StkAppService: simCount: 1
D CAT     : com.android.stk.StkAppService: slotId: 0
D CAT     : com.android.stk.StkAppService: onStart sim id: 0, op: 11, *****
D CAT     : com.android.stk.StkAppService: mStkService is: -1
D CAT     : StkAppInstaller: [setAppState]+
D CAT     : StkAppInstaller: Need not change app state!!
D CAT     : StkAppInstaller: [setAppState]-
D CAT     : com.android.stk.StkAppService: onDestroy()
D GsmSST  : [GsmSST] updateSpnDisplay: radio is on but out of service, set plmn='No service.'
D SubscriptionController: [getSubId]- sSlotIdxToSubId.size == 0, return DummySubIds slotIdx=0
D DCT     : [0]hasMatchedTetherApnSetting: APN=null
D GsmSST  : [GsmSST] updateSpnDisplay: changed sending intent rule=0 showPlmn='true' plmn='No service.' showSpn='false' spn='' dataSpn='' subId='-2'
D SubscriptionController: [getSubId]- sSlotIdxToSubId.size == 0, return DummySubIds slotIdx=0
D SubscriptionController: [getSubId]- sSlotIdxToSubId.size == 0, return DummySubIds slotIdx=0
D SubscriptionController: [setPlmnSpn] No valid subscription to store info
D SubscriptionController: notifySubscriptionInfoChanged:
D GsmSST  : [GsmSST] SubscriptionListener.onSubscriptionInfoChanged
D SubscriptionController: [getSubId]- sSlotIdxToSubId.size == 0, return DummySubIds slotIdx=0
D SubscriptionController: [getActiveSubInfoList]+
D SubscriptionController: selection:sim_id>=0 null
D SubscriptionController: [getActiveSubInfoList]- no info return
E PhoneBase: Error! unregisterForCallWaiting() in PhoneBase should not be called, CDMAPhone inactive.
D SubscriptionController: [getSubId]- sSlotIdxToSubId.size == 0, return DummySubIds slotIdx=0
D SubscriptionController: [getSubId]- sSlotIdxToSubId.size == 0, return DummySubIds slotIdx=0
D SubscriptionController: [getPhoneId]- invalid subId return=-1
D SubscriptionController: [getSubId]- sSlotIdxToSubId.size == 0, return DummySubIds slotIdx=0
D SubscriptionController: [getSubId]- sSlotIdxToSubId.size == 0, return DummySubIds slotIdx=0
D SubscriptionController: [getSubId]- sSlotIdxToSubId.size == 0, return DummySubIds slotIdx=0
D SubscriptionController: [getActiveSubInfoList]+
D SubscriptionController: [getActiveSubInfoList]+
D SubscriptionController: selection:sim_id>=0 null
D SubscriptionController: selection:sim_id>=0 null
D SubscriptionController: [getActiveSubInfoList]+
D SubscriptionController: selection:sim_id>=0 null
D SubscriptionController: [getActiveSubInfoList]- no info return
D SubscriptionController: [getActiveSubInfoList]- no info return
E PhoneBase: Error! registerForCallWaiting() in PhoneBase should not be called, CDMAPhone inactive.
D DCT     : [0]SubscriptionListener.onSubscriptionInfoChanged
D SubscriptionController: [getSubId]- sSlotIdxToSubId.size == 0, return DummySubIds slotIdx=0
D DctController: handleMessage msg={ when=-75ms what=107 target=com.android.internal.telephony.dataconnection.DctController }
D DctController: onSubInfoReady mPhoneNum=1
D SubscriptionController: [getSubId]- sSlotIdxToSubId.size == 0, return DummySubIds slotIdx=0
D DctController: onSubInfoReady handle pending requests subId=-2
D DctController: onSubInfoReady: SIM card absent on phoneId = 0
D SubscriptionController: [getSubId]- sSlotIdxToSubId.size == 0, return DummySubIds slotIdx=0
D DctController: [TNF -2]evalPendingRequest, pending request size is 1
D SubscriptionController: [getSubId]- sSlotIdxToSubId.size == 0, return DummySubIds slotIdx=0
D DctController: [TNF -2]evalPendingRequest: request = NetworkRequest [ id=1, legacyType=-1, [ Capabilities: INTERNET&NOT_RESTRICTED&TRUSTED&NOT_VPN] ]
D SubscriptionController: [getSubId]- sSlotIdxToSubId.size == 0, return DummySubIds slotIdx=0
D DctController: [TNF -2]Cellular needs Network for NetworkRequest [ id=1, legacyType=-1, [ Capabilities: INTERNET&NOT_RESTRICTED&TRUSTED&NOT_VPN] ]
D SubscriptionController: [getSubId]- sSlotIdxToSubId.size == 0, return DummySubIds slotIdx=0
D SubscriptionController: [getSubId]- sSlotIdxToSubId.size == 0, return DummySubIds slotIdx=0
D DctController: [TNF -2]Request not useable, pending request.
D DctController: processRequests
D SubscriptionController: [getSubId]- sSlotIdxToSubId.size == 0, return DummySubIds slotIdx=0
D DctController: handleMessage msg={ when=-1ms what=100 target=com.android.internal.telephony.dataconnection.DctController }
D DcSwitchAsyncChannel: [DcSwitchAsyncChannel-0]: rspIsIdle=true
D SubscriptionController: [getPhoneId]- invalid subId return=-1
D DcSwitchAsyncChannel: [DcSwitchAsyncChannel-0]: rspIsIdle=true
D DctController: onProcessRequest requestedPhoneId=-1, activePhoneId=-1
D SubscriptionController: [getActiveSubInfoList]- no info return
D SubscriptionController: [getActiveSubInfoList]+
D SubscriptionController: selection:sim_id>=0 null
D SubscriptionController: [getActiveSubInfoList]- no info return
D SubscriptionController: [getSubId]- sSlotIdxToSubId.size == 0, return DummySubIds slotIdx=0
D CAT     : com.android.stk.StkAppService: onCreate()+
D CAT     : com.android.stk.StkAppService: simCount: 1
D CAT     : com.android.stk.StkAppService: slotId: 0
D CAT     : com.android.stk.StkAppService: onStart sim id: 0, op: 11, *****
D CAT     : com.android.stk.StkAppService: mStkService is: -1
D CAT     : StkAppInstaller: [setAppState]+
D CAT     : StkAppInstaller: Need not change app state!!
D CAT     : StkAppInstaller: [setAppState]-
D CAT     : com.android.stk.StkAppService: onDestroy()
D SubscriptionController: getSimStateForSlotIdx:  simState=NOT_READY ordinal=6
D SubscriptionManager: getSimStateForSubscriber: simState=6 slotIdx=0
D SubscriptionController: getSimStateForSlotIdx:  simState=NOT_READY ordinal=6
D SubscriptionManager: getSimStateForSubscriber: simState=6 slotIdx=0
D SubscriptionController: getSimStateForSlotIdx:  simState=NOT_READY ordinal=6
D SubscriptionManager: getSimStateForSubscriber: simState=6 slotIdx=0
D DCT     : [0]hasMatchedTetherApnSetting: APN=null
D GsmSST  : [GsmSST] updateSpnDisplay: radio is on but out of service, set plmn='No service.'
D SubscriptionController: [getSubId]- sSlotIdxToSubId.size == 0, return DummySubIds slotIdx=0
D CAT     : com.android.stk.StkAppService: onCreate()+
D CAT     : com.android.stk.StkAppService: simCount: 1
D CAT     : com.android.stk.StkAppService: slotId: 0
D CAT     : com.android.stk.StkAppService: onStart sim id: 0, op: 11, *****
D CAT     : com.android.stk.StkAppService: mStkService is: -1
D CAT     : StkAppInstaller: [setAppState]+
D CAT     : StkAppInstaller: Need not change app state!!
D CAT     : StkAppInstaller: [setAppState]-
D CAT     : com.android.stk.StkAppService: onDestroy()
D SubscriptionController: getSimStateForSlotIdx:  simState=NOT_READY ordinal=6
D SubscriptionManager: getSimStateForSubscriber: simState=6 slotIdx=0
D SubscriptionController: getSimStateForSlotIdx:  simState=NOT_READY ordinal=6
D SubscriptionManager: getSimStateForSubscriber: simState=6 slotIdx=0
D SubscriptionController: getSimStateForSlotIdx:  simState=NOT_READY ordinal=6
D SubscriptionManager: getSimStateForSubscriber: simState=6 slotIdx=0
D DCT     : [0]hasMatchedTetherApnSetting: APN=null
D GsmSST  : [GsmSST] updateSpnDisplay: radio is on but out of service, set plmn='No service'
D SubscriptionController: [getSubId]- sSlotIdxToSubId.size == 0, return DummySubIds slotIdx=0
D GsmSST  : [GsmSST] updateSpnDisplay: changed sending intent rule=0 showPlmn='true' plmn='No service' showSpn='false' spn='' dataSpn='' subId='-2'
D SubscriptionController: [getSubId]- sSlotIdxToSubId.size == 0, return DummySubIds slotIdx=0
D SubscriptionController: [getSubId]- sSlotIdxToSubId.size == 0, return DummySubIds slotIdx=0
D SubscriptionController: [setPlmnSpn] No valid subscription to store info
D SubscriptionController: notifySubscriptionInfoChanged:
D GsmSST  : [GsmSST] SubscriptionListener.onSubscriptionInfoChanged
D SubscriptionController: [getSubId]- sSlotIdxToSubId.size == 0, return DummySubIds slotIdx=0
D DCT     : [0]SubscriptionListener.onSubscriptionInfoChanged
D SubscriptionController: [getSubId]- sSlotIdxToSubId.size == 0, return DummySubIds slotIdx=0
D SubscriptionController: [getActiveSubInfoList]+
D SubscriptionController: selection:sim_id>=0 null
D SubscriptionController: [getActiveSubInfoList]- no info return
E PhoneBase: Error! unregisterForCallWaiting() in PhoneBase should not be called, CDMAPhone inactive.
D SubscriptionController: [getSubId]- sSlotIdxToSubId.size == 0, return DummySubIds slotIdx=0
D SubscriptionController: [getSubId]- sSlotIdxToSubId.size == 0, return DummySubIds slotIdx=0
D SubscriptionController: [getPhoneId]- invalid subId return=-1
D SubscriptionController: [getSubId]- sSlotIdxToSubId.size == 0, return DummySubIds slotIdx=0
D SubscriptionController: [getSubId]- sSlotIdxToSubId.size == 0, return DummySubIds slotIdx=0
D SubscriptionController: [getSubId]- sSlotIdxToSubId.size == 0, return DummySubIds slotIdx=0
D SubscriptionController: [getActiveSubInfoList]+
E PhoneBase: Error! registerForCallWaiting() in PhoneBase should not be called, CDMAPhone inactive.
D SubscriptionController: selection:sim_id>=0 null
D SubscriptionController: [getActiveSubInfoList]+
D SubscriptionController: selection:sim_id>=0 null
D DctController: handleMessage msg={ when=-110ms what=107 target=com.android.internal.telephony.dataconnection.DctController }
D DctController: onSubInfoReady mPhoneNum=1
D SubscriptionController: [getSubId]- sSlotIdxToSubId.size == 0, return DummySubIds slotIdx=0
D DctController: onSubInfoReady handle pending requests subId=-2
D DctController: onSubInfoReady: SIM card absent on phoneId = 0
D SubscriptionController: [getSubId]- sSlotIdxToSubId.size == 0, return DummySubIds slotIdx=0
D DctController: [TNF -2]evalPendingRequest, pending request size is 1
D SubscriptionController: [getSubId]- sSlotIdxToSubId.size == 0, return DummySubIds slotIdx=0
D DctController: [TNF -2]evalPendingRequest: request = NetworkRequest [ id=1, legacyType=-1, [ Capabilities: INTERNET&NOT_RESTRICTED&TRUSTED&NOT_VPN] ]
D SubscriptionController: [getSubId]- sSlotIdxToSubId.size == 0, return DummySubIds slotIdx=0
D DctController: [TNF -2]Cellular needs Network for NetworkRequest [ id=1, legacyType=-1, [ Capabilities: INTERNET&NOT_RESTRICTED&TRUSTED&NOT_VPN] ]
D SubscriptionController: [getSubId]- sSlotIdxToSubId.size == 0, return DummySubIds slotIdx=0
D SubscriptionController: [getSubId]- sSlotIdxToSubId.size == 0, return DummySubIds slotIdx=0
D DctController: [TNF -2]Request not useable, pending request.
D DctController: processRequests
D SubscriptionController: [getSubId]- sSlotIdxToSubId.size == 0, return DummySubIds slotIdx=0
D DctController: handleMessage msg={ when=-2ms what=100 target=com.android.internal.telephony.dataconnection.DctController }
D DcSwitchAsyncChannel: [DcSwitchAsyncChannel-0]: rspIsIdle=true
D SubscriptionController: [getPhoneId]- invalid subId return=-1
D DcSwitchAsyncChannel: [DcSwitchAsyncChannel-0]: rspIsIdle=true
D DctController: onProcessRequest requestedPhoneId=-1, activePhoneId=-1
D SubscriptionController: [getActiveSubInfoList]+
D SubscriptionController: [getActiveSubInfoList]- no info return
D SubscriptionController: selection:sim_id>=0 null
D SubscriptionController: [getActiveSubInfoList]- no info return
D SubscriptionController: [getActiveSubInfoList]+
D SubscriptionController: selection:sim_id>=0 null
D SubscriptionController: [getActiveSubInfoList]- no info return
D SubscriptionController: [getActiveSubInfoList]- no info return
D SubscriptionController: [getSubId]- sSlotIdxToSubId.size == 0, return DummySubIds slotIdx=0
D CAT     : com.android.stk.StkAppService: onCreate()+
D CAT     : com.android.stk.StkAppService: simCount: 1
D CAT     : com.android.stk.StkAppService: slotId: 0
D CAT     : com.android.stk.StkAppService: onStart sim id: 0, op: 11, *****
D CAT     : com.android.stk.StkAppService: mStkService is: -1
D CAT     : StkAppInstaller: [setAppState]+
D CAT     : StkAppInstaller: Need not change app state!!
D CAT     : StkAppInstaller: [setAppState]-
D CAT     : com.android.stk.StkAppService: onDestroy()
D SubscriptionController: getSimStateForSlotIdx:  simState=NOT_READY ordinal=6
D SubscriptionManager: getSimStateForSubscriber: simState=6 slotIdx=0
D SubscriptionController: getSimStateForSlotIdx:  simState=NOT_READY ordinal=6
D SubscriptionManager: getSimStateForSubscriber: simState=6 slotIdx=0
D SubscriptionController: getSimStateForSlotIdx:  simState=NOT_READY ordinal=6
D SubscriptionManager: getSimStateForSubscriber: simState=6 slotIdx=0
D GsmSST  : [GsmSST] updateSpnDisplay: radio is on but out of service, set plmn='No service.'
D SubscriptionController: [getSubId]- sSlotIdxToSubId.size == 0, return DummySubIds slotIdx=0
D DCT     : [0]hasMatchedTetherApnSetting: APN=null
D GsmSST  : [GsmSST] updateSpnDisplay: changed sending intent rule=0 showPlmn='true' plmn='No service.' showSpn='false' spn='' dataSpn='' subId='-2'
D SubscriptionController: [getSubId]- sSlotIdxToSubId.size == 0, return DummySubIds slotIdx=0
D SubscriptionController: [getSubId]- sSlotIdxToSubId.size == 0, return DummySubIds slotIdx=0
D SubscriptionController: [setPlmnSpn] No valid subscription to store info
D SubscriptionController: notifySubscriptionInfoChanged:
D GsmSST  : [GsmSST] SubscriptionListener.onSubscriptionInfoChanged
D SubscriptionController: [getSubId]- sSlotIdxToSubId.size == 0, return DummySubIds slotIdx=0
D SubscriptionController: [getActiveSubInfoList]+
D SubscriptionController: selection:sim_id>=0 null
D SubscriptionController: [getActiveSubInfoList]- no info return
E PhoneBase: Error! unregisterForCallWaiting() in PhoneBase should not be called, CDMAPhone inactive.
D SubscriptionController: [getSubId]- sSlotIdxToSubId.size == 0, return DummySubIds slotIdx=0
D SubscriptionController: [getSubId]- sSlotIdxToSubId.size == 0, return DummySubIds slotIdx=0
D SubscriptionController: [getPhoneId]- invalid subId return=-1
D SubscriptionController: [getSubId]- sSlotIdxToSubId.size == 0, return DummySubIds slotIdx=0
D SubscriptionController: [getSubId]- sSlotIdxToSubId.size == 0, return DummySubIds slotIdx=0
D SubscriptionController: [getSubId]- sSlotIdxToSubId.size == 0, return DummySubIds slotIdx=0
D SubscriptionController: [getActiveSubInfoList]+
E PhoneBase: Error! registerForCallWaiting() in PhoneBase should not be called, CDMAPhone inactive.
D SubscriptionController: selection:sim_id>=0 null
D SubscriptionController: [getActiveSubInfoList]+
D SubscriptionController: selection:sim_id>=0 null
D DctController: handleMessage msg={ when=-127ms what=107 target=com.android.internal.telephony.dataconnection.DctController }
D DctController: onSubInfoReady mPhoneNum=1
D SubscriptionController: [getSubId]- sSlotIdxToSubId.size == 0, return DummySubIds slotIdx=0
D DctController: onSubInfoReady handle pending requests subId=-2
D DctController: onSubInfoReady: SIM card absent on phoneId = 0
D SubscriptionController: [getSubId]- sSlotIdxToSubId.size == 0, return DummySubIds slotIdx=0
D DctController: [TNF -2]evalPendingRequest, pending request size is 1
D SubscriptionController: [getSubId]- sSlotIdxToSubId.size == 0, return DummySubIds slotIdx=0
D DctController: [TNF -2]evalPendingRequest: request = NetworkRequest [ id=1, legacyType=-1, [ Capabilities: INTERNET&NOT_RESTRICTED&TRUSTED&NOT_VPN] ]
D SubscriptionController: [getSubId]- sSlotIdxToSubId.size == 0, return DummySubIds slotIdx=0
D DctController: [TNF -2]Cellular needs Network for NetworkRequest [ id=1, legacyType=-1, [ Capabilities: INTERNET&NOT_RESTRICTED&TRUSTED&NOT_VPN] ]
D SubscriptionController: [getSubId]- sSlotIdxToSubId.size == 0, return DummySubIds slotIdx=0
D SubscriptionController: [getSubId]- sSlotIdxToSubId.size == 0, return DummySubIds slotIdx=0
D DctController: [TNF -2]Request not useable, pending request.
D DctController: processRequests
D DCT     : [0]SubscriptionListener.onSubscriptionInfoChanged
D SubscriptionController: [getSubId]- sSlotIdxToSubId.size == 0, return DummySubIds slotIdx=0
D SubscriptionController: [getSubId]- sSlotIdxToSubId.size == 0, return DummySubIds slotIdx=0
D DctController: handleMessage msg={ when=-1ms what=100 target=com.android.internal.telephony.dataconnection.DctController }
D DcSwitchAsyncChannel: [DcSwitchAsyncChannel-0]: rspIsIdle=true
D SubscriptionController: [getPhoneId]- invalid subId return=-1
D DcSwitchAsyncChannel: [DcSwitchAsyncChannel-0]: rspIsIdle=true
D DctController: onProcessRequest requestedPhoneId=-1, activePhoneId=-1
D SubscriptionController: [getActiveSubInfoList]+
D SubscriptionController: selection:sim_id>=0 null
D SubscriptionController: [getActiveSubInfoList]- no info return
D SubscriptionController: [getActiveSubInfoList]+
D SubscriptionController: selection:sim_id>=0 null
D SubscriptionController: [getActiveSubInfoList]- no info return
D SubscriptionController: [getActiveSubInfoList]- no info return
D SubscriptionController: [getActiveSubInfoList]- no info return
D SubscriptionController: [getSubId]- sSlotIdxToSubId.size == 0, return DummySubIds slotIdx=0
D CAT     : com.android.stk.StkAppService: onCreate()+
D CAT     : com.android.stk.StkAppService: simCount: 1
D CAT     : com.android.stk.StkAppService: slotId: 0
D CAT     : com.android.stk.StkAppService: onStart sim id: 0, op: 11, *****
D CAT     : com.android.stk.StkAppService: mStkService is: -1
D CAT     : StkAppInstaller: [setAppState]+
D CAT     : StkAppInstaller: Need not change app state!!
D CAT     : StkAppInstaller: [setAppState]-
D CAT     : com.android.stk.StkAppService: onDestroy()
D SubscriptionController: getSimStateForSlotIdx:  simState=NOT_READY ordinal=6
D SubscriptionManager: getSimStateForSubscriber: simState=6 slotIdx=0
D SubscriptionController: getSimStateForSlotIdx:  simState=NOT_READY ordinal=6
D SubscriptionManager: getSimStateForSubscriber: simState=6 slotIdx=0
D SubscriptionController: getSimStateForSlotIdx:  simState=NOT_READY ordinal=6
D SubscriptionManager: getSimStateForSubscriber: simState=6 slotIdx=0
D GsmSST  : [GsmSST] updateSpnDisplay: radio is on but out of service, set plmn='No service'
D DCT     : [0]hasMatchedTetherApnSetting: APN=null
D SubscriptionController: [getSubId]- sSlotIdxToSubId.size == 0, return DummySubIds slotIdx=0
D GsmSST  : [GsmSST] updateSpnDisplay: changed sending intent rule=0 showPlmn='true' plmn='No service' showSpn='false' spn='' dataSpn='' subId='-2'
D SubscriptionController: [getSubId]- sSlotIdxToSubId.size == 0, return DummySubIds slotIdx=0
D SubscriptionController: [getSubId]- sSlotIdxToSubId.size == 0, return DummySubIds slotIdx=0
D SubscriptionController: [setPlmnSpn] No valid subscription to store info
D SubscriptionController: notifySubscriptionInfoChanged:
D GsmSST  : [GsmSST] SubscriptionListener.onSubscriptionInfoChanged
D SubscriptionController: [getSubId]- sSlotIdxToSubId.size == 0, return DummySubIds slotIdx=0
D DCT     : [0]SubscriptionListener.onSubscriptionInfoChanged
D SubscriptionController: [getSubId]- sSlotIdxToSubId.size == 0, return DummySubIds slotIdx=0
D SubscriptionController: [getActiveSubInfoList]+
D SubscriptionController: selection:sim_id>=0 null
D SubscriptionController: [getActiveSubInfoList]- no info return
E PhoneBase: Error! unregisterForCallWaiting() in PhoneBase should not be called, CDMAPhone inactive.
D SubscriptionController: [getSubId]- sSlotIdxToSubId.size == 0, return DummySubIds slotIdx=0
D SubscriptionController: [getSubId]- sSlotIdxToSubId.size == 0, return DummySubIds slotIdx=0
D SubscriptionController: [getPhoneId]- invalid subId return=-1
D SubscriptionController: [getSubId]- sSlotIdxToSubId.size == 0, return DummySubIds slotIdx=0
D SubscriptionController: [getSubId]- sSlotIdxToSubId.size == 0, return DummySubIds slotIdx=0
D SubscriptionController: [getSubId]- sSlotIdxToSubId.size == 0, return DummySubIds slotIdx=0
E PhoneBase: Error! registerForCallWaiting() in PhoneBase should not be called, CDMAPhone inactive.
D SubscriptionController: [getActiveSubInfoList]+
D DctController: handleMessage msg={ when=-53ms what=107 target=com.android.internal.telephony.dataconnection.DctController }
D DctController: onSubInfoReady mPhoneNum=1
D SubscriptionController: [getSubId]- sSlotIdxToSubId.size == 0, return DummySubIds slotIdx=0
D DctController: onSubInfoReady handle pending requests subId=-2
D DctController: onSubInfoReady: SIM card absent on phoneId = 0
D SubscriptionController: [getSubId]- sSlotIdxToSubId.size == 0, return DummySubIds slotIdx=0
D DctController: [TNF -2]evalPendingRequest, pending request size is 1
D SubscriptionController: [getSubId]- sSlotIdxToSubId.size == 0, return DummySubIds slotIdx=0
D DctController: [TNF -2]evalPendingRequest: request = NetworkRequest [ id=1, legacyType=-1, [ Capabilities: INTERNET&NOT_RESTRICTED&TRUSTED&NOT_VPN] ]
D SubscriptionController: [getSubId]- sSlotIdxToSubId.size == 0, return DummySubIds slotIdx=0
D DctController: [TNF -2]Cellular needs Network for NetworkRequest [ id=1, legacyType=-1, [ Capabilities: INTERNET&NOT_RESTRICTED&TRUSTED&NOT_VPN] ]
D SubscriptionController: [getSubId]- sSlotIdxToSubId.size == 0, return DummySubIds slotIdx=0
D SubscriptionController: [getSubId]- sSlotIdxToSubId.size == 0, return DummySubIds slotIdx=0
D DctController: [TNF -2]Request not useable, pending request.
D DctController: processRequests
D SubscriptionController: [getSubId]- sSlotIdxToSubId.size == 0, return DummySubIds slotIdx=0
D SubscriptionController: selection:sim_id>=0 null
D DctController: handleMessage msg={ when=-1ms what=100 target=com.android.internal.telephony.dataconnection.DctController }
D DcSwitchAsyncChannel: [DcSwitchAsyncChannel-0]: rspIsIdle=true
D SubscriptionController: [getPhoneId]- invalid subId return=-1
D DcSwitchAsyncChannel: [DcSwitchAsyncChannel-0]: rspIsIdle=true
D DctController: onProcessRequest requestedPhoneId=-1, activePhoneId=-1
D SubscriptionController: [getActiveSubInfoList]- no info return
D SubscriptionController: [getActiveSubInfoList]+
D SubscriptionController: selection:sim_id>=0 null
D SubscriptionController: [getActiveSubInfoList]- no info return
D SubscriptionController: [getActiveSubInfoList]+
D SubscriptionController: selection:sim_id>=0 null
D SubscriptionController: [getActiveSubInfoList]- no info return
D SubscriptionController: [getActiveSubInfoList]+
D SubscriptionController: selection:sim_id>=0 null
D SubscriptionController: [getSubId]- sSlotIdxToSubId.size == 0, return DummySubIds slotIdx=0
D SubscriptionController: [getActiveSubInfoList]- no info return
D CAT     : com.android.stk.StkAppService: onCreate()+
D CAT     : com.android.stk.StkAppService: simCount: 1
D CAT     : com.android.stk.StkAppService: slotId: 0
D CAT     : com.android.stk.StkAppService: onStart sim id: 0, op: 11, *****
D CAT     : com.android.stk.StkAppService: mStkService is: -1
D CAT     : StkAppInstaller: [setAppState]+
D CAT     : StkAppInstaller: Need not change app state!!
D CAT     : StkAppInstaller: [setAppState]-
D CAT     : com.android.stk.StkAppService: onDestroy()
D SubscriptionController: getSimStateForSlotIdx:  simState=NOT_READY ordinal=6
D SubscriptionManager: getSimStateForSubscriber: simState=6 slotIdx=0
D SubscriptionController: getSimStateForSlotIdx:  simState=NOT_READY ordinal=6
D SubscriptionManager: getSimStateForSubscriber: simState=6 slotIdx=0
D SubscriptionController: getSimStateForSlotIdx:  simState=NOT_READY ordinal=6
D SubscriptionManager: getSimStateForSubscriber: simState=6 slotIdx=0
D GsmSST  : [GsmSST] updateSpnDisplay: radio is on but out of service, set plmn='No service.'
D SubscriptionController: [getSubId]- sSlotIdxToSubId.size == 0, return DummySubIds slotIdx=0
D DCT     : [0]hasMatchedTetherApnSetting: APN=null
D GsmSST  : [GsmSST] updateSpnDisplay: changed sending intent rule=0 showPlmn='true' plmn='No service.' showSpn='false' spn='' dataSpn='' subId='-2'
D SubscriptionController: [getSubId]- sSlotIdxToSubId.size == 0, return DummySubIds slotIdx=0
D SubscriptionController: [getSubId]- sSlotIdxToSubId.size == 0, return DummySubIds slotIdx=0
D SubscriptionController: [setPlmnSpn] No valid subscription to store info
D SubscriptionController: notifySubscriptionInfoChanged:
D GsmSST  : [GsmSST] SubscriptionListener.onSubscriptionInfoChanged
D SubscriptionController: [getSubId]- sSlotIdxToSubId.size == 0, return DummySubIds slotIdx=0
D DCT     : [0]SubscriptionListener.onSubscriptionInfoChanged
D SubscriptionController: [getSubId]- sSlotIdxToSubId.size == 0, return DummySubIds slotIdx=0
D SubscriptionController: [getActiveSubInfoList]+
D SubscriptionController: selection:sim_id>=0 null
D SubscriptionController: [getActiveSubInfoList]- no info return
E PhoneBase: Error! unregisterForCallWaiting() in PhoneBase should not be called, CDMAPhone inactive.
D SubscriptionController: [getSubId]- sSlotIdxToSubId.size == 0, return DummySubIds slotIdx=0
D SubscriptionController: [getSubId]- sSlotIdxToSubId.size == 0, return DummySubIds slotIdx=0
D SubscriptionController: [getPhoneId]- invalid subId return=-1
D SubscriptionController: [getSubId]- sSlotIdxToSubId.size == 0, return DummySubIds slotIdx=0
D SubscriptionController: [getSubId]- sSlotIdxToSubId.size == 0, return DummySubIds slotIdx=0
D SubscriptionController: [getSubId]- sSlotIdxToSubId.size == 0, return DummySubIds slotIdx=0
D SubscriptionController: [getActiveSubInfoList]+
D SubscriptionController: selection:sim_id>=0 null
E PhoneBase: Error! registerForCallWaiting() in PhoneBase should not be called, CDMAPhone inactive.
D SubscriptionController: [getActiveSubInfoList]- no info return
D DctController: handleMessage msg={ when=-94ms what=107 target=com.android.internal.telephony.dataconnection.DctController }
D DctController: onSubInfoReady mPhoneNum=1
D SubscriptionController: [getSubId]- sSlotIdxToSubId.size == 0, return DummySubIds slotIdx=0
D DctController: onSubInfoReady handle pending requests subId=-2
D DctController: onSubInfoReady: SIM card absent on phoneId = 0
D SubscriptionController: [getSubId]- sSlotIdxToSubId.size == 0, return DummySubIds slotIdx=0
D DctController: [TNF -2]evalPendingRequest, pending request size is 1
D SubscriptionController: [getSubId]- sSlotIdxToSubId.size == 0, return DummySubIds slotIdx=0
D DctController: [TNF -2]evalPendingRequest: request = NetworkRequest [ id=1, legacyType=-1, [ Capabilities: INTERNET&NOT_RESTRICTED&TRUSTED&NOT_VPN] ]
D SubscriptionController: [getSubId]- sSlotIdxToSubId.size == 0, return DummySubIds slotIdx=0
D DctController: [TNF -2]Cellular needs Network for NetworkRequest [ id=1, legacyType=-1, [ Capabilities: INTERNET&NOT_RESTRICTED&TRUSTED&NOT_VPN] ]
D SubscriptionController: [getSubId]- sSlotIdxToSubId.size == 0, return DummySubIds slotIdx=0
D SubscriptionController: [getSubId]- sSlotIdxToSubId.size == 0, return DummySubIds slotIdx=0
D DctController: [TNF -2]Request not useable, pending request.
D DctController: processRequests
D SubscriptionController: [getSubId]- sSlotIdxToSubId.size == 0, return DummySubIds slotIdx=0
D SubscriptionController: [getActiveSubInfoList]+
D DctController: handleMessage msg={ when=-11ms what=100 target=com.android.internal.telephony.dataconnection.DctController }
D SubscriptionController: selection:sim_id>=0 null
D DcSwitchAsyncChannel: [DcSwitchAsyncChannel-0]: rspIsIdle=true
D SubscriptionController: [getPhoneId]- invalid subId return=-1
D DcSwitchAsyncChannel: [DcSwitchAsyncChannel-0]: rspIsIdle=true
D DctController: onProcessRequest requestedPhoneId=-1, activePhoneId=-1
D SubscriptionController: [getActiveSubInfoList]+
D SubscriptionController: [getActiveSubInfoList]+
D SubscriptionController: selection:sim_id>=0 null
D SubscriptionController: [getActiveSubInfoList]- no info return
D SubscriptionController: [getActiveSubInfoList]- no info return
D SubscriptionController: [getSubId]- sSlotIdxToSubId.size == 0, return DummySubIds slotIdx=0
D SubscriptionController: selection:sim_id>=0 null
D CAT     : com.android.stk.StkAppService: onCreate()+
D CAT     : com.android.stk.StkAppService: simCount: 1
D CAT     : com.android.stk.StkAppService: slotId: 0
D CAT     : com.android.stk.StkAppService: onStart sim id: 0, op: 11, *****
D CAT     : com.android.stk.StkAppService: mStkService is: -1
D CAT     : StkAppInstaller: [setAppState]+
D CAT     : StkAppInstaller: Need not change app state!!
D CAT     : StkAppInstaller: [setAppState]-
D CAT     : com.android.stk.StkAppService: onDestroy()
D SubscriptionController: [getActiveSubInfoList]- no info return
D SubscriptionController: getSimStateForSlotIdx:  simState=NOT_READY ordinal=6
D SubscriptionManager: getSimStateForSubscriber: simState=6 slotIdx=0
D SubscriptionController: getSimStateForSlotIdx:  simState=NOT_READY ordinal=6
D SubscriptionManager: getSimStateForSubscriber: simState=6 slotIdx=0
D SubscriptionController: getSimStateForSlotIdx:  simState=NOT_READY ordinal=6
D SubscriptionManager: getSimStateForSubscriber: simState=6 slotIdx=0
D GsmSST  : [GsmSST] updateSpnDisplay: radio is on but out of service, set plmn='No service.'
D SubscriptionController: [getSubId]- sSlotIdxToSubId.size == 0, return DummySubIds slotIdx=0
D DCT     : [0]hasMatchedTetherApnSetting: APN=null
D CAT     : com.android.stk.StkAppService: onCreate()+
D CAT     : com.android.stk.StkAppService: simCount: 1
D CAT     : com.android.stk.StkAppService: slotId: 0
D CAT     : com.android.stk.StkAppService: onStart sim id: 0, op: 11, *****
D CAT     : com.android.stk.StkAppService: mStkService is: -1
D CAT     : StkAppInstaller: [setAppState]+
D CAT     : StkAppInstaller: Need not change app state!!
D CAT     : StkAppInstaller: [setAppState]-
D CAT     : com.android.stk.StkAppService: onDestroy()
D SubscriptionController: getSimStateForSlotIdx:  simState=NOT_READY ordinal=6
D SubscriptionManager: getSimStateForSubscriber: simState=6 slotIdx=0
D SubscriptionController: getSimStateForSlotIdx:  simState=NOT_READY ordinal=6
D SubscriptionManager: getSimStateForSubscriber: simState=6 slotIdx=0
D SubscriptionController: getSimStateForSlotIdx:  simState=NOT_READY ordinal=6
D SubscriptionManager: getSimStateForSubscriber: simState=6 slotIdx=0
D GsmSST  : [GsmSST] updateSpnDisplay: radio is on but out of service, set plmn='No service'
D SubscriptionController: [getSubId]- sSlotIdxToSubId.size == 0, return DummySubIds slotIdx=0
D GsmSST  : [GsmSST] updateSpnDisplay: changed sending intent rule=0 showPlmn='true' plmn='No service' showSpn='false' spn='' dataSpn='' subId='-2'
D SubscriptionController: [getSubId]- sSlotIdxToSubId.size == 0, return DummySubIds slotIdx=0
D DCT     : [0]hasMatchedTetherApnSetting: APN=null
D SubscriptionController: [getSubId]- sSlotIdxToSubId.size == 0, return DummySubIds slotIdx=0
D SubscriptionController: [setPlmnSpn] No valid subscription to store info
D SubscriptionController: notifySubscriptionInfoChanged:
D GsmSST  : [GsmSST] SubscriptionListener.onSubscriptionInfoChanged
D SubscriptionController: [getSubId]- sSlotIdxToSubId.size == 0, return DummySubIds slotIdx=0
D DCT     : [0]SubscriptionListener.onSubscriptionInfoChanged
D SubscriptionController: [getSubId]- sSlotIdxToSubId.size == 0, return DummySubIds slotIdx=0
D SubscriptionController: [getActiveSubInfoList]+
D SubscriptionController: selection:sim_id>=0 null
D SubscriptionController: [getActiveSubInfoList]- no info return
E PhoneBase: Error! unregisterForCallWaiting() in PhoneBase should not be called, CDMAPhone inactive.
D SubscriptionController: [getSubId]- sSlotIdxToSubId.size == 0, return DummySubIds slotIdx=0
D SubscriptionController: [getSubId]- sSlotIdxToSubId.size == 0, return DummySubIds slotIdx=0
D SubscriptionController: [getPhoneId]- invalid subId return=-1
D SubscriptionController: [getSubId]- sSlotIdxToSubId.size == 0, return DummySubIds slotIdx=0
D SubscriptionController: [getSubId]- sSlotIdxToSubId.size == 0, return DummySubIds slotIdx=0
D SubscriptionController: [getSubId]- sSlotIdxToSubId.size == 0, return DummySubIds slotIdx=0
E PhoneBase: Error! registerForCallWaiting() in PhoneBase should not be called, CDMAPhone inactive.
D DctController: handleMessage msg={ when=-55ms what=107 target=com.android.internal.telephony.dataconnection.DctController }
D DctController: onSubInfoReady mPhoneNum=1
D SubscriptionController: [getSubId]- sSlotIdxToSubId.size == 0, return DummySubIds slotIdx=0
D DctController: onSubInfoReady handle pending requests subId=-2
D DctController: onSubInfoReady: SIM card absent on phoneId = 0
D SubscriptionController: [getSubId]- sSlotIdxToSubId.size == 0, return DummySubIds slotIdx=0
D DctController: [TNF -2]evalPendingRequest, pending request size is 1
D SubscriptionController: [getSubId]- sSlotIdxToSubId.size == 0, return DummySubIds slotIdx=0
D DctController: [TNF -2]evalPendingRequest: request = NetworkRequest [ id=1, legacyType=-1, [ Capabilities: INTERNET&NOT_RESTRICTED&TRUSTED&NOT_VPN] ]
D SubscriptionController: [getSubId]- sSlotIdxToSubId.size == 0, return DummySubIds slotIdx=0
D DctController: [TNF -2]Cellular needs Network for NetworkRequest [ id=1, legacyType=-1, [ Capabilities: INTERNET&NOT_RESTRICTED&TRUSTED&NOT_VPN] ]
D SubscriptionController: [getSubId]- sSlotIdxToSubId.size == 0, return DummySubIds slotIdx=0
D SubscriptionController: [getSubId]- sSlotIdxToSubId.size == 0, return DummySubIds slotIdx=0
D DctController: [TNF -2]Request not useable, pending request.
D DctController: processRequests
D SubscriptionController: [getSubId]- sSlotIdxToSubId.size == 0, return DummySubIds slotIdx=0
D DctController: handleMessage msg={ when=-2ms what=100 target=com.android.internal.telephony.dataconnection.DctController }
D DcSwitchAsyncChannel: [DcSwitchAsyncChannel-0]: rspIsIdle=true
D SubscriptionController: [getPhoneId]- invalid subId return=-1
D DcSwitchAsyncChannel: [DcSwitchAsyncChannel-0]: rspIsIdle=true
D DctController: onProcessRequest requestedPhoneId=-1, activePhoneId=-1
D SubscriptionController: [getActiveSubInfoList]+
D SubscriptionController: selection:sim_id>=0 null
D SubscriptionController: [getActiveSubInfoList]+
D SubscriptionController: selection:sim_id>=0 null
D SubscriptionController: [getActiveSubInfoList]+
D SubscriptionController: selection:sim_id>=0 null
D SubscriptionController: [getActiveSubInfoList]- no info return
D SubscriptionController: [getActiveSubInfoList]- no info return
D SubscriptionController: [getActiveSubInfoList]- no info return
D CAT     : com.android.stk.StkAppService: onCreate()+
D CAT     : com.android.stk.StkAppService: simCount: 1
D CAT     : com.android.stk.StkAppService: slotId: 0
D CAT     : com.android.stk.StkAppService: onStart sim id: 0, op: 11, *****
D CAT     : com.android.stk.StkAppService: mStkService is: -1
D CAT     : StkAppInstaller: [setAppState]+
D CAT     : StkAppInstaller: Need not change app state!!
D CAT     : StkAppInstaller: [setAppState]-
D CAT     : com.android.stk.StkAppService: onDestroy()
D SubscriptionController: [getActiveSubInfoList]+
D SubscriptionController: selection:sim_id>=0 null
D SubscriptionController: [getActiveSubInfoList]- no info return
D SubscriptionController: [getSubId]- sSlotIdxToSubId.size == 0, return DummySubIds slotIdx=0
D SubscriptionController: getSimStateForSlotIdx:  simState=NOT_READY ordinal=6
D SubscriptionManager: getSimStateForSubscriber: simState=6 slotIdx=0
D SubscriptionController: getSimStateForSlotIdx:  simState=NOT_READY ordinal=6
D SubscriptionManager: getSimStateForSubscriber: simState=6 slotIdx=0
D SubscriptionController: getSimStateForSlotIdx:  simState=NOT_READY ordinal=6
D SubscriptionManager: getSimStateForSubscriber: simState=6 slotIdx=0
D GsmSST  : [GsmSST] updateSpnDisplay: radio is on but out of service, set plmn='No service.'
D DCT     : [0]hasMatchedTetherApnSetting: APN=null
D SubscriptionController: [getSubId]- sSlotIdxToSubId.size == 0, return DummySubIds slotIdx=0
D GsmSST  : [GsmSST] updateSpnDisplay: changed sending intent rule=0 showPlmn='true' plmn='No service.' showSpn='false' spn='' dataSpn='' subId='-2'
D SubscriptionController: [getSubId]- sSlotIdxToSubId.size == 0, return DummySubIds slotIdx=0
D SubscriptionController: [getSubId]- sSlotIdxToSubId.size == 0, return DummySubIds slotIdx=0
D SubscriptionController: [setPlmnSpn] No valid subscription to store info
D SubscriptionController: notifySubscriptionInfoChanged:
D GsmSST  : [GsmSST] SubscriptionListener.onSubscriptionInfoChanged
D SubscriptionController: [getSubId]- sSlotIdxToSubId.size == 0, return DummySubIds slotIdx=0
D DCT     : [0]SubscriptionListener.onSubscriptionInfoChanged
D SubscriptionController: [getSubId]- sSlotIdxToSubId.size == 0, return DummySubIds slotIdx=0
E PhoneBase: Error! unregisterForCallWaiting() in PhoneBase should not be called, CDMAPhone inactive.
D SubscriptionController: [getSubId]- sSlotIdxToSubId.size == 0, return DummySubIds slotIdx=0
D SubscriptionController: [getSubId]- sSlotIdxToSubId.size == 0, return DummySubIds slotIdx=0
D SubscriptionController: [getPhoneId]- invalid subId return=-1
D SubscriptionController: [getSubId]- sSlotIdxToSubId.size == 0, return DummySubIds slotIdx=0
D SubscriptionController: [getSubId]- sSlotIdxToSubId.size == 0, return DummySubIds slotIdx=0
D SubscriptionController: [getSubId]- sSlotIdxToSubId.size == 0, return DummySubIds slotIdx=0
D SubscriptionController: [getActiveSubInfoList]+
D SubscriptionController: selection:sim_id>=0 null
D SubscriptionController: [getActiveSubInfoList]+
D SubscriptionController: [getActiveSubInfoList]- no info return
D SubscriptionController: [getActiveSubInfoList]+
E PhoneBase: Error! registerForCallWaiting() in PhoneBase should not be called, CDMAPhone inactive.
D SubscriptionController: selection:sim_id>=0 null
D SubscriptionController: [getActiveSubInfoList]+
D SubscriptionController: selection:sim_id>=0 null
D SubscriptionController: selection:sim_id>=0 null
D SubscriptionController: [getActiveSubInfoList]- no info return
D DctController: handleMessage msg={ when=-92ms what=107 target=com.android.internal.telephony.dataconnection.DctController }
D DctController: onSubInfoReady mPhoneNum=1
D SubscriptionController: [getSubId]- sSlotIdxToSubId.size == 0, return DummySubIds slotIdx=0
D DctController: onSubInfoReady handle pending requests subId=-2
D DctController: onSubInfoReady: SIM card absent on phoneId = 0
D SubscriptionController: [getSubId]- sSlotIdxToSubId.size == 0, return DummySubIds slotIdx=0
D DctController: [TNF -2]evalPendingRequest, pending request size is 1
D SubscriptionController: [getSubId]- sSlotIdxToSubId.size == 0, return DummySubIds slotIdx=0
D DctController: [TNF -2]evalPendingRequest: request = NetworkRequest [ id=1, legacyType=-1, [ Capabilities: INTERNET&NOT_RESTRICTED&TRUSTED&NOT_VPN] ]
D SubscriptionController: [getSubId]- sSlotIdxToSubId.size == 0, return DummySubIds slotIdx=0
D DctController: [TNF -2]Cellular needs Network for NetworkRequest [ id=1, legacyType=-1, [ Capabilities: INTERNET&NOT_RESTRICTED&TRUSTED&NOT_VPN] ]
D SubscriptionController: [getSubId]- sSlotIdxToSubId.size == 0, return DummySubIds slotIdx=0
D SubscriptionController: [getSubId]- sSlotIdxToSubId.size == 0, return DummySubIds slotIdx=0
D DctController: [TNF -2]Request not useable, pending request.
D DctController: processRequests
D SubscriptionController: [getSubId]- sSlotIdxToSubId.size == 0, return DummySubIds slotIdx=0
D DctController: handleMessage msg={ when=-1ms what=100 target=com.android.internal.telephony.dataconnection.DctController }
D DcSwitchAsyncChannel: [DcSwitchAsyncChannel-0]: rspIsIdle=true
D SubscriptionController: [getPhoneId]- invalid subId return=-1
D DcSwitchAsyncChannel: [DcSwitchAsyncChannel-0]: rspIsIdle=true
D DctController: onProcessRequest requestedPhoneId=-1, activePhoneId=-1
D SubscriptionController: [getActiveSubInfoList]- no info return
D SubscriptionController: [getActiveSubInfoList]- no info return
D SubscriptionController: [getActiveSubInfoList]+
D SubscriptionController: selection:sim_id>=0 null
D SubscriptionController: [getActiveSubInfoList]- no info return
D SubscriptionController: [getSubId]- sSlotIdxToSubId.size == 0, return DummySubIds slotIdx=0
D CAT     : com.android.stk.StkAppService: onCreate()+
D CAT     : com.android.stk.StkAppService: simCount: 1
D CAT     : com.android.stk.StkAppService: slotId: 0
D CAT     : com.android.stk.StkAppService: onStart sim id: 0, op: 11, *****
D CAT     : com.android.stk.StkAppService: mStkService is: -1
D CAT     : StkAppInstaller: [setAppState]+
D CAT     : StkAppInstaller: Need not change app state!!
D CAT     : StkAppInstaller: [setAppState]-
D CAT     : com.android.stk.StkAppService: onDestroy()
D SubscriptionController: getSimStateForSlotIdx:  simState=NOT_READY ordinal=6
D SubscriptionManager: getSimStateForSubscriber: simState=6 slotIdx=0
D SubscriptionController: getSimStateForSlotIdx:  simState=NOT_READY ordinal=6
D SubscriptionManager: getSimStateForSubscriber: simState=6 slotIdx=0
D SubscriptionController: getSimStateForSlotIdx:  simState=NOT_READY ordinal=6
D SubscriptionManager: getSimStateForSubscriber: simState=6 slotIdx=0
D GsmSST  : [GsmSST] updateSpnDisplay: radio is on but out of service, set plmn='No service.'
D SubscriptionController: [getSubId]- sSlotIdxToSubId.size == 0, return DummySubIds slotIdx=0
D DCT     : [0]hasMatchedTetherApnSetting: APN=null
D CAT     : com.android.stk.StkAppService: onCreate()+
D CAT     : com.android.stk.StkAppService: simCount: 1
D CAT     : com.android.stk.StkAppService: slotId: 0
D CAT     : com.android.stk.StkAppService: onStart sim id: 0, op: 11, *****
D CAT     : com.android.stk.StkAppService: mStkService is: -1
D CAT     : StkAppInstaller: [setAppState]+
D CAT     : StkAppInstaller: Need not change app state!!
D CAT     : StkAppInstaller: [setAppState]-
D CAT     : com.android.stk.StkAppService: onDestroy()
D SubscriptionController: getSimStateForSlotIdx:  simState=NOT_READY ordinal=6
D SubscriptionManager: getSimStateForSubscriber: simState=6 slotIdx=0
D SubscriptionController: getSimStateForSlotIdx:  simState=NOT_READY ordinal=6
D SubscriptionManager: getSimStateForSubscriber: simState=6 slotIdx=0
D SubscriptionController: getSimStateForSlotIdx:  simState=NOT_READY ordinal=6
D SubscriptionManager: getSimStateForSubscriber: simState=6 slotIdx=0
D GsmSST  : [GsmSST] updateSpnDisplay: radio is on but out of service, set plmn='No service.'
D SubscriptionController: [getSubId]- sSlotIdxToSubId.size == 0, return DummySubIds slotIdx=0
D DCT     : [0]hasMatchedTetherApnSetting: APN=null
D CAT     : com.android.stk.StkAppService: onCreate()+
D CAT     : com.android.stk.StkAppService: simCount: 1
D CAT     : com.android.stk.StkAppService: slotId: 0
D CAT     : com.android.stk.StkAppService: onStart sim id: 0, op: 11, *****
D CAT     : com.android.stk.StkAppService: mStkService is: -1
D CAT     : StkAppInstaller: [setAppState]+
D CAT     : StkAppInstaller: Need not change app state!!
D CAT     : StkAppInstaller: [setAppState]-
D CAT     : com.android.stk.StkAppService: onDestroy()
D SubscriptionController: getSimStateForSlotIdx:  simState=NOT_READY ordinal=6
D SubscriptionManager: getSimStateForSubscriber: simState=6 slotIdx=0
D SubscriptionController: getSimStateForSlotIdx:  simState=NOT_READY ordinal=6
D SubscriptionManager: getSimStateForSubscriber: simState=6 slotIdx=0
D SubscriptionController: getSimStateForSlotIdx:  simState=NOT_READY ordinal=6
D SubscriptionManager: getSimStateForSubscriber: simState=6 slotIdx=0
D RILJ    : NOTE: mWakeLockCount is 3at time of clearing
D RILJ    : WAKE_LOCK_TIMEOUT  mRequestList=3
D RILJ    : 0: [23] GET_SIM_STATUS
D RILJ    : 1: [40] GET_SIM_STATUS
D RILJ    : 2: [45] GET_SIM_STATUS
D SubscriptionController: [getSlotId]- subId invalid
D SubscriptionController: getSimStateForSlotIdx:  simState=NOT_READY ordinal=6
D SubscriptionManager: getSimStateForSubscriber: simState=6 slotIdx=0
D TelephonyManager: getSimState: default sim:-1, sim state for slotIdx=0 is 6, return state as unknown
D SubscriptionController: [getActiveSubInfoList]+
D SubscriptionController: selection:sim_id>=0 null
D SubscriptionController: [getActiveSubInfoList]- no info return
D SubscriptionController: [getSlotId]- subId invalid
D SubscriptionController: getSimStateForSlotIdx:  simState=NOT_READY ordinal=6
D SubscriptionManager: getSimStateForSubscriber: simState=6 slotIdx=0
D TelephonyManager: getSimState: default sim:-1, sim state for slotIdx=0 is 6, return state as unknown
D SubscriptionController: [getActiveSubInfoList]+
D SubscriptionController: selection:sim_id>=0 null
D SubscriptionController: [getActiveSubInfoList]- no info return
D SubscriptionController: [getPhoneId]- invalid subId return=-1
D SubscriptionController: [getPhoneId]- invalid subId return=-1
D SubscriptionController: [getPhoneId] asked for default subId=-1
D SubscriptionController: [getPhoneId]- invalid subId return=-1
D SubscriptionController: getSimStateForSlotIdx:  simState=NOT_READY ordinal=6
D SubscriptionManager: getSimStateForSubscriber: simState=6 slotIdx=0
D SubscriptionController: getSimStateForSlotIdx:  simState=NOT_READY ordinal=6
D SubscriptionManager: getSimStateForSubscriber: simState=6 slotIdx=0
D SubscriptionController: [getSlotId]- subId invalid
D SubscriptionController: getSimStateForSlotIdx: invalid slotIdx simState=UNKNOWN ordinal=0
D SubscriptionManager: getSimStateForSubscriber: simState=0 slotIdx=-1
D SubscriptionController: getSimStateForSlotIdx:  simState=NOT_READY ordinal=6
D SubscriptionManager: getSimStateForSubscriber: simState=6 slotIdx=0
D SubscriptionController: getSimStateForSlotIdx:  simState=NOT_READY ordinal=6
D SubscriptionManager: getSimStateForSubscriber: simState=6 slotIdx=0
D SubscriptionController: [getSlotId]- subId invalid
D SubscriptionController: getSimStateForSlotIdx:  simState=NOT_READY ordinal=6
D SubscriptionManager: getSimStateForSubscriber: simState=6 slotIdx=0
D TelephonyManager: getSimState: default sim:-1, sim state for slotIdx=0 is 6, return state as unknown
D DCT     : [0]hasMatchedTetherApnSetting: APN=null
D SubscriptionController: [getSlotId]- subId invalid
D SubscriptionController: getSimStateForSlotIdx:  simState=NOT_READY ordinal=6
D SubscriptionManager: getSimStateForSubscriber: simState=6 slotIdx=0
D TelephonyManager: getSimState: default sim:-1, sim state for slotIdx=0 is 6, return state as unknown
D DCT     : [0]hasMatchedTetherApnSetting: APN=null
D SubscriptionController: [getSlotId]- subId invalid
D SubscriptionController: getSimStateForSlotIdx:  simState=NOT_READY ordinal=6
D SubscriptionManager: getSimStateForSubscriber: simState=6 slotIdx=0
D TelephonyManager: getSimState: default sim:-1, sim state for slotIdx=0 is 6, return state as unknown
D SubscriptionController: [getActiveSubInfoList]+
D SubscriptionController: selection:sim_id>=0 null
D SubscriptionController: [getActiveSubInfoList]- no info return
D SubscriptionController: [getActiveSubInfoList]+
D SubscriptionController: selection:sim_id>=0 null
D SubscriptionController: [getActiveSubInfoList]- no info return
D SubscriptionController: [getActiveSubInfoList]+
D SubscriptionController: selection:sim_id>=0 null
D SubscriptionController: [getActiveSubInfoList]- no info return
D SubscriptionController: [getActiveSubInfoList]+
D SubscriptionController: selection:sim_id>=0 null
D SubscriptionController: [getActiveSubInfoList]- no info return
D SubscriptionController: [getActiveSubInfoList]+
D SubscriptionController: selection:sim_id>=0 null
D SubscriptionController: [getActiveSubInfoList]- no info return
D SubscriptionController: [getActiveSubInfoList]+
D SubscriptionController: selection:sim_id>=0 null
D SubscriptionController: [getActiveSubInfoList]- no info return
D SubscriptionController: [getActiveSubInfoList]+
D SubscriptionController: selection:sim_id>=0 null
D SubscriptionController: [getActiveSubInfoList]- no info return
D SubscriptionController: [getActiveSubInfoList]+
D SubscriptionController: selection:sim_id>=0 null
D SubscriptionController: [getActiveSubInfoList]- no info return
D SubscriptionController: [getActiveSubInfoList]+
D SubscriptionController: selection:sim_id>=0 null
D SubscriptionController: [getActiveSubInfoList]- no info return
D SubscriptionController: [getActiveSubInfoList]+
D SubscriptionController: selection:sim_id>=0 null
D SubscriptionController: [getActiveSubInfoList]- no info return
D SubscriptionController: [getActiveSubInfoList]+
D SubscriptionController: selection:sim_id>=0 null
D SubscriptionController: [getActiveSubInfoList]- no info return
D SubscriptionController: [getActiveSubInfoList]+
D SubscriptionController: selection:sim_id>=0 null
D SubscriptionController: [getActiveSubInfoList]- no info return
D SubscriptionController: [getActiveSubInfoList]+
D SubscriptionController: selection:sim_id>=0 null
D SubscriptionController: [getActiveSubInfoList]- no info return
D SubscriptionController: [getActiveSubInfoList]+
D SubscriptionController: selection:sim_id>=0 null
D SubscriptionController: [getActiveSubInfoList]- no info return
D SubscriptionController: [getActiveSubInfoList]+
D SubscriptionController: selection:sim_id>=0 null
D SubscriptionController: [getActiveSubInfoList]- no info return
D RILJ    : [3706]> SCREEN_STATE: false [SUB0]
D use-Rlog/RLOG-RIL: 4 RIL requests in the queue (1 pending, 1 handled, 2 unhandled)
D use-Rlog/RLOG-RIL: 3 RIL requests in the queue (0 pending, 1 handled, 2 unhandled)
D RILJ    : [3706]< SCREEN_STATE  [SUB0]
D DCT     : [0]onReceive: action=android.intent.action.SCREEN_ON
D DCT     : [0]stopNetStatPoll
D SubscriptionController: [getSubId]- sSlotIdxToSubId.size == 0, return DummySubIds slotIdx=0
D DCT     : [0]overall state is IDLE
D SubscriptionController: [getSubId]- sSlotIdxToSubId.size == 0, return DummySubIds slotIdx=0
D DCT     : [0]onReceive: action=android.intent.action.SCREEN_OFF
D DCT     : [0]stopNetStatPoll
D SubscriptionController: [getSubId]- sSlotIdxToSubId.size == 0, return DummySubIds slotIdx=0
D DCT     : [0]overall state is IDLE
D SubscriptionController: [getSubId]- sSlotIdxToSubId.size == 0, return DummySubIds slotIdx=0
D DCT     : [0]hasMatchedTetherApnSetting: APN=null
D SubscriptionController: [getSlotId]- subId invalid
D SubscriptionController: getSimStateForSlotIdx:  simState=NOT_READY ordinal=6
D SubscriptionManager: getSimStateForSubscriber: simState=6 slotIdx=0
D TelephonyManager: getSimState: default sim:-1, sim state for slotIdx=0 is 6, return state as unknown
D DCT     : [0]hasMatchedTetherApnSetting: APN=null
D DCT     : [0]onReceive: action=android.intent.action.SCREEN_ON
D DCT     : [0]stopNetStatPoll
D SubscriptionController: [getSubId]- sSlotIdxToSubId.size == 0, return DummySubIds slotIdx=0
D DCT     : [0]overall state is IDLE
D SubscriptionController: [getSubId]- sSlotIdxToSubId.size == 0, return DummySubIds slotIdx=0
D RILJ    : [3707]> SCREEN_STATE: true [SUB0]
D use-Rlog/RLOG-RIL: 4 RIL requests in the queue (1 pending, 1 handled, 2 unhandled)
D use-Rlog/RLOG-RIL: 3 RIL requests in the queue (0 pending, 1 handled, 2 unhandled)
D RILJ    : [UNSL]< UNSOL_RESPONSE_VOICE_NETWORK_STATE_CHANGED [SUB0]
D RILJ    : [3707]< SCREEN_STATE  [SUB0]
D RILJ    : [3708]> OPERATOR [SUB0]
D RILJ    : [3709]> DATA_REGISTRATION_STATE [SUB0]
D use-Rlog/RLOG-RIL: 4 RIL requests in the queue (1 pending, 1 handled, 2 unhandled)
D use-Rlog/RLOG-RIL-IPC: 
D use-Rlog/RLOG-RIL-IPC: xmm626_sec_modem_fmt_send: Sent FMT message
D use-Rlog/RLOG-RIL-IPC: xmm626_sec_modem_fmt_send: Message: mseq=0x18, command=IPC_NET_SERVING_NETWORK, type=IPC_TYPE_GET, size=0
D RILJ    : [3710]> VOICE_REGISTRATION_STATE [SUB0]
D use-Rlog/RLOG-RIL: 5 RIL requests in the queue (1 pending, 2 handled, 2 unhandled)
D use-Rlog/RLOG-RIL-IPC: 
D use-Rlog/RLOG-RIL-IPC: xmm626_sec_modem_fmt_send: Sent FMT message
D use-Rlog/RLOG-RIL-IPC: xmm626_sec_modem_fmt_send: Message: mseq=0x19, command=IPC_NET_REGIST, type=IPC_TYPE_GET, size=2
D use-Rlog/RLOG-RIL-IPC: ================================= IPC FMT data =================================
D use-Rlog/RLOG-RIL-IPC: [0000]   FF 03                                              ..
D use-Rlog/RLOG-RIL-IPC: ================================================================================
D RILJ    : [3711]> QUERY_NETWORK_SELECTION_MODE [SUB0]
D use-Rlog/RLOG-RIL: 6 RIL requests in the queue (1 pending, 3 handled, 2 unhandled)
D use-Rlog/RLOG-RIL-IPC: 
D use-Rlog/RLOG-RIL-IPC: xmm626_sec_modem_fmt_send: Sent FMT message
D use-Rlog/RLOG-RIL-IPC: xmm626_sec_modem_fmt_send: Message: mseq=0x1a, command=IPC_NET_REGIST, type=IPC_TYPE_GET, size=2
D use-Rlog/RLOG-RIL-IPC: ================================= IPC FMT data =================================
D use-Rlog/RLOG-RIL-IPC: [0000]   FF 02                                              ..
D use-Rlog/RLOG-RIL-IPC: ================================================================================
D use-Rlog/RLOG-RIL: 7 RIL requests in the queue (1 pending, 4 handled, 2 unhandled)
D use-Rlog/RLOG-RIL-IPC: 
D use-Rlog/RLOG-RIL-IPC: xmm626_sec_modem_fmt_send: Sent FMT message
D use-Rlog/RLOG-RIL-IPC: xmm626_sec_modem_fmt_send: Message: mseq=0x1b, command=IPC_NET_PLMN_SEL, type=IPC_TYPE_GET, size=0
D DCT     : [0]hasMatchedTetherApnSetting: APN=null
D SubscriptionController: [getActiveSubInfoList]+
D SubscriptionController: selection:sim_id>=0 null
D SubscriptionController: [getActiveSubInfoList]- no info return
D SubscriptionController: [getActiveSubInfoList]+
D SubscriptionController: selection:sim_id>=0 null
D SubscriptionController: [getActiveSubInfoList]- no info return
D SubscriptionController: [getActiveSubInfoList]+
D SubscriptionController: selection:sim_id>=0 null
D SubscriptionController: [getActiveSubInfoList]- no info return
D SubscriptionController: [getActiveSubInfoList]+
D SubscriptionController: selection:sim_id>=0 null
D SubscriptionController: [getActiveSubInfoList]- no info return
D RILJ    : [3712]> SCREEN_STATE: false [SUB0]
D use-Rlog/RLOG-RIL: 8 RIL requests in the queue (1 pending, 5 handled, 2 unhandled)
D use-Rlog/RLOG-RIL: 7 RIL requests in the queue (0 pending, 5 handled, 2 unhandled)
D RILJ    : [3712]< SCREEN_STATE  [SUB0]
D DCT     : [0]onReceive: action=android.intent.action.SCREEN_OFF
D DCT     : [0]stopNetStatPoll
D SubscriptionController: [getSubId]- sSlotIdxToSubId.size == 0, return DummySubIds slotIdx=0
D DCT     : [0]overall state is IDLE
D SubscriptionController: [getSubId]- sSlotIdxToSubId.size == 0, return DummySubIds slotIdx=0
D DCT     : [0]hasMatchedTetherApnSetting: APN=null
D SubscriptionController: [getSlotId]- subId invalid
D SubscriptionController: getSimStateForSlotIdx:  simState=NOT_READY ordinal=6
D SubscriptionManager: getSimStateForSubscriber: simState=6 slotIdx=0
D TelephonyManager: getSimState: default sim:-1, sim state for slotIdx=0 is 6, return state as unknown
D DCT     : [0]hasMatchedTetherApnSetting: APN=null
D RILJ    : NOTE: mWakeLockCount is 4at time of clearing
D RILJ    : WAKE_LOCK_TIMEOUT  mRequestList=7
D RILJ    : 0: [23] GET_SIM_STATUS
D RILJ    : 1: [40] GET_SIM_STATUS
D RILJ    : 2: [45] GET_SIM_STATUS
D RILJ    : 3: [60] OPERATOR
D RILJ    : 4: [61] DATA_REGISTRATION_STATE
D RILJ    : 5: [62] VOICE_REGISTRATION_STATE
D RILJ    : 6: [63] QUERY_NETWORK_SELECTION_MODE
D DCT     : [0]onReceive: action=android.intent.action.SCREEN_ON
D DCT     : [0]stopNetStatPoll
D SubscriptionController: [getSubId]- sSlotIdxToSubId.size == 0, return DummySubIds slotIdx=0
D DCT     : [0]overall state is IDLE
D SubscriptionController: [getSubId]- sSlotIdxToSubId.size == 0, return DummySubIds slotIdx=0
D RILJ    : [3713]> SCREEN_STATE: true [SUB0]
D use-Rlog/RLOG-RIL: 8 RIL requests in the queue (1 pending, 5 handled, 2 unhandled)
D use-Rlog/RLOG-RIL: 7 RIL requests in the queue (0 pending, 5 handled, 2 unhandled)
D RILJ    : [UNSL]< UNSOL_RESPONSE_VOICE_NETWORK_STATE_CHANGED [SUB0]
D RILJ    : [3713]< SCREEN_STATE  [SUB0]
D RILJ    : [3714]> OPERATOR [SUB0]
D RILJ    : [3715]> DATA_REGISTRATION_STATE [SUB0]
D use-Rlog/RLOG-RIL: 8 RIL requests in the queue (1 pending, 5 handled, 2 unhandled)
D RILJ    : [3716]> VOICE_REGISTRATION_STATE [SUB0]
D use-Rlog/RLOG-RIL: 9 RIL requests in the queue (1 pending, 5 handled, 3 unhandled)
D RILJ    : [3717]> QUERY_NETWORK_SELECTION_MODE [SUB0]
D use-Rlog/RLOG-RIL: 10 RIL requests in the queue (1 pending, 5 handled, 4 unhandled)
D use-Rlog/RLOG-RIL: 11 RIL requests in the queue (1 pending, 5 handled, 5 unhandled)
D use-Rlog/RLOG-RIL-IPC: 
D use-Rlog/RLOG-RIL-IPC: xmm626_sec_modem_fmt_send: Sent FMT message
D use-Rlog/RLOG-RIL-IPC: xmm626_sec_modem_fmt_send: Message: mseq=0x1c, command=IPC_NET_PLMN_SEL, type=IPC_TYPE_GET, size=0
D RILJ    : [3718]> SCREEN_STATE: false [SUB0]
D use-Rlog/RLOG-RIL: 12 RIL requests in the queue (1 pending, 6 handled, 5 unhandled)
D use-Rlog/RLOG-RIL: 11 RIL requests in the queue (0 pending, 6 handled, 5 unhandled)
D RILJ    : [3718]< SCREEN_STATE  [SUB0]
D DCT     : [0]onReceive: action=android.intent.action.SCREEN_OFF
D DCT     : [0]stopNetStatPoll
D SubscriptionController: [getSubId]- sSlotIdxToSubId.size == 0, return DummySubIds slotIdx=0
D DCT     : [0]overall state is IDLE
D SubscriptionController: [getSubId]- sSlotIdxToSubId.size == 0, return DummySubIds slotIdx=0
D RILJ    : NOTE: mWakeLockCount is 4at time of clearing
D RILJ    : WAKE_LOCK_TIMEOUT  mRequestList=11
D RILJ    : 0: [23] GET_SIM_STATUS
D RILJ    : 1: [40] GET_SIM_STATUS
D RILJ    : 2: [45] GET_SIM_STATUS
D RILJ    : 3: [60] OPERATOR
D RILJ    : 4: [61] DATA_REGISTRATION_STATE
D RILJ    : 5: [62] VOICE_REGISTRATION_STATE
D RILJ    : 6: [63] QUERY_NETWORK_SELECTION_MODE
D RILJ    : 7: [66] OPERATOR
D RILJ    : 8: [67] DATA_REGISTRATION_STATE
D RILJ    : 9: [68] VOICE_REGISTRATION_STATE
D RILJ    : 10: [69] QUERY_NETWORK_SELECTION_MODE
D RILJ    : [3719]> SCREEN_STATE: true [SUB0]
D use-Rlog/RLOG-RIL: 12 RIL requests in the queue (1 pending, 6 handled, 5 unhandled)
D use-Rlog/RLOG-RIL: 11 RIL requests in the queue (0 pending, 6 handled, 5 unhandled)
D RILJ    : [UNSL]< UNSOL_RESPONSE_VOICE_NETWORK_STATE_CHANGED [SUB0]
D RILJ    : [3719]< SCREEN_STATE  [SUB0]
D RILJ    : [3720]> OPERATOR [SUB0]
D use-Rlog/RLOG-RIL: 12 RIL requests in the queue (1 pending, 6 handled, 5 unhandled)
D RILJ    : [3721]> DATA_REGISTRATION_STATE [SUB0]
D RILJ    : [3722]> VOICE_REGISTRATION_STATE [SUB0]
D use-Rlog/RLOG-RIL: 13 RIL requests in the queue (1 pending, 6 handled, 6 unhandled)
D RILJ    : [3723]> QUERY_NETWORK_SELECTION_MODE [SUB0]
D use-Rlog/RLOG-RIL: 14 RIL requests in the queue (1 pending, 6 handled, 7 unhandled)
D use-Rlog/RLOG-RIL: 15 RIL requests in the queue (1 pending, 6 handled, 8 unhandled)
D use-Rlog/RLOG-RIL-IPC: 
D use-Rlog/RLOG-RIL-IPC: xmm626_sec_modem_fmt_send: Sent FMT message
D use-Rlog/RLOG-RIL-IPC: xmm626_sec_modem_fmt_send: Message: mseq=0x1d, command=IPC_NET_PLMN_SEL, type=IPC_TYPE_GET, size=0
D DCT     : [0]onReceive: action=android.intent.action.SCREEN_ON
D DCT     : [0]stopNetStatPoll
D SubscriptionController: [getSubId]- sSlotIdxToSubId.size == 0, return DummySubIds slotIdx=0
D DCT     : [0]overall state is IDLE
D SubscriptionController: [getSubId]- sSlotIdxToSubId.size == 0, return DummySubIds slotIdx=0
D RILJ    : [3724]> SCREEN_STATE: false [SUB0]
D use-Rlog/RLOG-RIL: 16 RIL requests in the queue (1 pending, 7 handled, 8 unhandled)
D use-Rlog/RLOG-RIL: 15 RIL requests in the queue (0 pending, 7 handled, 8 unhandled)
D RILJ    : [3724]< SCREEN_STATE  [SUB0]
D DCT     : [0]onReceive: action=android.intent.action.SCREEN_OFF
D DCT     : [0]stopNetStatPoll
D SubscriptionController: [getSubId]- sSlotIdxToSubId.size == 0, return DummySubIds slotIdx=0
D DCT     : [0]overall state is IDLE
D SubscriptionController: [getSubId]- sSlotIdxToSubId.size == 0, return DummySubIds slotIdx=0
D RILJ    : [3725]> SCREEN_STATE: true [SUB0]
D use-Rlog/RLOG-RIL: 16 RIL requests in the queue (1 pending, 7 handled, 8 unhandled)
D use-Rlog/RLOG-RIL: 15 RIL requests in the queue (0 pending, 7 handled, 8 unhandled)
D RILJ    : [UNSL]< UNSOL_RESPONSE_VOICE_NETWORK_STATE_CHANGED [SUB0]
D RILJ    : [3725]< SCREEN_STATE  [SUB0]
D RILJ    : [3726]> OPERATOR [SUB0]
D RILJ    : [3727]> DATA_REGISTRATION_STATE [SUB0]
D use-Rlog/RLOG-RIL: 16 RIL requests in the queue (1 pending, 7 handled, 8 unhandled)
D RILJ    : [3728]> VOICE_REGISTRATION_STATE [SUB0]
D use-Rlog/RLOG-RIL: 17 RIL requests in the queue (1 pending, 7 handled, 9 unhandled)
D RILJ    : [3729]> QUERY_NETWORK_SELECTION_MODE [SUB0]
D use-Rlog/RLOG-RIL: 18 RIL requests in the queue (1 pending, 7 handled, 10 unhandled)
D use-Rlog/RLOG-RIL: 19 RIL requests in the queue (1 pending, 7 handled, 11 unhandled)
D use-Rlog/RLOG-RIL-IPC: 
D use-Rlog/RLOG-RIL-IPC: xmm626_sec_modem_fmt_send: Sent FMT message
D use-Rlog/RLOG-RIL-IPC: xmm626_sec_modem_fmt_send: Message: mseq=0x1e, command=IPC_NET_PLMN_SEL, type=IPC_TYPE_GET, size=0
D DCT     : [0]onReceive: action=android.intent.action.SCREEN_ON
D DCT     : [0]stopNetStatPoll
D SubscriptionController: [getSubId]- sSlotIdxToSubId.size == 0, return DummySubIds slotIdx=0
D DCT     : [0]overall state is IDLE
D SubscriptionController: [getSubId]- sSlotIdxToSubId.size == 0, return DummySubIds slotIdx=0
D DCT     : [0]onReceive: action=android.intent.action.SCREEN_OFF
D DCT     : [0]stopNetStatPoll
D SubscriptionController: [getSubId]- sSlotIdxToSubId.size == 0, return DummySubIds slotIdx=0
D DCT     : [0]overall state is IDLE
D SubscriptionController: [getSubId]- sSlotIdxToSubId.size == 0, return DummySubIds slotIdx=0
D DCT     : [0]onReceive: action=android.intent.action.SCREEN_ON
D DCT     : [0]stopNetStatPoll
D SubscriptionController: [getSubId]- sSlotIdxToSubId.size == 0, return DummySubIds slotIdx=0
D DCT     : [0]overall state is IDLE
D SubscriptionController: [getSubId]- sSlotIdxToSubId.size == 0, return DummySubIds slotIdx=0
D DCT     : [0]hasMatchedTetherApnSetting: APN=null
D SubscriptionController: [getPhoneId]- invalid subId return=-1
D SubscriptionController: [getPhoneId]- invalid subId return=-1
D SubscriptionController: [getSlotId]- subId invalid
D SubscriptionController: [getSubId]- invalid slotIdx=-1
D DCT     : [0]hasMatchedTetherApnSetting: APN=null
D DCT     : [0]onReceive: action=android.net.wifi.WIFI_STATE_CHANGED
D DCT     : [0]WIFI_STATE_CHANGED_ACTION: enabled=false mIsWifiConnected=false
D RILJ    : NOTE: mWakeLockCount is 8at time of clearing
D RILJ    : WAKE_LOCK_TIMEOUT  mRequestList=19
D RILJ    : 0: [23] GET_SIM_STATUS
D RILJ    : 1: [40] GET_SIM_STATUS
D RILJ    : 2: [45] GET_SIM_STATUS
D RILJ    : 3: [60] OPERATOR
D RILJ    : 4: [61] DATA_REGISTRATION_STATE
D RILJ    : 5: [62] VOICE_REGISTRATION_STATE
D RILJ    : 6: [63] QUERY_NETWORK_SELECTION_MODE
D RILJ    : 7: [66] OPERATOR
D RILJ    : 8: [67] DATA_REGISTRATION_STATE
D RILJ    : 9: [68] VOICE_REGISTRATION_STATE
D RILJ    : 10: [69] QUERY_NETWORK_SELECTION_MODE
D RILJ    : 11: [72] OPERATOR
D RILJ    : 12: [73] DATA_REGISTRATION_STATE
D RILJ    : 13: [74] VOICE_REGISTRATION_STATE
D RILJ    : 14: [75] QUERY_NETWORK_SELECTION_MODE
D RILJ    : 15: [78] OPERATOR
D RILJ    : 16: [79] DATA_REGISTRATION_STATE
D RILJ    : 17: [80] VOICE_REGISTRATION_STATE
D RILJ    : 18: [81] QUERY_NETWORK_SELECTION_MODE
D SubscriptionController: [getPhoneId]- invalid subId return=-1
D DCT     : [0]hasMatchedTetherApnSetting: APN=null
D DCT     : [0]hasMatchedTetherApnSetting: APN=null
D SubscriptionController: [getSlotId]- subId invalid
D SubscriptionController: getSimStateForSlotIdx:  simState=NOT_READY ordinal=6
D SubscriptionManager: getSimStateForSubscriber: simState=6 slotIdx=0
D TelephonyManager: getSimState: default sim:-1, sim state for slotIdx=0 is 6, return state as unknown
D GsmSST  : [GsmSST] mDeviceShuttingDown = false
D GsmSST  : [GsmSST] mDesiredPowerState = false
D GsmSST  : [GsmSST] getRadioState = RADIO_ON
D GsmSST  : [GsmSST] mPowerOffDelayNeed = true
D GsmSST  : [GsmSST] mAlarmSwitch = false
D SubscriptionController: [getSubId]- sSlotIdxToSubId.size == 0, return DummySubIds slotIdx=0
D SubscriptionController: [getSubId]- sSlotIdxToSubId.size == 0, return DummySubIds slotIdx=0
D SubscriptionController: [getPhoneId]- invalid subId return=-1
D DCT     : [0]cleanUpAllConnections
D GsmSST  : [GsmSST] Data disconnected, turn off radio right away.
D RILJ    : [3730]> RADIO_POWER off [SUB0]
D DCT     : [0]handleMessage msg={ when=-100ms what=270365 obj=radioTurnedOff target=com.android.internal.telephony.dataconnection.DcTracker }
D DCT     : [0]cleanUpAllConnections: tearDown=true reason=radioTurnedOff
D DCT     : [0]cleanUpConnection: tearDown=true reason=radioTurnedOff apnContext={mApnType=default mState=IDLE mWaitingApns={null} mWaitingApnsPermanentFailureCountDown=0 mApnSetting={null} mReason=radioTurnedOff mDataEnabled=false mDependencyMet=true}
D DCT     : [0]setupDataForSinglePdn: reason = radioTurnedOff isDisconnected = true
D DCT     : [0]isOnlySingleDcAllowed(0): false
D DCT     : [0]cleanUpConnection: X tearDown=true reason=radioTurnedOff apnContext={mApnType=default mState=IDLE mWaitingApns={null} mWaitingApnsPermanentFailureCountDown=0 mApnSetting={null} mReason=radioTurnedOff mDataEnabled=false mDependencyMet=true} dcac=null
D DCT     : [0]cleanUpConnection: tearDown=true reason=radioTurnedOff apnContext={mApnType=mms mState=IDLE mWaitingApns={null} mWaitingApnsPermanentFailureCountDown=0 mApnSetting={null} mReason=radioTurnedOff mDataEnabled=false mDependencyMet=true}
D DCT     : [0]setupDataForSinglePdn: reason = radioTurnedOff isDisconnected = true
D DCT     : [0]isOnlySingleDcAllowed(0): false
D DCT     : [0]cleanUpConnection: X tearDown=true reason=radioTurnedOff apnContext={mApnType=mms mState=IDLE mWaitingApns={null} mWaitingApnsPermanentFailureCountDown=0 mApnSetting={null} mReason=radioTurnedOff mDataEnabled=false mDependencyMet=true} dcac=null
D DCT     : [0]cleanUpConnection: tearDown=true reason=radioTurnedOff apnContext={mApnType=supl mState=IDLE mWaitingApns={null} mWaitingApnsPermanentFailureCountDown=0 mApnSetting={null} mReason=radioTurnedOff mDataEnabled=false mDependencyMet=true}
D DCT     : [0]setupDataForSinglePdn: reason = radioTurnedOff isDisconnected = true
D DCT     : [0]isOnlySingleDcAllowed(0): false
D DCT     : [0]cleanUpConnection: X tearDown=true reason=radioTurnedOff apnContext={mApnType=supl mState=IDLE mWaitingApns={null} mWaitingApnsPermanentFailureCountDown=0 mApnSetting={null} mReason=radioTurnedOff mDataEnabled=false mDependencyMet=true} dcac=null
D DCT     : [0]cleanUpConnection: tearDown=true reason=radioTurnedOff apnContext={mApnType=dun mState=IDLE mWaitingApns={null} mWaitingApnsPermanentFailureCountDown=0 mApnSetting={null} mReason=radioTurnedOff mDataEnabled=false mDependencyMet=true}
D DCT     : [0]setupDataForSinglePdn: reason = radioTurnedOff isDisconnected = true
D DCT     : [0]isOnlySingleDcAllowed(0): false
D DCT     : [0]cleanUpConnection: X tearDown=true reason=radioTurnedOff apnContext={mApnType=dun mState=IDLE mWaitingApns={null} mWaitingApnsPermanentFailureCountDown=0 mApnSetting={null} mReason=radioTurnedOff mDataEnabled=false mDependencyMet=true} dcac=null
D DCT     : [0]cleanUpConnection: tearDown=true reason=radioTurnedOff apnContext={mApnType=hipri mState=IDLE mWaitingApns={null} mWaitingApnsPermanentFailureCountDown=0 mApnSetting={null} mReason=radioTurnedOff mDataEnabled=false mDependencyMet=true}
D DCT     : [0]setupDataForSinglePdn: reason = radioTurnedOff isDisconnected = true
D DCT     : [0]isOnlySingleDcAllowed(0): false
D DCT     : [0]cleanUpConnection: X tearDown=true reason=radioTurnedOff apnContext={mApnType=hipri mState=IDLE mWaitingApns={null} mWaitingApnsPermanentFailureCountDown=0 mApnSetting={null} mReason=radioTurnedOff mDataEnabled=false mDependencyMet=true} dcac=null
D DCT     : [0]stopNetStatPoll
D SubscriptionController: [getSubId]- sSlotIdxToSubId.size == 0, return DummySubIds slotIdx=0
D use-Rlog/RLOG-RIL: 20 RIL requests in the queue (1 pending, 8 handled, 11 unhandled)
D use-Rlog/RLOG-RIL: Requesting low power mode power state
D use-Rlog/RLOG-RIL-IPC: 
D use-Rlog/RLOG-RIL-IPC: xmm626_sec_modem_fmt_send: Sent FMT message
D use-Rlog/RLOG-RIL-IPC: xmm626_sec_modem_fmt_send: Message: mseq=0x1f, command=IPC_PWR_PHONE_STATE, type=IPC_TYPE_EXEC, size=2
D use-Rlog/RLOG-RIL-IPC: ================================= IPC FMT data =================================
D use-Rlog/RLOG-RIL-IPC: [0000]   01 00                                              ..
D use-Rlog/RLOG-RIL-IPC: ================================================================================
D DCT     : [0]cleanUpConnection: mDisconnectPendingCount = 0
D DCT     : [0]notifyDataDisconnectComplete
D SubscriptionController: [getSubId]- sSlotIdxToSubId.size == 0, return DummySubIds slotIdx=0
D SubscriptionController: [getSlotId]- subId invalid
D SubscriptionController: getSimStateForSlotIdx:  simState=NOT_READY ordinal=6
D SubscriptionManager: getSimStateForSubscriber: simState=6 slotIdx=0
D TelephonyManager: getSimState: default sim:-1, sim state for slotIdx=0 is 6, return state as unknown
D SubscriptionController: [getPhoneId]- invalid subId return=-1
D SubscriptionController: [getPhoneId]- invalid subId return=-1
D GsmSST  : [GsmSST] mDeviceShuttingDown = false
D GsmSST  : [GsmSST] mDesiredPowerState = true
D GsmSST  : [GsmSST] getRadioState = RADIO_ON
D GsmSST  : [GsmSST] mPowerOffDelayNeed = true
D GsmSST  : [GsmSST] mAlarmSwitch = false
D SubscriptionController: [getPhoneId]- invalid subId return=-1
D SubscriptionController: [getPhoneId]- invalid subId return=-1
D SubscriptionController: [getSubId]- sSlotIdxToSubId.size == 0, return DummySubIds slotIdx=0
D SubscriptionController: [getSlotId]- subId invalid
D SubscriptionController: getSimStateForSlotIdx:  simState=NOT_READY ordinal=6
D SubscriptionManager: getSimStateForSubscriber: simState=6 slotIdx=0
D TelephonyManager: getSimState: default sim:-1, sim state for slotIdx=0 is 6, return state as unknown
D DCT     : [0]onReceive: action=android.net.wifi.WIFI_STATE_CHANGED
D DCT     : [0]WIFI_STATE_CHANGED_ACTION: enabled=false mIsWifiConnected=false
D DCT     : [0]hasMatchedTetherApnSetting: APN=null
D DCT     : [0]hasMatchedTetherApnSetting: APN=null
D SubscriptionController: [getPhoneId]- invalid subId return=-1
D SubscriptionController: [getPhoneId]- invalid subId return=-1
D DCT     : [0]hasMatchedTetherApnSetting: APN=null
