D/RIL     ( 1891): Created IPC FMT client

D/RIL     ( 1891): Created IPC RFS client

D/RIL     ( 1891): Created SRS client

D/RIL-IPC ( 1891): Starting i9300 modem boot

D/RIL-IPC ( 1891): Opened modem image device

D/RIL-IPC ( 1891): Mapped modem image data to memory

D/RIL-IPC ( 1891): Opened modem boot device

D/RIL-IPC ( 1891): Opened modem link device

D/RIL-IPC ( 1891): Turned the modem off

D/RIL-IPC ( 1891): Turned the modem on

D/RIL-IPC ( 1891): Waited for link connected

D/RIL-IPC ( 1891): Wrote ATAT in ASCII

D/RIL-IPC ( 1891): Read chip id (0x16)

D/RIL-IPC ( 1891): Wrote PSI header

D/RIL-IPC ( 1891): Wrote PSI, CRC is 0xc8

D/RIL-IPC ( 1891): Wrote PSI CRC (0xc8)

D/RIL-IPC ( 1891): Read PSI CRC ACK

D/RIL-IPC ( 1891): Read PSI ACK

D/RIL-IPC ( 1891): Sent XMM626 HSIC PSI

D/RIL-IPC ( 1891): Wrote EBL size

D/RIL-IPC ( 1891): Wrote EBL, CRC is 0xb5

D/RIL-IPC ( 1891): Wrote EBL CRC (0xb5)

D/RIL-IPC ( 1891): Sent XMM626 HSIC EBL

D/RIL-IPC ( 1891): Read port config

D/RIL-IPC ( 1891): Sent XMM626 HSIC port config

D/RIL-IPC ( 1891): Sent XMM626 HSIC SEC start

D/RIL-IPC ( 1891): Sent XMM626 HSIC firmware

D/RIL-IPC ( 1891): Checked nv_data path

D/RIL-IPC ( 1891): Checked nv_data md5 path

D/RIL-IPC ( 1891): Calculated nv_data md5: 1455f7aaa8936eda837ebc27acf1c818

D/RIL-IPC ( 1891): Read nv_data md5: 1455f7aaa8936eda837ebc27acf1c818

D/RIL-IPC ( 1891): Checked nv_data backup path

D/RIL-IPC ( 1891): Loaded nv_data

D/RIL-IPC ( 1891): Sent XMM626 HSIC nv_data

D/RIL-IPC ( 1891): Sent XMM626 HSIC SEC end

D/RIL-IPC ( 1891): Sent XMM626 HSIC HW reset

D/RIL-IPC ( 1891): Waiting for host wake failed

D/RIL-IPC ( 1891): Waited for host wake

D/RIL-IPC ( 1891): Waited for link connected

D/RIL     ( 1891): Opened IPC FMT client

D/RIL     ( 1891): Started IPC FMT client loop

D/RIL     ( 1891): Opened IPC RFS client

D/RIL     ( 1891): Started IPC RFS client loop

D/RIL-SRS ( 1891): Started SRS server loop

D/RIL     ( 1891): Opened SRS client

D/RIL     ( 1891): Started SRS client loop

E/RILC    ( 1891): RIL_register: RIL version 7

D/RIL-IPC ( 1891): 

D/RIL-IPC ( 1891): xmm626_sec_modem_fmt_recv: Received FMT message

D/RIL-IPC ( 1891): xmm626_sec_modem_fmt_recv: Message: aseq=0xff, command=IPC_PWR_PHONE_PWR_UP, type=IPC_TYPE_NOTI, size=0

D/RIL     ( 1891): Updating RIL radio state to 0

D/RIL-IPC ( 1891): 

D/RIL-IPC ( 1891): xmm626_sec_modem_fmt_recv: Received FMT message

D/RIL-IPC ( 1891): xmm626_sec_modem_fmt_recv: Message: aseq=0x00, command=IPC_MISC_ME_IMSI, type=IPC_TYPE_NOTI, size=16

D/RIL-IPC ( 1891): ================================= IPC FMT data =================================

D/RIL-IPC ( 1891): [0000]   0F 30 30 30 30 30 30 30  30 30 30 30 30 30 30 30   .0000000 00000000

D/RIL-IPC ( 1891): ================================================================================

D/RIL-IPC ( 1891): 

D/RIL-IPC ( 1891): xmm626_sec_modem_fmt_recv: Received FMT message

D/RIL-IPC ( 1891): xmm626_sec_modem_fmt_recv: Message: aseq=0xff, command=IPC_NET_REGIST, type=IPC_TYPE_NOTI, size=11

D/RIL-IPC ( 1891): ================================= IPC FMT data =================================

D/RIL-IPC ( 1891): [0000]   FF 02 01 00 00 00 00 00  00 00 00                  ........ ...

D/RIL-IPC ( 1891): ================================================================================

D/RIL-IPC ( 1891): 

D/RIL-IPC ( 1891): xmm626_sec_modem_fmt_recv: Received FMT message

D/RIL-IPC ( 1891): xmm626_sec_modem_fmt_recv: Message: aseq=0xff, command=IPC_NET_REGIST, type=IPC_TYPE_NOTI, size=11

D/RIL-IPC ( 1891): ================================= IPC FMT data =================================

D/RIL-IPC ( 1891): [0000]   FF 03 01 00 00 00 00 00  00 00 00                  ........ ...

D/RIL-IPC ( 1891): ================================================================================

D/RIL-IPC ( 1891): 

D/RIL-IPC ( 1891): xmm626_sec_modem_fmt_recv: Received FMT message

D/RIL-IPC ( 1891): xmm626_sec_modem_fmt_recv: Message: aseq=0x00, command=IPC_DISP_ICON_INFO, type=IPC_TYPE_NOTI, size=4

D/RIL-IPC ( 1891): ================================= IPC FMT data =================================

D/RIL-IPC ( 1891): [0000]   FF 00 00 00                                        ....

D/RIL-IPC ( 1891): ================================================================================

D/RIL-IPC ( 1891): 

D/RIL-IPC ( 1891): xmm626_sec_modem_fmt_recv: Received FMT message

D/RIL-IPC ( 1891): xmm626_sec_modem_fmt_recv: Message: aseq=0xff, command=IPC_SEC_SIM_ICC_TYPE, type=IPC_TYPE_NOTI, size=1

D/RIL-IPC ( 1891): ================================= IPC FMT data =================================

D/RIL-IPC ( 1891): [0000]   02                                                 .

D/RIL-IPC ( 1891): ================================================================================

D/RIL-IPC ( 1891): 

D/RIL-IPC ( 1891): xmm626_sec_modem_fmt_recv: Received FMT message

D/RIL-IPC ( 1891): xmm626_sec_modem_fmt_recv: Message: aseq=0xff, command=IPC_SEC_PIN_STATUS, type=IPC_TYPE_NOTI, size=2

D/RIL-IPC ( 1891): ================================= IPC FMT data =================================

D/RIL-IPC ( 1891): [0000]   03 01                                              ..

D/RIL-IPC ( 1891): ================================================================================

D/RIL-IPC ( 1891): 

D/RIL-IPC ( 1891): xmm626_sec_modem_fmt_recv: Received FMT message

D/RIL-IPC ( 1891): xmm626_sec_modem_fmt_recv: Message: aseq=0xff, command=IPC_SAT_PROACTIVE_CMD, type=IPC_TYPE_INDI, size=13

D/RIL-IPC ( 1891): ================================= IPC FMT data =================================

D/RIL-IPC ( 1891): [0000]   0B 00 D0 09 81 03 01 02  00 82 02 81 82            ........ .....

D/RIL-IPC ( 1891): ================================================================================

D/RIL-IPC ( 1891): Unhandled IPC FMT message: IPC_SAT_PROACTIVE_CMD

I/PHONE   ( 2563): Network Mode set to 0

I/PHONE   ( 2563): Cdma Subscription set to 1

I/PHONE   ( 2563): RILClassname is RIL

D/RILJ    ( 2563): RIL(context, preferredNetworkType=0 cdmaSubscription=1)

D/RILJ    ( 2563): Starting RILReceiver

I/RILJ    ( 2563): Connected to 'rild' socket

I/RILC    ( 1891): libril: new connection

I/RILC    ( 1891): RIL Daemon version: Samsung-RIL

D/RILJ    ( 2563): [UNSL]< UNSOL_RIL_CONNECTED {7}

D/RILJ    ( 2563): [0000]> RADIO_POWER off

D/RILJ    ( 2563): [0001]> REQUEST_SET_PREFERRED_NETWORK_TYPE : 0

D/RIL     ( 1891): 1 RIL request in the queue (1 pending, 0 handled, 0 unhandled)

D/RIL     ( 1891): Requesting low power mode power state

D/RIL-IPC ( 1891): 

D/RIL-IPC ( 1891): xmm626_sec_modem_fmt_send: Sent FMT message

D/RIL-IPC ( 1891): xmm626_sec_modem_fmt_send: Message: mseq=0x01, command=IPC_PWR_PHONE_STATE, type=IPC_TYPE_EXEC, size=2

D/RIL-IPC ( 1891): ================================= IPC FMT data =================================

D/RIL-IPC ( 1891): [0000]   01 00                                              ..

D/RIL-IPC ( 1891): ================================================================================

D/RIL_UiccController( 2563): Creating UiccController

I/PHONE   ( 2563): Creating GSMPhone

D/RILJ    ( 2563): [0002]> RIL_REQUEST_CDMA_SET_SUBSCRIPTION_SOURCE : 1

D/RILJ    ( 2563): [UNSL]< UNSOL_RESPONSE_RADIO_STATE_CHANGED RADIO_OFF

D/RILB    ( 2563): Notifying: radio available

D/RILJ    ( 2563): [0003]> SCREEN_STATE: true

D/PHONE   ( 2563): mDoesRilSendMultipleCallRing=false

D/PHONE   ( 2563): mCallRingDelay=3000

D/RIL     ( 1891): 2 RIL requests in the queue (1 pending, 1 handled, 0 unhandled)

D/RIL     ( 1891): 3 RIL requests in the queue (2 pending, 1 handled, 0 unhandled)

D/RIL-IPC ( 1891): 

D/RIL-IPC ( 1891): xmm626_sec_modem_fmt_send: Sent FMT message

D/RIL-IPC ( 1891): xmm626_sec_modem_fmt_send: Message: mseq=0x02, command=IPC_NET_MODE_SEL, type=IPC_TYPE_SET, size=1

D/RIL-IPC ( 1891): ================================= IPC FMT data =================================

D/RIL-IPC ( 1891): [0000]   01                                                 .

D/RIL-IPC ( 1891): ================================================================================

D/RIL     ( 1891): Unhandled RIL request: 77

D/RIL     ( 1891): 2 RIL requests in the queue (0 pending, 2 handled, 0 unhandled)

D/RIL     ( 1891): 3 RIL requests in the queue (1 pending, 2 handled, 0 unhandled)

D/RILJ    ( 2563): [0002]< RIL_REQUEST_CDMA_SET_SUBSCRIPTION_SOURCE error: com.android.internal.telephony.CommandException: REQUEST_NOT_SUPPORTED

D/RILJ    ( 2563): setPhoneType=1 old value=0

D/SMS     ( 2563): SMSDispatcher: ctor mSmsCapable=true format=3gpp mSmsReceiveDisabled=false mSmsSendDisabled=false

D/GSM     ( 2563): [GsmDCT] DCT.constructor

D/GSM     ( 2563): [GsmDCT] GsmDCT.constructor

D/GSM     ( 2563): [ApnContext:default] set mDependencyMet as false current state is true

D/GSM     ( 2563): [ApnContext:default] set enabled as true, current state is false

D/GSM     ( 2563): [GsmDCT] applyNewState(default, true(true), true(false))

D/GSM     ( 2563): [ApnContext:default] set reason as dependencyMet,current state IDLE

D/GSM     ( 2563): [ApnContext:default] set enabled as true, current state is true

D/GSM     ( 2563): [ApnContext:default] set mDependencyMet as true current state is false

D/GSM     ( 2563): [GsmDCT] trySetupData for type:default due to dependencyMet

D/GSM     ( 2563): [GsmDCT] trySetupData with mIsPsRestricted=false

D/GSM     ( 2563): [GsmDCT] isDataAllowed: not allowed due to - gprs= 1 - SIM not loaded

D/GSM     ( 2563): [GsmDCT] notifyOffApnsOfAvailability skipped apn due to isReady==false: {mApnType=default mState=IDLE mWaitingApns=null mWaitingApnsPermanentFailureCountDown=0 mApnSetting=null mDataConnectionAc=null mReason=dependencyMet mRetryCount=0 mDataEnabled=true mDependencyMet=true}

D/GSM     ( 2563): [ApnContext:mms] set mDependencyMet as false current state is true

D/GSM     ( 2563): [GsmDCT] applyNewState(mms, false(false), true(false))

D/GSM     ( 2563): [ApnContext:mms] set enabled as false, current state is false

D/GSM     ( 2563): [ApnContext:mms] set mDependencyMet as true current state is false

D/GSM     ( 2563): [ApnContext:supl] set mDependencyMet as false current state is true

D/GSM     ( 2563): [GsmDCT] applyNewState(supl, false(false), true(false))

D/GSM     ( 2563): [ApnContext:supl] set enabled as false, current state is false

D/GSM     ( 2563): [ApnContext:supl] set mDependencyMet as true current state is false

D/GSM     ( 2563): [ApnContext:dun] set mDependencyMet as false current state is true

D/GSM     ( 2563): [GsmDCT] applyNewState(dun, false(false), true(false))

D/GSM     ( 2563): [ApnContext:dun] set enabled as false, current state is false

D/GSM     ( 2563): [ApnContext:dun] set mDependencyMet as true current state is false

D/GSM     ( 2563): [ApnContext:hipri] set mDependencyMet as false current state is true

D/GSM     ( 2563): [GsmDCT] applyNewState(hipri, false(false), true(false))

D/GSM     ( 2563): [ApnContext:hipri] set enabled as false, current state is false

D/GSM     ( 2563): [ApnContext:hipri] set mDependencyMet as true current state is false

D/RILB    ( 2563): registerForRilConnected h=Handler (com.android.internal.telephony.PhoneProxy) {416f1308} w=4

D/RILB    ( 2563): Notifying: ril connected mRilVersion=7

D/RIL_IccCardProxy( 2563): Creating

D/RIL_IccCardProxy( 2563): Broadcasting intent ACTION_SIM_STATE_CHANGED NOT_READY reason null

D/RIL-IPC ( 1891): 

D/RIL-IPC ( 1891): xmm626_sec_modem_fmt_recv: Received FMT message

D/RIL-IPC ( 1891): xmm626_sec_modem_fmt_recv: Message: aseq=0x01, command=IPC_GEN_PHONE_RES, type=IPC_TYPE_RESP, size=5

D/RIL-IPC ( 1891): ================================= IPC FMT data =================================

D/RIL-IPC ( 1891): [0000]   01 07 01 00 80                                     .....

D/RIL-IPC ( 1891): ================================================================================

D/RIL     ( 1891): Generic response was expected

D/RIL-IPC ( 1891): 

D/RIL-IPC ( 1891): xmm626_sec_modem_fmt_recv: Received FMT message

D/RIL-IPC ( 1891): xmm626_sec_modem_fmt_recv: Message: aseq=0x01, command=IPC_PWR_PHONE_STATE, type=IPC_TYPE_NOTI, size=1

D/RIL-IPC ( 1891): ================================= IPC FMT data =================================

D/RIL-IPC ( 1891): [0000]   01                                                 .

D/RIL-IPC ( 1891): ================================================================================

D/RIL     ( 1891): Power state is low power mode

D/RIL     ( 1891): 2 RIL requests in the queue (0 pending, 1 handled, 1 unhandled)

D/RILJ    ( 2563): [0000]< RADIO_POWER 

D/RIL-IPC ( 1891): 

D/RIL-IPC ( 1891): xmm626_sec_modem_fmt_recv: Received FMT message

D/RIL-IPC ( 1891): xmm626_sec_modem_fmt_recv: Message: aseq=0x02, command=IPC_GEN_PHONE_RES, type=IPC_TYPE_RESP, size=5

D/RIL-IPC ( 1891): ================================= IPC FMT data =================================

D/RIL-IPC ( 1891): [0000]   08 0A 03 00 80                                     .....

D/RIL-IPC ( 1891): ================================================================================

D/RIL     ( 1891): Generic response was expected

D/RIL     ( 1891): 1 RIL request in the queue (0 pending, 0 handled, 1 unhandled)

D/RILJ    ( 2563): [0001]< REQUEST_SET_PREFERRED_NETWORK_TYPE 

D/RIL_IccCardProxy( 2563): Setting radio tech UMTS

D/RIL_IccCardProxy( 2563): updateQuietMode: 3GPP subscription -> newQuietMode=false

D/RIL_IccCardProxy( 2563): updateQuietMode: QuietMode is false (app_type=1 isLteOnCdmaMode=false cdmaSource=-1)

D/RILJ    ( 2563): [0004]> SET_SUPP_SVC_NOTIFICATION

D/RIL     ( 1891): 2 RIL requests in the queue (1 pending, 0 handled, 1 unhandled)

D/RIL     ( 1891): Unhandled RIL request: 62

D/RIL     ( 1891): 1 RIL request in the queue (0 pending, 0 handled, 1 unhandled)

D/RILJ    ( 2563): [0004]< SET_SUPP_SVC_NOTIFICATION error: com.android.internal.telephony.CommandException: REQUEST_NOT_SUPPORTED

D/RILJ    ( 2563): [0005]> RADIO_POWER on

D/RIL     ( 1891): 2 RIL requests in the queue (1 pending, 0 handled, 1 unhandled)

D/RIL     ( 1891): Requesting normal power state

D/RIL-IPC ( 1891): 

D/RIL-IPC ( 1891): xmm626_sec_modem_fmt_send: Sent FMT message

D/RIL-IPC ( 1891): xmm626_sec_modem_fmt_send: Message: mseq=0x03, command=IPC_PWR_PHONE_STATE, type=IPC_TYPE_EXEC, size=2

D/RIL-IPC ( 1891): ================================= IPC FMT data =================================

D/RIL-IPC ( 1891): [0000]   02 02                                              ..

D/RIL-IPC ( 1891): ================================================================================

D/GSM     ( 2563): [GsmSST] Poll ServiceState done:  oldSS=[1 home null null null  Unknown CSS not supported 0 0 RoamInd=0 DefRoamInd=0 EmergOnly=false] newSS=[3 home null null null  Unknown CSS not supported -1 -1 RoamInd=-1 DefRoamInd=-1 EmergOnly=false] oldGprs=1 newData=1 oldMaxDataCalls=1 mNewMaxDataCalls=1 oldReasonDataDenied=-1 mNewReasonDataDenied=-1 oldType=Unknown newType=Unknown

D/GSM     ( 2563): [GsmSST] updateSpnDisplay: radio is off w/ showPlmn=false plmn=null

D/GSM     ( 2563): [GsmSST] updateSpnDisplay: changed sending intent rule=0 showPlmn='false' plmn='null' showSpn='false' spn=''

D/GSM     ( 2563): [GsmSST] operatorNumeric is null

D/GSM     ( 2563): [GsmDCT] handleMessage msg={ what=270369 when=-130ms obj=android.os.AsyncResult@41701918 }

D/GSM     ( 2563): [GsmDCT] handleMessage msg={ what=270337 when=-124ms obj=android.os.AsyncResult@417024f0 }

D/GSM     ( 2563): [GsmDCT] onRadioAvailable

D/RIL-IPC ( 1891): 

D/RIL-IPC ( 1891): xmm626_sec_modem_fmt_recv: Received FMT message

D/RIL-IPC ( 1891): xmm626_sec_modem_fmt_recv: Message: aseq=0x03, command=IPC_GEN_PHONE_RES, type=IPC_TYPE_RESP, size=5

D/RIL-IPC ( 1891): ================================= IPC FMT data =================================

D/RIL-IPC ( 1891): [0000]   01 07 01 00 80                                     .....

D/RIL-IPC ( 1891): ================================================================================

D/RIL     ( 1891): Generic response was expected

D/RIL-IPC ( 1891): 

D/RIL-IPC ( 1891): xmm626_sec_modem_fmt_recv: Received FMT message

D/RIL-IPC ( 1891): xmm626_sec_modem_fmt_recv: Message: aseq=0x03, command=IPC_PWR_PHONE_STATE, type=IPC_TYPE_NOTI, size=1

D/RIL-IPC ( 1891): ================================= IPC FMT data =================================

D/RIL-IPC ( 1891): [0000]   02                                                 .

D/RIL-IPC ( 1891): ================================================================================

D/RIL     ( 1891): Power state is normal

D/RIL     ( 1891): 1 RIL request in the queue (0 pending, 0 handled, 1 unhandled)

D/RIL     ( 1891): Updating RIL radio state to 2

D/RIL-IPC ( 1891): 

D/RIL-IPC ( 1891): xmm626_sec_modem_fmt_recv: Received FMT message

D/RIL-IPC ( 1891): xmm626_sec_modem_fmt_recv: Message: aseq=0x03, command=IPC_SEC_SIM_ICC_TYPE, type=IPC_TYPE_NOTI, size=1

D/RIL-IPC ( 1891): ================================= IPC FMT data =================================

D/RIL-IPC ( 1891): [0000]   02                                                 .

D/RIL-IPC ( 1891): ================================================================================

D/GSM     ( 2563): [GsmDCT] overall state is IDLE

D/RIL-IPC ( 1891): 

D/RIL-IPC ( 1891): xmm626_sec_modem_fmt_recv: Received FMT message

D/RIL-IPC ( 1891): xmm626_sec_modem_fmt_recv: Message: aseq=0x03, command=IPC_SEC_PIN_STATUS, type=IPC_TYPE_NOTI, size=2

D/RIL-IPC ( 1891): ================================= IPC FMT data =================================

D/RIL-IPC ( 1891): [0000]   03 01                                              ..

D/RIL-IPC ( 1891): ================================================================================

D/RIL     ( 1891): ipc2ril_sec_pin_status_response: Selecting status application 3 on 10

D/RIL     ( 1891): Updating RIL radio state to 3

D/GSM     ( 2563): [GsmDCT] handleMessage msg={ what=270342 when=-125ms obj=android.os.AsyncResult@417025e0 }

D/GSM     ( 2563): [ApnContext:dun] setRetryCount: 0

D/RIL-IPC ( 1891): 

D/RIL-IPC ( 1891): xmm626_sec_modem_fmt_recv: Received FMT message

D/GSM     ( 2563): [ApnContext:supl] setRetryCount: 0

D/RIL-IPC ( 1891): xmm626_sec_modem_fmt_recv: Message: aseq=0x03, command=IPC_SAT_PROACTIVE_CMD, type=IPC_TYPE_INDI, size=13

D/RIL-IPC ( 1891): ================================= IPC FMT data =================================

D/RIL-IPC ( 1891): [0000]   0B 00 D0 09 81 03 01 02  00 82 02 81 82            ........ .....

D/RIL-IPC ( 1891): ================================================================================

D/RIL-IPC ( 1891): Unhandled IPC FMT message: IPC_SAT_PROACTIVE_CMD

D/GSM     ( 2563): [ApnContext:hipri] setRetryCount: 0

D/GSM     ( 2563): [ApnContext:default] setRetryCount: 0

D/RIL     ( 1891): 0 RIL request in the queue (0 pending, 0 handled, 0 unhandled)

D/RIL     ( 1891): 1 RIL request data in the queue

D/GSM     ( 2563): [ApnContext:mms] setRetryCount: 0

D/GSM     ( 2563): [GsmDCT] onRadioOffOrNotAvailable: is off and clean up all connections

D/GSM     ( 2563): [GsmDCT] cleanUpAllConnections: tearDown=false reason=radioTurnedOff

D/GSM     ( 2563): [ApnContext:dun] set reason as radioTurnedOff,current state IDLE

D/RIL-IPC ( 1891): 

D/RIL-IPC ( 1891): xmm626_sec_modem_rfs_recv: Received RFS message

D/RIL-IPC ( 1891): xmm626_sec_modem_rfs_recv: Message: aseq=0x01, command=IPC_RFS_NV_WRITE_ITEM, size=12

D/RIL-IPC ( 1891): ================================= IPC RFS data =================================

D/RIL-IPC ( 1891): [0000]   09 00 1A 00 04 00 00 00  0F 00 93 40               ........ ...@

D/RIL-IPC ( 1891): ================================================================================

D/RIL-IPC ( 1891): Checked nv_data path

D/GSM     ( 2563): [GsmDCT] cleanUpConnection: E tearDown=false reason=radioTurnedOff apnContext={mApnType=dun mState=IDLE mWaitingApns=null mWaitingApnsPermanentFailureCountDown=0 mApnSetting=null mDataConnectionAc=null mReason=radioTurnedOff mRetryCount=0 mDataEnabled=false mDependencyMet=true}

D/RILJ    ( 2563): [0005]< RADIO_POWER 

D/GSM     ( 2563): [ApnContext:dun] setState: IDLE, previous state:IDLE

D/RILJ    ( 2563): [UNSL]< UNSOL_VOICE_RADIO_TECH_CHANGED {3}

D/RILJ    ( 2563): [UNSL]< UNSOL_RESPONSE_RADIO_STATE_CHANGED RADIO_ON

D/RILB    ( 2563): Notifying: Radio On

D/GSM     ( 2563): [GsmDCT] isDataAllowed: not allowed due to - gprs= 1 - SIM not loaded

D/RILJ    ( 2563): [UNSL]< UNSOL_RESPONSE_SIM_STATUS_CHANGED

D/RILJ    ( 2563): [UNSL]< UNSOL_RESPONSE_RADIO_STATE_CHANGED RADIO_ON

D/RILJ    ( 2563): [UNSL]< UNSOL_RESPONSE_SIM_STATUS_CHANGED

D/GSM     ( 2563): [GsmDCT] isDataPossible(dun): possible=false isDataAllowed=false apnTypePossible=true apnContextisEnabled=false apnContextState()=IDLE

D/GSM     ( 2563): [GsmDCT] get active apn string for type:dun

D/RILJ    ( 2563): [UNSL]< UNSOL_RESPONSE_VOICE_NETWORK_STATE_CHANGED

D/RILJ    ( 2563): [0003]< SCREEN_STATE 

D/GSM     ( 2563): [ApnContext:dun] setDataConnection: old dc=null new dc=null this={mApnType=dun mState=IDLE mWaitingApns=null mWaitingApnsPermanentFailureCountDown=0 mApnSetting=null mDataConnectionAc=null mReason=radioTurnedOff mRetryCount=0 mDataEnabled=false mDependencyMet=true}

D/GSM     ( 2563): [ApnContext:dun] setDataConnectionAc: old dcac=null new dcac=null

D/GSM     ( 2563): [GsmDCT] cleanUpConnection: X tearDown=false reason=radioTurnedOff apnContext={mApnType=dun mState=IDLE mWaitingApns=null mWaitingApnsPermanentFailureCountDown=0 mApnSetting=null mDataConnectionAc=null mReason=radioTurnedOff mRetryCount=0 mDataEnabled=false mDependencyMet=true} dc=null

D/GSM     ( 2563): [ApnContext:supl] set reason as radioTurnedOff,current state IDLE

D/GSM     ( 2563): [GsmDCT] cleanUpConnection: E tearDown=false reason=radioTurnedOff apnContext={mApnType=supl mState=IDLE mWaitingApns=null mWaitingApnsPermanentFailureCountDown=0 mApnSetting=null mDataConnectionAc=null mReason=radioTurnedOff mRetryCount=0 mDataEnabled=false mDependencyMet=true}

D/GSM     ( 2563): [ApnContext:supl] setState: IDLE, previous state:IDLE

D/GSM     ( 2563): [GsmDCT] isDataAllowed: not allowed due to - gprs= 1 - SIM not loaded

D/GSM     ( 2563): [GsmDCT] isDataPossible(supl): possible=false isDataAllowed=false apnTypePossible=true apnContextisEnabled=false apnContextState()=IDLE

D/GSM     ( 2563): [GsmDCT] get active apn string for type:supl

D/GSM     ( 2563): [ApnContext:supl] setDataConnection: old dc=null new dc=null this={mApnType=supl mState=IDLE mWaitingApns=null mWaitingApnsPermanentFailureCountDown=0 mApnSetting=null mDataConnectionAc=null mReason=radioTurnedOff mRetryCount=0 mDataEnabled=false mDependencyMet=true}

D/GSM     ( 2563): [ApnContext:supl] setDataConnectionAc: old dcac=null new dcac=null

D/GSM     ( 2563): [GsmDCT] cleanUpConnection: X tearDown=false reason=radioTurnedOff apnContext={mApnType=supl mState=IDLE mWaitingApns=null mWaitingApnsPermanentFailureCountDown=0 mApnSetting=null mDataConnectionAc=null mReason=radioTurnedOff mRetryCount=0 mDataEnabled=false mDependencyMet=true} dc=null

D/GSM     ( 2563): [ApnContext:hipri] set reason as radioTurnedOff,current state IDLE

D/GSM     ( 2563): [GsmDCT] cleanUpConnection: E tearDown=false reason=radioTurnedOff apnContext={mApnType=hipri mState=IDLE mWaitingApns=null mWaitingApnsPermanentFailureCountDown=0 mApnSetting=null mDataConnectionAc=null mReason=radioTurnedOff mRetryCount=0 mDataEnabled=false mDependencyMet=true}

D/GSM     ( 2563): [ApnContext:hipri] setState: IDLE, previous state:IDLE

D/GSM     ( 2563): [GsmDCT] isDataAllowed: not allowed due to - gprs= 1 - SIM not loaded

D/GSM     ( 2563): [GsmDCT] isDataPossible(hipri): possible=false isDataAllowed=false apnTypePossible=true apnContextisEnabled=false apnContextState()=IDLE

D/GSM     ( 2563): [GsmDCT] get active apn string for type:hipri

D/GSM     ( 2563): [ApnContext:hipri] setDataConnection: old dc=null new dc=null this={mApnType=hipri mState=IDLE mWaitingApns=null mWaitingApnsPermanentFailureCountDown=0 mApnSetting=null mDataConnectionAc=null mReason=radioTurnedOff mRetryCount=0 mDataEnabled=false mDependencyMet=true}

D/GSM     ( 2563): [ApnContext:hipri] setDataConnectionAc: old dcac=null new dcac=null

D/GSM     ( 2563): [GsmDCT] cleanUpConnection: X tearDown=false reason=radioTurnedOff apnContext={mApnType=hipri mState=IDLE mWaitingApns=null mWaitingApnsPermanentFailureCountDown=0 mApnSetting=null mDataConnectionAc=null mReason=radioTurnedOff mRetryCount=0 mDataEnabled=false mDependencyMet=true} dc=null

D/GSM     ( 2563): [ApnContext:default] set reason as radioTurnedOff,current state IDLE

D/GSM     ( 2563): [GsmDCT] cleanUpConnection: E tearDown=false reason=radioTurnedOff apnContext={mApnType=default mState=IDLE mWaitingApns=null mWaitingApnsPermanentFailureCountDown=0 mApnSetting=null mDataConnectionAc=null mReason=radioTurnedOff mRetryCount=0 mDataEnabled=true mDependencyMet=true}

D/GSM     ( 2563): [ApnContext:default] setState: IDLE, previous state:IDLE

D/GSM     ( 2563): [GsmDCT] isDataAllowed: not allowed due to - gprs= 1 - SIM not loaded

D/GSM     ( 2563): [GsmDCT] isDataPossible(default): possible=false isDataAllowed=false apnTypePossible=true apnContextisEnabled=true apnContextState()=IDLE

D/GSM     ( 2563): [GsmDCT] get active apn string for type:default

D/GSM     ( 2563): [ApnContext:default] setDataConnection: old dc=null new dc=null this={mApnType=default mState=IDLE mWaitingApns=null mWaitingApnsPermanentFailureCountDown=0 mApnSetting=null mDataConnectionAc=null mReason=radioTurnedOff mRetryCount=0 mDataEnabled=true mDependencyMet=true}

D/GSM     ( 2563): [ApnContext:default] setDataConnectionAc: old dcac=null new dcac=null

D/GSM     ( 2563): [GsmDCT] cleanUpConnection: X tearDown=false reason=radioTurnedOff apnContext={mApnType=default mState=IDLE mWaitingApns=null mWaitingApnsPermanentFailureCountDown=0 mApnSetting=null mDataConnectionAc=null mReason=radioTurnedOff mRetryCount=0 mDataEnabled=true mDependencyMet=true} dc=null

D/GSM     ( 2563): [ApnContext:mms] set reason as radioTurnedOff,current state IDLE

D/GSM     ( 2563): [GsmDCT] cleanUpConnection: E tearDown=false reason=radioTurnedOff apnContext={mApnType=mms mState=IDLE mWaitingApns=null mWaitingApnsPermanentFailureCountDown=0 mApnSetting=null mDataConnectionAc=null mReason=radioTurnedOff mRetryCount=0 mDataEnabled=false mDependencyMet=true}

D/GSM     ( 2563): [ApnContext:mms] setState: IDLE, previous state:IDLE

D/GSM     ( 2563): [GsmDCT] isDataAllowed: not allowed due to - gprs= 1 - SIM not loaded

D/GSM     ( 2563): [GsmDCT] isDataPossible(mms): possible=false isDataAllowed=false apnTypePossible=true apnContextisEnabled=false apnContextState()=IDLE

D/GSM     ( 2563): [GsmDCT] get active apn string for type:mms

D/RIL-RFS ( 1891): Wrote 4 nv_data byte(s) at offset 0x1a0009

D/RIL-IPC ( 1891): 

D/RIL-IPC ( 1891): xmm626_sec_modem_rfs_send: Sent RFS message

D/RIL-IPC ( 1891): xmm626_sec_modem_rfs_send: Message: mseq=0x01, command=IPC_RFS_NV_WRITE_ITEM, size=9

D/RIL-IPC ( 1891): ================================= IPC RFS data =================================

D/RIL-IPC ( 1891): [0000]   01 09 00 1A 00 04 00 00  00                        ........ .

D/RIL-IPC ( 1891): ================================================================================

D/RIL-IPC ( 1891): 

D/RIL-IPC ( 1891): xmm626_sec_modem_fmt_recv: Received FMT message

D/RIL-IPC ( 1891): xmm626_sec_modem_fmt_recv: Message: aseq=0xff, command=IPC_NET_REGIST, type=IPC_TYPE_NOTI, size=11

D/RIL-IPC ( 1891): ================================= IPC FMT data =================================

D/RIL-IPC ( 1891): [0000]   FF 02 01 00 00 00 00 00  00 00 00                  ........ ...

D/RIL-IPC ( 1891): ================================================================================

D/RIL-IPC ( 1891): 

D/RIL-IPC ( 1891): xmm626_sec_modem_fmt_recv: Received FMT message

D/RIL-IPC ( 1891): xmm626_sec_modem_fmt_recv: Message: aseq=0xff, command=IPC_NET_REGIST, type=IPC_TYPE_NOTI, size=11

D/RIL-IPC ( 1891): ================================= IPC FMT data =================================

D/RIL-IPC ( 1891): [0000]   FF 03 01 00 00 00 00 00  00 00 00                  ........ ...

D/RIL-IPC ( 1891): ================================================================================

D/RIL-IPC ( 1891): 

D/RIL-IPC ( 1891): xmm626_sec_modem_fmt_recv: Received FMT message

D/RIL-IPC ( 1891): xmm626_sec_modem_fmt_recv: Message: aseq=0x00, command=IPC_DISP_ICON_INFO, type=IPC_TYPE_NOTI, size=4

D/RIL-IPC ( 1891): ================================= IPC FMT data =================================

D/RIL-IPC ( 1891): [0000]   FF 00 00 05                                        ....

D/RIL-IPC ( 1891): ================================================================================

D/RIL     ( 1891): Signal strength is 1

D/RIL-IPC ( 1891): 

D/RIL-IPC ( 1891): xmm626_sec_modem_fmt_recv: Received FMT message

D/RIL-IPC ( 1891): xmm626_sec_modem_fmt_recv: Message: aseq=0xff, command=IPC_NET_REGIST, type=IPC_TYPE_NOTI, size=11

D/RIL-IPC ( 1891): ================================= IPC FMT data =================================

D/RIL-IPC ( 1891): [0000]   FF 02 04 00 00 00 00 00  00 00 00                  ........ ...

D/RIL-IPC ( 1891): ================================================================================

D/RIL-IPC ( 1891): 

D/RIL-IPC ( 1891): xmm626_sec_modem_fmt_recv: Received FMT message

D/RIL-IPC ( 1891): xmm626_sec_modem_fmt_recv: Message: aseq=0xff, command=IPC_NET_REGIST, type=IPC_TYPE_NOTI, size=11

D/RIL-IPC ( 1891): ================================= IPC FMT data =================================

D/RIL-IPC ( 1891): [0000]   FF 03 01 00 00 00 00 00  00 00 00                  ........ ...

D/RIL-IPC ( 1891): ================================================================================

D/RIL-IPC ( 1891): 

D/RIL-IPC ( 1891): xmm626_sec_modem_fmt_recv: Received FMT message

D/RIL-IPC ( 1891): xmm626_sec_modem_fmt_recv: Message: aseq=0x00, command=IPC_NET_SERVING_NETWORK, type=IPC_TYPE_NOTI, size=11

D/RIL-IPC ( 1891): ================================= IPC FMT data =================================

D/RIL-IPC ( 1891): [0000]   02 04 FF 32 30 36 30 31  23 00 00                  ...20601 #..

D/RIL-IPC ( 1891): ================================================================================

D/RILJ    ( 2563): [UNSL]< UNSOL_RESPONSE_VOICE_NETWORK_STATE_CHANGED

D/RILJ    ( 2563): [UNSL]< UNSOL_RESPONSE_VOICE_NETWORK_STATE_CHANGED

D/RILJ    ( 2563): [UNSL]< UNSOL_RESPONSE_VOICE_NETWORK_STATE_CHANGED

D/RILJ    ( 2563): [UNSL]< UNSOL_RESPONSE_VOICE_NETWORK_STATE_CHANGED

D/RILJ    ( 2563): [UNSL]< UNSOL_RESPONSE_VOICE_NETWORK_STATE_CHANGED

D/GSM     ( 2563): [ApnContext:mms] setDataConnection: old dc=null new dc=null this={mApnType=mms mState=IDLE mWaitingApns=null mWaitingApnsPermanentFailureCountDown=0 mApnSetting=null mDataConnectionAc=null mReason=radioTurnedOff mRetryCount=0 mDataEnabled=false mDependencyMet=true}

D/GSM     ( 2563): [ApnContext:mms] setDataConnectionAc: old dcac=null new dcac=null

D/RIL-IPC ( 1891): 

D/RIL-IPC ( 1891): xmm626_sec_modem_rfs_recv: Received RFS message

D/RIL-IPC ( 1891): xmm626_sec_modem_rfs_recv: Message: aseq=0x01, command=IPC_RFS_NV_WRITE_ITEM, size=9

D/RIL-IPC ( 1891): ================================= IPC RFS data =================================

D/RIL-IPC ( 1891): [0000]   10 00 1A 00 01 00 00 00  02                        ........ .

D/RIL-IPC ( 1891): ================================================================================

D/GSM     ( 2563): [GsmDCT] cleanUpConnection: X tearDown=false reason=radioTurnedOff apnContext={mApnType=mms mState=IDLE mWaitingApns=null mWaitingApnsPermanentFailureCountDown=0 mApnSetting=null mDataConnectionAc=null mReason=radioTurnedOff mRetryCount=0 mDataEnabled=false mDependencyMet=true} dc=null

D/RIL-IPC ( 1891): Checked nv_data path

D/GSM     ( 2563): [GsmDCT] stopNetStatPoll

D/GSM     ( 2563): [GsmDCT] notifyOffApnOfAvailability type:dun

D/GSM     ( 2563): [GsmDCT] isDataAllowed: not allowed due to - gprs= 1 - SIM not loaded

D/GSM     ( 2563): [GsmDCT] isDataPossible(dun): possible=false isDataAllowed=false apnTypePossible=true apnContextisEnabled=false apnContextState()=IDLE

D/GSM     ( 2563): [GsmDCT] get active apn string for type:dun

D/GSM     ( 2563): [GsmDCT] notifyOffApnOfAvailability type:supl

D/GSM     ( 2563): [GsmDCT] isDataAllowed: not allowed due to - gprs= 1 - SIM not loaded

D/GSM     ( 2563): [GsmDCT] isDataPossible(supl): possible=false isDataAllowed=false apnTypePossible=true apnContextisEnabled=false apnContextState()=IDLE

D/GSM     ( 2563): [GsmDCT] get active apn string for type:supl

D/GSM     ( 2563): [GsmDCT] notifyOffApnOfAvailability type:hipri

D/GSM     ( 2563): [GsmDCT] isDataAllowed: not allowed due to - gprs= 1 - SIM not loaded

D/GSM     ( 2563): [GsmDCT] isDataPossible(hipri): possible=false isDataAllowed=false apnTypePossible=true apnContextisEnabled=false apnContextState()=IDLE

D/GSM     ( 2563): [GsmDCT] get active apn string for type:hipri

D/GSM     ( 2563): [GsmDCT] notifyOffApnsOfAvailability skipped apn due to isReady==false: {mApnType=default mState=IDLE mWaitingApns=null mWaitingApnsPermanentFailureCountDown=0 mApnSetting=null mDataConnectionAc=null mReason=radioTurnedOff mRetryCount=0 mDataEnabled=true mDependencyMet=true}

D/GSM     ( 2563): [GsmDCT] notifyOffApnOfAvailability type:mms

D/GSM     ( 2563): [GsmDCT] isDataAllowed: not allowed due to - gprs= 1 - SIM not loaded

D/GSM     ( 2563): [GsmDCT] isDataPossible(mms): possible=false isDataAllowed=false apnTypePossible=true apnContextisEnabled=false apnContextState()=IDLE

D/GSM     ( 2563): [GsmDCT] get active apn string for type:mms

D/GSM     ( 2563): [GsmDCT] handleMessage msg={ what=270345 when=-188ms obj=android.os.AsyncResult@417028b8 }

D/GSM     ( 2563): [GsmDCT] onDataConnectionDetached: stop polling and notify detached

D/GSM     ( 2563): [GsmDCT] stopNetStatPoll

D/GSM     ( 2563): [GsmDCT] notifyDataConnection: reason=dataDetached

D/GSM     ( 2563): [GsmDCT] notifyDataConnection: type:default

D/GSM     ( 2563): [GsmDCT] isDataAllowed: not allowed due to - gprs= 1 - SIM not loaded

D/GSM     ( 2563): [GsmDCT] isDataPossible(default): possible=false isDataAllowed=false apnTypePossible=true apnContextisEnabled=true apnContextState()=IDLE

D/GSM     ( 2563): [GsmDCT] get active apn string for type:default

D/GSM     ( 2563): [GsmDCT] notifyOffApnOfAvailability type:dun

D/GSM     ( 2563): [GsmDCT] isDataAllowed: not allowed due to - gprs= 1 - SIM not loaded

D/GSM     ( 2563): [GsmDCT] isDataPossible(dun): possible=false isDataAllowed=false apnTypePossible=true apnContextisEnabled=false apnContextState()=IDLE

D/GSM     ( 2563): [GsmDCT] get active apn string for type:dun

D/GSM     ( 2563): [GsmDCT] notifyOffApnOfAvailability type:supl

D/GSM     ( 2563): [GsmDCT] isDataAllowed: not allowed due to - gprs= 1 - SIM not loaded

D/GSM     ( 2563): [GsmDCT] isDataPossible(supl): possible=false isDataAllowed=false apnTypePossible=true apnContextisEnabled=false apnContextState()=IDLE

D/GSM     ( 2563): [GsmDCT] get active apn string for type:supl

D/GSM     ( 2563): [GsmDCT] notifyOffApnOfAvailability type:hipri

D/GSM     ( 2563): [GsmDCT] isDataAllowed: not allowed due to - gprs= 1 - SIM not loaded

D/GSM     ( 2563): [GsmDCT] isDataPossible(hipri): possible=false isDataAllowed=false apnTypePossible=true apnContextisEnabled=false apnContextState()=IDLE

D/GSM     ( 2563): [GsmDCT] get active apn string for type:hipri

D/GSM     ( 2563): [GsmDCT] notifyOffApnsOfAvailability skipped apn due to isReady==false: {mApnType=default mState=IDLE mWaitingApns=null mWaitingApnsPermanentFailureCountDown=0 mApnSetting=null mDataConnectionAc=null mReason=radioTurnedOff mRetryCount=0 mDataEnabled=true mDependencyMet=true}

D/GSM     ( 2563): [GsmDCT] notifyOffApnOfAvailability type:mms

D/GSM     ( 2563): [GsmDCT] isDataAllowed: not allowed due to - gprs= 1 - SIM not loaded

D/GSM     ( 2563): [GsmDCT] isDataPossible(mms): possible=false isDataAllowed=false apnTypePossible=true apnContextisEnabled=false apnContextState()=IDLE

D/GSM     ( 2563): [GsmDCT] get active apn string for type:mms

D/RIL-RFS ( 1891): Wrote 1 nv_data byte(s) at offset 0x1a0010

D/RIL-IPC ( 1891): 

D/RIL-IPC ( 1891): xmm626_sec_modem_rfs_send: Sent RFS message

D/RIL-IPC ( 1891): xmm626_sec_modem_rfs_send: Message: mseq=0x01, command=IPC_RFS_NV_WRITE_ITEM, size=9

D/RIL-IPC ( 1891): ================================= IPC RFS data =================================

D/RIL-IPC ( 1891): [0000]   01 10 00 1A 00 01 00 00  00                        ........ .

D/RIL-IPC ( 1891): ================================================================================

D/GSM     ( 2563): [GsmDCT] handleMessage msg={ what=270348 when=-198ms obj=android.os.AsyncResult@41702a10 }

D/GSM     ( 2563): [ApnContext:dun] setRetryCount: 0

D/GSM     ( 2563): [ApnContext:supl] setRetryCount: 0

D/GSM     ( 2563): [ApnContext:hipri] setRetryCount: 0

D/GSM     ( 2563): [ApnContext:default] setRetryCount: 0

D/GSM     ( 2563): [ApnContext:mms] setRetryCount: 0

D/GSM     ( 2563): [GsmDCT] onRoamingOff

D/RILJ    ( 2563): [0006]> BASEBAND_VERSION

D/RILJ    ( 2563): [0007]> GET_IMEI

D/RIL     ( 1891): 1 RIL request in the queue (1 pending, 0 handled, 0 unhandled)

D/RIL     ( 1891): 6 RIL requests data in the queue

D/RIL-IPC ( 1891): 

D/RIL-IPC ( 1891): xmm626_sec_modem_fmt_send: Sent FMT message

D/RIL-IPC ( 1891): xmm626_sec_modem_fmt_send: Message: mseq=0x04, command=IPC_MISC_ME_VERSION, type=IPC_TYPE_GET, size=1

D/RIL-IPC ( 1891): ================================= IPC FMT data =================================

D/RIL-IPC ( 1891): [0000]   FF                                                 .

D/RIL-IPC ( 1891): ================================================================================

D/RILJ    ( 2563): [0008]> GET_IMEISV

D/RIL-IPC ( 1891): 

D/RIL-IPC ( 1891): xmm626_sec_modem_fmt_recv: Received FMT message

D/RIL-IPC ( 1891): xmm626_sec_modem_fmt_recv: Message: aseq=0x04, command=IPC_MISC_ME_VERSION, type=IPC_TYPE_RESP, size=148

D/RIL-IPC ( 1891): ================================= IPC FMT data =================================

D/RIL-IPC ( 1891): [0000]   1F 49 39 33 30 30 58 58  55 47 4E 41 38 00 00 00   .I9300XX UGNA8...

D/RIL-IPC ( 1891): [0010]   00 00 00 00 00 00 00 00  00 00 00 00 00 00 00 00   ........ ........

D/RIL-IPC ( 1891): [0020]   00 4D 50 20 31 2E 31 30  30 00 00 00 00 00 00 00   .MP 1.10 0.......

D/RIL-IPC ( 1891): [0030]   00 00 00 00 00 00 00 00  00 00 00 00 00 00 00 00   ........ ........

D/RIL-IPC ( 1891): [0040]   00 32 30 31 32 2E 37 2E  34 00 00 00 00 00 00 00   .2012.7. 4.......

D/RIL-IPC ( 1891): [0050]   00 00 00 00 00 00 00 00  00 00 00 00 00 00 00 00   ........ ........

D/RIL-IPC ( 1891): [0060]   00 47 54 2D 49 39 33 30  30 4D 42 44 43 59 4F 00   .GT-I930 0MBDCYO.

D/RIL-IPC ( 1891): [0070]   00 00 00 00 00 00 00 00  00 00 00 00 00 00 00 00   ........ ........

D/RIL-IPC ( 1891): [0080]   00 49 39 33 30 30 00 00  00 00 00 00 00 00 00 00   .I9300.. ........

D/RIL-IPC ( 1891): [0090]   00 00 00 00                                        ....

D/RIL-IPC ( 1891): ================================================================================

D/RIL     ( 1891): 0 RIL request in the queue (0 pending, 0 handled, 0 unhandled)

D/RIL     ( 1891): 6 RIL requests data in the queue

D/RIL     ( 1891): 1 RIL request in the queue (1 pending, 0 handled, 0 unhandled)

D/RIL     ( 1891): 6 RIL requests data in the queue

D/RIL-IPC ( 1891): 

D/RIL-IPC ( 1891): xmm626_sec_modem_fmt_send: Sent FMT message

D/RIL-IPC ( 1891): xmm626_sec_modem_fmt_send: Message: mseq=0x05, command=IPC_MISC_ME_SN, type=IPC_TYPE_GET, size=1

D/RIL-IPC ( 1891): ================================= IPC FMT data =================================

D/RILJ    ( 2563): [0006]< BASEBAND_VERSION I9300XXUGNA8

D/RIL-IPC ( 1891): [0000]   01                                                 .

D/RIL-IPC ( 1891): ================================================================================

D/RIL     ( 1891): 2 RIL requests in the queue (1 pending, 1 handled, 0 unhandled)

D/RIL     ( 1891): 6 RIL requests data in the queue

D/RIL-IPC ( 1891): 

D/RIL-IPC ( 1891): xmm626_sec_modem_fmt_recv: Received FMT message

D/RIL-IPC ( 1891): xmm626_sec_modem_fmt_recv: Message: aseq=0x05, command=IPC_MISC_ME_SN, type=IPC_TYPE_RESP, size=34

D/RIL-IPC ( 1891): ================================= IPC FMT data =================================

D/RIL-IPC ( 1891): [0000]   01 11 33 35 33 38 31 37  30 35 31 38 32 38 37 31   ..353817 05182871

D/RIL-IPC ( 1891): [0010]   33 30 31 00 00 00 00 00  00 00 00 00 00 00 00 00   301..... ........

D/RIL-IPC ( 1891): [0020]   00 4D                                              .M

D/RIL-IPC ( 1891): ================================================================================

D/RIL     ( 1891): 1 RIL request in the queue (0 pending, 1 handled, 0 unhandled)

D/RIL     ( 1891): 6 RIL requests data in the queue

D/RIL     ( 1891): 0 RIL request in the queue (0 pending, 0 handled, 0 unhandled)

D/RIL     ( 1891): 6 RIL requests data in the queue

D/RILJ    ( 2563): [0007]< GET_IMEI 

D/RILJ    ( 2563): [0008]< GET_IMEISV 

D/PHONE   ( 2563): [PhoneProxy] Ignoring voice radio technology changed message. newVoiceRadioTech = 3 Active Phone = GSM

D/RILJ    ( 2563): [0009]> OPERATOR

D/RIL     ( 1891): 1 RIL request in the queue (1 pending, 0 handled, 0 unhandled)

D/RIL     ( 1891): 6 RIL requests data in the queue

D/RIL     ( 1891): 0 RIL request in the queue (0 pending, 0 handled, 0 unhandled)

D/RILJ    ( 2563): [0010]> DATA_REGISTRATION_STATE

D/RIL     ( 1891): 5 RIL requests data in the queue

D/RILJ    ( 2563): [0009]< OPERATOR {Proximus, Proximus, 20601}

D/RIL     ( 1891): 1 RIL request in the queue (1 pending, 0 handled, 0 unhandled)

D/RIL     ( 1891): 5 RIL requests data in the queue

D/RIL     ( 1891): 0 RIL request in the queue (0 pending, 0 handled, 0 unhandled)

D/RIL     ( 1891): 4 RIL requests data in the queue

D/RILJ    ( 2563): [0011]> VOICE_REGISTRATION_STATE

D/RIL     ( 1891): 1 RIL request in the queue (1 pending, 0 handled, 0 unhandled)

D/RIL     ( 1891): 4 RIL requests data in the queue

D/RIL     ( 1891): 0 RIL request in the queue (0 pending, 0 handled, 0 unhandled)

D/RIL     ( 1891): 3 RIL requests data in the queue

D/RILJ    ( 2563): [0012]> QUERY_NETWORK_SELECTION_MODE

D/RIL     ( 1891): 1 RIL request in the queue (1 pending, 0 handled, 0 unhandled)

D/RIL     ( 1891): 3 RIL requests data in the queue

D/RIL-IPC ( 1891): 

D/RIL-IPC ( 1891): xmm626_sec_modem_fmt_send: Sent FMT message

D/RIL-IPC ( 1891): xmm626_sec_modem_fmt_send: Message: mseq=0x06, command=IPC_NET_PLMN_SEL, type=IPC_TYPE_GET, size=0

D/RILJ    ( 2563): [0010]< DATA_REGISTRATION_STATE {0, 0, 0, 0, 3}

D/RILJ    ( 2563): [0011]< VOICE_REGISTRATION_STATE {0, 0, 0, 0, null, null, null, null, null, null, null, null, null, null, null}

D/RIL_UiccController( 2563): Received EVENT_ICC_STATUS_CHANGED, calling getIccCardStatus

D/RILJ    ( 2563): [0013]> GET_SIM_STATUS

D/RIL-IPC ( 1891): 

D/RIL-IPC ( 1891): xmm626_sec_modem_fmt_recv: Received FMT message

D/RIL-IPC ( 1891): xmm626_sec_modem_fmt_recv: Message: aseq=0x06, command=IPC_NET_PLMN_SEL, type=IPC_TYPE_RESP, size=1

D/RIL-IPC ( 1891): ================================= IPC FMT data =================================

D/RIL-IPC ( 1891): [0000]   02                                                 .

D/RIL-IPC ( 1891): ================================================================================

D/RIL     ( 1891): 0 RIL request in the queue (0 pending, 0 handled, 0 unhandled)

D/RIL     ( 1891): 3 RIL requests data in the queue

D/RILJ    ( 2563): [0012]< QUERY_NETWORK_SELECTION_MODE {0}

D/RIL     ( 1891): 1 RIL request in the queue (1 pending, 0 handled, 0 unhandled)

D/RIL     ( 1891): 3 RIL requests data in the queue

D/RIL     ( 1891): 0 RIL request in the queue (0 pending, 0 handled, 0 unhandled)

D/RIL     ( 1891): 2 RIL requests data in the queue

D/RILJ    ( 2563): [0014]> GET_CURRENT_CALLS

D/RILJ    ( 2563): [0013]< GET_SIM_STATUS IccCardState {CARDSTATE_PRESENT,PINSTATE_UNKNOWN,num_apps=1,gsm_id=0{APPTYPE_SIM,APPSTATE_PIN},cdma_id=-1,ims_id=-1}

D/RIL     ( 1891): 1 RIL request in the queue (1 pending, 0 handled, 0 unhandled)

D/RIL     ( 1891): 2 RIL requests data in the queue

D/RIL-IPC ( 1891): 

D/RIL-IPC ( 1891): xmm626_sec_modem_fmt_send: Sent FMT message

D/RIL-IPC ( 1891): xmm626_sec_modem_fmt_send: Message: mseq=0x07, command=IPC_CALL_LIST, type=IPC_TYPE_GET, size=0

D/RILJ    ( 2563): [0015]> RIL_REQUEST_VOICE_RADIO_TECH

D/RILJ    ( 2563): [0015]< RIL_REQUEST_VOICE_RADIO_TECH {3}

D/RILJ    ( 2563): [0016]> RIL_REQUEST_CDMA_GET_SUBSCRIPTION_SOURCE

D/RIL-IPC ( 1891): 

D/RIL-IPC ( 1891): xmm626_sec_modem_fmt_recv: Received FMT message

D/RIL-IPC ( 1891): xmm626_sec_modem_fmt_recv: Message: aseq=0x07, command=IPC_CALL_LIST, type=IPC_TYPE_RESP, size=1

D/RIL-IPC ( 1891): ================================= IPC FMT data =================================

D/RIL-IPC ( 1891): [0000]   00                                                 .

D/RIL-IPC ( 1891): ================================================================================

D/RIL     ( 1891): 0 RIL request in the queue (0 pending, 0 handled, 0 unhandled)

D/RIL     ( 1891): 2 RIL requests data in the queue

D/RILJ    ( 2563): [0014]< GET_CURRENT_CALLS  

D/RIL_UiccController( 2563): Received EVENT_ICC_STATUS_CHANGED, calling getIccCardStatus

D/RILJ    ( 2563): [0016]< RIL_REQUEST_CDMA_GET_SUBSCRIPTION_SOURCE {0}

D/RILJ    ( 2563): [0017]> GET_SIM_STATUS

D/RIL_UiccController( 2563): Received EVENT_ICC_STATUS_CHANGED, calling getIccCardStatus

D/RILJ    ( 2563): [0018]> GET_SIM_STATUS

D/RIL     ( 1891): 1 RIL request in the queue (1 pending, 0 handled, 0 unhandled)

D/RIL     ( 1891): 2 RIL requests data in the queue

D/RIL-IPC ( 1891): 

D/RIL-IPC ( 1891): xmm626_sec_modem_fmt_send: Sent FMT message

D/RIL-IPC ( 1891): xmm626_sec_modem_fmt_send: Message: mseq=0x08, command=IPC_SEC_PIN_STATUS, type=IPC_TYPE_GET, size=0

D/RIL-IPC ( 1891): 

D/RIL-IPC ( 1891): xmm626_sec_modem_fmt_recv: Received FMT message

D/RIL-IPC ( 1891): xmm626_sec_modem_fmt_recv: Message: aseq=0x08, command=IPC_SEC_PIN_STATUS, type=IPC_TYPE_RESP, size=2

D/RIL-IPC ( 1891): ================================= IPC FMT data =================================

D/RIL-IPC ( 1891): [0000]   03 01                                              ..

D/RIL-IPC ( 1891): ================================================================================

D/RIL     ( 1891): ipc2ril_sec_pin_status_response: Selecting status application 3 on 10

D/RIL     ( 1891): 0 RIL request in the queue (0 pending, 0 handled, 0 unhandled)

D/RIL     ( 1891): 2 RIL requests data in the queue

D/RIL     ( 1891): 1 RIL request in the queue (1 pending, 0 handled, 0 unhandled)

D/RIL     ( 1891): 2 RIL requests data in the queue

D/RIL-IPC ( 1891): 

D/RIL-IPC ( 1891): xmm626_sec_modem_fmt_send: Sent FMT message

D/RIL-IPC ( 1891): xmm626_sec_modem_fmt_send: Message: mseq=0x09, command=IPC_SEC_PIN_STATUS, type=IPC_TYPE_GET, size=0

D/RILJ    ( 2563): [0017]< GET_SIM_STATUS IccCardState {CARDSTATE_PRESENT,PINSTATE_UNKNOWN,num_apps=1,gsm_id=0{APPTYPE_SIM,APPSTATE_PIN},cdma_id=-1,ims_id=-1}

D/RIL-IPC ( 1891): 

D/RIL-IPC ( 1891): xmm626_sec_modem_fmt_recv: Received FMT message

D/RILJ    ( 2563): [0019]> OPERATOR

D/RIL-IPC ( 1891): xmm626_sec_modem_fmt_recv: Message: aseq=0x09, command=IPC_SEC_PIN_STATUS, type=IPC_TYPE_RESP, size=2

D/RIL-IPC ( 1891): ================================= IPC FMT data =================================

D/RIL-IPC ( 1891): [0000]   03 01                                              ..

D/RIL-IPC ( 1891): ================================================================================

D/RIL     ( 1891): ipc2ril_sec_pin_status_response: Selecting status application 3 on 10

D/RIL     ( 1891): 0 RIL request in the queue (0 pending, 0 handled, 0 unhandled)

D/RIL     ( 1891): 2 RIL requests data in the queue

D/RILJ    ( 2563): [0018]< GET_SIM_STATUS IccCardState {CARDSTATE_PRESENT,PINSTATE_UNKNOWN,num_apps=1,gsm_id=0{APPTYPE_SIM,APPSTATE_PIN},cdma_id=-1,ims_id=-1}

D/RILJ    ( 2563): [0020]> DATA_REGISTRATION_STATE

D/RIL     ( 1891): 1 RIL request in the queue (1 pending, 0 handled, 0 unhandled)

D/RIL     ( 1891): 2 RIL requests data in the queue

D/RIL-IPC ( 1891): 

D/RIL-IPC ( 1891): xmm626_sec_modem_fmt_send: Sent FMT message

D/RIL-IPC ( 1891): xmm626_sec_modem_fmt_send: Message: mseq=0x0a, command=IPC_NET_SERVING_NETWORK, type=IPC_TYPE_GET, size=0

D/RILJ    ( 2563): [0021]> VOICE_REGISTRATION_STATE

D/RIL     ( 1891): 2 RIL requests in the queue (1 pending, 1 handled, 0 unhandled)

D/RIL     ( 1891): 2 RIL requests data in the queue

D/RIL     ( 1891): 1 RIL request in the queue (0 pending, 1 handled, 0 unhandled)

D/RIL     ( 1891): 1 RIL request data in the queue

D/RIL-IPC ( 1891): 

D/RIL-IPC ( 1891): xmm626_sec_modem_fmt_recv: Received FMT message

D/RIL-IPC ( 1891): xmm626_sec_modem_fmt_recv: Message: aseq=0x0a, command=IPC_NET_SERVING_NETWORK, type=IPC_TYPE_RESP, size=11

D/RIL-IPC ( 1891): ================================= IPC FMT data =================================

D/RIL-IPC ( 1891): [0000]   02 04 FF 32 30 36 30 31  23 00 00                  ...20601 #..

D/RIL-IPC ( 1891): ================================================================================

D/RILJ    ( 2563): [0020]< DATA_REGISTRATION_STATE {0, 0, 0, 0, 3}

D/RIL     ( 1891): 0 RIL request in the queue (0 pending, 0 handled, 0 unhandled)

D/RIL     ( 1891): 1 RIL request data in the queue

D/RIL     ( 1891): 1 RIL request in the queue (1 pending, 0 handled, 0 unhandled)

D/RIL     ( 1891): 1 RIL request data in the queue

D/RIL     ( 1891): 0 RIL request in the queue (0 pending, 0 handled, 0 unhandled)

D/RILJ    ( 2563): [0022]> QUERY_NETWORK_SELECTION_MODE

D/RILJ    ( 2563): [0019]< OPERATOR {Proximus, Proximus, 20601}

D/RIL     ( 1891): 1 RIL request in the queue (1 pending, 0 handled, 0 unhandled)

D/RIL-IPC ( 1891): 

D/RIL-IPC ( 1891): xmm626_sec_modem_fmt_send: Sent FMT message

D/RIL-IPC ( 1891): xmm626_sec_modem_fmt_send: Message: mseq=0x0b, command=IPC_NET_PLMN_SEL, type=IPC_TYPE_GET, size=0

D/RILJ    ( 2563): [0021]< VOICE_REGISTRATION_STATE {10, 0, 0, 0, null, null, null, null, null, null, null, null, null, null, null}

D/RIL-IPC ( 1891): 

D/RIL-IPC ( 1891): xmm626_sec_modem_fmt_recv: Received FMT message

D/RIL-IPC ( 1891): xmm626_sec_modem_fmt_recv: Message: aseq=0x0b, command=IPC_NET_PLMN_SEL, type=IPC_TYPE_RESP, size=1

D/RIL-IPC ( 1891): ================================= IPC FMT data =================================

D/RIL-IPC ( 1891): [0000]   02                                                 .

D/RIL-IPC ( 1891): ================================================================================

D/RIL     ( 1891): 0 RIL request in the queue (0 pending, 0 handled, 0 unhandled)

D/RILJ    ( 2563): [0022]< QUERY_NETWORK_SELECTION_MODE {0}

D/RILJ    ( 2563): [0023]> OPERATOR

D/RILJ    ( 2563): [0024]> DATA_REGISTRATION_STATE

D/RIL     ( 1891): 1 RIL request in the queue (1 pending, 0 handled, 0 unhandled)

D/RIL-IPC ( 1891): 

D/RIL-IPC ( 1891): xmm626_sec_modem_fmt_send: Sent FMT message

D/RIL-IPC ( 1891): xmm626_sec_modem_fmt_send: Message: mseq=0x0c, command=IPC_NET_SERVING_NETWORK, type=IPC_TYPE_GET, size=0

D/RILJ    ( 2563): [0025]> VOICE_REGISTRATION_STATE

D/RIL     ( 1891): 2 RIL requests in the queue (1 pending, 1 handled, 0 unhandled)

D/RIL-IPC ( 1891): 

D/RIL-IPC ( 1891): xmm626_sec_modem_fmt_send: Sent FMT message

D/RIL-IPC ( 1891): xmm626_sec_modem_fmt_send: Message: mseq=0x0d, command=IPC_NET_REGIST, type=IPC_TYPE_GET, size=2

D/RIL-IPC ( 1891): ================================= IPC FMT data =================================

D/RIL-IPC ( 1891): [0000]   FF 03                                              ..

D/RIL-IPC ( 1891): ================================================================================

D/RIL-IPC ( 1891): 

D/RIL-IPC ( 1891): xmm626_sec_modem_fmt_recv: Received FMT message

D/RIL-IPC ( 1891): xmm626_sec_modem_fmt_recv: Message: aseq=0x0c, command=IPC_NET_SERVING_NETWORK, type=IPC_TYPE_RESP, size=11

D/RIL-IPC ( 1891): ================================= IPC FMT data =================================

D/RIL-IPC ( 1891): [0000]   02 04 FF 32 30 36 30 31  23 00 00                  ...20601 #..

D/RIL-IPC ( 1891): ================================================================================

D/RIL     ( 1891): 1 RIL request in the queue (0 pending, 1 handled, 0 unhandled)

D/RILJ    ( 2563): [0023]< OPERATOR {Proximus, Proximus, 20601}

D/RILJ    ( 2563): [0026]> QUERY_NETWORK_SELECTION_MODE

D/RIL-IPC ( 1891): 

D/RIL-IPC ( 1891): xmm626_sec_modem_fmt_recv: Received FMT message

D/RIL-IPC ( 1891): xmm626_sec_modem_fmt_recv: Message: aseq=0x0d, command=IPC_NET_REGIST, type=IPC_TYPE_RESP, size=11

D/RIL-IPC ( 1891): ================================= IPC FMT data =================================

D/RIL-IPC ( 1891): [0000]   FF 03 01 00 00 00 00 00  00 00 00                  ........ ...

D/RIL-IPC ( 1891): ================================================================================

D/RILJ    ( 2563): [0027]> OPERATOR

D/RIL     ( 1891): 0 RIL request in the queue (0 pending, 0 handled, 0 unhandled)

D/RILJ    ( 2563): [0028]> DATA_REGISTRATION_STATE

D/RILJ    ( 2563): [0029]> VOICE_REGISTRATION_STATE

D/RILJ    ( 2563): [0030]> QUERY_NETWORK_SELECTION_MODE

D/RILJ    ( 2563): [0024]< DATA_REGISTRATION_STATE {0, 0, 0, 0, 3}

D/RIL     ( 1891): 1 RIL request in the queue (1 pending, 0 handled, 0 unhandled)

D/RIL-IPC ( 1891): 

D/RIL-IPC ( 1891): xmm626_sec_modem_fmt_send: Sent FMT message

D/RIL-IPC ( 1891): xmm626_sec_modem_fmt_send: Message: mseq=0x0e, command=IPC_NET_REGIST, type=IPC_TYPE_GET, size=2

D/RIL-IPC ( 1891): ================================= IPC FMT data =================================

D/RIL-IPC ( 1891): [0000]   FF 02                                              ..

D/RIL-IPC ( 1891): ================================================================================

D/RIL     ( 1891): 2 RIL requests in the queue (1 pending, 1 handled, 0 unhandled)

D/RIL-IPC ( 1891): 

D/RIL-IPC ( 1891): xmm626_sec_modem_fmt_send: Sent FMT message

D/RIL-IPC ( 1891): xmm626_sec_modem_fmt_send: Message: mseq=0x0f, command=IPC_NET_PLMN_SEL, type=IPC_TYPE_GET, size=0

D/RIL     ( 1891): 3 RIL requests in the queue (1 pending, 2 handled, 0 unhandled)

D/RIL-IPC ( 1891): 

D/RIL-IPC ( 1891): xmm626_sec_modem_fmt_send: Sent FMT message

D/RIL-IPC ( 1891): xmm626_sec_modem_fmt_send: Message: mseq=0x10, command=IPC_NET_SERVING_NETWORK, type=IPC_TYPE_GET, size=0

D/RIL     ( 1891): 4 RIL requests in the queue (1 pending, 3 handled, 0 unhandled)

D/RIL-IPC ( 1891): 

D/RIL-IPC ( 1891): xmm626_sec_modem_fmt_send: Sent FMT message

D/RIL-IPC ( 1891): xmm626_sec_modem_fmt_send: Message: mseq=0x11, command=IPC_NET_REGIST, type=IPC_TYPE_GET, size=2

D/RIL-IPC ( 1891): ================================= IPC FMT data =================================

D/RIL-IPC ( 1891): [0000]   FF 03                                              ..

D/RIL-IPC ( 1891): ================================================================================

D/RIL-IPC ( 1891): 

D/RIL-IPC ( 1891): xmm626_sec_modem_fmt_recv: Received FMT message

D/RIL-IPC ( 1891): xmm626_sec_modem_fmt_recv: Message: aseq=0x0e, command=IPC_NET_REGIST, type=IPC_TYPE_RESP, size=11

D/RIL-IPC ( 1891): ================================= IPC FMT data =================================

D/RIL-IPC ( 1891): [0000]   FF 02 04 00 00 00 00 00  00 00 00                  ........ ...

D/RIL-IPC ( 1891): ================================================================================

D/RIL     ( 1891): 3 RIL requests in the queue (0 pending, 3 handled, 0 unhandled)

D/RIL     ( 1891): 4 RIL requests in the queue (1 pending, 3 handled, 0 unhandled)

D/RIL-IPC ( 1891): 

D/RIL-IPC ( 1891): xmm626_sec_modem_fmt_send: Sent FMT message

D/RIL-IPC ( 1891): xmm626_sec_modem_fmt_send: Message: mseq=0x12, command=IPC_NET_REGIST, type=IPC_TYPE_GET, size=2

D/RIL-IPC ( 1891): ================================= IPC FMT data =================================

D/RIL-IPC ( 1891): [0000]   FF 02                                              ..

D/RIL-IPC ( 1891): ================================================================================

D/RIL     ( 1891): 5 RIL requests in the queue (1 pending, 4 handled, 0 unhandled)

D/RIL-IPC ( 1891): 

D/RIL-IPC ( 1891): xmm626_sec_modem_fmt_send: Sent FMT message

D/RIL-IPC ( 1891): xmm626_sec_modem_fmt_send: Message: mseq=0x13, command=IPC_NET_PLMN_SEL, type=IPC_TYPE_GET, size=0

D/RILJ    ( 2563): [0025]< VOICE_REGISTRATION_STATE {10, 0, 0, 0, null, null, null, null, null, null, null, null, null, null, null}

D/RIL-IPC ( 1891): 

D/RIL-IPC ( 1891): xmm626_sec_modem_fmt_recv: Received FMT message

D/RIL-IPC ( 1891): xmm626_sec_modem_fmt_recv: Message: aseq=0x0f, command=IPC_NET_PLMN_SEL, type=IPC_TYPE_RESP, size=1

D/RIL-IPC ( 1891): ================================= IPC FMT data =================================

D/RIL-IPC ( 1891): [0000]   02                                                 .

D/RIL-IPC ( 1891): ================================================================================

D/RIL     ( 1891): 4 RIL requests in the queue (0 pending, 4 handled, 0 unhandled)

D/RILJ    ( 2563): [0026]< QUERY_NETWORK_SELECTION_MODE {0}

D/RILJ    ( 2563): [0031]> OPERATOR

D/RIL-IPC ( 1891): 

D/RIL-IPC ( 1891): xmm626_sec_modem_fmt_recv: Received FMT message

D/RIL-IPC ( 1891): xmm626_sec_modem_fmt_recv: Message: aseq=0x10, command=IPC_NET_SERVING_NETWORK, type=IPC_TYPE_RESP, size=11

D/RIL-IPC ( 1891): ================================= IPC FMT data =================================

D/RIL-IPC ( 1891): [0000]   02 04 FF 32 30 36 30 31  23 00 00                  ...20601 #..

D/RIL-IPC ( 1891): ================================================================================

D/RIL     ( 1891): 3 RIL requests in the queue (0 pending, 3 handled, 0 unhandled)

D/RILJ    ( 2563): [0027]< OPERATOR {Proximus, Proximus, 20601}

D/RILJ    ( 2563): [0032]> DATA_REGISTRATION_STATE

D/RIL     ( 1891): 4 RIL requests in the queue (1 pending, 3 handled, 0 unhandled)

D/RIL-IPC ( 1891): 

D/RIL-IPC ( 1891): xmm626_sec_modem_fmt_send: Sent FMT message

D/RIL-IPC ( 1891): xmm626_sec_modem_fmt_send: Message: mseq=0x14, command=IPC_NET_SERVING_NETWORK, type=IPC_TYPE_GET, size=0

D/RILJ    ( 2563): [0033]> VOICE_REGISTRATION_STATE

D/RIL     ( 1891): 5 RIL requests in the queue (1 pending, 4 handled, 0 unhandled)

D/RIL-IPC ( 1891): 

D/RIL-IPC ( 1891): xmm626_sec_modem_fmt_recv: Received FMT message

D/RIL-IPC ( 1891): xmm626_sec_modem_fmt_recv: Message: aseq=0x11, command=IPC_NET_REGIST, type=IPC_TYPE_RESP, size=11

D/RIL-IPC ( 1891): ================================= IPC FMT data =================================

D/RIL-IPC ( 1891): [0000]   FF 03 01 00 00 00 00 00  00 00 00                  ........ ...

D/RIL-IPC ( 1891): ================================================================================

D/RIL     ( 1891): 4 RIL requests in the queue (0 pending, 3 handled, 1 unhandled)

D/RIL-IPC ( 1891): 

D/RIL-IPC ( 1891): xmm626_sec_modem_fmt_recv: Received FMT message

D/RIL-IPC ( 1891): xmm626_sec_modem_fmt_recv: Message: aseq=0x12, command=IPC_NET_REGIST, type=IPC_TYPE_RESP, size=11

D/RIL-IPC ( 1891): ================================= IPC FMT data =================================

D/RIL-IPC ( 1891): [0000]   FF 02 04 00 00 00 00 00  00 00 00                  ........ ...

D/RIL-IPC ( 1891): ================================================================================

D/RIL     ( 1891): 3 RIL requests in the queue (0 pending, 2 handled, 1 unhandled)

D/RIL-IPC ( 1891): 

D/RIL-IPC ( 1891): xmm626_sec_modem_fmt_send: Sent FMT message

D/RIL-IPC ( 1891): xmm626_sec_modem_fmt_send: Message: mseq=0x15, command=IPC_NET_REGIST, type=IPC_TYPE_GET, size=2

D/RIL-IPC ( 1891): ================================= IPC FMT data =================================

D/RIL-IPC ( 1891): [0000]   FF 03                                              ..

D/RIL-IPC ( 1891): ================================================================================

D/RILJ    ( 2563): [0034]> QUERY_NETWORK_SELECTION_MODE

D/RILJ    ( 2563): [0028]< DATA_REGISTRATION_STATE {0, 0, 0, 0, 3}

D/RIL-IPC ( 1891): 

D/RIL-IPC ( 1891): xmm626_sec_modem_fmt_recv: Received FMT message

D/RIL-IPC ( 1891): xmm626_sec_modem_fmt_recv: Message: aseq=0x13, command=IPC_NET_PLMN_SEL, type=IPC_TYPE_RESP, size=1

D/RIL-IPC ( 1891): ================================= IPC FMT data =================================

D/RIL-IPC ( 1891): [0000]   02                                                 .

D/RIL-IPC ( 1891): ================================================================================

D/RIL     ( 1891): 2 RIL requests in the queue (0 pending, 2 handled, 0 unhandled)

D/RILJ    ( 2563): [0035]> OPERATOR

D/RIL-IPC ( 1891): 

D/RIL-IPC ( 1891): xmm626_sec_modem_fmt_recv: Received FMT message

D/RIL-IPC ( 1891): xmm626_sec_modem_fmt_recv: Message: aseq=0x14, command=IPC_NET_SERVING_NETWORK, type=IPC_TYPE_RESP, size=11

D/RIL-IPC ( 1891): ================================= IPC FMT data =================================

D/RIL-IPC ( 1891): [0000]   02 04 FF 32 30 36 30 31  23 00 00                  ...20601 #..

D/RIL-IPC ( 1891): ================================================================================

D/RIL     ( 1891): 1 RIL request in the queue (0 pending, 1 handled, 0 unhandled)

D/RIL-IPC ( 1891): 

D/RIL-IPC ( 1891): xmm626_sec_modem_fmt_recv: Received FMT message

D/RIL-IPC ( 1891): xmm626_sec_modem_fmt_recv: Message: aseq=0x15, command=IPC_NET_REGIST, type=IPC_TYPE_RESP, size=11

D/RIL-IPC ( 1891): ================================= IPC FMT data =================================

D/RIL-IPC ( 1891): [0000]   FF 03 01 00 00 00 00 00  00 00 00                  ........ ...

D/RIL-IPC ( 1891): ================================================================================

D/RIL     ( 1891): 0 RIL request in the queue (0 pending, 0 handled, 0 unhandled)

D/RILJ    ( 2563): [0029]< VOICE_REGISTRATION_STATE {10, 0, 0, 0, null, null, null, null, null, null, null, null, null, null, null}

D/RILJ    ( 2563): [0036]> DATA_REGISTRATION_STATE

D/RILJ    ( 2563): [0030]< QUERY_NETWORK_SELECTION_MODE {0}

D/RILJ    ( 2563): [0037]> VOICE_REGISTRATION_STATE

D/RILJ    ( 2563): [0031]< OPERATOR {Proximus, Proximus, 20601}

D/RILJ    ( 2563): [0038]> QUERY_NETWORK_SELECTION_MODE

D/RILJ    ( 2563): [0032]< DATA_REGISTRATION_STATE {0, 0, 0, 0, 3}

D/RILJ    ( 2563): [0039]> OPERATOR

D/RIL     ( 1891): 1 RIL request in the queue (1 pending, 0 handled, 0 unhandled)

D/RIL-IPC ( 1891): 

D/RIL-IPC ( 1891): xmm626_sec_modem_fmt_send: Sent FMT message

D/RIL-IPC ( 1891): xmm626_sec_modem_fmt_send: Message: mseq=0x16, command=IPC_NET_REGIST, type=IPC_TYPE_GET, size=2

D/RIL-IPC ( 1891): ================================= IPC FMT data =================================

D/RIL-IPC ( 1891): [0000]   FF 02                                              ..

D/RIL-IPC ( 1891): ================================================================================

D/RILJ    ( 2563): [0040]> DATA_REGISTRATION_STATE

D/RILJ    ( 2563): [0041]> VOICE_REGISTRATION_STATE

D/RIL     ( 1891): 2 RIL requests in the queue (1 pending, 1 handled, 0 unhandled)

D/RIL-IPC ( 1891): 

D/RIL-IPC ( 1891): xmm626_sec_modem_fmt_send: Sent FMT message

D/RIL-IPC ( 1891): xmm626_sec_modem_fmt_send: Message: mseq=0x17, command=IPC_NET_PLMN_SEL, type=IPC_TYPE_GET, size=0

D/RIL-IPC ( 1891): 

D/RIL-IPC ( 1891): xmm626_sec_modem_fmt_recv: Received FMT message

D/RIL-IPC ( 1891): xmm626_sec_modem_fmt_recv: Message: aseq=0x16, command=IPC_NET_REGIST, type=IPC_TYPE_RESP, size=11

D/RIL-IPC ( 1891): ================================= IPC FMT data =================================

D/RIL-IPC ( 1891): [0000]   FF 02 04 00 00 00 00 00  00 00 00                  ........ ...

D/RIL-IPC ( 1891): ================================================================================

D/RIL     ( 1891): 1 RIL request in the queue (0 pending, 1 handled, 0 unhandled)

D/RILJ    ( 2563): [0042]> QUERY_NETWORK_SELECTION_MODE

D/RILJ    ( 2563): [0033]< VOICE_REGISTRATION_STATE {10, 0, 0, 0, null, null, null, null, null, null, null, null, null, null, null}

D/RIL-IPC ( 1891): 

D/RIL-IPC ( 1891): xmm626_sec_modem_fmt_recv: Received FMT message

D/RIL-IPC ( 1891): xmm626_sec_modem_fmt_recv: Message: aseq=0x17, command=IPC_NET_PLMN_SEL, type=IPC_TYPE_RESP, size=1

D/RIL-IPC ( 1891): ================================= IPC FMT data =================================

D/RIL-IPC ( 1891): [0000]   02                                                 .

D/RIL-IPC ( 1891): ================================================================================

D/RIL     ( 1891): 0 RIL request in the queue (0 pending, 0 handled, 0 unhandled)

D/GSM     ( 2563): Baseband version: I9300XXUGNA8

D/RIL     ( 1891): 1 RIL request in the queue (1 pending, 0 handled, 0 unhandled)

D/RILJ    ( 2563): [0034]< QUERY_NETWORK_SELECTION_MODE {0}

D/RIL     ( 1891): 2 RIL requests in the queue (2 pending, 0 handled, 0 unhandled)

D/RIL-IPC ( 1891): 

D/RIL-IPC ( 1891): xmm626_sec_modem_fmt_send: Sent FMT message

D/RIL-IPC ( 1891): xmm626_sec_modem_fmt_send: Message: mseq=0x18, command=IPC_NET_SERVING_NETWORK, type=IPC_TYPE_GET, size=0

D/RIL-IPC ( 1891): 

D/RIL-IPC ( 1891): xmm626_sec_modem_fmt_send: Sent FMT message

D/RIL-IPC ( 1891): xmm626_sec_modem_fmt_send: Message: mseq=0x19, command=IPC_NET_REGIST, type=IPC_TYPE_GET, size=2

D/RIL-IPC ( 1891): ================================= IPC FMT data =================================

D/RIL-IPC ( 1891): [0000]   FF 03                                              ..

D/RIL-IPC ( 1891): ================================================================================

D/RIL     ( 1891): 3 RIL requests in the queue (1 pending, 2 handled, 0 unhandled)

D/RIL-IPC ( 1891): 

D/RIL-IPC ( 1891): xmm626_sec_modem_fmt_send: Sent FMT message

D/RIL-IPC ( 1891): xmm626_sec_modem_fmt_send: Message: mseq=0x1a, command=IPC_NET_REGIST, type=IPC_TYPE_GET, size=2

D/RIL-IPC ( 1891): ================================= IPC FMT data =================================

D/RIL-IPC ( 1891): [0000]   FF 02                                              ..

D/RIL-IPC ( 1891): ================================================================================

D/RIL     ( 1891): 4 RIL requests in the queue (1 pending, 3 handled, 0 unhandled)

D/RIL     ( 1891): 5 RIL requests in the queue (2 pending, 3 handled, 0 unhandled)

D/RIL     ( 1891): 6 RIL requests in the queue (3 pending, 3 handled, 0 unhandled)

D/RIL     ( 1891): 7 RIL requests in the queue (4 pending, 3 handled, 0 unhandled)

D/RIL     ( 1891): 8 RIL requests in the queue (5 pending, 3 handled, 0 unhandled)

D/RIL-IPC ( 1891): 

D/RIL-IPC ( 1891): xmm626_sec_modem_fmt_send: Sent FMT message

D/RIL-IPC ( 1891): xmm626_sec_modem_fmt_send: Message: mseq=0x1b, command=IPC_NET_PLMN_SEL, type=IPC_TYPE_GET, size=0

D/RIL-IPC ( 1891): 

D/RIL-IPC ( 1891): xmm626_sec_modem_fmt_send: Sent FMT message

D/RIL-IPC ( 1891): xmm626_sec_modem_fmt_send: Message: mseq=0x1c, command=IPC_NET_PLMN_SEL, type=IPC_TYPE_GET, size=0

D/RIL-IPC ( 1891): 

D/RIL-IPC ( 1891): xmm626_sec_modem_fmt_recv: Received FMT message

D/RIL-IPC ( 1891): xmm626_sec_modem_fmt_recv: Message: aseq=0x18, command=IPC_NET_SERVING_NETWORK, type=IPC_TYPE_RESP, size=11

D/RIL-IPC ( 1891): ================================= IPC FMT data =================================

D/RIL-IPC ( 1891): [0000]   02 04 FF 32 30 36 30 31  23 00 00                  ...20601 #..

D/RIL-IPC ( 1891): ================================================================================

D/RIL     ( 1891): 7 RIL requests in the queue (0 pending, 4 handled, 3 unhandled)

D/RIL-IPC ( 1891): 

D/RIL-IPC ( 1891): xmm626_sec_modem_fmt_send: Sent FMT message

D/RIL-IPC ( 1891): xmm626_sec_modem_fmt_send: Message: mseq=0x1d, command=IPC_NET_SERVING_NETWORK, type=IPC_TYPE_GET, size=0

D/RILJ    ( 2563): [0035]< OPERATOR {Proximus, Proximus, 20601}

D/RIL-IPC ( 1891): 

D/RIL-IPC ( 1891): xmm626_sec_modem_fmt_recv: Received FMT message

D/RIL-IPC ( 1891): xmm626_sec_modem_fmt_recv: Message: aseq=0x19, command=IPC_NET_REGIST, type=IPC_TYPE_RESP, size=11

D/RIL-IPC ( 1891): ================================= IPC FMT data =================================

D/RIL-IPC ( 1891): [0000]   FF 03 01 00 00 00 00 00  00 00 00                  ........ ...

D/RIL-IPC ( 1891): ================================================================================

D/RIL     ( 1891): 6 RIL requests in the queue (0 pending, 4 handled, 2 unhandled)

D/RIL-IPC ( 1891): 

D/RIL-IPC ( 1891): xmm626_sec_modem_fmt_send: Sent FMT message

D/RIL-IPC ( 1891): xmm626_sec_modem_fmt_send: Message: mseq=0x1e, command=IPC_NET_REGIST, type=IPC_TYPE_GET, size=2

D/RIL-IPC ( 1891): ================================= IPC FMT data =================================

D/RIL-IPC ( 1891): [0000]   FF 03                                              ..

D/RIL-IPC ( 1891): ================================================================================

D/RIL_UiccController( 2563): Received EVENT_GET_ICC_STATUS_DONE

D/RIL-IPC ( 1891): 

D/RIL-IPC ( 1891): xmm626_sec_modem_fmt_recv: Received FMT message

D/RIL-IPC ( 1891): xmm626_sec_modem_fmt_recv: Message: aseq=0x1a, command=IPC_NET_REGIST, type=IPC_TYPE_RESP, size=11

D/RIL-IPC ( 1891): ================================= IPC FMT data =================================

D/RIL-IPC ( 1891): [0000]   FF 02 04 00 00 00 00 00  00 00 00                  ........ ...

D/RIL-IPC ( 1891): ================================================================================

D/RIL     ( 1891): 5 RIL requests in the queue (0 pending, 4 handled, 1 unhandled)

D/RIL-IPC ( 1891): 

D/RIL-IPC ( 1891): xmm626_sec_modem_fmt_send: Sent FMT message

D/RIL-IPC ( 1891): xmm626_sec_modem_fmt_send: Message: mseq=0x1f, command=IPC_NET_REGIST, type=IPC_TYPE_GET, size=2

D/RIL-IPC ( 1891): ================================= IPC FMT data =================================

D/RIL-IPC ( 1891): [0000]   FF 02                                              ..

D/RIL-IPC ( 1891): ================================================================================

D/RILJ    ( 2563): [0036]< DATA_REGISTRATION_STATE {0, 0, 0, 0, 3}

D/RILJ    ( 2563): [0037]< VOICE_REGISTRATION_STATE {10, 0, 0, 0, null, null, null, null, null, null, null, null, null, null, null}

D/RIL-IPC ( 1891): 

D/RIL-IPC ( 1891): xmm626_sec_modem_fmt_recv: Received FMT message

D/RIL-IPC ( 1891): xmm626_sec_modem_fmt_recv: Message: aseq=0x1b, command=IPC_NET_PLMN_SEL, type=IPC_TYPE_RESP, size=1

D/RIL-IPC ( 1891): ================================= IPC FMT data =================================

D/RIL-IPC ( 1891): [0000]   02                                                 .

D/RIL-IPC ( 1891): ================================================================================

D/RIL     ( 1891): 4 RIL requests in the queue (0 pending, 4 handled, 0 unhandled)

D/RILJ    ( 2563): [0038]< QUERY_NETWORK_SELECTION_MODE {0}

D/RIL-IPC ( 1891): 

D/RIL-IPC ( 1891): xmm626_sec_modem_fmt_recv: Received FMT message

D/RIL-IPC ( 1891): xmm626_sec_modem_fmt_recv: Message: aseq=0x1c, command=IPC_NET_PLMN_SEL, type=IPC_TYPE_RESP, size=1

D/RIL-IPC ( 1891): ================================= IPC FMT data =================================

D/RIL-IPC ( 1891): [0000]   02                                                 .

D/RIL-IPC ( 1891): ================================================================================

D/RIL     ( 1891): 3 RIL requests in the queue (0 pending, 3 handled, 0 unhandled)

D/RIL-IPC ( 1891): 

D/RIL-IPC ( 1891): xmm626_sec_modem_fmt_recv: Received FMT message

D/RIL-IPC ( 1891): xmm626_sec_modem_fmt_recv: Message: aseq=0x1d, command=IPC_NET_SERVING_NETWORK, type=IPC_TYPE_RESP, size=11

D/RIL-IPC ( 1891): ================================= IPC FMT data =================================

D/RIL-IPC ( 1891): [0000]   02 04 FF 32 30 36 30 31  23 00 00                  ...20601 #..

D/RIL-IPC ( 1891): ================================================================================

D/RIL     ( 1891): 2 RIL requests in the queue (0 pending, 2 handled, 0 unhandled)

D/RIL_UiccCard( 2563): Creating

D/RILJ    ( 2563): [0042]< QUERY_NETWORK_SELECTION_MODE {0}

D/RIL_UiccCard( 2563): 1 applications

D/RIL_UiccCardApplication( 2563): Creating UiccApp: {APPTYPE_SIM,APPSTATE_PIN}

D/RIL-IPC ( 1891): 

D/RIL-IPC ( 1891): xmm626_sec_modem_fmt_recv: Received FMT message

D/RIL-IPC ( 1891): xmm626_sec_modem_fmt_recv: Message: aseq=0x1e, command=IPC_NET_REGIST, type=IPC_TYPE_RESP, size=11

D/RIL-IPC ( 1891): ================================= IPC FMT data =================================

D/RIL-IPC ( 1891): [0000]   FF 03 01 00 00 00 00 00  00 00 00                  ........ ...

D/RIL-IPC ( 1891): ================================================================================

D/RIL     ( 1891): 1 RIL request in the queue (0 pending, 1 handled, 0 unhandled)

D/RILJ    ( 2563): [0039]< OPERATOR {Proximus, Proximus, 20601}

D/RILJ    ( 2563): [0040]< DATA_REGISTRATION_STATE {0, 0, 0, 0, 3}

D/RIL-IPC ( 1891): 

D/RIL-IPC ( 1891): xmm626_sec_modem_fmt_recv: Received FMT message

D/RIL-IPC ( 1891): xmm626_sec_modem_fmt_recv: Message: aseq=0x1f, command=IPC_NET_REGIST, type=IPC_TYPE_RESP, size=11

D/RIL-IPC ( 1891): ================================= IPC FMT data =================================

D/RIL-IPC ( 1891): [0000]   FF 02 04 00 00 00 00 00  00 00 00                  ........ ...

D/RIL-IPC ( 1891): ================================================================================

D/RIL     ( 1891): 0 RIL request in the queue (0 pending, 0 handled, 0 unhandled)

D/RILJ    ( 2563): [0041]< VOICE_REGISTRATION_STATE {10, 0, 0, 0, null, null, null, null, null, null, null, null, null, null, null}

W/GSM     ( 2563): Can't open /system/etc/voicemail-conf.xml

D/GSM     ( 2563): [SIMRecords] SIMRecords: onRadioOffOrNotAvailable set 'gsm.sim.operator.numeric' to operator=null

D/RIL_UiccCard( 2563): update: radioState=RADIO_ON mLastRadioState=RADIO_UNAVAILABLE

D/RIL_UiccController( 2563): Notifying IccChangedRegistrants

D/PHONE   ( 2563): [PhoneProxy] Ignoring voice radio technology changed message. newVoiceRadioTech = 3 Active Phone = GSM

D/CDMA    ( 2563): [CdmaSSM] CDMA_SUBSCRIPTION_SOURCE event = 2

D/CDMA    ( 2563): [CdmaSSM] Subscription Source Changed : 1 >> 0

D/RIL_UiccController( 2563): Received EVENT_GET_ICC_STATUS_DONE

D/RIL_UiccCard( 2563): 1 applications

D/RIL_UiccCardApplication( 2563): APPTYPE_SIM update. New {APPTYPE_SIM,APPSTATE_PIN}

D/RIL_UiccCard( 2563): update: radioState=RADIO_ON mLastRadioState=RADIO_ON

D/RIL_UiccController( 2563): Notifying IccChangedRegistrants

D/RIL_UiccController( 2563): Received EVENT_GET_ICC_STATUS_DONE

D/RIL_UiccCard( 2563): 1 applications

D/RIL_UiccCardApplication( 2563): APPTYPE_SIM update. New {APPTYPE_SIM,APPSTATE_PIN}

D/RIL_UiccCard( 2563): update: radioState=RADIO_ON mLastRadioState=RADIO_ON

D/RIL_UiccController( 2563): Notifying IccChangedRegistrants

D/GSM     ( 2563): [GsmSST] Poll ServiceState done:  oldSS=[3 home null null null  Unknown CSS not supported -1 -1 RoamInd=-1 DefRoamInd=-1 EmergOnly=false] newSS=[1 home Proximus Proximus 20601  Unknown CSS not supported -1 -1 RoamInd=-1 DefRoamInd=-1 EmergOnly=true] oldGprs=1 newData=1 oldMaxDataCalls=1 mNewMaxDataCalls=1 oldReasonDataDenied=-1 mNewReasonDataDenied=-1 oldType=Unknown newType=Unknown

D/GSM     ( 2563): [GsmSST] updateSpnDisplay: radio is on but out of service, set plmn='Emergency calls only'

D/GSM     ( 2563): [GsmSST] updateSpnDisplay: changed sending intent rule=0 showPlmn='true' plmn='Emergency calls only' showSpn='false' spn=''

D/GSM     ( 2563): [GsmSST] pollStateDone: no nitz but one TZ for iso-cc=be with zone.getID=Europe/Brussels testOneUniqueOffsetPath=false

D/GSM     ( 2563): [GsmSST] setAndBroadcastNetworkSetTimeZone: setTimeZone=Europe/Brussels

D/GSM     ( 2563): [GsmSST] setAndBroadcastNetworkSetTimeZone: call alarm.setTimeZone and broadcast zoneId=Europe/Brussels

D/GSM     ( 2563): [GsmSST] shouldFixTimeZoneNow: retVal=false iccCardExist=false operatorNumeric=20601 mcc=206 prevOperatorNumeric= prevMcc=207 needToFixTimeZone=false ltod=06-01 18:27:34.561

D/GSM     ( 2563): [GSMPhone] New Uicc application found

D/GSM     ( 2563): [GsmSST] New card found

D/GSM     ( 2563): [GsmDCT] handleMessage msg={ what=270369 when=-136ms obj=android.os.AsyncResult@417b85f0 }

D/GSM     ( 2563): [GsmDCT] New records found

D/RIL_IccCardProxy( 2563): Icc changed. Reregestering.

D/RIL_UiccCardApplication( 2563): Notifying 1 registrant: LOCKED

D/RIL_IccCardProxy( 2563): Broadcasting intent ACTION_SIM_STATE_CHANGED LOCKED reason PIN

D/RIL_IccCardProxy( 2563): updateQuietMode: 3GPP subscription -> newQuietMode=false

D/RIL_IccCardProxy( 2563): updateQuietMode: QuietMode is false (app_type=1 isLteOnCdmaMode=false cdmaSource=-1)

D/GSM     ( 2563): [GsmDCT] handleMessage msg={ what=270369 when=-128ms obj=android.os.AsyncResult@417b99c8 }

D/GSM     ( 2563): [GsmDCT] handleMessage msg={ what=270369 when=-128ms obj=android.os.AsyncResult@417b9f28 }

D/RILJ    ( 2563): [0043]> OEM_HOOK_RAW[01010007011400]

D/RILJ    ( 2563): [0044]> OEM_HOOK_RAW[010300063200]

D/RIL     ( 1891): 1 RIL request in the queue (1 pending, 0 handled, 0 unhandled)

D/RIL-IPC ( 1891): 

D/RIL-IPC ( 1891): xmm626_sec_modem_fmt_send: Sent FMT message

D/RIL-IPC ( 1891): xmm626_sec_modem_fmt_send: Message: mseq=0x20, command=IPC_SVC_ENTER, type=IPC_TYPE_SET, size=3

D/RIL-IPC ( 1891): ================================= IPC FMT data =================================

D/RIL-IPC ( 1891): [0000]   01 14 10                                           ...

D/RIL-IPC ( 1891): ================================================================================

D/RIL     ( 1891): 2 RIL requests in the queue (1 pending, 1 handled, 0 unhandled)

D/RILJ    ( 2563): [0045]> OEM_HOOK_RAW[010300063300]

D/RIL     ( 1891): 3 RIL requests in the queue (1 pending, 1 handled, 1 unhandled)

D/RILJ    ( 2563): [0046]> OEM_HOOK_RAW[0102000501]

D/RIL     ( 1891): 4 RIL requests in the queue (1 pending, 1 handled, 2 unhandled)

D/RIL-IPC ( 1891): 

D/RIL-IPC ( 1891): xmm626_sec_modem_fmt_recv: Received FMT message

D/RIL-IPC ( 1891): xmm626_sec_modem_fmt_recv: Message: aseq=0x20, command=IPC_GEN_PHONE_RES, type=IPC_TYPE_RESP, size=5

D/RIL-IPC ( 1891): ================================= IPC FMT data =================================

D/RIL-IPC ( 1891): [0000]   0B 01 03 00 80                                     .....

D/RIL-IPC ( 1891): ================================================================================

D/RIL     ( 1891): Generic response was expected

D/RIL-IPC ( 1891): 

D/RIL-IPC ( 1891): xmm626_sec_modem_fmt_recv: Received FMT message

D/RIL-IPC ( 1891): xmm626_sec_modem_fmt_recv: Message: aseq=0xff, command=IPC_SVC_SCREEN_CFG, type=IPC_TYPE_NOTI, size=2

D/RIL-IPC ( 1891): ================================= IPC FMT data =================================

D/RIL-IPC ( 1891): [0000]   0B 01                                              ..

D/RIL-IPC ( 1891): ================================================================================

D/RIL-IPC ( 1891): Unhandled IPC FMT message: IPC_SVC_SCREEN_CFG

D/RIL-IPC ( 1891): 

D/RIL-IPC ( 1891): xmm626_sec_modem_fmt_recv: Received FMT message

D/RIL-IPC ( 1891): xmm626_sec_modem_fmt_recv: Message: aseq=0x00, command=IPC_SVC_DISPLAY_SCREEN, type=IPC_TYPE_NOTI, size=545

D/RIL-IPC ( 1891): ================================= IPC FMT data =================================

D/RIL-IPC ( 1891): [0000]   10 00 00 20 52 52 43 28  48 53 50 41 29 20 43 4F   ... RRC( HSPA) CO

D/RIL-IPC ( 1891): [0010]   4E 54 52 4F 4C 00 20 20  20 20 20 20 20 20 20 20   NTROL.           

D/RIL-IPC ( 1891): [0020]   20 20 00 01 00 20 5B 31  5D 20 44 49 53 50 4C 41     ... [1 ] DISPLA

D/RIL-IPC ( 1891): [0030]   59 20 52 45 56 49 53 49  4F 4E 00 20 20 20 20 20   Y REVISI ON.     

D/RIL-IPC ( 1891): [0040]   20 20 20 20 00 02 00 20  5B 32 5D 20 43 48 41 4E       ...  [2] CHAN

D/RIL-IPC ( 1891): [0050]   47 45 20 52 45 56 49 53  49 4F 4E 00 20 20 20 20   GE REVIS ION.    

D/RIL-IPC ( 1891): [0060]   20 20 20 20 20 20 00 03  00 20 20 20 20 20 20 20         .. .       

D/RIL-IPC ( 1891): [0070]   20 20 20 20 20 20 20 20  20 20 20 20 20 20 20 20                    

D/RIL-IPC ( 1891): [0080]   20 20 20 20 20 20 20 20  00 04 00 20 20 20 20 20            ...     

D/RIL-IPC ( 1891): [0090]   20 20 20 20 20 20 20 20  20 20 20 20 20 20 20 20                    

D/RIL-IPC ( 1891): [00a0]   20 20 20 20 20 20 20 20  20 20 00 05 00 20 20 20              ...   

D/RIL-IPC ( 1891): [00b0]   20 20 20 20 20 20 20 20  20 20 20 20 20 20 20 20                    

D/RIL-IPC ( 1891): [00c0]   20 20 20 20 20 20 20 20  20 20 20 20 00 06 00 20                ... 

D/RIL-IPC ( 1891): [00d0]   20 20 20 20 20 20 20 20  20 20 20 20 20 20 20 20                    

D/RIL-IPC ( 1891): [00e0]   20 20 20 20 20 20 20 20  20 20 20 20 20 20 00 07                  ..

D/RIL-IPC ( 1891): [00f0]   00 20 20 20 20 20 20 20  20 20 20 20 20 20 20 20   .                

D/RIL-IPC ( 1891): ================================================================================

D/RIL     ( 1891): 3 RIL requests in the queue (0 pending, 0 handled, 3 unhandled)

D/RIL-IPC ( 1891): 

D/RIL-IPC ( 1891): xmm626_sec_modem_fmt_recv: Received FMT message

D/RIL-IPC ( 1891): xmm626_sec_modem_fmt_recv: Message: aseq=0x00, command=IPC_SVC_DISPLAY_SCREEN, type=IPC_TYPE_NOTI, size=35

D/RIL-IPC ( 1891): ================================= IPC FMT data =================================

D/RIL-IPC ( 1891): [0000]   01 00 01 20 52 52 43 28  48 53 50 41 29 20 43 4F   ... RRC( HSPA) CO

D/RIL-IPC ( 1891): [0010]   4E 54 52 4F 4C 00 20 20  20 20 20 20 20 20 20 20   NTROL.           

D/RIL-IPC ( 1891): [0020]   20 20 00                                             .

D/RIL-IPC ( 1891): ================================================================================

D/RIL-IPC ( 1891): 

D/RIL-IPC ( 1891): xmm626_sec_modem_fmt_send: Sent FMT message

D/RIL-IPC ( 1891): xmm626_sec_modem_fmt_send: Message: mseq=0x21, command=IPC_SVC_PRO_KEYCODE, type=IPC_TYPE_SET, size=1

D/RIL-IPC ( 1891): ================================= IPC FMT data =================================

D/RIL-IPC ( 1891): [0000]   32                                                 2

D/RIL-IPC ( 1891): ================================================================================

D/RILJ    ( 2563): [0043]< OEM_HOOK_RAW [B@417fbe00

D/RIL-IPC ( 1891): 

D/RIL-IPC ( 1891): xmm626_sec_modem_fmt_recv: Received FMT message

D/RIL-IPC ( 1891): xmm626_sec_modem_fmt_recv: Message: aseq=0x21, command=IPC_GEN_PHONE_RES, type=IPC_TYPE_RESP, size=5

D/RIL-IPC ( 1891): ================================= IPC FMT data =================================

D/RIL-IPC ( 1891): [0000]   0B 03 03 00 80                                     .....

D/RIL-IPC ( 1891): ================================================================================

D/RIL     ( 1891): Generic response was expected

D/RIL-IPC ( 1891): 

D/RIL-IPC ( 1891): xmm626_sec_modem_fmt_recv: Received FMT message

D/RIL-IPC ( 1891): xmm626_sec_modem_fmt_recv: Message: aseq=0xff, command=IPC_SVC_DISPLAY_SCREEN, type=IPC_TYPE_NOTI, size=35

D/RIL-IPC ( 1891): ================================= IPC FMT data =================================

D/RIL-IPC ( 1891): [0000]   01 09 00 20 32 00 20 20  20 20 20 20 20 20 20 20   ... 2.           

D/RIL-IPC ( 1891): [0010]   20 20 20 20 20 20 20 20  20 20 20 20 20 20 20 20                    

D/RIL-IPC ( 1891): [0020]   20 20 00                                             .

D/RIL-IPC ( 1891): ================================================================================

D/RIL-IPC ( 1891): 

D/RIL-IPC ( 1891): xmm626_sec_modem_fmt_recv: Received FMT message

D/RIL-IPC ( 1891): xmm626_sec_modem_fmt_recv: Message: aseq=0x00, command=IPC_SVC_DISPLAY_SCREEN, type=IPC_TYPE_NOTI, size=545

D/RIL-IPC ( 1891): ================================= IPC FMT data =================================

D/RIL-IPC ( 1891): [0000]   10 00 00 20 43 48 41 4E  47 45 20 48 53 50 41 20   ... CHAN GE HSPA 

D/RIL-IPC ( 1891): [0010]   52 45 56 49 53 49 4F 4E  00 20 20 20 20 20 20 20   REVISION .       

D/RIL-IPC ( 1891): [0020]   20 20 00 01 00 20 5B 31  5D 20 52 45 4C 45 41 53     ... [1 ] RELEAS

D/RIL-IPC ( 1891): [0030]   45 20 52 39 39 28 48 53  50 41 20 4F 46 46 29 00   E R99(HS PA OFF).

D/RIL-IPC ( 1891): [0040]   20 20 20 20 00 02 00 20  5B 32 5D 20 52 45 4C 45       ...  [2] RELE

D/RIL-IPC ( 1891): [0050]   41 53 45 20 35 28 48 53  44 50 41 20 4F 4E 4C 59   ASE 5(HS DPA ONLY

D/RIL-IPC ( 1891): [0060]   29 00 20 20 20 20 00 03  00 20 5B 33 5D 20 52 45   ).    .. . [3] RE

D/RIL-IPC ( 1891): [0070]   4C 45 41 53 45 20 36 28  48 53 44 50 41 2F 48 53   LEASE 6( HSDPA/HS

D/RIL-IPC ( 1891): [0080]   55 50 41 29 00 20 20 20  00 04 00 20 20 20 20 20   UPA).    ...     

D/RIL-IPC ( 1891): [0090]   20 20 20 20 20 20 20 20  20 20 20 20 20 20 20 20                    

D/RIL-IPC ( 1891): [00a0]   20 20 20 20 20 20 20 20  20 20 00 05 00 20 20 20              ...   

D/RIL-IPC ( 1891): [00b0]   20 20 20 20 20 20 20 20  20 20 20 20 20 20 20 20                    

D/RIL-IPC ( 1891): [00c0]   20 20 20 20 20 20 20 20  20 20 20 20 00 06 00 20                ... 

D/RIL-IPC ( 1891): [00d0]   20 20 20 20 20 20 20 20  20 20 20 20 20 20 20 20                    

D/RIL-IPC ( 1891): [00e0]   20 20 20 20 20 20 20 20  20 20 20 20 20 20 00 07                  ..

D/RIL-IPC ( 1891): [00f0]   00 20 20 20 20 20 20 20  20 20 20 20 20 20 20 20   .                

D/RIL-IPC ( 1891): ================================================================================

D/RIL     ( 1891): 2 RIL requests in the queue (0 pending, 0 handled, 2 unhandled)

D/RIL-IPC ( 1891): 

D/RIL-IPC ( 1891): xmm626_sec_modem_fmt_recv: Received FMT message

D/RIL-IPC ( 1891): xmm626_sec_modem_fmt_recv: Message: aseq=0x00, command=IPC_SVC_DISPLAY_SCREEN, type=IPC_TYPE_NOTI, size=35

D/RIL-IPC ( 1891): ================================= IPC FMT data =================================

D/RIL-IPC ( 1891): [0000]   01 00 01 20 43 48 41 4E  47 45 20 48 53 50 41 20   ... CHAN GE HSPA 

D/RIL-IPC ( 1891): [0010]   52 45 56 49 53 49 4F 4E  00 20 20 20 20 20 20 20   REVISION .       

D/RIL-IPC ( 1891): [0020]   20 20 00                                             .

D/RIL-IPC ( 1891): ================================================================================

D/RIL-IPC ( 1891): 

D/RIL-IPC ( 1891): xmm626_sec_modem_fmt_send: Sent FMT message

D/RIL-IPC ( 1891): xmm626_sec_modem_fmt_send: Message: mseq=0x22, command=IPC_SVC_PRO_KEYCODE, type=IPC_TYPE_SET, size=1

D/RILJ    ( 2563): [0044]< OEM_HOOK_RAW [B@417fd250

D/RIL-IPC ( 1891): ================================= IPC FMT data =================================

D/RIL-IPC ( 1891): [0000]   33                                                 3

D/RIL-IPC ( 1891): ================================================================================

D/RIL-IPC ( 1891): 

D/RIL-IPC ( 1891): xmm626_sec_modem_fmt_recv: Received FMT message

D/RIL-IPC ( 1891): xmm626_sec_modem_fmt_recv: Message: aseq=0x22, command=IPC_GEN_PHONE_RES, type=IPC_TYPE_RESP, size=5

D/RIL-IPC ( 1891): ================================= IPC FMT data =================================

D/RIL-IPC ( 1891): [0000]   0B 03 03 00 80                                     .....

D/RIL-IPC ( 1891): ================================================================================

D/RIL     ( 1891): Generic response was expected

D/RIL-IPC ( 1891): 

D/RIL-IPC ( 1891): xmm626_sec_modem_fmt_recv: Received FMT message

D/RIL-IPC ( 1891): xmm626_sec_modem_fmt_recv: Message: aseq=0xff, command=IPC_SVC_DISPLAY_SCREEN, type=IPC_TYPE_NOTI, size=35

D/RIL-IPC ( 1891): ================================= IPC FMT data =================================

D/RIL-IPC ( 1891): [0000]   01 09 00 20 33 00 20 20  20 20 20 20 20 20 20 20   ... 3.           

D/RIL-IPC ( 1891): [0010]   20 20 20 20 20 20 20 20  20 20 20 20 20 20 20 20                    

D/RIL-IPC ( 1891): [0020]   20 20 00                                             .

D/RIL-IPC ( 1891): ================================================================================

D/RIL-IPC ( 1891): 

D/RIL-IPC ( 1891): xmm626_sec_modem_fmt_recv: Received FMT message

D/RIL-IPC ( 1891): xmm626_sec_modem_fmt_recv: Message: aseq=0x00, command=IPC_SVC_DISPLAY_SCREEN, type=IPC_TYPE_NOTI, size=545

D/RIL-IPC ( 1891): ================================= IPC FMT data =================================

D/RIL-IPC ( 1891): [0000]   10 00 00 43 48 41 4E 47  45 5F 52 45 4C 35 00 20   ...CHANG E_REL5. 

D/RIL-IPC ( 1891): [0010]   52 45 56 49 53 49 4F 4E  00 20 20 20 20 20 20 20   REVISION .       

D/RIL-IPC ( 1891): [0020]   20 20 00 01 00 48 53 44  50 41 20 4F 4E 2C 20 48     ...HSD PA ON, H

D/RIL-IPC ( 1891): [0030]   53 55 50 41 20 4F 4E 00  50 41 20 4F 46 46 29 00   SUPA ON. PA OFF).

D/RIL-IPC ( 1891): [0040]   20 20 20 20 00 02 00 20  20 20 20 20 20 20 20 20       ...          

D/RIL-IPC ( 1891): [0050]   20 20 20 20 20 20 20 20  20 20 20 20 20 20 20 20                    

D/RIL-IPC ( 1891): [0060]   20 20 20 20 20 20 00 03  00 20 20 20 20 20 20 20         .. .       

D/RIL-IPC ( 1891): [0070]   20 20 20 20 20 20 20 20  20 20 20 20 20 20 20 20                    

D/RIL-IPC ( 1891): [0080]   20 20 20 20 20 20 20 20  00 04 00 20 20 20 20 20            ...     

D/RIL-IPC ( 1891): [0090]   20 20 20 20 20 20 20 20  20 20 20 20 20 20 20 20                    

D/RIL-IPC ( 1891): [00a0]   20 20 20 20 20 20 20 20  20 20 00 05 00 20 20 20              ...   

D/RIL-IPC ( 1891): [00b0]   20 20 20 20 20 20 20 20  20 20 20 20 20 20 20 20                    

D/RIL-IPC ( 1891): [00c0]   20 20 20 20 20 20 20 20  20 20 20 20 00 06 00 20                ... 

D/RIL-IPC ( 1891): [00d0]   20 20 20 20 20 20 20 20  20 20 20 20 20 20 20 20                    

D/RIL-IPC ( 1891): [00e0]   20 20 20 20 20 20 20 20  20 20 20 20 20 20 00 07                  ..

D/RIL-IPC ( 1891): [00f0]   00 20 20 20 20 20 20 20  20 20 20 20 20 20 20 20   .                

D/RIL-IPC ( 1891): ================================================================================

D/RIL     ( 1891): 1 RIL request in the queue (0 pending, 0 handled, 1 unhandled)

D/RIL-IPC ( 1891): 

D/RIL-IPC ( 1891): xmm626_sec_modem_fmt_recv: Received FMT message

D/RIL-IPC ( 1891): xmm626_sec_modem_fmt_recv: Message: aseq=0x00, command=IPC_SVC_DISPLAY_SCREEN, type=IPC_TYPE_NOTI, size=35

D/RIL-IPC ( 1891): ================================= IPC FMT data =================================

D/RIL-IPC ( 1891): [0000]   01 00 01 43 48 41 4E 47  45 5F 52 45 4C 35 00 20   ...CHANG E_REL5. 

D/RIL-IPC ( 1891): [0010]   52 45 56 49 53 49 4F 4E  00 20 20 20 20 20 20 20   REVISION .       

D/RIL-IPC ( 1891): [0020]   20 20 00                                             .

D/RIL-IPC ( 1891): ================================================================================

D/RIL-IPC ( 1891): 

D/RIL-IPC ( 1891): xmm626_sec_modem_fmt_send: Sent FMT message

D/RIL-IPC ( 1891): xmm626_sec_modem_fmt_send: Message: mseq=0x23, command=IPC_SVC_END, type=IPC_TYPE_SET, size=1

D/RIL-IPC ( 1891): ================================= IPC FMT data =================================

D/RIL-IPC ( 1891): [0000]   01                                                 .

D/RILJ    ( 2563): [0045]< OEM_HOOK_RAW [B@417fd728

D/RIL-IPC ( 1891): ================================================================================

D/RIL-IPC ( 1891): 

D/RIL-IPC ( 1891): xmm626_sec_modem_fmt_recv: Received FMT message

D/RIL-IPC ( 1891): xmm626_sec_modem_fmt_recv: Message: aseq=0x23, command=IPC_GEN_PHONE_RES, type=IPC_TYPE_RESP, size=5

D/RIL-IPC ( 1891): ================================= IPC FMT data =================================

D/RIL-IPC ( 1891): [0000]   0B 02 03 00 80                                     .....

D/RIL-IPC ( 1891): ================================================================================

D/RIL     ( 1891): Generic response was expected

D/RIL     ( 1891): 0 RIL request in the queue (0 pending, 0 handled, 0 unhandled)

D/RILJ    ( 2563): [0046]< OEM_HOOK_RAW [B@417feba0

D/RIL-IPC ( 1891): 

D/RIL-IPC ( 1891): xmm626_sec_modem_fmt_recv: Received FMT message

D/RIL-IPC ( 1891): xmm626_sec_modem_fmt_recv: Message: aseq=0x23, command=IPC_GPRS_HSDPA_STATUS, type=IPC_TYPE_NOTI, size=1

D/RIL-IPC ( 1891): ================================= IPC FMT data =================================

D/RIL-IPC ( 1891): [0000]   01                                                 .

D/RIL-IPC ( 1891): ================================================================================

D/RIL-IPC ( 1891): 

D/RIL-IPC ( 1891): xmm626_sec_modem_fmt_recv: Received FMT message

D/RIL-IPC ( 1891): xmm626_sec_modem_fmt_recv: Message: aseq=0xff, command=IPC_NET_REGIST, type=IPC_TYPE_NOTI, size=11

D/RIL-IPC ( 1891): ================================= IPC FMT data =================================

D/RIL-IPC ( 1891): [0000]   04 02 04 01 CC 42 07 D4  07 00 00                  .....B.. ...

D/RIL-IPC ( 1891): ================================================================================

D/RIL-IPC ( 1891): 

D/RIL-IPC ( 1891): xmm626_sec_modem_fmt_recv: Received FMT message

D/RIL-IPC ( 1891): xmm626_sec_modem_fmt_recv: Message: aseq=0xff, command=IPC_NET_REGIST, type=IPC_TYPE_NOTI, size=11

D/RIL-IPC ( 1891): ================================= IPC FMT data =================================

D/RIL-IPC ( 1891): [0000]   04 03 01 01 CC 42 07 D4  07 00 00                  .....B.. ...

D/RIL-IPC ( 1891): ================================================================================

D/RILJ    ( 2563): [UNSL]< UNSOL_RESPONSE_VOICE_NETWORK_STATE_CHANGED

D/RIL-IPC ( 1891): 

D/RIL-IPC ( 1891): xmm626_sec_modem_fmt_recv: Received FMT message

D/RIL-IPC ( 1891): xmm626_sec_modem_fmt_recv: Message: aseq=0x00, command=IPC_NET_SERVING_NETWORK, type=IPC_TYPE_NOTI, size=11

D/RIL-IPC ( 1891): ================================= IPC FMT data =================================

D/RIL-IPC ( 1891): [0000]   02 04 04 32 30 36 31 30  23 CC 42                  ...20610 #.B

D/RIL-IPC ( 1891): ================================================================================

D/RILJ    ( 2563): [UNSL]< UNSOL_RESPONSE_VOICE_NETWORK_STATE_CHANGED

D/RILJ    ( 2563): [0047]> OPERATOR

D/RILJ    ( 2563): [0048]> DATA_REGISTRATION_STATE

D/RILJ    ( 2563): [UNSL]< UNSOL_RESPONSE_VOICE_NETWORK_STATE_CHANGED

D/RIL     ( 1891): 1 RIL request in the queue (1 pending, 0 handled, 0 unhandled)

D/RIL     ( 1891): 3 RIL requests data in the queue

D/RIL     ( 1891): 0 RIL request in the queue (0 pending, 0 handled, 0 unhandled)

D/RIL     ( 1891): 2 RIL requests data in the queue

D/RILJ    ( 2563): [0049]> VOICE_REGISTRATION_STATE

D/RILJ    ( 2563): [0050]> QUERY_NETWORK_SELECTION_MODE

D/RIL     ( 1891): 1 RIL request in the queue (1 pending, 0 handled, 0 unhandled)

D/RIL     ( 1891): 2 RIL requests data in the queue

D/RILJ    ( 2563): [0051]> OPERATOR

D/RIL     ( 1891): 0 RIL request in the queue (0 pending, 0 handled, 0 unhandled)

D/RIL     ( 1891): 1 RIL request data in the queue

D/RIL     ( 1891): 1 RIL request in the queue (1 pending, 0 handled, 0 unhandled)

D/RIL     ( 1891): 1 RIL request data in the queue

D/RIL     ( 1891): 0 RIL request in the queue (0 pending, 0 handled, 0 unhandled)

D/RILJ    ( 2563): [0052]> DATA_REGISTRATION_STATE

D/RIL     ( 1891): 1 RIL request in the queue (1 pending, 0 handled, 0 unhandled)

D/RIL-IPC ( 1891): 

D/RIL-IPC ( 1891): xmm626_sec_modem_fmt_send: Sent FMT message

D/RIL-IPC ( 1891): xmm626_sec_modem_fmt_send: Message: mseq=0x24, command=IPC_NET_PLMN_SEL, type=IPC_TYPE_GET, size=0

D/RILJ    ( 2563): [0053]> VOICE_REGISTRATION_STATE

D/RIL     ( 1891): 2 RIL requests in the queue (1 pending, 1 handled, 0 unhandled)

D/RIL-IPC ( 1891): 

D/RIL-IPC ( 1891): xmm626_sec_modem_fmt_send: Sent FMT message

D/RIL-IPC ( 1891): xmm626_sec_modem_fmt_send: Message: mseq=0x25, command=IPC_NET_SERVING_NETWORK, type=IPC_TYPE_GET, size=0

D/RILJ    ( 2563): [UNSL]< UNSOL_RESPONSE_VOICE_NETWORK_STATE_CHANGED

D/RIL-IPC ( 1891): 

D/RIL-IPC ( 1891): xmm626_sec_modem_fmt_recv: Received FMT message

D/RIL-IPC ( 1891): xmm626_sec_modem_fmt_recv: Message: aseq=0x24, command=IPC_NET_PLMN_SEL, type=IPC_TYPE_RESP, size=1

D/RIL-IPC ( 1891): ================================= IPC FMT data =================================

D/RIL-IPC ( 1891): [0000]   02                                                 .

D/RIL-IPC ( 1891): ================================================================================

D/RIL     ( 1891): 1 RIL request in the queue (0 pending, 1 handled, 0 unhandled)

D/RILJ    ( 2563): [0047]< OPERATOR {Mobistar, Mobistar, 20610}

D/RIL-IPC ( 1891): 

D/RIL-IPC ( 1891): xmm626_sec_modem_fmt_recv: Received FMT message

D/RIL-IPC ( 1891): xmm626_sec_modem_fmt_recv: Message: aseq=0x25, command=IPC_NET_SERVING_NETWORK, type=IPC_TYPE_RESP, size=11

D/RIL-IPC ( 1891): ================================= IPC FMT data =================================

D/RIL-IPC ( 1891): [0000]   02 04 04 32 30 36 31 30  23 CC 42                  ...20610 #.B

D/RIL-IPC ( 1891): ================================================================================

D/RILJ    ( 2563): [0048]< DATA_REGISTRATION_STATE {0, 42cc, 7d407, 9, 3}

D/RIL     ( 1891): 0 RIL request in the queue (0 pending, 0 handled, 0 unhandled)

D/RILJ    ( 2563): [0049]< VOICE_REGISTRATION_STATE {10, 42cc, 7d407, 9, null, null, null, null, null, null, null, null, null, null, null}

D/RIL     ( 1891): 1 RIL request in the queue (1 pending, 0 handled, 0 unhandled)

D/RIL-IPC ( 1891): 

D/RIL-IPC ( 1891): xmm626_sec_modem_fmt_send: Sent FMT message

D/RILJ    ( 2563): [0050]< QUERY_NETWORK_SELECTION_MODE {0}

D/RIL-IPC ( 1891): xmm626_sec_modem_fmt_send: Message: mseq=0x26, command=IPC_NET_REGIST, type=IPC_TYPE_GET, size=2

D/RIL-IPC ( 1891): ================================= IPC FMT data =================================

D/RIL-IPC ( 1891): [0000]   FF 03                                              ..

D/RIL-IPC ( 1891): ================================================================================

D/RIL     ( 1891): 2 RIL requests in the queue (1 pending, 1 handled, 0 unhandled)

D/RIL-IPC ( 1891): 

D/RIL-IPC ( 1891): xmm626_sec_modem_fmt_send: Sent FMT message

D/RIL-IPC ( 1891): xmm626_sec_modem_fmt_send: Message: mseq=0x27, command=IPC_NET_REGIST, type=IPC_TYPE_GET, size=2

D/RIL-IPC ( 1891): ================================= IPC FMT data =================================

D/RIL-IPC ( 1891): [0000]   FF 02                                              ..

D/RIL-IPC ( 1891): ================================================================================

D/RIL-IPC ( 1891): 

D/RIL-IPC ( 1891): xmm626_sec_modem_fmt_recv: Received FMT message

D/RIL-IPC ( 1891): xmm626_sec_modem_fmt_recv: Message: aseq=0x26, command=IPC_NET_REGIST, type=IPC_TYPE_RESP, size=11

D/RIL-IPC ( 1891): ================================= IPC FMT data =================================

D/RIL-IPC ( 1891): [0000]   04 03 01 01 CC 42 07 D4  07 00 00                  .....B.. ...

D/RIL-IPC ( 1891): ================================================================================

D/RIL     ( 1891): 1 RIL request in the queue (0 pending, 1 handled, 0 unhandled)

D/RILJ    ( 2563): [0054]> QUERY_NETWORK_SELECTION_MODE

D/RIL-IPC ( 1891): 

D/RIL-IPC ( 1891): xmm626_sec_modem_fmt_recv: Received FMT message

D/RIL-IPC ( 1891): xmm626_sec_modem_fmt_recv: Message: aseq=0x27, command=IPC_NET_REGIST, type=IPC_TYPE_RESP, size=11

D/RIL-IPC ( 1891): ================================= IPC FMT data =================================

D/RIL-IPC ( 1891): [0000]   04 02 04 01 CC 42 07 D4  07 00 00                  .....B.. ...

D/RIL-IPC ( 1891): ================================================================================

D/RIL     ( 1891): 0 RIL request in the queue (0 pending, 0 handled, 0 unhandled)

D/RILJ    ( 2563): [0051]< OPERATOR {Mobistar, Mobistar, 20610}

D/RIL     ( 1891): 1 RIL request in the queue (1 pending, 0 handled, 0 unhandled)

D/RIL-IPC ( 1891): 

D/RIL-IPC ( 1891): xmm626_sec_modem_fmt_send: Sent FMT message

D/RIL-IPC ( 1891): xmm626_sec_modem_fmt_send: Message: mseq=0x28, command=IPC_NET_PLMN_SEL, type=IPC_TYPE_GET, size=0

D/RILJ    ( 2563): [0055]> OPERATOR

D/RILJ    ( 2563): [0052]< DATA_REGISTRATION_STATE {0, 42cc, 7d407, 9, 3}

D/RIL-IPC ( 1891): 

D/RIL-IPC ( 1891): xmm626_sec_modem_fmt_recv: Received FMT message

D/RIL-IPC ( 1891): xmm626_sec_modem_fmt_recv: Message: aseq=0x28, command=IPC_NET_PLMN_SEL, type=IPC_TYPE_RESP, size=1

D/RIL-IPC ( 1891): ================================= IPC FMT data =================================

D/RIL-IPC ( 1891): [0000]   02                                                 .

D/RIL-IPC ( 1891): ================================================================================

D/RIL     ( 1891): 0 RIL request in the queue (0 pending, 0 handled, 0 unhandled)

D/RILJ    ( 2563): [0053]< VOICE_REGISTRATION_STATE {10, 42cc, 7d407, 9, null, null, null, null, null, null, null, null, null, null, null}

D/RIL     ( 1891): 1 RIL request in the queue (1 pending, 0 handled, 0 unhandled)

D/RIL-IPC ( 1891): 

D/RIL-IPC ( 1891): xmm626_sec_modem_fmt_send: Sent FMT message

D/RIL-IPC ( 1891): xmm626_sec_modem_fmt_send: Message: mseq=0x29, command=IPC_NET_SERVING_NETWORK, type=IPC_TYPE_GET, size=0

D/RILJ    ( 2563): [0056]> DATA_REGISTRATION_STATE

D/RILJ    ( 2563): [0054]< QUERY_NETWORK_SELECTION_MODE {0}

D/RIL-IPC ( 1891): 

D/RIL-IPC ( 1891): xmm626_sec_modem_fmt_recv: Received FMT message

D/RIL-IPC ( 1891): xmm626_sec_modem_fmt_recv: Message: aseq=0x29, command=IPC_NET_SERVING_NETWORK, type=IPC_TYPE_RESP, size=11

D/RIL-IPC ( 1891): ================================= IPC FMT data =================================

D/RIL-IPC ( 1891): [0000]   02 04 04 32 30 36 31 30  23 CC 42                  ...20610 #.B

D/RIL-IPC ( 1891): ================================================================================

D/RIL     ( 1891): 0 RIL request in the queue (0 pending, 0 handled, 0 unhandled)

D/RILJ    ( 2563): [0055]< OPERATOR {Mobistar, Mobistar, 20610}

D/RIL     ( 1891): 1 RIL request in the queue (1 pending, 0 handled, 0 unhandled)

D/RIL-IPC ( 1891): 

D/RIL-IPC ( 1891): xmm626_sec_modem_fmt_send: Sent FMT message

D/RIL-IPC ( 1891): xmm626_sec_modem_fmt_send: Message: mseq=0x2a, command=IPC_NET_REGIST, type=IPC_TYPE_GET, size=2

D/RIL-IPC ( 1891): ================================= IPC FMT data =================================

D/RIL-IPC ( 1891): [0000]   FF 03                                              ..

D/RIL-IPC ( 1891): ================================================================================

D/RILJ    ( 2563): [0057]> VOICE_REGISTRATION_STATE

D/RIL-IPC ( 1891): 

D/RIL-IPC ( 1891): xmm626_sec_modem_fmt_recv: Received FMT message

D/RIL-IPC ( 1891): xmm626_sec_modem_fmt_recv: Message: aseq=0x2a, command=IPC_NET_REGIST, type=IPC_TYPE_RESP, size=11

D/RIL-IPC ( 1891): ================================= IPC FMT data =================================

D/RIL-IPC ( 1891): [0000]   04 03 01 01 CC 42 07 D4  07 00 00                  .....B.. ...

D/RIL-IPC ( 1891): ================================================================================

D/RIL     ( 1891): 0 RIL request in the queue (0 pending, 0 handled, 0 unhandled)

D/RIL     ( 1891): 1 RIL request in the queue (1 pending, 0 handled, 0 unhandled)

D/RIL-IPC ( 1891): 

D/RIL-IPC ( 1891): xmm626_sec_modem_fmt_send: Sent FMT message

D/RIL-IPC ( 1891): xmm626_sec_modem_fmt_send: Message: mseq=0x2b, command=IPC_NET_REGIST, type=IPC_TYPE_GET, size=2

D/RIL-IPC ( 1891): ================================= IPC FMT data =================================

D/RIL-IPC ( 1891): [0000]   FF 02                                              ..

D/RIL-IPC ( 1891): ================================================================================

D/RILJ    ( 2563): [0056]< DATA_REGISTRATION_STATE {0, 42cc, 7d407, 9, 3}

D/RILJ    ( 2563): [0058]> QUERY_NETWORK_SELECTION_MODE

D/RIL-IPC ( 1891): 

D/RIL-IPC ( 1891): xmm626_sec_modem_fmt_recv: Received FMT message

D/RIL-IPC ( 1891): xmm626_sec_modem_fmt_recv: Message: aseq=0x2b, command=IPC_NET_REGIST, type=IPC_TYPE_RESP, size=11

D/RIL-IPC ( 1891): ================================= IPC FMT data =================================

D/RIL-IPC ( 1891): [0000]   04 02 04 01 CC 42 07 D4  07 00 00                  .....B.. ...

D/RIL-IPC ( 1891): ================================================================================

D/RIL     ( 1891): 0 RIL request in the queue (0 pending, 0 handled, 0 unhandled)

D/RIL     ( 1891): 1 RIL request in the queue (1 pending, 0 handled, 0 unhandled)

D/RIL-IPC ( 1891): 

D/RIL-IPC ( 1891): xmm626_sec_modem_fmt_send: Sent FMT message

D/RIL-IPC ( 1891): xmm626_sec_modem_fmt_send: Message: mseq=0x2c, command=IPC_NET_PLMN_SEL, type=IPC_TYPE_GET, size=0

D/RILJ    ( 2563): [0057]< VOICE_REGISTRATION_STATE {10, 42cc, 7d407, 9, null, null, null, null, null, null, null, null, null, null, null}

D/RILJ    ( 2563): [0059]> OPERATOR

D/RIL-IPC ( 1891): 

D/RIL-IPC ( 1891): xmm626_sec_modem_fmt_recv: Received FMT message

D/RIL-IPC ( 1891): xmm626_sec_modem_fmt_recv: Message: aseq=0x2c, command=IPC_NET_PLMN_SEL, type=IPC_TYPE_RESP, size=1

D/RIL-IPC ( 1891): ================================= IPC FMT data =================================

D/RIL-IPC ( 1891): [0000]   02                                                 .

D/RIL-IPC ( 1891): ================================================================================

D/RIL     ( 1891): 0 RIL request in the queue (0 pending, 0 handled, 0 unhandled)

D/RIL     ( 1891): 1 RIL request in the queue (1 pending, 0 handled, 0 unhandled)

D/RILJ    ( 2563): [0058]< QUERY_NETWORK_SELECTION_MODE {0}

D/RIL-IPC ( 1891): 

D/RIL-IPC ( 1891): xmm626_sec_modem_fmt_send: Sent FMT message

D/RIL-IPC ( 1891): xmm626_sec_modem_fmt_send: Message: mseq=0x2d, command=IPC_NET_SERVING_NETWORK, type=IPC_TYPE_GET, size=0

D/RILJ    ( 2563): [0060]> DATA_REGISTRATION_STATE

D/RIL-IPC ( 1891): 

D/RIL-IPC ( 1891): xmm626_sec_modem_fmt_recv: Received FMT message

D/RIL-IPC ( 1891): xmm626_sec_modem_fmt_recv: Message: aseq=0x2d, command=IPC_NET_SERVING_NETWORK, type=IPC_TYPE_RESP, size=11

D/RIL-IPC ( 1891): ================================= IPC FMT data =================================

D/RIL-IPC ( 1891): [0000]   02 04 04 32 30 36 31 30  23 CC 42                  ...20610 #.B

D/RIL-IPC ( 1891): ================================================================================

D/RIL     ( 1891): 0 RIL request in the queue (0 pending, 0 handled, 0 unhandled)

D/RILJ    ( 2563): [0059]< OPERATOR {Mobistar, Mobistar, 20610}

D/RIL     ( 1891): 1 RIL request in the queue (1 pending, 0 handled, 0 unhandled)

D/RIL-IPC ( 1891): 

D/RIL-IPC ( 1891): xmm626_sec_modem_fmt_send: Sent FMT message

D/RIL-IPC ( 1891): xmm626_sec_modem_fmt_send: Message: mseq=0x2e, command=IPC_NET_REGIST, type=IPC_TYPE_GET, size=2

D/RIL-IPC ( 1891): ================================= IPC FMT data =================================

D/RIL-IPC ( 1891): [0000]   FF 03                                              ..

D/RIL-IPC ( 1891): ================================================================================

D/RILJ    ( 2563): [0061]> VOICE_REGISTRATION_STATE

D/RIL-IPC ( 1891): 

D/RIL-IPC ( 1891): xmm626_sec_modem_fmt_recv: Received FMT message

D/RIL-IPC ( 1891): xmm626_sec_modem_fmt_recv: Message: aseq=0x2e, command=IPC_NET_REGIST, type=IPC_TYPE_RESP, size=11

D/RIL-IPC ( 1891): ================================= IPC FMT data =================================

D/RIL-IPC ( 1891): [0000]   04 03 01 01 CC 42 07 D4  07 00 00                  .....B.. ...

D/RIL-IPC ( 1891): ================================================================================

D/RIL     ( 1891): 0 RIL request in the queue (0 pending, 0 handled, 0 unhandled)

D/RIL     ( 1891): 1 RIL request in the queue (1 pending, 0 handled, 0 unhandled)

D/RIL-IPC ( 1891): 

D/RIL-IPC ( 1891): xmm626_sec_modem_fmt_send: Sent FMT message

D/RIL-IPC ( 1891): xmm626_sec_modem_fmt_send: Message: mseq=0x2f, command=IPC_NET_REGIST, type=IPC_TYPE_GET, size=2

D/RIL-IPC ( 1891): ================================= IPC FMT data =================================

D/RIL-IPC ( 1891): [0000]   FF 02                                              ..

D/RIL-IPC ( 1891): ================================================================================

D/RILJ    ( 2563): [0060]< DATA_REGISTRATION_STATE {0, 42cc, 7d407, 9, 3}

D/RILJ    ( 2563): [0062]> QUERY_NETWORK_SELECTION_MODE

D/RIL-IPC ( 1891): 

D/RIL-IPC ( 1891): xmm626_sec_modem_fmt_recv: Received FMT message

D/RIL-IPC ( 1891): xmm626_sec_modem_fmt_recv: Message: aseq=0x2f, command=IPC_NET_REGIST, type=IPC_TYPE_RESP, size=11

D/RIL-IPC ( 1891): ================================= IPC FMT data =================================

D/RIL-IPC ( 1891): [0000]   04 02 04 01 CC 42 07 D4  07 00 00                  .....B.. ...

D/RIL-IPC ( 1891): ================================================================================

D/RIL     ( 1891): 0 RIL request in the queue (0 pending, 0 handled, 0 unhandled)

D/RILJ    ( 2563): [0061]< VOICE_REGISTRATION_STATE {10, 42cc, 7d407, 9, null, null, null, null, null, null, null, null, null, null, null}

D/RIL     ( 1891): 1 RIL request in the queue (1 pending, 0 handled, 0 unhandled)

D/RIL-IPC ( 1891): 

D/RIL-IPC ( 1891): xmm626_sec_modem_fmt_send: Sent FMT message

D/RIL-IPC ( 1891): xmm626_sec_modem_fmt_send: Message: mseq=0x30, command=IPC_NET_PLMN_SEL, type=IPC_TYPE_GET, size=0

D/RIL-IPC ( 1891): 

D/RIL-IPC ( 1891): xmm626_sec_modem_fmt_recv: Received FMT message

D/RIL-IPC ( 1891): xmm626_sec_modem_fmt_recv: Message: aseq=0x30, command=IPC_NET_PLMN_SEL, type=IPC_TYPE_RESP, size=1

D/RIL-IPC ( 1891): ================================= IPC FMT data =================================

D/RIL-IPC ( 1891): [0000]   02                                                 .

D/RIL-IPC ( 1891): ================================================================================

D/RIL     ( 1891): 0 RIL request in the queue (0 pending, 0 handled, 0 unhandled)

D/RILJ    ( 2563): [0062]< QUERY_NETWORK_SELECTION_MODE {0}

D/GSM     ( 2563): [GsmSST] Poll ServiceState done:  oldSS=[1 home Proximus Proximus 20601  Unknown CSS not supported -1 -1 RoamInd=-1 DefRoamInd=-1 EmergOnly=true] newSS=[1 home Mobistar Mobistar 20610  HSDPA CSS not supported -1 -1 RoamInd=-1 DefRoamInd=-1 EmergOnly=true] oldGprs=1 newData=1 oldMaxDataCalls=1 mNewMaxDataCalls=1 oldReasonDataDenied=-1 mNewReasonDataDenied=-1 oldType=Unknown newType=HSDPA

D/GSM     ( 2563): [GsmSST] RAT switched Unknown -> HSDPA at cell 513031

D/GSM     ( 2563): [GsmSST] updateSpnDisplay: radio is on but out of service, set plmn='Emergency calls only'

D/GSM     ( 2563): [GsmSST] updateSpnDisplay: changed sending intent rule=2 showPlmn='true' plmn='Emergency calls only' showSpn='false' spn='null'

D/GSM     ( 2563): [GsmSST] pollStateDone: no nitz but one TZ for iso-cc=be with zone.getID=Europe/Brussels testOneUniqueOffsetPath=false

D/GSM     ( 2563): [GsmSST] setAndBroadcastNetworkSetTimeZone: setTimeZone=Europe/Brussels

D/GSM     ( 2563): [GsmSST] setAndBroadcastNetworkSetTimeZone: call alarm.setTimeZone and broadcast zoneId=Europe/Brussels

D/GSM     ( 2563): [GsmSST] shouldFixTimeZoneNow: retVal=false iccCardExist=true operatorNumeric=20610 mcc=206 prevOperatorNumeric=20601 prevMcc=206 needToFixTimeZone=false ltod=06-01 18:27:38.019

D/GSM     ( 2563): [GsmDCT] get all active apn types

D/GSM     ( 2563): [GsmDCT] isDataAllowed: not allowed due to - gprs= 1 - SIM not loaded

D/GSM     ( 2563): [GsmDCT] isDataPossible(default): possible=false isDataAllowed=false apnTypePossible=true apnContextisEnabled=true apnContextState()=IDLE

D/GSM     ( 2563): [GsmDCT] get active apn string for type:default

D/RIL-IPC ( 1891): 

D/RIL-IPC ( 1891): xmm626_sec_modem_fmt_recv: Received FMT message

D/RIL-IPC ( 1891): xmm626_sec_modem_fmt_recv: Message: aseq=0x30, command=IPC_DISP_ICON_INFO, type=IPC_TYPE_NOTI, size=4

D/RIL-IPC ( 1891): ================================= IPC FMT data =================================

D/RIL-IPC ( 1891): [0000]   FF 04 00 05                                        ....

D/RIL-IPC ( 1891): ================================================================================

D/RIL     ( 1891): Signal strength is 12

D/RIL-IPC ( 1891): 

D/RIL-IPC ( 1891): xmm626_sec_modem_fmt_recv: Received FMT message

D/RIL-IPC ( 1891): xmm626_sec_modem_fmt_recv: Message: aseq=0x30, command=IPC_DISP_RSSI_INFO, type=IPC_TYPE_NOTI, size=1

D/RIL-IPC ( 1891): ================================= IPC FMT data =================================

D/RIL-IPC ( 1891): [0000]   56                                                 V

D/RIL-IPC ( 1891): ================================================================================

D/RIL     ( 1891): Signal strength is 13

D/RILJ    ( 2563): [0063]> ENTER_SIM_PIN

D/RIL     ( 1891): 1 RIL request in the queue (1 pending, 0 handled, 0 unhandled)

D/RIL-IPC ( 1891): 

D/RIL-IPC ( 1891): xmm626_sec_modem_fmt_send: Sent FMT message

D/RIL-IPC ( 1891): xmm626_sec_modem_fmt_send: Message: mseq=0x31, command=IPC_SEC_PIN_STATUS, type=IPC_TYPE_SET, size=19

D/RIL-IPC ( 1891): ================================= IPC FMT data =================================

D/RIL-IPC ( 1891): [0000]   03 04 00 34 31 34 30 00  00 00 00 00 00 00 00 00   ...PIN CODE APPEARS HERE AND HAS BEEN REMOVED. ........

D/RIL-IPC ( 1891): [0010]   00 00 00                                           ...

D/RIL-IPC ( 1891): ================================================================================

D/RIL-IPC ( 1891): 

D/RIL-IPC ( 1891): xmm626_sec_modem_fmt_recv: Received FMT message

D/RIL-IPC ( 1891): xmm626_sec_modem_fmt_recv: Message: aseq=0x31, command=IPC_GEN_PHONE_RES, type=IPC_TYPE_RESP, size=5

D/RIL-IPC ( 1891): ================================= IPC FMT data =================================

D/RIL-IPC ( 1891): [0000]   05 01 03 00 80                                     .....

D/RIL-IPC ( 1891): ================================================================================

D/RIL     ( 1891): Generic response was expected

D/RIL-IPC ( 1891): 

D/RIL-IPC ( 1891): xmm626_sec_modem_fmt_send: Sent FMT message

D/RIL-IPC ( 1891): xmm626_sec_modem_fmt_send: Message: mseq=0x31, command=IPC_SEC_LOCK_INFOMATION, type=IPC_TYPE_GET, size=2

D/RIL-IPC ( 1891): ================================= IPC FMT data =================================

D/RIL-IPC ( 1891): [0000]   01 03                                              ..

D/RIL-IPC ( 1891): ================================================================================

D/RIL-IPC ( 1891): 

D/RIL-IPC ( 1891): xmm626_sec_modem_fmt_recv: Received FMT message

D/RIL-IPC ( 1891): xmm626_sec_modem_fmt_recv: Message: aseq=0x31, command=IPC_SEC_LOCK_INFOMATION, type=IPC_TYPE_RESP, size=4

D/RIL-IPC ( 1891): ================================= IPC FMT data =================================

D/RIL-IPC ( 1891): [0000]   01 03 00 03                                        ....

D/RIL-IPC ( 1891): ================================================================================

D/RIL     ( 1891): 0 RIL request in the queue (0 pending, 0 handled, 0 unhandled)

D/RILJ    ( 2563): [0063]< ENTER_SIM_PIN {3}

D/RIL-IPC ( 1891): 

D/RIL-IPC ( 1891): xmm626_sec_modem_fmt_recv: Received FMT message

D/RIL-IPC ( 1891): xmm626_sec_modem_fmt_recv: Message: aseq=0x31, command=IPC_SEC_PIN_STATUS, type=IPC_TYPE_NOTI, size=2

D/RIL-IPC ( 1891): ================================= IPC FMT data =================================

D/RIL-IPC ( 1891): [0000]   00 00                                              ..

D/RIL-IPC ( 1891): ================================================================================

D/RIL     ( 1891): ipc2ril_sec_pin_status_response: Selecting status application 2 on 10

D/RIL     ( 1891): Updating RIL radio state to 4

D/RIL-IPC ( 1891): 

D/RIL-IPC ( 1891): xmm626_sec_modem_fmt_recv: Received FMT message

D/RIL-IPC ( 1891): xmm626_sec_modem_fmt_recv: Message: aseq=0xff, command=IPC_SEC_PIN_STATUS, type=IPC_TYPE_NOTI, size=2

D/RIL-IPC ( 1891): ================================= IPC FMT data =================================

D/RIL-IPC ( 1891): [0000]   82 00                                              ..

D/RIL-IPC ( 1891): ================================================================================

D/RIL     ( 1891): ipc2ril_sec_pin_status_response: Selecting status application 2 on 10

D/RIL-IPC ( 1891): 

D/RIL-IPC ( 1891): xmm626_sec_modem_fmt_recv: Received FMT message

D/RIL-IPC ( 1891): xmm626_sec_modem_fmt_recv: Message: aseq=0x00, command=IPC_SMS_DEVICE_READY, type=IPC_TYPE_NOTI, size=1

D/RIL-IPC ( 1891): ================================= IPC FMT data =================================

D/RIL-IPC ( 1891): [0000]   02                                                 .

D/RIL-IPC ( 1891): ================================================================================

D/RIL-IPC ( 1891): Unhandled IPC FMT message: IPC_SMS_DEVICE_READY

D/RILJ    ( 2563): [UNSL]< UNSOL_RESPONSE_SIM_STATUS_CHANGED

D/RILJ    ( 2563): [UNSL]< UNSOL_RESPONSE_RADIO_STATE_CHANGED RADIO_ON

D/RILJ    ( 2563): [UNSL]< UNSOL_RESPONSE_SIM_STATUS_CHANGED

D/RILJ    ( 2563): [UNSL]< UNSOL_RESPONSE_SIM_STATUS_CHANGED

D/RIL_UiccController( 2563): Received EVENT_ICC_STATUS_CHANGED, calling getIccCardStatus

D/RILJ    ( 2563): [0064]> GET_SIM_STATUS

D/RIL_UiccController( 2563): Received EVENT_ICC_STATUS_CHANGED, calling getIccCardStatus

D/RILJ    ( 2563): [0065]> GET_SIM_STATUS

D/RIL     ( 1891): 1 RIL request in the queue (1 pending, 0 handled, 0 unhandled)

D/RIL     ( 1891): 1 RIL request data in the queue

D/RIL     ( 1891): 0 RIL request in the queue (0 pending, 0 handled, 0 unhandled)

D/RIL_UiccController( 2563): Received EVENT_ICC_STATUS_CHANGED, calling getIccCardStatus

D/RIL     ( 1891): 1 RIL request in the queue (1 pending, 0 handled, 0 unhandled)

D/RIL-IPC ( 1891): 

D/RIL-IPC ( 1891): xmm626_sec_modem_fmt_send: Sent FMT message

D/RIL-IPC ( 1891): xmm626_sec_modem_fmt_send: Message: mseq=0x32, command=IPC_SEC_PIN_STATUS, type=IPC_TYPE_GET, size=0

D/RILJ    ( 2563): [0066]> GET_SIM_STATUS

D/RILJ    ( 2563): [0064]< GET_SIM_STATUS IccCardState {CARDSTATE_PRESENT,PINSTATE_UNKNOWN,num_apps=1,gsm_id=0{APPTYPE_SIM,APPSTATE_READY},cdma_id=-1,ims_id=-1}

D/RIL_UiccController( 2563): Received EVENT_GET_ICC_STATUS_DONE

D/RIL_UiccCard( 2563): 1 applications

D/RIL_UiccCardApplication( 2563): APPTYPE_SIM update. New {APPTYPE_SIM,APPSTATE_READY}

D/RIL_UiccCardApplication( 2563): APPTYPE_SIM changed state: APPSTATE_PIN -> APPSTATE_READY

D/RIL     ( 1891): 2 RIL requests in the queue (1 pending, 1 handled, 0 unhandled)

D/RILJ    ( 2563): [0067]> QUERY_FACILITY_LOCK

D/RIL-IPC ( 1891): 

D/RIL-IPC ( 1891): xmm626_sec_modem_fmt_recv: Received FMT message

D/RIL-IPC ( 1891): xmm626_sec_modem_fmt_recv: Message: aseq=0x32, command=IPC_SEC_PIN_STATUS, type=IPC_TYPE_RESP, size=2

D/RIL-IPC ( 1891): ================================= IPC FMT data =================================

D/RIL-IPC ( 1891): [0000]   00 00                                              ..

D/RIL-IPC ( 1891): ================================================================================

D/RIL     ( 1891): ipc2ril_sec_pin_status_response: Selecting status application 2 on 10

D/RIL     ( 1891): 1 RIL request in the queue (0 pending, 0 handled, 1 unhandled)

D/RIL-IPC ( 1891): 

D/RIL-IPC ( 1891): xmm626_sec_modem_fmt_send: Sent FMT message

D/RIL-IPC ( 1891): xmm626_sec_modem_fmt_send: Message: mseq=0x33, command=IPC_SEC_PIN_STATUS, type=IPC_TYPE_GET, size=0

D/RILJ    ( 2563): [0068]> QUERY_FACILITY_LOCK

D/RILJ    ( 2563): [0065]< GET_SIM_STATUS IccCardState {CARDSTATE_PRESENT,PINSTATE_UNKNOWN,num_apps=1,gsm_id=0{APPTYPE_SIM,APPSTATE_READY},cdma_id=-1,ims_id=-1}

D/RIL_UiccCardApplication( 2563): Notifying registrants: READY

D/RIL_UiccCard( 2563): update: radioState=RADIO_ON mLastRadioState=RADIO_ON

D/RIL_UiccController( 2563): Notifying IccChangedRegistrants

D/RIL     ( 1891): 2 RIL requests in the queue (1 pending, 1 handled, 0 unhandled)

D/RIL-IPC ( 1891): 

D/RIL-IPC ( 1891): xmm626_sec_modem_fmt_send: Sent FMT message

D/RIL-IPC ( 1891): xmm626_sec_modem_fmt_send: Message: mseq=0x34, command=IPC_SEC_PHONE_LOCK, type=IPC_TYPE_GET, size=1

D/RIL_UiccController( 2563): Received EVENT_GET_ICC_STATUS_DONE

D/RIL-IPC ( 1891): ================================= IPC FMT data =================================

D/RIL-IPC ( 1891): [0000]   04                                                 .

D/RIL-IPC ( 1891): ================================================================================

D/RIL_UiccCard( 2563): 1 applications

D/RIL_UiccCardApplication( 2563): APPTYPE_SIM update. New {APPTYPE_SIM,APPSTATE_READY}

D/RIL-IPC ( 1891): 

D/RIL-IPC ( 1891): xmm626_sec_modem_fmt_recv: Received FMT message

D/RIL-IPC ( 1891): xmm626_sec_modem_fmt_recv: Message: aseq=0x33, command=IPC_SEC_PIN_STATUS, type=IPC_TYPE_RESP, size=2

D/RIL-IPC ( 1891): ================================= IPC FMT data =================================

D/RIL-IPC ( 1891): [0000]   00 00                                              ..

D/RIL-IPC ( 1891): ================================================================================

D/RIL     ( 1891): ipc2ril_sec_pin_status_response: Selecting status application 2 on 10

D/RIL     ( 1891): 1 RIL request in the queue (0 pending, 1 handled, 0 unhandled)

D/RIL_UiccCard( 2563): update: radioState=RADIO_ON mLastRadioState=RADIO_ON

D/RIL_UiccController( 2563): Notifying IccChangedRegistrants

D/GSM     ( 2563): [SIMRecords] fetchSimRecords 0

D/RIL     ( 1891): 2 RIL requests in the queue (1 pending, 1 handled, 0 unhandled)

D/RIL-IPC ( 1891): 

D/RIL-IPC ( 1891): xmm626_sec_modem_fmt_send: Sent FMT message

D/RIL-IPC ( 1891): xmm626_sec_modem_fmt_send: Message: mseq=0x35, command=IPC_SEC_PHONE_LOCK, type=IPC_TYPE_GET, size=1

D/RIL-IPC ( 1891): ================================= IPC FMT data =================================

D/RIL-IPC ( 1891): [0000]   03                                                 .

D/RILJ    ( 2563): [0069]> getIMSI: GET_IMSI aid: null

D/RIL-IPC ( 1891): ================================================================================

D/RIL     ( 1891): 3 RIL requests in the queue (1 pending, 2 handled, 0 unhandled)

D/RILJ    ( 2563): [0070]> iccIO: SIM_IO 0xc0 0x2fe2  path: 3F00,0,0,15 aid: null

D/RIL-IPC ( 1891): 

D/RIL-IPC ( 1891): xmm626_sec_modem_fmt_send: Sent FMT message

D/RIL-IPC ( 1891): xmm626_sec_modem_fmt_send: Message: mseq=0x36, command=IPC_MISC_ME_IMSI, type=IPC_TYPE_GET, size=0

D/RIL-IPC ( 1891): 

D/RIL-IPC ( 1891): xmm626_sec_modem_fmt_recv: Received FMT message

D/RIL-IPC ( 1891): xmm626_sec_modem_fmt_recv: Message: aseq=0x34, command=IPC_SEC_PHONE_LOCK, type=IPC_TYPE_RESP, size=2

D/RIL-IPC ( 1891): ================================= IPC FMT data =================================

D/RIL-IPC ( 1891): [0000]   04 00                                              ..

D/RIL-IPC ( 1891): ================================================================================

D/RIL     ( 1891): 2 RIL requests in the queue (0 pending, 2 handled, 0 unhandled)

D/RIL     ( 1891): 3 RIL requests in the queue (1 pending, 2 handled, 0 unhandled)

D/RIL-IPC ( 1891): 

D/RIL-IPC ( 1891): xmm626_sec_modem_fmt_send: Sent FMT message

D/RIL-IPC ( 1891): xmm626_sec_modem_fmt_send: Message: mseq=0x37, command=IPC_SEC_RSIM_ACCESS, type=IPC_TYPE_GET, size=6

D/RIL-IPC ( 1891): ================================= IPC FMT data =================================

D/RIL-IPC ( 1891): [0000]   C0 E2 2F 00 00 0F                                  ../...

D/RIL-IPC ( 1891): ================================================================================

D/RILJ    ( 2563): [0071]> iccIO: SIM_IO 0xc0 0x6f40  path: 3F007F10,0,0,15 aid: null

D/RILJ    ( 2563): [0066]< GET_SIM_STATUS IccCardState {CARDSTATE_PRESENT,PINSTATE_UNKNOWN,num_apps=1,gsm_id=0{APPTYPE_SIM,APPSTATE_READY},cdma_id=-1,ims_id=-1}

D/RILJ    ( 2563): [0072]> iccIO: SIM_IO 0xc0 0x6fc9  path: 3F007F20,0,0,15 aid: null

D/RIL     ( 1891): 4 RIL requests in the queue (1 pending, 3 handled, 0 unhandled)

D/RIL-IPC ( 1891): 

D/RIL-IPC ( 1891): xmm626_sec_modem_fmt_recv: Received FMT message

D/RIL-IPC ( 1891): xmm626_sec_modem_fmt_recv: Message: aseq=0x35, command=IPC_SEC_PHONE_LOCK, type=IPC_TYPE_RESP, size=2

D/RIL-IPC ( 1891): ================================= IPC FMT data =================================

D/RIL-IPC ( 1891): [0000]   03 01                                              ..

D/RIL-IPC ( 1891): ================================================================================

D/RIL     ( 1891): 3 RIL requests in the queue (0 pending, 2 handled, 1 unhandled)

D/RIL-IPC ( 1891): 

D/RIL-IPC ( 1891): xmm626_sec_modem_fmt_recv: Received FMT message

D/RIL-IPC ( 1891): xmm626_sec_modem_fmt_recv: Message: aseq=0x36, command=IPC_MISC_ME_IMSI, type=IPC_TYPE_RESP, size=16

D/RIL-IPC ( 1891): ================================= IPC FMT data =================================

D/RIL-IPC ( 1891): [0000]   0F 32 30 36 30 31 32 32  31 37 37 31 34 39 30 32   .2060122 17714902

D/RIL-IPC ( 1891): ================================================================================

D/RIL     ( 1891): 2 RIL requests in the queue (0 pending, 1 handled, 1 unhandled)

D/RIL     ( 1891): 3 RIL requests in the queue (1 pending, 1 handled, 1 unhandled)

D/RILJ    ( 2563): [0073]> iccIO: SIM_IO 0xc0 0x6fad  path: 3F007F20,0,0,15 aid: null

D/RILJ    ( 2563): [0067]< QUERY_FACILITY_LOCK {0}

D/RIL     ( 1891): 4 RIL requests in the queue (1 pending, 1 handled, 2 unhandled)

D/RILJ    ( 2563): [0074]> iccIO: SIM_IO 0xc0 0x6fca  path: 3F007F20,0,0,15 aid: null

D/RILJ    ( 2563): [0068]< QUERY_FACILITY_LOCK {1}

D/RILJ    ( 2563): [0075]> iccIO: SIM_IO 0xc0 0x6f11  path: 3F007F20,0,0,15 aid: null

D/RILJ    ( 2563): [0069]< GET_IMSI 

D/RIL     ( 1891): 5 RIL requests in the queue (1 pending, 1 handled, 3 unhandled)

D/RIL     ( 1891): 6 RIL requests in the queue (2 pending, 1 handled, 3 unhandled)

D/RILJ    ( 2563): [0076]> iccIO: SIM_IO 0xc0 0x6fcb  path: 3F007F20,0,0,15 aid: null

D/RIL     ( 1891): 7 RIL requests in the queue (1 pending, 1 handled, 5 unhandled)

D/RILJ    ( 2563): [0077]> iccIO: SIM_IO 0xc0 0x6f13  path: 3F007F20,0,0,15 aid: null

D/RIL     ( 1891): 8 RIL requests in the queue (1 pending, 1 handled, 6 unhandled)

D/RILJ    ( 2563): [0078]> iccIO: SIM_IO 0xc0 0x6f46  path: 3F007F20,0,0,15 aid: null

D/RILJ    ( 2563): [0079]> iccIO: SIM_IO 0xc0 0x6fcd  path: 3F007F20,0,0,15 aid: null

D/RIL     ( 1891): 9 RIL requests in the queue (1 pending, 1 handled, 7 unhandled)

D/RIL     ( 1891): 10 RIL requests in the queue (1 pending, 1 handled, 8 unhandled)

D/RILJ    ( 2563): [0080]> iccIO: SIM_IO 0xc0 0x6fc5  path: 3F007F20,0,0,15 aid: null

D/RIL     ( 1891): 11 RIL requests in the queue (1 pending, 1 handled, 9 unhandled)

D/RILJ    ( 2563): [0081]> iccIO: SIM_IO 0xc0 0x6f38  path: 3F007F20,0,0,15 aid: null

D/RIL     ( 1891): 12 RIL requests in the queue (1 pending, 1 handled, 10 unhandled)

D/RILJ    ( 2563): [0082]> iccIO: SIM_IO 0xc0 0x6f16  path: 3F007F20,0,0,15 aid: null

D/RIL     ( 1891): 13 RIL requests in the queue (1 pending, 1 handled, 11 unhandled)

D/RILJ    ( 2563): [0083]> iccIO: SIM_IO 0xc0 0x6f15  path: 3F007F20,0,0,15 aid: null

D/RIL     ( 1891): 14 RIL requests in the queue (1 pending, 1 handled, 12 unhandled)

D/GSM     ( 2563): [SIMRecords] fetchSimRecords 15 requested: true

D/RILJ    ( 2563): [0084]> RIL_REQUEST_REPORT_STK_SERVICE_IS_RUNNING

D/RIL     ( 1891): 15 RIL requests in the queue (1 pending, 1 handled, 13 unhandled)

D/RIL     ( 1891): Unhandled RIL request: 103

D/RIL     ( 1891): 14 RIL requests in the queue (0 pending, 1 handled, 13 unhandled)

D/RILJ    ( 2563): [0084]< RIL_REQUEST_REPORT_STK_SERVICE_IS_RUNNING error: com.android.internal.telephony.CommandException: REQUEST_NOT_SUPPORTED

D/RILJ    ( 2563): setCurrentPreferredNetworkType: 0

D/RILJ    ( 2563): [0085]> REQUEST_SET_PREFERRED_NETWORK_TYPE : 0

D/RIL     ( 1891): 15 RIL requests in the queue (1 pending, 1 handled, 13 unhandled)

D/RIL-IPC ( 1891): 

D/RIL-IPC ( 1891): xmm626_sec_modem_fmt_send: Sent FMT message

D/RIL-IPC ( 1891): xmm626_sec_modem_fmt_send: Message: mseq=0x38, command=IPC_NET_MODE_SEL, type=IPC_TYPE_SET, size=1

D/RIL-IPC ( 1891): ================================= IPC FMT data =================================

D/RIL-IPC ( 1891): [0000]   01                                                 .

D/RIL-IPC ( 1891): ================================================================================

D/RILJ    ( 2563): [0086]> SET_NETWORK_SELECTION_AUTOMATIC

D/RIL     ( 1891): 16 RIL requests in the queue (1 pending, 2 handled, 13 unhandled)

D/RIL-IPC ( 1891): 

D/RIL-IPC ( 1891): xmm626_sec_modem_fmt_send: Sent FMT message

D/RIL-IPC ( 1891): xmm626_sec_modem_fmt_send: Message: mseq=0x39, command=IPC_NET_PLMN_SEL, type=IPC_TYPE_SET, size=8

D/RIL-IPC ( 1891): ================================= IPC FMT data =================================

D/RIL-IPC ( 1891): [0000]   02 00 00 00 00 00 00 FF                            ........

D/RIL-IPC ( 1891): ================================================================================

D/RILJ    ( 2563): [0087]> OPERATOR

D/RIL-IPC ( 1891): 

D/RIL-IPC ( 1891): xmm626_sec_modem_fmt_recv: Received FMT message

D/RIL-IPC ( 1891): xmm626_sec_modem_fmt_recv: Message: aseq=0x38, command=IPC_GEN_PHONE_RES, type=IPC_TYPE_RESP, size=5

D/RIL-IPC ( 1891): ================================= IPC FMT data =================================

D/RIL-IPC ( 1891): [0000]   08 0A 03 00 80                                     .....

D/RIL-IPC ( 1891): ================================================================================

D/RIL     ( 1891): Generic response was expected

D/RIL     ( 1891): 15 RIL requests in the queue (0 pending, 2 handled, 13 unhandled)

D/RILJ    ( 2563): [0085]< REQUEST_SET_PREFERRED_NETWORK_TYPE 

D/RIL     ( 1891): 16 RIL requests in the queue (1 pending, 2 handled, 13 unhandled)

D/RIL-IPC ( 1891): 

D/RIL-IPC ( 1891): xmm626_sec_modem_fmt_send: Sent FMT message

D/RIL-IPC ( 1891): xmm626_sec_modem_fmt_send: Message: mseq=0x3a, command=IPC_NET_SERVING_NETWORK, type=IPC_TYPE_GET, size=0

D/RIL-IPC ( 1891): 

D/RIL-IPC ( 1891): xmm626_sec_modem_fmt_recv: Received FMT message

D/RIL-IPC ( 1891): xmm626_sec_modem_fmt_recv: Message: aseq=0x39, command=IPC_GEN_PHONE_RES, type=IPC_TYPE_RESP, size=5

D/RIL-IPC ( 1891): ================================= IPC FMT data =================================

D/RIL-IPC ( 1891): [0000]   08 02 03 00 80                                     .....

D/RIL-IPC ( 1891): ================================================================================

D/RIL     ( 1891): Generic response was expected

D/RIL     ( 1891): 15 RIL requests in the queue (0 pending, 2 handled, 13 unhandled)

D/RILJ    ( 2563): [0086]< SET_NETWORK_SELECTION_AUTOMATIC 

D/RILJ    ( 2563): [0088]> DATA_REGISTRATION_STATE

D/RIL-IPC ( 1891): 

D/RIL-IPC ( 1891): xmm626_sec_modem_fmt_recv: Received FMT message

D/RIL-IPC ( 1891): xmm626_sec_modem_fmt_recv: Message: aseq=0x3a, command=IPC_NET_SERVING_NETWORK, type=IPC_TYPE_RESP, size=11

D/RIL-IPC ( 1891): ================================= IPC FMT data =================================

D/RIL-IPC ( 1891): [0000]   02 04 04 32 30 36 31 30  23 CC 42                  ...20610 #.B

D/RIL-IPC ( 1891): ================================================================================

D/RIL     ( 1891): 14 RIL requests in the queue (0 pending, 1 handled, 13 unhandled)

D/RILJ    ( 2563): [0087]< OPERATOR {Mobistar, Mobistar, 20610}

D/RIL     ( 1891): 15 RIL requests in the queue (1 pending, 1 handled, 13 unhandled)

D/RIL-IPC ( 1891): 

D/RIL-IPC ( 1891): xmm626_sec_modem_fmt_send: Sent FMT message

D/RIL-IPC ( 1891): xmm626_sec_modem_fmt_send: Message: mseq=0x3b, command=IPC_NET_REGIST, type=IPC_TYPE_GET, size=2

D/RIL-IPC ( 1891): ================================= IPC FMT data =================================

D/RIL-IPC ( 1891): [0000]   FF 03                                              ..

D/RIL-IPC ( 1891): ================================================================================

D/RILJ    ( 2563): [0089]> VOICE_REGISTRATION_STATE

D/RIL     ( 1891): 16 RIL requests in the queue (1 pending, 2 handled, 13 unhandled)

D/RIL-IPC ( 1891): 

D/RIL-IPC ( 1891): xmm626_sec_modem_fmt_send: Sent FMT message

D/RIL-IPC ( 1891): xmm626_sec_modem_fmt_send: Message: mseq=0x3c, command=IPC_NET_REGIST, type=IPC_TYPE_GET, size=2

D/RIL-IPC ( 1891): ================================= IPC FMT data =================================

D/RIL-IPC ( 1891): [0000]   FF 02                                              ..

D/RIL-IPC ( 1891): ================================================================================

D/RIL-IPC ( 1891): 

D/RIL-IPC ( 1891): xmm626_sec_modem_fmt_recv: Received FMT message

D/RIL-IPC ( 1891): xmm626_sec_modem_fmt_recv: Message: aseq=0x3b, command=IPC_NET_REGIST, type=IPC_TYPE_RESP, size=11

D/RIL-IPC ( 1891): ================================= IPC FMT data =================================

D/RIL-IPC ( 1891): [0000]   04 03 01 01 CC 42 07 D4  07 00 00                  .....B.. ...

D/RIL-IPC ( 1891): ================================================================================

D/RIL     ( 1891): 15 RIL requests in the queue (0 pending, 2 handled, 13 unhandled)

D/RILJ    ( 2563): [0088]< DATA_REGISTRATION_STATE {0, 42cc, 7d407, 9, 3}

D/RILJ    ( 2563): [0090]> QUERY_NETWORK_SELECTION_MODE

D/RIL     ( 1891): 16 RIL requests in the queue (1 pending, 2 handled, 13 unhandled)

D/RIL-IPC ( 1891): 

D/RIL-IPC ( 1891): xmm626_sec_modem_fmt_send: Sent FMT message

D/RIL-IPC ( 1891): xmm626_sec_modem_fmt_send: Message: mseq=0x3d, command=IPC_NET_PLMN_SEL, type=IPC_TYPE_GET, size=0

D/RIL-IPC ( 1891): 

D/RIL-IPC ( 1891): xmm626_sec_modem_fmt_recv: Received FMT message

D/RIL-IPC ( 1891): xmm626_sec_modem_fmt_recv: Message: aseq=0x3c, command=IPC_NET_REGIST, type=IPC_TYPE_RESP, size=11

D/RIL-IPC ( 1891): ================================= IPC FMT data =================================

D/RIL-IPC ( 1891): [0000]   04 02 04 01 CC 42 07 D4  07 00 00                  .....B.. ...

D/RIL-IPC ( 1891): ================================================================================

D/RIL     ( 1891): 15 RIL requests in the queue (0 pending, 2 handled, 13 unhandled)

D/RILJ    ( 2563): [0089]< VOICE_REGISTRATION_STATE {10, 42cc, 7d407, 9, null, null, null, null, null, null, null, null, null, null, null}

D/RIL_IccCardProxy( 2563): Broadcasting intent ACTION_SIM_STATE_CHANGED READY reason null

D/RIL-IPC ( 1891): 

D/RIL-IPC ( 1891): xmm626_sec_modem_fmt_recv: Received FMT message

D/RIL-IPC ( 1891): xmm626_sec_modem_fmt_recv: Message: aseq=0x3d, command=IPC_NET_PLMN_SEL, type=IPC_TYPE_RESP, size=1

D/RIL-IPC ( 1891): ================================= IPC FMT data =================================

D/RIL-IPC ( 1891): [0000]   02                                                 .

D/RIL-IPC ( 1891): ================================================================================

D/RIL     ( 1891): 14 RIL requests in the queue (0 pending, 1 handled, 13 unhandled)

D/RILJ    ( 2563): [0090]< QUERY_NETWORK_SELECTION_MODE {0}

D/GSM     ( 2563): [GsmDCT] handleMessage msg={ what=270369 when=-25ms obj=android.os.AsyncResult@4180e810 }

D/GSM     ( 2563): [GsmDCT] handleMessage msg={ what=270369 when=-26ms obj=android.os.AsyncResult@4180ede8 }

D/RIL_UiccController( 2563): Received EVENT_GET_ICC_STATUS_DONE

D/RIL_UiccCard( 2563): 1 applications

D/RIL_UiccCardApplication( 2563): APPTYPE_SIM update. New {APPTYPE_SIM,APPSTATE_READY}

D/RIL_UiccCard( 2563): update: radioState=RADIO_ON mLastRadioState=RADIO_ON

D/RIL_UiccController( 2563): Notifying IccChangedRegistrants

D/RIL_UiccCardApplication( 2563): Query facility lock : false

D/RIL_UiccCardApplication( 2563): Query facility lock : 1

D/GSM     ( 2563): [SIMRecords] IMSI: xxxxxxx

D/GSM     ( 2563): [SIMRecords] onRecordLoaded 14 requested: true

D/GSM     ( 2563): [GsmSST] Poll ServiceState done:  oldSS=[1 home Mobistar Mobistar 20610  HSDPA CSS not supported -1 -1 RoamInd=-1 DefRoamInd=-1 EmergOnly=true] newSS=[1 home Mobistar Mobistar 20610  HSDPA CSS not supported -1 -1 RoamInd=-1 DefRoamInd=-1 EmergOnly=true] oldGprs=1 newData=1 oldMaxDataCalls=1 mNewMaxDataCalls=1 oldReasonDataDenied=-1 mNewReasonDataDenied=-1 oldType=HSDPA newType=HSDPA

D/GSM     ( 2563): [GsmDCT] handleMessage msg={ what=270369 when=-3ms obj=android.os.AsyncResult@41818810 }

D/RIL_IccCardProxy( 2563): Broadcasting intent ACTION_SIM_STATE_CHANGED IMSI reason null

D/RIL-IPC ( 1891): 

D/RIL-IPC ( 1891): xmm626_sec_modem_fmt_recv: Received FMT message

D/RIL-IPC ( 1891): xmm626_sec_modem_fmt_recv: Message: aseq=0x37, command=IPC_SEC_RSIM_ACCESS, type=IPC_TYPE_RESP, size=37

D/RIL-IPC ( 1891): ================================= IPC FMT data =================================

D/RIL-IPC ( 1891): [0000]   90 00 22 62 20 82 02 41  21 83 02 2F E2 A5 03 C0   .."b ..A !../....

D/RIL-IPC ( 1891): [0010]   01 40 8A 01 05 8B 06 2F  06 01 01 00 00 80 02 00   .@...../ ........

D/RIL-IPC ( 1891): [0020]   0A 81 02 00 1C                                     .....

D/RIL-IPC ( 1891): ================================================================================

D/RIL     ( 1891): 13 RIL requests in the queue (0 pending, 0 handled, 13 unhandled)

D/RIL-IPC ( 1891): 

D/RIL-IPC ( 1891): xmm626_sec_modem_fmt_send: Sent FMT message

D/RIL-IPC ( 1891): xmm626_sec_modem_fmt_send: Message: mseq=0x3e, command=IPC_SEC_RSIM_ACCESS, type=IPC_TYPE_GET, size=6

D/RIL-IPC ( 1891): ================================= IPC FMT data =================================

D/RIL-IPC ( 1891): [0000]   C0 40 6F 00 00 0F                                  .@o...

D/RIL-IPC ( 1891): ================================================================================

D/RILJ    ( 2563): [0070]< SIM_IO IccIoResponse sw1:0x90 sw2:0x0

D/GSM     ( 2563): [SIMRecords] onRecordLoaded 13 requested: true

D/RIL-IPC ( 1891): 

D/RIL-IPC ( 1891): xmm626_sec_modem_fmt_recv: Received FMT message

D/RIL-IPC ( 1891): xmm626_sec_modem_fmt_recv: Message: aseq=0x3e, command=IPC_SEC_RSIM_ACCESS, type=IPC_TYPE_RESP, size=42

D/RIL-IPC ( 1891): ================================= IPC FMT data =================================

D/RIL-IPC ( 1891): [0000]   90 00 27 62 25 82 05 42  21 00 27 05 83 02 6F 40   ..'b%..B !.'...o@

D/RIL-IPC ( 1891): [0010]   A5 03 C0 01 00 8A 01 05  8B 06 6F 06 01 06 00 00   ........ ..o.....

D/RIL-IPC ( 1891): [0020]   80 02 00 C3 81 02 00 D7  88 00                     ........ ..

D/RIL-IPC ( 1891): ================================================================================

D/RIL     ( 1891): 12 RIL requests in the queue (0 pending, 0 handled, 12 unhandled)

D/RIL-IPC ( 1891): 

D/RIL-IPC ( 1891): xmm626_sec_modem_fmt_send: Sent FMT message

D/RIL-IPC ( 1891): xmm626_sec_modem_fmt_send: Message: mseq=0x3f, command=IPC_SEC_RSIM_ACCESS, type=IPC_TYPE_GET, size=6

D/RIL-IPC ( 1891): ================================= IPC FMT data =================================

D/RIL-IPC ( 1891): [0000]   C0 C9 6F 00 00 0F                                  ..o...

D/RIL-IPC ( 1891): ================================================================================

D/RILJ    ( 2563): [0071]< SIM_IO IccIoResponse sw1:0x90 sw2:0x0

D/RILJ    ( 2563): [0091]> iccIO: SIM_IO 0xb2 0x6f40  path: 3F007F10,1,4,39 aid: null

D/RIL     ( 1891): 13 RIL requests in the queue (1 pending, 1 handled, 11 unhandled)

D/RIL-IPC ( 1891): 

D/RIL-IPC ( 1891): xmm626_sec_modem_fmt_recv: Received FMT message

D/RIL-IPC ( 1891): xmm626_sec_modem_fmt_recv: Message: aseq=0x3f, command=IPC_SEC_RSIM_ACCESS, type=IPC_TYPE_RESP, size=42

D/RIL-IPC ( 1891): ================================= IPC FMT data =================================

D/RIL-IPC ( 1891): [0000]   90 00 27 62 25 82 05 42  21 00 04 01 83 02 6F C9   ..'b%..B !.....o.

D/RIL-IPC ( 1891): [0010]   A5 03 C0 01 00 8A 01 05  8B 06 6F 06 01 11 00 00   ........ ..o.....

D/RIL-IPC ( 1891): [0020]   80 02 00 04 81 02 00 18  88 00                     ........ ..

D/RIL-IPC ( 1891): ================================================================================

D/RIL     ( 1891): 12 RIL requests in the queue (0 pending, 0 handled, 12 unhandled)

D/RIL-IPC ( 1891): 

D/RIL-IPC ( 1891): xmm626_sec_modem_fmt_send: Sent FMT message

D/RIL-IPC ( 1891): xmm626_sec_modem_fmt_send: Message: mseq=0x40, command=IPC_SEC_RSIM_ACCESS, type=IPC_TYPE_GET, size=6

D/RIL-IPC ( 1891): ================================= IPC FMT data =================================

D/RIL-IPC ( 1891): [0000]   C0 AD 6F 00 00 0F                                  ..o...

D/RIL-IPC ( 1891): ================================================================================

D/RILJ    ( 2563): [0072]< SIM_IO IccIoResponse sw1:0x90 sw2:0x0

D/RILJ    ( 2563): [0092]> iccIO: SIM_IO 0xb2 0x6fc9  path: 3F007F20,1,4,4 aid: null

D/RIL     ( 1891): 13 RIL requests in the queue (1 pending, 1 handled, 11 unhandled)

D/RIL-IPC ( 1891): 

D/RIL-IPC ( 1891): xmm626_sec_modem_fmt_recv: Received FMT message

D/RIL-IPC ( 1891): xmm626_sec_modem_fmt_recv: Message: aseq=0x40, command=IPC_SEC_RSIM_ACCESS, type=IPC_TYPE_RESP, size=40

D/RIL-IPC ( 1891): ================================= IPC FMT data =================================

D/RIL-IPC ( 1891): [0000]   90 00 25 62 23 82 02 41  21 83 02 6F AD A5 03 C0   ..%b#..A !..o....

D/RIL-IPC ( 1891): [0010]   01 00 8A 01 05 8B 06 6F  06 01 02 00 00 80 02 00   .......o ........

D/RIL-IPC ( 1891): [0020]   04 81 02 00 16 88 01 18                            ........

D/RIL-IPC ( 1891): ================================================================================

D/RIL     ( 1891): 12 RIL requests in the queue (0 pending, 0 handled, 12 unhandled)

D/RIL-IPC ( 1891): 

D/RIL-IPC ( 1891): xmm626_sec_modem_fmt_recv: Received FMT message

D/RIL-IPC ( 1891): xmm626_sec_modem_fmt_recv: Message: aseq=0xff, command=IPC_NET_REGIST, type=IPC_TYPE_NOTI, size=11

D/RIL-IPC ( 1891): ================================= IPC FMT data =================================

D/RIL-IPC ( 1891): [0000]   04 02 04 01 CC 42 F4 A7  07 00 00                  .....B.. ...

D/RIL-IPC ( 1891): ================================================================================

D/RIL-IPC ( 1891): 

D/RIL-IPC ( 1891): xmm626_sec_modem_fmt_send: Sent FMT message

D/RIL-IPC ( 1891): xmm626_sec_modem_fmt_send: Message: mseq=0x41, command=IPC_SEC_RSIM_ACCESS, type=IPC_TYPE_GET, size=6

D/RIL-IPC ( 1891): ================================= IPC FMT data =================================

D/RIL-IPC ( 1891): [0000]   C0 CA 6F 00 00 0F                                  ..o...

D/RIL-IPC ( 1891): ================================================================================

D/RIL-IPC ( 1891): 

D/RIL-IPC ( 1891): xmm626_sec_modem_fmt_recv: Received FMT message

D/RIL-IPC ( 1891): xmm626_sec_modem_fmt_recv: Message: aseq=0xff, command=IPC_NET_REGIST, type=IPC_TYPE_NOTI, size=11

D/RIL-IPC ( 1891): ================================= IPC FMT data =================================

D/RIL-IPC ( 1891): [0000]   04 03 01 01 CC 42 F4 A7  07 00 00                  .....B.. ...

D/RIL-IPC ( 1891): ================================================================================

D/RILJ    ( 2563): [0073]< SIM_IO IccIoResponse sw1:0x90 sw2:0x0

D/RILJ    ( 2563): [UNSL]< UNSOL_RESPONSE_VOICE_NETWORK_STATE_CHANGED

D/RILJ    ( 2563): [UNSL]< UNSOL_RESPONSE_VOICE_NETWORK_STATE_CHANGED

D/RILJ    ( 2563): [0093]> iccIO: SIM_IO 0xb0 0x6fad  path: 3F007F20,0,0,22 aid: null

D/RILJ    ( 2563): [0094]> OPERATOR

D/RIL     ( 1891): 13 RIL requests in the queue (1 pending, 1 handled, 11 unhandled)

D/RIL     ( 1891): 2 RIL requests data in the queue

D/RILJ    ( 2563): [0095]> DATA_REGISTRATION_STATE

D/RIL     ( 1891): 14 RIL requests in the queue (1 pending, 1 handled, 12 unhandled)

D/RIL     ( 1891): 2 RIL requests data in the queue

D/RIL-IPC ( 1891): 

D/RIL-IPC ( 1891): xmm626_sec_modem_fmt_send: Sent FMT message

D/RIL-IPC ( 1891): xmm626_sec_modem_fmt_send: Message: mseq=0x42, command=IPC_NET_SERVING_NETWORK, type=IPC_TYPE_GET, size=0

D/RILJ    ( 2563): [0096]> VOICE_REGISTRATION_STATE

D/RIL     ( 1891): 15 RIL requests in the queue (1 pending, 2 handled, 12 unhandled)

D/RIL     ( 1891): 2 RIL requests data in the queue

D/RIL     ( 1891): 14 RIL requests in the queue (0 pending, 2 handled, 12 unhandled)

D/RIL     ( 1891): 1 RIL request data in the queue

D/RILJ    ( 2563): [0095]< DATA_REGISTRATION_STATE {0, 42cc, 7a7f4, 9, 3}

D/RILJ    ( 2563): [0097]> QUERY_NETWORK_SELECTION_MODE

D/RIL-IPC ( 1891): 

D/RIL-IPC ( 1891): xmm626_sec_modem_fmt_recv: Received FMT message

D/RIL-IPC ( 1891): xmm626_sec_modem_fmt_recv: Message: aseq=0x42, command=IPC_NET_SERVING_NETWORK, type=IPC_TYPE_RESP, size=11

D/RIL-IPC ( 1891): ================================= IPC FMT data =================================

D/RIL-IPC ( 1891): [0000]   02 04 04 32 30 36 31 30  23 CC 42                  ...20610 #.B

D/RIL-IPC ( 1891): ================================================================================

D/RIL     ( 1891): 13 RIL requests in the queue (0 pending, 1 handled, 12 unhandled)

D/RIL     ( 1891): 1 RIL request data in the queue

D/RILJ    ( 2563): [0098]> OPERATOR

D/RILJ    ( 2563): [0099]> DATA_REGISTRATION_STATE

D/RIL     ( 1891): 14 RIL requests in the queue (1 pending, 1 handled, 12 unhandled)

D/RIL     ( 1891): 1 RIL request data in the queue

D/RIL     ( 1891): 13 RIL requests in the queue (0 pending, 1 handled, 12 unhandled)

D/RILJ    ( 2563): [0100]> VOICE_REGISTRATION_STATE

D/RILJ    ( 2563): [0094]< OPERATOR {Mobistar, Mobistar, 20610}

D/RILJ    ( 2563): [0101]> QUERY_NETWORK_SELECTION_MODE

D/RILJ    ( 2563): [0096]< VOICE_REGISTRATION_STATE {10, 42cc, 7a7f4, 9, null, null, null, null, null, null, null, null, null, null, null}

D/RIL     ( 1891): 14 RIL requests in the queue (1 pending, 1 handled, 12 unhandled)

D/RIL-IPC ( 1891): 

D/RIL-IPC ( 1891): xmm626_sec_modem_fmt_send: Sent FMT message

D/RIL-IPC ( 1891): xmm626_sec_modem_fmt_send: Message: mseq=0x43, command=IPC_NET_PLMN_SEL, type=IPC_TYPE_GET, size=0

D/RIL     ( 1891): 15 RIL requests in the queue (1 pending, 2 handled, 12 unhandled)

D/RIL-IPC ( 1891): 

D/RIL-IPC ( 1891): xmm626_sec_modem_fmt_send: Sent FMT message

D/RIL-IPC ( 1891): xmm626_sec_modem_fmt_send: Message: mseq=0x44, command=IPC_NET_SERVING_NETWORK, type=IPC_TYPE_GET, size=0

D/RIL     ( 1891): 16 RIL requests in the queue (1 pending, 3 handled, 12 unhandled)

D/RIL     ( 1891): 17 RIL requests in the queue (2 pending, 3 handled, 12 unhandled)

D/RIL-IPC ( 1891): 

D/RIL-IPC ( 1891): xmm626_sec_modem_fmt_send: Sent FMT message

D/RIL-IPC ( 1891): xmm626_sec_modem_fmt_send: Message: mseq=0x45, command=IPC_NET_REGIST, type=IPC_TYPE_GET, size=2

D/RIL-IPC ( 1891): ================================= IPC FMT data =================================

D/RIL-IPC ( 1891): [0000]   FF 03                                              ..

D/RIL-IPC ( 1891): ================================================================================

D/RIL-IPC ( 1891): 

D/RIL-IPC ( 1891): xmm626_sec_modem_fmt_send: Sent FMT message

D/RIL-IPC ( 1891): xmm626_sec_modem_fmt_send: Message: mseq=0x46, command=IPC_NET_REGIST, type=IPC_TYPE_GET, size=2

D/RIL-IPC ( 1891): ================================= IPC FMT data =================================

D/RIL-IPC ( 1891): [0000]   FF 02                                              ..

D/RIL-IPC ( 1891): ================================================================================

D/RIL     ( 1891): 18 RIL requests in the queue (1 pending, 5 handled, 12 unhandled)

D/RIL-IPC ( 1891): 

D/RIL-IPC ( 1891): xmm626_sec_modem_fmt_send: Sent FMT message

D/RIL-IPC ( 1891): xmm626_sec_modem_fmt_send: Message: mseq=0x47, command=IPC_NET_PLMN_SEL, type=IPC_TYPE_GET, size=0

D/RIL-IPC ( 1891): 

D/RIL-IPC ( 1891): xmm626_sec_modem_fmt_recv: Received FMT message

D/RIL-IPC ( 1891): xmm626_sec_modem_fmt_recv: Message: aseq=0x43, command=IPC_NET_PLMN_SEL, type=IPC_TYPE_RESP, size=1

D/RIL-IPC ( 1891): ================================= IPC FMT data =================================

D/RIL-IPC ( 1891): [0000]   02                                                 .

D/RIL-IPC ( 1891): ================================================================================

D/RIL     ( 1891): 17 RIL requests in the queue (0 pending, 5 handled, 12 unhandled)

D/RILJ    ( 2563): [0097]< QUERY_NETWORK_SELECTION_MODE {0}

D/RIL-IPC ( 1891): 

D/RIL-IPC ( 1891): xmm626_sec_modem_fmt_recv: Received FMT message

D/RIL-IPC ( 1891): xmm626_sec_modem_fmt_recv: Message: aseq=0x44, command=IPC_NET_SERVING_NETWORK, type=IPC_TYPE_RESP, size=11

D/RIL-IPC ( 1891): ================================= IPC FMT data =================================

D/RIL-IPC ( 1891): [0000]   02 04 04 32 30 36 31 30  23 CC 42                  ...20610 #.B

D/RIL-IPC ( 1891): ================================================================================

D/RIL     ( 1891): 16 RIL requests in the queue (0 pending, 4 handled, 12 unhandled)

D/RILJ    ( 2563): [0098]< OPERATOR {Mobistar, Mobistar, 20610}

D/RIL-IPC ( 1891): 

D/RIL-IPC ( 1891): xmm626_sec_modem_fmt_recv: Received FMT message

D/RIL-IPC ( 1891): xmm626_sec_modem_fmt_recv: Message: aseq=0x45, command=IPC_NET_REGIST, type=IPC_TYPE_RESP, size=11

D/RIL-IPC ( 1891): ================================= IPC FMT data =================================

D/RIL-IPC ( 1891): [0000]   04 03 01 01 CC 42 F4 A7  07 00 00                  .....B.. ...

D/RIL-IPC ( 1891): ================================================================================

D/RIL     ( 1891): 15 RIL requests in the queue (0 pending, 3 handled, 12 unhandled)

D/RILJ    ( 2563): [0099]< DATA_REGISTRATION_STATE {0, 42cc, 7a7f4, 9, 3}

D/RIL-IPC ( 1891): 

D/RIL-IPC ( 1891): xmm626_sec_modem_fmt_recv: Received FMT message

D/RIL-IPC ( 1891): xmm626_sec_modem_fmt_recv: Message: aseq=0x46, command=IPC_NET_REGIST, type=IPC_TYPE_RESP, size=11

D/RIL-IPC ( 1891): ================================= IPC FMT data =================================

D/RIL-IPC ( 1891): [0000]   04 02 04 01 CC 42 F4 A7  07 00 00                  .....B.. ...

D/RIL-IPC ( 1891): ================================================================================

D/RIL     ( 1891): 14 RIL requests in the queue (0 pending, 2 handled, 12 unhandled)

D/RILJ    ( 2563): [0100]< VOICE_REGISTRATION_STATE {10, 42cc, 7a7f4, 9, null, null, null, null, null, null, null, null, null, null, null}

D/RIL-IPC ( 1891): 

D/RIL-IPC ( 1891): xmm626_sec_modem_fmt_recv: Received FMT message

D/RIL-IPC ( 1891): xmm626_sec_modem_fmt_recv: Message: aseq=0x47, command=IPC_NET_PLMN_SEL, type=IPC_TYPE_RESP, size=1

D/RIL-IPC ( 1891): ================================= IPC FMT data =================================

D/RIL-IPC ( 1891): [0000]   02                                                 .

D/RIL-IPC ( 1891): ================================================================================

D/RIL     ( 1891): 13 RIL requests in the queue (0 pending, 1 handled, 12 unhandled)

D/RILJ    ( 2563): [0101]< QUERY_NETWORK_SELECTION_MODE {0}

D/GSM     ( 2563): [GsmSST] Poll ServiceState done:  oldSS=[1 home Mobistar Mobistar 20610  HSDPA CSS not supported -1 -1 RoamInd=-1 DefRoamInd=-1 EmergOnly=true] newSS=[1 home Mobistar Mobistar 20610  HSDPA CSS not supported -1 -1 RoamInd=-1 DefRoamInd=-1 EmergOnly=true] oldGprs=1 newData=1 oldMaxDataCalls=1 mNewMaxDataCalls=1 oldReasonDataDenied=-1 mNewReasonDataDenied=-1 oldType=HSDPA newType=HSDPA

D/RIL-IPC ( 1891): 

D/RIL-IPC ( 1891): xmm626_sec_modem_fmt_recv: Received FMT message

D/RIL-IPC ( 1891): xmm626_sec_modem_fmt_recv: Message: aseq=0x41, command=IPC_SEC_RSIM_ACCESS, type=IPC_TYPE_RESP, size=42

D/RIL-IPC ( 1891): ================================= IPC FMT data =================================

D/RIL-IPC ( 1891): [0000]   90 00 27 62 25 82 05 42  21 00 05 01 83 02 6F CA   ..'b%..B !.....o.

D/RIL-IPC ( 1891): [0010]   A5 03 C0 01 00 8A 01 05  8B 06 6F 06 01 06 00 00   ........ ..o.....

D/RIL-IPC ( 1891): [0020]   80 02 00 05 81 02 00 19  88 00                     ........ ..

D/RIL-IPC ( 1891): ================================================================================

D/RIL     ( 1891): 12 RIL requests in the queue (0 pending, 0 handled, 12 unhandled)

D/RIL-IPC ( 1891): 

D/RIL-IPC ( 1891): xmm626_sec_modem_fmt_send: Sent FMT message

D/RIL-IPC ( 1891): xmm626_sec_modem_fmt_send: Message: mseq=0x48, command=IPC_SEC_RSIM_ACCESS, type=IPC_TYPE_GET, size=6

D/RIL-IPC ( 1891): ================================= IPC FMT data =================================

D/RIL-IPC ( 1891): [0000]   C0 11 6F 00 00 0F                                  ..o...

D/RIL-IPC ( 1891): ================================================================================

D/RILJ    ( 2563): [0074]< SIM_IO IccIoResponse sw1:0x90 sw2:0x0

D/RILJ    ( 2563): [0102]> iccIO: SIM_IO 0xb2 0x6fca  path: 3F007F20,1,4,5 aid: null

D/RIL     ( 1891): 13 RIL requests in the queue (1 pending, 1 handled, 11 unhandled)

D/RIL-IPC ( 1891): 

D/RIL-IPC ( 1891): xmm626_sec_modem_fmt_recv: Received FMT message

D/RIL-IPC ( 1891): xmm626_sec_modem_fmt_recv: Message: aseq=0x48, command=IPC_SEC_RSIM_ACCESS, type=IPC_TYPE_RESP, size=3

D/RIL-IPC ( 1891): ================================= IPC FMT data =================================

D/RIL-IPC ( 1891): [0000]   6A 82 00                                           j..

D/RIL-IPC ( 1891): ================================================================================

D/RIL     ( 1891): 12 RIL requests in the queue (0 pending, 0 handled, 12 unhandled)

D/RIL-IPC ( 1891): 

D/RIL-IPC ( 1891): xmm626_sec_modem_fmt_send: Sent FMT message

D/RIL-IPC ( 1891): xmm626_sec_modem_fmt_send: Message: mseq=0x49, command=IPC_SEC_RSIM_ACCESS, type=IPC_TYPE_GET, size=6

D/RIL-IPC ( 1891): ================================= IPC FMT data =================================

D/RIL-IPC ( 1891): [0000]   C0 CB 6F 00 00 0F                                  ..o...

D/RIL-IPC ( 1891): ================================================================================

D/RILJ    ( 2563): [0075]< SIM_IO IccIoResponse sw1:0x6a sw2:0x82

D/GSM     ( 2563): [SIMRecords] onRecordLoaded 12 requested: true

D/RIL-IPC ( 1891): 

D/RIL-IPC ( 1891): xmm626_sec_modem_fmt_recv: Received FMT message

D/RIL-IPC ( 1891): xmm626_sec_modem_fmt_recv: Message: aseq=0x49, command=IPC_SEC_RSIM_ACCESS, type=IPC_TYPE_RESP, size=42

D/RIL-IPC ( 1891): ================================= IPC FMT data =================================

D/RIL-IPC ( 1891): [0000]   90 00 27 62 25 82 05 42  21 00 10 01 83 02 6F CB   ..'b%..B !.....o.

D/RIL-IPC ( 1891): [0010]   A5 03 C0 01 00 8A 01 05  8B 06 6F 06 01 06 00 00   ........ ..o.....

D/RIL-IPC ( 1891): [0020]   80 02 00 10 81 02 00 24  88 00                     .......$ ..

D/RIL-IPC ( 1891): ================================================================================

D/RIL     ( 1891): 11 RIL requests in the queue (0 pending, 0 handled, 11 unhandled)

D/RIL-IPC ( 1891): 

D/RIL-IPC ( 1891): xmm626_sec_modem_fmt_send: Sent FMT message

D/RIL-IPC ( 1891): xmm626_sec_modem_fmt_send: Message: mseq=0x4a, command=IPC_SEC_RSIM_ACCESS, type=IPC_TYPE_GET, size=6

D/RIL-IPC ( 1891): ================================= IPC FMT data =================================

D/RIL-IPC ( 1891): [0000]   C0 13 6F 00 00 0F                                  ..o...

D/RIL-IPC ( 1891): ================================================================================

D/RILJ    ( 2563): [0076]< SIM_IO IccIoResponse sw1:0x90 sw2:0x0

D/RILJ    ( 2563): [0103]> iccIO: SIM_IO 0xb2 0x6fcb  path: 3F007F20,1,4,16 aid: null

D/RIL     ( 1891): 12 RIL requests in the queue (1 pending, 1 handled, 10 unhandled)

D/RIL-IPC ( 1891): 

D/RIL-IPC ( 1891): xmm626_sec_modem_fmt_recv: Received FMT message

D/RIL-IPC ( 1891): xmm626_sec_modem_fmt_recv: Message: aseq=0x4a, command=IPC_SEC_RSIM_ACCESS, type=IPC_TYPE_RESP, size=3

D/RIL-IPC ( 1891): ================================= IPC FMT data =================================

D/RIL-IPC ( 1891): [0000]   6A 82 00                                           j..

D/RIL-IPC ( 1891): ================================================================================

D/RIL     ( 1891): 11 RIL requests in the queue (0 pending, 0 handled, 11 unhandled)

D/RIL-IPC ( 1891): 

D/RIL-IPC ( 1891): xmm626_sec_modem_fmt_send: Sent FMT message

D/RIL-IPC ( 1891): xmm626_sec_modem_fmt_send: Message: mseq=0x4b, command=IPC_SEC_RSIM_ACCESS, type=IPC_TYPE_GET, size=6

D/RIL-IPC ( 1891): ================================= IPC FMT data =================================

D/RIL-IPC ( 1891): [0000]   C0 46 6F 00 00 0F                                  .Fo...

D/RIL-IPC ( 1891): ================================================================================

D/RILJ    ( 2563): [0077]< SIM_IO IccIoResponse sw1:0x6a sw2:0x82

D/GSM     ( 2563): [SIMRecords] onRecordLoaded 11 requested: true

D/RIL-IPC ( 1891): 

D/RIL-IPC ( 1891): xmm626_sec_modem_fmt_recv: Received FMT message

D/RIL-IPC ( 1891): xmm626_sec_modem_fmt_recv: Message: aseq=0x4b, command=IPC_SEC_RSIM_ACCESS, type=IPC_TYPE_RESP, size=39

D/RIL-IPC ( 1891): ================================= IPC FMT data =================================

D/RIL-IPC ( 1891): [0000]   90 00 24 62 22 82 02 41  21 83 02 6F 46 A5 03 C0   ..$b"..A !..oF...

D/RIL-IPC ( 1891): [0010]   01 00 8A 01 05 8B 06 6F  06 01 02 00 00 80 02 00   .......o ........

D/RIL-IPC ( 1891): [0020]   11 81 02 00 23 88 00                               ....#..

D/RIL-IPC ( 1891): ================================================================================

D/RIL     ( 1891): 10 RIL requests in the queue (0 pending, 0 handled, 10 unhandled)

D/RIL-IPC ( 1891): 

D/RIL-IPC ( 1891): xmm626_sec_modem_fmt_send: Sent FMT message

D/RIL-IPC ( 1891): xmm626_sec_modem_fmt_send: Message: mseq=0x4c, command=IPC_SEC_RSIM_ACCESS, type=IPC_TYPE_GET, size=6

D/RIL-IPC ( 1891): ================================= IPC FMT data =================================

D/RIL-IPC ( 1891): [0000]   C0 CD 6F 00 00 0F                                  ..o...

D/RIL-IPC ( 1891): ================================================================================

D/RILJ    ( 2563): [0078]< SIM_IO IccIoResponse sw1:0x90 sw2:0x0

D/RILJ    ( 2563): [0104]> iccIO: SIM_IO 0xb0 0x6f46  path: 3F007F20,0,0,35 aid: null

D/RIL     ( 1891): 11 RIL requests in the queue (1 pending, 1 handled, 9 unhandled)

D/RIL-IPC ( 1891): 

D/RIL-IPC ( 1891): xmm626_sec_modem_fmt_recv: Received FMT message

D/RIL-IPC ( 1891): xmm626_sec_modem_fmt_recv: Message: aseq=0x4c, command=IPC_SEC_RSIM_ACCESS, type=IPC_TYPE_RESP, size=3

D/RIL-IPC ( 1891): ================================= IPC FMT data =================================

D/RIL-IPC ( 1891): [0000]   6A 82 00                                           j..

D/RIL-IPC ( 1891): ================================================================================

D/RIL     ( 1891): 10 RIL requests in the queue (0 pending, 0 handled, 10 unhandled)

D/RIL-IPC ( 1891): 

D/RIL-IPC ( 1891): xmm626_sec_modem_fmt_send: Sent FMT message

D/RIL-IPC ( 1891): xmm626_sec_modem_fmt_send: Message: mseq=0x4d, command=IPC_SEC_RSIM_ACCESS, type=IPC_TYPE_GET, size=6

D/RIL-IPC ( 1891): ================================= IPC FMT data =================================

D/RIL-IPC ( 1891): [0000]   C0 C5 6F 00 00 0F                                  ..o...

D/RIL-IPC ( 1891): ================================================================================

D/RILJ    ( 2563): [0079]< SIM_IO IccIoResponse sw1:0x6a sw2:0x82

D/GSM     ( 2563): [SIMRecords] onRecordLoaded 10 requested: true

D/RIL-IPC ( 1891): 

D/RIL-IPC ( 1891): xmm626_sec_modem_fmt_recv: Received FMT message

D/RIL-IPC ( 1891): xmm626_sec_modem_fmt_recv: Message: aseq=0x4d, command=IPC_SEC_RSIM_ACCESS, type=IPC_TYPE_RESP, size=3

D/RIL-IPC ( 1891): ================================= IPC FMT data =================================

D/RIL-IPC ( 1891): [0000]   6A 82 00                                           j..

D/RIL-IPC ( 1891): ================================================================================

D/RIL     ( 1891): 9 RIL requests in the queue (0 pending, 0 handled, 9 unhandled)

D/RIL-IPC ( 1891): 

D/RIL-IPC ( 1891): xmm626_sec_modem_fmt_send: Sent FMT message

D/RIL-IPC ( 1891): xmm626_sec_modem_fmt_send: Message: mseq=0x4e, command=IPC_SEC_RSIM_ACCESS, type=IPC_TYPE_GET, size=6

D/RIL-IPC ( 1891): ================================= IPC FMT data =================================

D/RIL-IPC ( 1891): [0000]   C0 38 6F 00 00 0F                                  .8o...

D/RIL-IPC ( 1891): ================================================================================

D/RILJ    ( 2563): [0080]< SIM_IO IccIoResponse sw1:0x6a sw2:0x82

D/GSM     ( 2563): [SIMRecords] onRecordLoaded 9 requested: true

D/RIL-IPC ( 1891): 

D/RIL-IPC ( 1891): xmm626_sec_modem_fmt_recv: Received FMT message

D/RIL-IPC ( 1891): xmm626_sec_modem_fmt_recv: Message: aseq=0x4e, command=IPC_SEC_RSIM_ACCESS, type=IPC_TYPE_RESP, size=40

D/RIL-IPC ( 1891): ================================= IPC FMT data =================================

D/RIL-IPC ( 1891): [0000]   90 00 25 62 23 82 02 41  21 83 02 6F 38 A5 03 C0   ..%b#..A !..o8...

D/RIL-IPC ( 1891): [0010]   01 00 8A 01 05 8B 06 6F  06 01 11 00 00 80 02 00   .......o ........

D/RIL-IPC ( 1891): [0020]   07 81 02 00 19 88 01 20                            ....... 

D/RIL-IPC ( 1891): ================================================================================

D/RIL     ( 1891): 8 RIL requests in the queue (0 pending, 0 handled, 8 unhandled)

D/RIL-IPC ( 1891): 

D/RIL-IPC ( 1891): xmm626_sec_modem_fmt_send: Sent FMT message

D/RIL-IPC ( 1891): xmm626_sec_modem_fmt_send: Message: mseq=0x4f, command=IPC_SEC_RSIM_ACCESS, type=IPC_TYPE_GET, size=6

D/RIL-IPC ( 1891): ================================= IPC FMT data =================================

D/RIL-IPC ( 1891): [0000]   C0 16 6F 00 00 0F                                  ..o...

D/RIL-IPC ( 1891): ================================================================================

D/RILJ    ( 2563): [0081]< SIM_IO IccIoResponse sw1:0x90 sw2:0x0

D/RILJ    ( 2563): [0105]> iccIO: SIM_IO 0xb0 0x6f38  path: 3F007F20,0,0,25 aid: null

D/RIL     ( 1891): 9 RIL requests in the queue (1 pending, 1 handled, 7 unhandled)

D/RIL-IPC ( 1891): 

D/RIL-IPC ( 1891): xmm626_sec_modem_fmt_recv: Received FMT message

D/RIL-IPC ( 1891): xmm626_sec_modem_fmt_recv: Message: aseq=0x4f, command=IPC_SEC_RSIM_ACCESS, type=IPC_TYPE_RESP, size=3

D/RIL-IPC ( 1891): ================================= IPC FMT data =================================

D/RIL-IPC ( 1891): [0000]   6A 82 00                                           j..

D/RIL-IPC ( 1891): ================================================================================

D/RIL     ( 1891): 8 RIL requests in the queue (0 pending, 0 handled, 8 unhandled)

D/RIL-IPC ( 1891): 

D/RIL-IPC ( 1891): xmm626_sec_modem_fmt_send: Sent FMT message

D/RIL-IPC ( 1891): xmm626_sec_modem_fmt_send: Message: mseq=0x50, command=IPC_SEC_RSIM_ACCESS, type=IPC_TYPE_GET, size=6

D/RIL-IPC ( 1891): ================================= IPC FMT data =================================

D/RIL-IPC ( 1891): [0000]   C0 15 6F 00 00 0F                                  ..o...

D/RIL-IPC ( 1891): ================================================================================

D/RILJ    ( 2563): [0082]< SIM_IO IccIoResponse sw1:0x6a sw2:0x82

D/GSM     ( 2563): [SIMRecords] onRecordLoaded 8 requested: true

D/RIL-IPC ( 1891): 

D/RIL-IPC ( 1891): xmm626_sec_modem_fmt_recv: Received FMT message

D/RIL-IPC ( 1891): xmm626_sec_modem_fmt_recv: Message: aseq=0x50, command=IPC_SEC_RSIM_ACCESS, type=IPC_TYPE_RESP, size=3

D/RIL-IPC ( 1891): ================================= IPC FMT data =================================

D/RIL-IPC ( 1891): [0000]   6A 82 00                                           j..

D/RIL-IPC ( 1891): ================================================================================

D/RIL     ( 1891): 7 RIL requests in the queue (0 pending, 0 handled, 7 unhandled)

D/RIL-IPC ( 1891): 

D/RIL-IPC ( 1891): xmm626_sec_modem_fmt_send: Sent FMT message

D/RIL-IPC ( 1891): xmm626_sec_modem_fmt_send: Message: mseq=0x51, command=IPC_SEC_RSIM_ACCESS, type=IPC_TYPE_GET, size=6

D/RIL-IPC ( 1891): ================================= IPC FMT data =================================

D/RIL-IPC ( 1891): [0000]   B2 40 6F 01 04 27                                  .@o..'

D/RIL-IPC ( 1891): ================================================================================

D/RILJ    ( 2563): [0083]< SIM_IO IccIoResponse sw1:0x6a sw2:0x82

E/GSM     ( 2563): [SIMRecords] Exception in fetching EF_CSP data com.android.internal.telephony.IccException: sw1:106 sw2:130

D/GSM     ( 2563): [SIMRecords] onRecordLoaded 7 requested: true

D/RIL-IPC ( 1891): 

D/RIL-IPC ( 1891): xmm626_sec_modem_fmt_recv: Received FMT message

D/RIL-IPC ( 1891): xmm626_sec_modem_fmt_recv: Message: aseq=0x51, command=IPC_SEC_RSIM_ACCESS, type=IPC_TYPE_RESP, size=42

D/RIL-IPC ( 1891): ================================= IPC FMT data =================================

D/RIL-IPC ( 1891): [0000]   90 00 27 47 53 4D 20 4E  75 6D 62 65 72 FF FF FF   ..'GSM N umber...

D/RIL-IPC ( 1891): [0010]   FF FF FF FF FF FF FF FF  FF FF FF FF FF FF FF FF   ........ ........

D/RIL-IPC ( 1891): [0020]   FF FF FF FF FF FF FF FF  FF FF                     ........ ..

D/RIL-IPC ( 1891): ================================================================================

D/RIL     ( 1891): 6 RIL requests in the queue (0 pending, 0 handled, 6 unhandled)

D/RIL-IPC ( 1891): 

D/RIL-IPC ( 1891): xmm626_sec_modem_fmt_send: Sent FMT message

D/RIL-IPC ( 1891): xmm626_sec_modem_fmt_send: Message: mseq=0x52, command=IPC_SEC_RSIM_ACCESS, type=IPC_TYPE_GET, size=6

D/RIL-IPC ( 1891): ================================= IPC FMT data =================================

D/RIL-IPC ( 1891): [0000]   B2 C9 6F 01 04 04                                  ..o...

D/RIL-IPC ( 1891): ================================================================================

D/RILJ    ( 2563): [0091]< SIM_IO IccIoResponse sw1:0x90 sw2:0x0

D/GSM     ( 2563): [SIMRecords] MSISDN: xxxxxxx

D/GSM     ( 2563): [SIMRecords] onRecordLoaded 6 requested: true

D/RIL-IPC ( 1891): 

D/RIL-IPC ( 1891): xmm626_sec_modem_fmt_recv: Received FMT message

D/RIL-IPC ( 1891): xmm626_sec_modem_fmt_recv: Message: aseq=0x52, command=IPC_SEC_RSIM_ACCESS, type=IPC_TYPE_RESP, size=7

D/RIL-IPC ( 1891): ================================= IPC FMT data =================================

D/RIL-IPC ( 1891): [0000]   90 00 04 01 00 00 00                               .......

D/RIL-IPC ( 1891): ================================================================================

D/RIL     ( 1891): 5 RIL requests in the queue (0 pending, 0 handled, 5 unhandled)

D/RIL-IPC ( 1891): 

D/RIL-IPC ( 1891): xmm626_sec_modem_fmt_send: Sent FMT message

D/RIL-IPC ( 1891): xmm626_sec_modem_fmt_send: Message: mseq=0x53, command=IPC_SEC_RSIM_ACCESS, type=IPC_TYPE_GET, size=6

D/RIL-IPC ( 1891): ================================= IPC FMT data =================================

D/RIL-IPC ( 1891): [0000]   B0 AD 6F 00 00 16                                  ..o...

D/RIL-IPC ( 1891): ================================================================================

D/RILJ    ( 2563): [0092]< SIM_IO IccIoResponse sw1:0x90 sw2:0x0

D/GSM     ( 2563): [SIMRecords] EF_MBI: 01000000

D/GSM     ( 2563): [SIMRecords] Got valid mailbox number for MBDN

D/RILJ    ( 2563): [0106]> iccIO: SIM_IO 0xc0 0x6fc7  path: 3F007F20,0,0,15 aid: null

D/GSM     ( 2563): [SIMRecords] onRecordLoaded 6 requested: true

D/RIL     ( 1891): 6 RIL requests in the queue (1 pending, 1 handled, 4 unhandled)

D/RIL-IPC ( 1891): 

D/RIL-IPC ( 1891): xmm626_sec_modem_fmt_recv: Received FMT message

D/RIL-IPC ( 1891): xmm626_sec_modem_fmt_recv: Message: aseq=0x53, command=IPC_SEC_RSIM_ACCESS, type=IPC_TYPE_RESP, size=3

D/RIL-IPC ( 1891): ================================= IPC FMT data =================================

D/RIL-IPC ( 1891): [0000]   67 00 00                                           g..

D/RIL-IPC ( 1891): ================================================================================

D/RIL     ( 1891): 5 RIL requests in the queue (0 pending, 0 handled, 5 unhandled)

D/RIL-IPC ( 1891): 

D/RIL-IPC ( 1891): xmm626_sec_modem_fmt_send: Sent FMT message

D/RIL-IPC ( 1891): xmm626_sec_modem_fmt_send: Message: mseq=0x54, command=IPC_SEC_RSIM_ACCESS, type=IPC_TYPE_GET, size=6

D/RIL-IPC ( 1891): ================================= IPC FMT data =================================

D/RIL-IPC ( 1891): [0000]   B2 CA 6F 01 04 05                                  ..o...

D/RIL-IPC ( 1891): ================================================================================

D/RILJ    ( 2563): [0093]< SIM_IO IccIoResponse sw1:0x67 sw2:0x0

D/GSM     ( 2563): [SIMRecords] onRecordLoaded 5 requested: true

D/RIL-IPC ( 1891): 

D/RIL-IPC ( 1891): xmm626_sec_modem_fmt_recv: Received FMT message

D/RIL-IPC ( 1891): xmm626_sec_modem_fmt_recv: Message: aseq=0x54, command=IPC_SEC_RSIM_ACCESS, type=IPC_TYPE_RESP, size=8

D/RIL-IPC ( 1891): ================================= IPC FMT data =================================

D/RIL-IPC ( 1891): [0000]   90 00 05 00 00 00 00 00                            ........

D/RIL-IPC ( 1891): ================================================================================

D/RIL     ( 1891): 4 RIL requests in the queue (0 pending, 0 handled, 4 unhandled)

D/RIL-IPC ( 1891): 

D/RIL-IPC ( 1891): xmm626_sec_modem_fmt_send: Sent FMT message

D/RIL-IPC ( 1891): xmm626_sec_modem_fmt_send: Message: mseq=0x55, command=IPC_SEC_RSIM_ACCESS, type=IPC_TYPE_GET, size=6

D/RIL-IPC ( 1891): ================================= IPC FMT data =================================

D/RIL-IPC ( 1891): [0000]   B2 CB 6F 01 04 10                                  ..o...

D/RIL-IPC ( 1891): ================================================================================

D/RILJ    ( 2563): [0102]< SIM_IO IccIoResponse sw1:0x90 sw2:0x0

D/GSM     ( 2563): [SIMRecords] EF_MWIS: 0000000000

D/GSM     ( 2563): [SIMRecords] onRecordLoaded 4 requested: true

D/RIL-IPC ( 1891): 

D/RIL-IPC ( 1891): xmm626_sec_modem_fmt_recv: Received FMT message

D/RIL-IPC ( 1891): xmm626_sec_modem_fmt_recv: Message: aseq=0x55, command=IPC_SEC_RSIM_ACCESS, type=IPC_TYPE_RESP, size=19

D/RIL-IPC ( 1891): ================================= IPC FMT data =================================

D/RIL-IPC ( 1891): [0000]   90 00 10 01 00 FF FF FF  FF FF FF FF FF FF FF FF   ........ ........

D/RIL-IPC ( 1891): [0010]   FF FF FF                                           ...

D/RIL-IPC ( 1891): ================================================================================

D/RIL     ( 1891): 3 RIL requests in the queue (0 pending, 0 handled, 3 unhandled)

D/RIL-IPC ( 1891): 

D/RIL-IPC ( 1891): xmm626_sec_modem_fmt_send: Sent FMT message

D/RIL-IPC ( 1891): xmm626_sec_modem_fmt_send: Message: mseq=0x56, command=IPC_SEC_RSIM_ACCESS, type=IPC_TYPE_GET, size=6

D/RIL-IPC ( 1891): ================================= IPC FMT data =================================

D/RIL-IPC ( 1891): [0000]   B0 46 6F 00 00 23                                  .Fo..#

D/RIL-IPC ( 1891): ================================================================================

D/RILJ    ( 2563): [0103]< SIM_IO IccIoResponse sw1:0x90 sw2:0x0

D/GSM     ( 2563): [SIMRecords] EF_CFIS: 0100ffffffffffffffffffffffffffff

D/GSM     ( 2563): [SIMRecords] EF_CFIS: callFordwardingEnabled=false

D/GSM     ( 2563): [SIMRecords] onRecordLoaded 3 requested: true

D/RIL-IPC ( 1891): 

D/RIL-IPC ( 1891): xmm626_sec_modem_fmt_recv: Received FMT message

D/RIL-IPC ( 1891): xmm626_sec_modem_fmt_recv: Message: aseq=0x56, command=IPC_SEC_RSIM_ACCESS, type=IPC_TYPE_RESP, size=3

D/RIL-IPC ( 1891): ================================= IPC FMT data =================================

D/RIL-IPC ( 1891): [0000]   67 00 00                                           g..

D/RIL-IPC ( 1891): ================================================================================

D/RIL     ( 1891): 2 RIL requests in the queue (0 pending, 0 handled, 2 unhandled)

D/RIL-IPC ( 1891): 

D/RIL-IPC ( 1891): xmm626_sec_modem_fmt_send: Sent FMT message

D/RIL-IPC ( 1891): xmm626_sec_modem_fmt_send: Message: mseq=0x57, command=IPC_SEC_RSIM_ACCESS, type=IPC_TYPE_GET, size=6

D/RIL-IPC ( 1891): ================================= IPC FMT data =================================

D/RIL-IPC ( 1891): [0000]   B0 38 6F 00 00 19                                  .8o...

D/RIL-IPC ( 1891): ================================================================================

D/RILJ    ( 2563): [0104]< SIM_IO IccIoResponse sw1:0x67 sw2:0x0

D/RILJ    ( 2563): [0107]> iccIO: SIM_IO 0xc0 0x6f14  path: 3F007F20,0,0,15 aid: null

D/GSM     ( 2563): [SIMRecords] onRecordLoaded 3 requested: true

D/RIL     ( 1891): 3 RIL requests in the queue (1 pending, 1 handled, 1 unhandled)

D/RIL-IPC ( 1891): 

D/RIL-IPC ( 1891): xmm626_sec_modem_fmt_recv: Received FMT message

D/RIL-IPC ( 1891): xmm626_sec_modem_fmt_recv: Message: aseq=0x57, command=IPC_SEC_RSIM_ACCESS, type=IPC_TYPE_RESP, size=3

D/RIL-IPC ( 1891): ================================= IPC FMT data =================================

D/RIL-IPC ( 1891): [0000]   67 00 00                                           g..

D/RIL-IPC ( 1891): ================================================================================

D/RIL     ( 1891): 2 RIL requests in the queue (0 pending, 0 handled, 2 unhandled)

D/RIL-IPC ( 1891): 

D/RIL-IPC ( 1891): xmm626_sec_modem_fmt_send: Sent FMT message

D/RIL-IPC ( 1891): xmm626_sec_modem_fmt_send: Message: mseq=0x58, command=IPC_SEC_RSIM_ACCESS, type=IPC_TYPE_GET, size=6

D/RIL-IPC ( 1891): ================================= IPC FMT data =================================

D/RIL-IPC ( 1891): [0000]   C0 C7 6F 00 00 0F                                  ..o...

D/RIL-IPC ( 1891): ================================================================================

D/RILJ    ( 2563): [0105]< SIM_IO IccIoResponse sw1:0x67 sw2:0x0

D/GSM     ( 2563): [SIMRecords] onRecordLoaded 2 requested: true

D/RIL-IPC ( 1891): 

D/RIL-IPC ( 1891): xmm626_sec_modem_fmt_recv: Received FMT message

D/RIL-IPC ( 1891): xmm626_sec_modem_fmt_recv: Message: aseq=0x58, command=IPC_SEC_RSIM_ACCESS, type=IPC_TYPE_RESP, size=42

D/RIL-IPC ( 1891): ================================= IPC FMT data =================================

D/RIL-IPC ( 1891): [0000]   90 00 27 62 25 82 05 42  21 00 18 03 83 02 6F C7   ..'b%..B !.....o.

D/RIL-IPC ( 1891): [0010]   A5 03 C0 01 00 8A 01 05  8B 06 6F 06 01 11 00 00   ........ ..o.....

D/RIL-IPC ( 1891): [0020]   80 02 00 48 81 02 00 5C  88 00                     ...H...\ ..

D/RIL-IPC ( 1891): ================================================================================

D/RIL     ( 1891): 1 RIL request in the queue (0 pending, 0 handled, 1 unhandled)

D/RIL-IPC ( 1891): 

D/RIL-IPC ( 1891): xmm626_sec_modem_fmt_send: Sent FMT message

D/RIL-IPC ( 1891): xmm626_sec_modem_fmt_send: Message: mseq=0x59, command=IPC_SEC_RSIM_ACCESS, type=IPC_TYPE_GET, size=6

D/RIL-IPC ( 1891): ================================= IPC FMT data =================================

D/RIL-IPC ( 1891): [0000]   C0 14 6F 00 00 0F                                  ..o...

D/RIL-IPC ( 1891): ================================================================================

D/RILJ    ( 2563): [0106]< SIM_IO IccIoResponse sw1:0x90 sw2:0x0

D/RILJ    ( 2563): [0108]> iccIO: SIM_IO 0xb2 0x6fc7  path: 3F007F20,1,4,24 aid: null

D/RIL     ( 1891): 2 RIL requests in the queue (1 pending, 1 handled, 0 unhandled)

D/RIL-IPC ( 1891): 

D/RIL-IPC ( 1891): xmm626_sec_modem_fmt_recv: Received FMT message

D/RIL-IPC ( 1891): xmm626_sec_modem_fmt_recv: Message: aseq=0x59, command=IPC_SEC_RSIM_ACCESS, type=IPC_TYPE_RESP, size=3

D/RIL-IPC ( 1891): ================================= IPC FMT data =================================

D/RIL-IPC ( 1891): [0000]   6A 82 00                                           j..

D/RIL-IPC ( 1891): ================================================================================

D/RIL     ( 1891): 1 RIL request in the queue (0 pending, 0 handled, 1 unhandled)

D/RIL-IPC ( 1891): 

D/RIL-IPC ( 1891): xmm626_sec_modem_fmt_send: Sent FMT message

D/RIL-IPC ( 1891): xmm626_sec_modem_fmt_send: Message: mseq=0x5a, command=IPC_SEC_RSIM_ACCESS, type=IPC_TYPE_GET, size=6

D/RIL-IPC ( 1891): ================================= IPC FMT data =================================

D/RIL-IPC ( 1891): [0000]   B2 C7 6F 01 04 18                                  ..o...

D/RIL-IPC ( 1891): ================================================================================

D/RILJ    ( 2563): [0107]< SIM_IO IccIoResponse sw1:0x6a sw2:0x82

D/RILJ    ( 2563): [0109]> iccIO: SIM_IO 0xc0 0x6f18  path: 3F007F20,0,0,15 aid: null

D/GSM     ( 2563): [SIMRecords] onRecordLoaded 2 requested: true

D/RIL     ( 1891): 2 RIL requests in the queue (1 pending, 1 handled, 0 unhandled)

D/RIL-IPC ( 1891): 

D/RIL-IPC ( 1891): xmm626_sec_modem_fmt_recv: Received FMT message

D/RIL-IPC ( 1891): xmm626_sec_modem_fmt_recv: Message: aseq=0xff, command=IPC_NET_REGIST, type=IPC_TYPE_NOTI, size=11

D/RIL-IPC ( 1891): ================================= IPC FMT data =================================

D/RIL-IPC ( 1891): [0000]   04 02 02 9B DD 07 FE 4E  EE 03 00                  .......N ...

D/RIL-IPC ( 1891): ================================================================================

D/RIL-IPC ( 1891): 

D/RIL-IPC ( 1891): xmm626_sec_modem_fmt_recv: Received FMT message

D/RIL-IPC ( 1891): xmm626_sec_modem_fmt_recv: Message: aseq=0xff, command=IPC_NET_REGIST, type=IPC_TYPE_NOTI, size=11

D/RIL-IPC ( 1891): ================================= IPC FMT data =================================

D/RIL-IPC ( 1891): [0000]   04 03 03 9B DD 07 FE 4E  EE 03 00                  .......N ...

D/RIL-IPC ( 1891): ================================================================================

D/RIL-IPC ( 1891): 

D/RIL-IPC ( 1891): xmm626_sec_modem_fmt_recv: Received FMT message

D/RIL-IPC ( 1891): xmm626_sec_modem_fmt_recv: Message: aseq=0x00, command=IPC_NET_SERVING_NETWORK, type=IPC_TYPE_NOTI, size=11

D/RIL-IPC ( 1891): ================================= IPC FMT data =================================

D/RIL-IPC ( 1891): [0000]   02 02 04 32 30 36 30 31  23 DD 07                  ...20601 #..

D/RIL-IPC ( 1891): ================================================================================

D/RILJ    ( 2563): [UNSL]< UNSOL_RESPONSE_VOICE_NETWORK_STATE_CHANGED

D/RIL-IPC ( 1891): 

D/RIL-IPC ( 1891): xmm626_sec_modem_fmt_recv: Received FMT message

D/RIL-IPC ( 1891): xmm626_sec_modem_fmt_recv: Message: aseq=0x5a, command=IPC_SEC_RSIM_ACCESS, type=IPC_TYPE_RESP, size=27

D/RIL-IPC ( 1891): ================================= IPC FMT data =================================

D/RIL-IPC ( 1891): [0000]   90 00 18 56 6F 69 63 65  6D 61 69 6C FF 07 91 23   ...Voice mail...#

D/RIL-IPC ( 1891): [0010]   74 15 15 69 F9 FF FF FF  FF FF FF                  t..i.... ...

D/RIL-IPC ( 1891): ================================================================================

D/RILJ    ( 2563): [UNSL]< UNSOL_RESPONSE_VOICE_NETWORK_STATE_CHANGED

D/RIL     ( 1891): 1 RIL request in the queue (0 pending, 0 handled, 1 unhandled)

D/RIL     ( 1891): 3 RIL requests data in the queue

D/RIL-IPC ( 1891): 

D/RIL-IPC ( 1891): xmm626_sec_modem_fmt_send: Sent FMT message

D/RIL-IPC ( 1891): xmm626_sec_modem_fmt_send: Message: mseq=0x5b, command=IPC_SEC_RSIM_ACCESS, type=IPC_TYPE_GET, size=6

D/RIL-IPC ( 1891): ================================= IPC FMT data =================================

D/RIL-IPC ( 1891): [0000]   C0 18 6F 00 00 0F                                  ..o...

D/RIL-IPC ( 1891): ================================================================================

D/RILJ    ( 2563): [0110]> OPERATOR

D/RILJ    ( 2563): [UNSL]< UNSOL_RESPONSE_VOICE_NETWORK_STATE_CHANGED

D/RIL     ( 1891): 2 RIL requests in the queue (1 pending, 1 handled, 0 unhandled)

D/RIL     ( 1891): 3 RIL requests data in the queue

D/RIL     ( 1891): 1 RIL request in the queue (0 pending, 1 handled, 0 unhandled)

D/RIL     ( 1891): 2 RIL requests data in the queue

D/RILJ    ( 2563): [0108]< SIM_IO IccIoResponse sw1:0x90 sw2:0x0

D/RILJ    ( 2563): [0111]> DATA_REGISTRATION_STATE

D/RILJ    ( 2563): [0110]< OPERATOR {Proximus, Proximus, 20601}

D/RIL     ( 1891): 2 RIL requests in the queue (1 pending, 1 handled, 0 unhandled)

D/RIL     ( 1891): 2 RIL requests data in the queue

D/RIL     ( 1891): 1 RIL request in the queue (0 pending, 1 handled, 0 unhandled)

D/RIL     ( 1891): 1 RIL request data in the queue

D/RILJ    ( 2563): [0112]> VOICE_REGISTRATION_STATE

D/RILJ    ( 2563): [0111]< DATA_REGISTRATION_STATE {2, 7dd, 3ee4efe, 9, 3}

D/RIL     ( 1891): 2 RIL requests in the queue (1 pending, 1 handled, 0 unhandled)

D/RIL     ( 1891): 1 RIL request data in the queue

D/RIL     ( 1891): 1 RIL request in the queue (0 pending, 1 handled, 0 unhandled)

D/RILJ    ( 2563): [0113]> QUERY_NETWORK_SELECTION_MODE

D/RILJ    ( 2563): [0112]< VOICE_REGISTRATION_STATE {1, 7dd, 3ee4efe, 9, null, null, null, null, null, null, null, null, null, null, null}

D/RIL     ( 1891): 2 RIL requests in the queue (1 pending, 1 handled, 0 unhandled)

D/RIL-IPC ( 1891): 

D/RIL-IPC ( 1891): xmm626_sec_modem_fmt_send: Sent FMT message

D/RIL-IPC ( 1891): xmm626_sec_modem_fmt_send: Message: mseq=0x5c, command=IPC_NET_PLMN_SEL, type=IPC_TYPE_GET, size=0

D/RILJ    ( 2563): [0114]> OPERATOR

D/RIL-IPC ( 1891): 

D/RIL-IPC ( 1891): xmm626_sec_modem_fmt_recv: Received FMT message

D/RIL-IPC ( 1891): xmm626_sec_modem_fmt_recv: Message: aseq=0x5c, command=IPC_NET_PLMN_SEL, type=IPC_TYPE_RESP, size=1

D/RIL-IPC ( 1891): ================================= IPC FMT data =================================

D/RIL-IPC ( 1891): [0000]   02                                                 .

D/RIL-IPC ( 1891): ================================================================================

D/RIL     ( 1891): 1 RIL request in the queue (0 pending, 1 handled, 0 unhandled)

D/RILJ    ( 2563): [0113]< QUERY_NETWORK_SELECTION_MODE {0}

D/RIL     ( 1891): 2 RIL requests in the queue (1 pending, 1 handled, 0 unhandled)

D/RIL-IPC ( 1891): 

D/RIL-IPC ( 1891): xmm626_sec_modem_fmt_send: Sent FMT message

D/RIL-IPC ( 1891): xmm626_sec_modem_fmt_send: Message: mseq=0x5d, command=IPC_NET_SERVING_NETWORK, type=IPC_TYPE_GET, size=0

D/RILJ    ( 2563): [0115]> DATA_REGISTRATION_STATE

D/RIL-IPC ( 1891): 

D/RIL-IPC ( 1891): xmm626_sec_modem_fmt_recv: Received FMT message

D/RIL-IPC ( 1891): xmm626_sec_modem_fmt_recv: Message: aseq=0x5d, command=IPC_NET_SERVING_NETWORK, type=IPC_TYPE_RESP, size=11

D/RIL-IPC ( 1891): ================================= IPC FMT data =================================

D/RIL-IPC ( 1891): [0000]   02 02 04 32 30 36 30 31  23 DD 07                  ...20601 #..

D/RIL-IPC ( 1891): ================================================================================

D/RIL     ( 1891): 1 RIL request in the queue (0 pending, 1 handled, 0 unhandled)

D/RILJ    ( 2563): [0114]< OPERATOR {Proximus, Proximus, 20601}

D/RIL     ( 1891): 2 RIL requests in the queue (1 pending, 1 handled, 0 unhandled)

D/RIL-IPC ( 1891): 

D/RIL-IPC ( 1891): xmm626_sec_modem_fmt_send: Sent FMT message

D/RIL-IPC ( 1891): xmm626_sec_modem_fmt_send: Message: mseq=0x5e, command=IPC_NET_REGIST, type=IPC_TYPE_GET, size=2

D/RIL-IPC ( 1891): ================================= IPC FMT data =================================

D/RIL-IPC ( 1891): [0000]   FF 03                                              ..

D/RIL-IPC ( 1891): ================================================================================

D/RILJ    ( 2563): [0116]> VOICE_REGISTRATION_STATE

D/RIL     ( 1891): 3 RIL requests in the queue (1 pending, 2 handled, 0 unhandled)

D/RIL-IPC ( 1891): 

D/RIL-IPC ( 1891): xmm626_sec_modem_fmt_send: Sent FMT message

D/RIL-IPC ( 1891): xmm626_sec_modem_fmt_send: Message: mseq=0x5f, command=IPC_NET_REGIST, type=IPC_TYPE_GET, size=2

D/RIL-IPC ( 1891): ================================= IPC FMT data =================================

D/RIL-IPC ( 1891): [0000]   FF 02                                              ..

D/RIL-IPC ( 1891): ================================================================================

D/RILJ    ( 2563): [0117]> QUERY_NETWORK_SELECTION_MODE

D/RIL-IPC ( 1891): 

D/RIL-IPC ( 1891): xmm626_sec_modem_fmt_recv: Received FMT message

D/RIL-IPC ( 1891): xmm626_sec_modem_fmt_recv: Message: aseq=0x5e, command=IPC_NET_REGIST, type=IPC_TYPE_RESP, size=11

D/RIL-IPC ( 1891): ================================= IPC FMT data =================================

D/RIL-IPC ( 1891): [0000]   04 03 03 9B DD 07 FE 4E  EE 03 00                  .......N ...

D/RIL-IPC ( 1891): ================================================================================

D/RIL     ( 1891): 2 RIL requests in the queue (0 pending, 2 handled, 0 unhandled)

D/RIL-IPC ( 1891): 

D/RIL-IPC ( 1891): xmm626_sec_modem_fmt_recv: Received FMT message

D/RIL-IPC ( 1891): xmm626_sec_modem_fmt_recv: Message: aseq=0x5f, command=IPC_NET_REGIST, type=IPC_TYPE_RESP, size=11

D/RIL-IPC ( 1891): ================================= IPC FMT data =================================

D/RIL-IPC ( 1891): [0000]   04 02 02 9B DD 07 FE 4E  EE 03 00                  .......N ...

D/RIL-IPC ( 1891): ================================================================================

D/RIL     ( 1891): 1 RIL request in the queue (0 pending, 1 handled, 0 unhandled)

D/RIL     ( 1891): 2 RIL requests in the queue (1 pending, 1 handled, 0 unhandled)

D/RIL-IPC ( 1891): 

D/RIL-IPC ( 1891): xmm626_sec_modem_fmt_send: Sent FMT message

D/RIL-IPC ( 1891): xmm626_sec_modem_fmt_send: Message: mseq=0x60, command=IPC_NET_PLMN_SEL, type=IPC_TYPE_GET, size=0

D/RILJ    ( 2563): [0118]> OPERATOR

D/RIL     ( 1891): 3 RIL requests in the queue (1 pending, 2 handled, 0 unhandled)

D/RIL-IPC ( 1891): 

D/RIL-IPC ( 1891): xmm626_sec_modem_fmt_send: Sent FMT message

D/RIL-IPC ( 1891): xmm626_sec_modem_fmt_send: Message: mseq=0x61, command=IPC_NET_SERVING_NETWORK, type=IPC_TYPE_GET, size=0

D/RILJ    ( 2563): [0115]< DATA_REGISTRATION_STATE {2, 7dd, 3ee4efe, 9, 3}

D/RILJ    ( 2563): [0119]> DATA_REGISTRATION_STATE

D/RILJ    ( 2563): [0116]< VOICE_REGISTRATION_STATE {1, 7dd, 3ee4efe, 9, null, null, null, null, null, null, null, null, null, null, null}

D/RIL-IPC ( 1891): 

D/RIL-IPC ( 1891): xmm626_sec_modem_fmt_recv: Received FMT message

D/RIL-IPC ( 1891): xmm626_sec_modem_fmt_recv: Message: aseq=0x60, command=IPC_NET_PLMN_SEL, type=IPC_TYPE_RESP, size=1

D/RIL-IPC ( 1891): ================================= IPC FMT data =================================

D/RIL-IPC ( 1891): [0000]   02                                                 .

D/RIL-IPC ( 1891): ================================================================================

D/RIL     ( 1891): 2 RIL requests in the queue (0 pending, 2 handled, 0 unhandled)

D/RILJ    ( 2563): [0117]< QUERY_NETWORK_SELECTION_MODE {0}

D/RIL-IPC ( 1891): 

D/RIL-IPC ( 1891): xmm626_sec_modem_fmt_recv: Received FMT message

D/RIL-IPC ( 1891): xmm626_sec_modem_fmt_recv: Message: aseq=0x61, command=IPC_NET_SERVING_NETWORK, type=IPC_TYPE_RESP, size=11

D/RIL-IPC ( 1891): ================================= IPC FMT data =================================

D/RIL-IPC ( 1891): [0000]   02 02 04 32 30 36 30 31  23 DD 07                  ...20601 #..

D/RIL-IPC ( 1891): ================================================================================

D/RIL     ( 1891): 1 RIL request in the queue (0 pending, 1 handled, 0 unhandled)

D/RIL     ( 1891): 2 RIL requests in the queue (1 pending, 1 handled, 0 unhandled)

D/RIL-IPC ( 1891): 

D/RIL-IPC ( 1891): xmm626_sec_modem_fmt_send: Sent FMT message

D/RIL-IPC ( 1891): xmm626_sec_modem_fmt_send: Message: mseq=0x62, command=IPC_NET_REGIST, type=IPC_TYPE_GET, size=2

D/RIL-IPC ( 1891): ================================= IPC FMT data =================================

D/RIL-IPC ( 1891): [0000]   FF 03                                              ..

D/RIL-IPC ( 1891): ================================================================================

D/RILJ    ( 2563): [0120]> VOICE_REGISTRATION_STATE

D/RILJ    ( 2563): [0118]< OPERATOR {Proximus, Proximus, 20601}

D/RIL     ( 1891): 3 RIL requests in the queue (1 pending, 2 handled, 0 unhandled)

D/RIL-IPC ( 1891): 

D/RIL-IPC ( 1891): xmm626_sec_modem_fmt_send: Sent FMT message

D/RIL-IPC ( 1891): xmm626_sec_modem_fmt_send: Message: mseq=0x63, command=IPC_NET_REGIST, type=IPC_TYPE_GET, size=2

D/RIL-IPC ( 1891): ================================= IPC FMT data =================================

D/RIL-IPC ( 1891): [0000]   FF 02                                              ..

D/RIL-IPC ( 1891): ================================================================================

D/RIL-IPC ( 1891): 

D/RIL-IPC ( 1891): xmm626_sec_modem_fmt_recv: Received FMT message

D/RIL-IPC ( 1891): xmm626_sec_modem_fmt_recv: Message: aseq=0x62, command=IPC_NET_REGIST, type=IPC_TYPE_RESP, size=11

D/RIL-IPC ( 1891): ================================= IPC FMT data =================================

D/RIL-IPC ( 1891): [0000]   04 03 03 9B DD 07 FE 4E  EE 03 00                  .......N ...

D/RIL-IPC ( 1891): ================================================================================

D/RIL     ( 1891): 2 RIL requests in the queue (0 pending, 2 handled, 0 unhandled)

D/RILJ    ( 2563): [0121]> QUERY_NETWORK_SELECTION_MODE

D/RILJ    ( 2563): [0119]< DATA_REGISTRATION_STATE {2, 7dd, 3ee4efe, 9, 3}

D/RIL     ( 1891): 3 RIL requests in the queue (1 pending, 2 handled, 0 unhandled)

D/RIL-IPC ( 1891): 

D/RIL-IPC ( 1891): xmm626_sec_modem_fmt_send: Sent FMT message

D/RIL-IPC ( 1891): xmm626_sec_modem_fmt_send: Message: mseq=0x64, command=IPC_NET_PLMN_SEL, type=IPC_TYPE_GET, size=0

D/RIL-IPC ( 1891): 

D/RIL-IPC ( 1891): xmm626_sec_modem_fmt_recv: Received FMT message

D/RIL-IPC ( 1891): xmm626_sec_modem_fmt_recv: Message: aseq=0x63, command=IPC_NET_REGIST, type=IPC_TYPE_RESP, size=11

D/RIL-IPC ( 1891): ================================= IPC FMT data =================================

D/RIL-IPC ( 1891): [0000]   04 02 02 9B DD 07 FE 4E  EE 03 00                  .......N ...

D/RIL-IPC ( 1891): ================================================================================

D/RIL     ( 1891): 2 RIL requests in the queue (0 pending, 2 handled, 0 unhandled)

D/RILJ    ( 2563): [0120]< VOICE_REGISTRATION_STATE {1, 7dd, 3ee4efe, 9, null, null, null, null, null, null, null, null, null, null, null}

D/RIL-IPC ( 1891): 

D/RIL-IPC ( 1891): xmm626_sec_modem_fmt_recv: Received FMT message

D/RIL-IPC ( 1891): xmm626_sec_modem_fmt_recv: Message: aseq=0x64, command=IPC_NET_PLMN_SEL, type=IPC_TYPE_RESP, size=1

D/RIL-IPC ( 1891): ================================= IPC FMT data =================================

D/RIL-IPC ( 1891): [0000]   02                                                 .

D/RIL-IPC ( 1891): ================================================================================

D/RIL     ( 1891): 1 RIL request in the queue (0 pending, 1 handled, 0 unhandled)

D/RILJ    ( 2563): [0121]< QUERY_NETWORK_SELECTION_MODE {0}

D/GSM     ( 2563): [SIMRecords] VM: ADN Record 'Voicemail' '+32475151969 null' EF[MBDN]

D/GSM     ( 2563): [SIMRecords] onRecordLoaded 1 requested: true

D/GSM     ( 2563): [GsmSST] Poll ServiceState done:  oldSS=[1 home Mobistar Mobistar 20610  HSDPA CSS not supported -1 -1 RoamInd=-1 DefRoamInd=-1 EmergOnly=true] newSS=[0 home Proximus Proximus 20601  HSDPA CSS not supported -1 -1 RoamInd=-1 DefRoamInd=-1 EmergOnly=false] oldGprs=1 newData=1 oldMaxDataCalls=1 mNewMaxDataCalls=1 oldReasonDataDenied=-1 mNewReasonDataDenied=-1 oldType=HSDPA newType=HSDPA

D/GSM     ( 2563): [GsmSST] pollStateDone: registering current mNitzUpdatedTime=false changing to false

D/GSM     ( 2563): [GsmSST] updateSpnDisplay: changed sending intent rule=2 showPlmn='true' plmn='Proximus' showSpn='false' spn='null'

D/GSM     ( 2563): [GsmSST] pollStateDone: no nitz but one TZ for iso-cc=be with zone.getID=Europe/Brussels testOneUniqueOffsetPath=false

D/GSM     ( 2563): [GsmSST] setAndBroadcastNetworkSetTimeZone: setTimeZone=Europe/Brussels

D/GSM     ( 2563): [GsmSST] setAndBroadcastNetworkSetTimeZone: call alarm.setTimeZone and broadcast zoneId=Europe/Brussels

D/GSM     ( 2563): [GsmSST] shouldFixTimeZoneNow: retVal=false iccCardExist=true operatorNumeric=20601 mcc=206 prevOperatorNumeric=20610 prevMcc=206 needToFixTimeZone=false ltod=06-01 18:27:45.966

D/GSM     ( 2563): [SimSmsInterfaceManager] enableCellBroadcastRange

D/GSM     ( 2563): [SimSmsInterfaceManager] Calling setGsmBroadcastConfig with 1 configurations

D/RILJ    ( 2563): [0122]> RIL_REQUEST_GSM_SET_BROADCAST_CONFIG with 1 configs : 

D/RILJ    ( 2563): SmsBroadcastConfigInfo: Id [4352,6399] Code [0,255] ENABLED

D/RIL     ( 1891): Detected string with a size of 15 bytes

D/RIL     ( 1891): 2 RIL requests in the queue (1 pending, 1 handled, 0 unhandled)

D/RIL     ( 1891): Unhandled RIL request: 90

D/RIL     ( 1891): 1 RIL request in the queue (0 pending, 1 handled, 0 unhandled)

D/RILJ    ( 2563): [0122]< RIL_REQUEST_GSM_SET_BROADCAST_CONFIG error: com.android.internal.telephony.CommandException: REQUEST_NOT_SUPPORTED

D/GSM     ( 2563): [SimSmsInterfaceManager] Failed to add cell broadcast subscription for MID range 4352 to 6399 from client com.android.cellbroadcastreceiver

D/GSM     ( 2563): [SimSmsInterfaceManager] disableCellBroadcastRange

D/GSM     ( 2563): [SimSmsInterfaceManager] Failed to remove cell broadcast subscription for MID range 50 to 50 from client com.android.cellbroadcastreceiver

D/RIL-IPC ( 1891): 

D/RIL-IPC ( 1891): xmm626_sec_modem_fmt_recv: Received FMT message

D/RIL-IPC ( 1891): xmm626_sec_modem_fmt_recv: Message: aseq=0x5b, command=IPC_SEC_RSIM_ACCESS, type=IPC_TYPE_RESP, size=3

D/RIL-IPC ( 1891): ================================= IPC FMT data =================================

D/RIL-IPC ( 1891): [0000]   6A 82 00                                           j..

D/RIL-IPC ( 1891): ================================================================================

D/RIL     ( 1891): 0 RIL request in the queue (0 pending, 0 handled, 0 unhandled)

D/RILJ    ( 2563): [0109]< SIM_IO IccIoResponse sw1:0x6a sw2:0x82

D/GSM     ( 2563): [SIMRecords] No SPN loaded in either CHPS or 3GPP

D/GSM     ( 2563): [SIMRecords] onRecordLoaded 0 requested: true

D/GSM     ( 2563): [SIMRecords] SIMRecords: onAllRecordsLoaded set 'gsm.sim.operator.numeric' to operator='20601'

D/RIL-IPC ( 1891): 

D/RIL-IPC ( 1891): xmm626_sec_modem_fmt_recv: Received FMT message

D/RIL-IPC ( 1891): xmm626_sec_modem_fmt_recv: Message: aseq=0x5b, command=IPC_DISP_RSSI_INFO, type=IPC_TYPE_NOTI, size=1

D/RIL-IPC ( 1891): ================================= IPC FMT data =================================

D/RIL-IPC ( 1891): [0000]   54                                                 T

D/RIL-IPC ( 1891): ================================================================================

D/RIL     ( 1891): Signal strength is 14

D/GSM     ( 2563): [GsmDCT] handleMessage msg={ what=270338 when=-815ms obj=android.os.AsyncResult@418574d0 }

D/GSM     ( 2563): [GsmDCT] onRecordsLoaded: createAllApnList

D/GSM     ( 2563): [GsmDCT] createAllApnList: selection=numeric = '20601' and carrier_enabled = 1

D/GSM     ( 2563): [GsmDCT] createApnList: X result=[[ApnSettingV2] Proximus MMS, 28, 20601, event.proximus.be, null, http://mmsc.proximus.be/mms, 10.55.14.75, 8080, null, -1, mms, IP, IP, true, 0, [ApnSettingV2] Proximus Internet, 29, 20601, internet.proximus.be, null, null, null, null, null, -1, default | supl, IP, IP, true, 0]

D/GSM     ( 2563): [GsmDCT] getPreferredApn: X not found

D/GSM     ( 2563): [GsmDCT] createAllApnList: mPreferredApn=null

D/GSM     ( 2563): [GsmDCT] createAllApnList: X mAllApns=[[ApnSettingV2] Proximus MMS, 28, 20601, event.proximus.be, null, http://mmsc.proximus.be/mms, 10.55.14.75, 8080, null, -1, mms, IP, IP, true, 0, [ApnSettingV2] Proximus Internet, 29, 20601, internet.proximus.be, null, null, null, null, null, -1, default | supl, IP, IP, true, 0]

D/GSM     ( 2563): [GsmDCT] onRecordsLoaded: notifying data availability

D/GSM     ( 2563): [GsmDCT] notifyOffApnOfAvailability type:dun

D/GSM     ( 2563): [GsmDCT] isDataAllowed: not allowed due to - gprs= 1

D/GSM     ( 2563): [GsmDCT] isDataPossible(dun): possible=false isDataAllowed=false apnTypePossible=true apnContextisEnabled=false apnContextState()=IDLE

D/GSM     ( 2563): [GsmDCT] get active apn string for type:dun

D/GSM     ( 2563): [GsmDCT] notifyOffApnOfAvailability type:supl

D/GSM     ( 2563): [GsmDCT] isDataAllowed: not allowed due to - gprs= 1

D/GSM     ( 2563): [GsmDCT] isDataPossible(supl): possible=false isDataAllowed=false apnTypePossible=true apnContextisEnabled=false apnContextState()=IDLE

D/GSM     ( 2563): [GsmDCT] get active apn string for type:supl

D/GSM     ( 2563): [GsmDCT] notifyOffApnOfAvailability type:hipri

D/GSM     ( 2563): [GsmDCT] isDataAllowed: not allowed due to - gprs= 1

D/GSM     ( 2563): [GsmDCT] isDataPossible(hipri): possible=false isDataAllowed=false apnTypePossible=true apnContextisEnabled=false apnContextState()=IDLE

D/GSM     ( 2563): [GsmDCT] get active apn string for type:hipri

D/GSM     ( 2563): [GsmDCT] notifyOffApnsOfAvailability skipped apn due to isReady==false: {mApnType=default mState=IDLE mWaitingApns=null mWaitingApnsPermanentFailureCountDown=0 mApnSetting=null mDataConnectionAc=null mReason=radioTurnedOff mRetryCount=0 mDataEnabled=true mDependencyMet=true}

D/GSM     ( 2563): [GsmDCT] notifyOffApnOfAvailability type:mms

D/GSM     ( 2563): [GsmDCT] isDataAllowed: not allowed due to - gprs= 1

D/GSM     ( 2563): [GsmDCT] isDataPossible(mms): possible=false isDataAllowed=false apnTypePossible=true apnContextisEnabled=false apnContextState()=IDLE

D/GSM     ( 2563): [GsmDCT] get active apn string for type:mms

D/GSM     ( 2563): [ApnContext:dun] setRetryCount: 0

D/GSM     ( 2563): [ApnContext:supl] setRetryCount: 0

D/GSM     ( 2563): [ApnContext:hipri] setRetryCount: 0

D/GSM     ( 2563): [ApnContext:default] setRetryCount: 0

D/GSM     ( 2563): [ApnContext:mms] setRetryCount: 0

D/GSM     ( 2563): [ApnContext:default] set reason as simLoaded,current state IDLE

D/GSM     ( 2563): [GsmDCT] trySetupData for type:default due to simLoaded

D/GSM     ( 2563): [GsmDCT] trySetupData with mIsPsRestricted=false

D/GSM     ( 2563): [GsmDCT] isDataAllowed: not allowed due to - gprs= 1

D/GSM     ( 2563): [GsmDCT] notifyOffApnOfAvailability type:dun

D/GSM     ( 2563): [GsmDCT] isDataAllowed: not allowed due to - gprs= 1

D/GSM     ( 2563): [GsmDCT] isDataPossible(dun): possible=false isDataAllowed=false apnTypePossible=true apnContextisEnabled=false apnContextState()=IDLE

D/GSM     ( 2563): [GsmDCT] get active apn string for type:dun

D/GSM     ( 2563): [GsmDCT] notifyOffApnOfAvailability type:supl

D/GSM     ( 2563): [GsmDCT] isDataAllowed: not allowed due to - gprs= 1

D/GSM     ( 2563): [GsmDCT] isDataPossible(supl): possible=false isDataAllowed=false apnTypePossible=true apnContextisEnabled=false apnContextState()=IDLE

D/GSM     ( 2563): [GsmDCT] get active apn string for type:supl

D/GSM     ( 2563): [GsmDCT] notifyOffApnOfAvailability type:hipri

D/GSM     ( 2563): [GsmDCT] isDataAllowed: not allowed due to - gprs= 1

D/GSM     ( 2563): [GsmDCT] isDataPossible(hipri): possible=false isDataAllowed=false apnTypePossible=true apnContextisEnabled=false apnContextState()=IDLE

D/GSM     ( 2563): [GsmDCT] get active apn string for type:hipri

D/GSM     ( 2563): [GsmDCT] notifyOffApnsOfAvailability skipped apn due to isReady==false: {mApnType=default mState=IDLE mWaitingApns=null mWaitingApnsPermanentFailureCountDown=0 mApnSetting=null mDataConnectionAc=null mReason=simLoaded mRetryCount=0 mDataEnabled=true mDependencyMet=true}

D/GSM     ( 2563): [GsmDCT] notifyOffApnOfAvailability type:mms

D/GSM     ( 2563): [GsmDCT] isDataAllowed: not allowed due to - gprs= 1

D/GSM     ( 2563): [GsmDCT] isDataPossible(mms): possible=false isDataAllowed=false apnTypePossible=true apnContextisEnabled=false apnContextState()=IDLE

D/GSM     ( 2563): [GsmDCT] get active apn string for type:mms

D/RIL_IccCardProxy( 2563): Broadcasting intent ACTION_SIM_STATE_CHANGED LOADED reason null

D/RIL-IPC ( 1891): 

D/RIL-IPC ( 1891): xmm626_sec_modem_fmt_recv: Received FMT message

D/RIL-IPC ( 1891): xmm626_sec_modem_fmt_recv: Message: aseq=0xff, command=IPC_NET_REGIST, type=IPC_TYPE_NOTI, size=11

D/RIL-IPC ( 1891): ================================= IPC FMT data =================================

D/RIL-IPC ( 1891): [0000]   04 02 02 9B DD 07 FE 4E  EE 03 00                  .......N ...

D/RIL-IPC ( 1891): ================================================================================

D/RIL-IPC ( 1891): 

D/RIL-IPC ( 1891): xmm626_sec_modem_fmt_recv: Received FMT message

D/RIL-IPC ( 1891): xmm626_sec_modem_fmt_recv: Message: aseq=0xff, command=IPC_NET_REGIST, type=IPC_TYPE_NOTI, size=11

D/RIL-IPC ( 1891): ================================= IPC FMT data =================================

D/RIL-IPC ( 1891): [0000]   04 03 03 9B DD 07 FE 4E  EE 03 00                  .......N ...

D/RIL-IPC ( 1891): ================================================================================

D/RIL-IPC ( 1891): 

D/RIL-IPC ( 1891): xmm626_sec_modem_fmt_recv: Received FMT message

D/RILJ    ( 2563): [UNSL]< UNSOL_RESPONSE_VOICE_NETWORK_STATE_CHANGED

D/RIL-IPC ( 1891): xmm626_sec_modem_fmt_recv: Message: aseq=0x00, command=IPC_NET_SERVING_NETWORK, type=IPC_TYPE_NOTI, size=11

D/RIL-IPC ( 1891): ================================= IPC FMT data =================================

D/RIL-IPC ( 1891): [0000]   02 02 04 32 30 36 30 31  23 DD 07                  ...20601 #..

D/RIL-IPC ( 1891): ================================================================================

D/RILJ    ( 2563): [UNSL]< UNSOL_RESPONSE_VOICE_NETWORK_STATE_CHANGED

D/RILJ    ( 2563): [UNSL]< UNSOL_RESPONSE_VOICE_NETWORK_STATE_CHANGED

D/RILJ    ( 2563): [0123]> OPERATOR

D/RILJ    ( 2563): [0124]> DATA_REGISTRATION_STATE

D/RIL     ( 1891): 1 RIL request in the queue (1 pending, 0 handled, 0 unhandled)

D/RIL     ( 1891): 3 RIL requests data in the queue

D/RIL     ( 1891): 0 RIL request in the queue (0 pending, 0 handled, 0 unhandled)

D/RIL     ( 1891): 2 RIL requests data in the queue

D/RILJ    ( 2563): [0123]< OPERATOR {Proximus, Proximus, 20601}

D/RIL     ( 1891): 1 RIL request in the queue (1 pending, 0 handled, 0 unhandled)

D/RIL     ( 1891): 2 RIL requests data in the queue

D/RIL     ( 1891): 0 RIL request in the queue (0 pending, 0 handled, 0 unhandled)

D/RIL     ( 1891): 1 RIL request data in the queue

D/RILJ    ( 2563): [0125]> VOICE_REGISTRATION_STATE

D/RIL     ( 1891): 1 RIL request in the queue (1 pending, 0 handled, 0 unhandled)

D/RILJ    ( 2563): [0124]< DATA_REGISTRATION_STATE {2, 7dd, 3ee4efe, 9, 3}

D/RIL     ( 1891): 1 RIL request data in the queue

D/RIL     ( 1891): 0 RIL request in the queue (0 pending, 0 handled, 0 unhandled)

D/RILJ    ( 2563): [0126]> QUERY_NETWORK_SELECTION_MODE

D/RILJ    ( 2563): [0127]> OPERATOR

D/RIL     ( 1891): 1 RIL request in the queue (1 pending, 0 handled, 0 unhandled)

D/RIL-IPC ( 1891): 

D/RIL-IPC ( 1891): xmm626_sec_modem_fmt_send: Sent FMT message

D/RIL-IPC ( 1891): xmm626_sec_modem_fmt_send: Message: mseq=0x65, command=IPC_NET_PLMN_SEL, type=IPC_TYPE_GET, size=0

D/RILJ    ( 2563): [0125]< VOICE_REGISTRATION_STATE {1, 7dd, 3ee4efe, 9, null, null, null, null, null, null, null, null, null, null, null}

D/RIL     ( 1891): 2 RIL requests in the queue (1 pending, 1 handled, 0 unhandled)

D/RIL-IPC ( 1891): 

D/RIL-IPC ( 1891): xmm626_sec_modem_fmt_send: Sent FMT message

D/RIL-IPC ( 1891): xmm626_sec_modem_fmt_send: Message: mseq=0x66, command=IPC_NET_SERVING_NETWORK, type=IPC_TYPE_GET, size=0

D/RILJ    ( 2563): [0128]> DATA_REGISTRATION_STATE

D/RIL-IPC ( 1891): 

D/RIL-IPC ( 1891): xmm626_sec_modem_fmt_recv: Received FMT message

D/RIL-IPC ( 1891): xmm626_sec_modem_fmt_recv: Message: aseq=0x65, command=IPC_NET_PLMN_SEL, type=IPC_TYPE_RESP, size=1

D/RIL-IPC ( 1891): ================================= IPC FMT data =================================

D/RIL-IPC ( 1891): [0000]   02                                                 .

D/RIL-IPC ( 1891): ================================================================================

D/RIL     ( 1891): 1 RIL request in the queue (0 pending, 1 handled, 0 unhandled)

D/RIL-IPC ( 1891): 

D/RIL-IPC ( 1891): xmm626_sec_modem_fmt_recv: Received FMT message

D/RIL-IPC ( 1891): xmm626_sec_modem_fmt_recv: Message: aseq=0x66, command=IPC_NET_SERVING_NETWORK, type=IPC_TYPE_RESP, size=11

D/RIL-IPC ( 1891): ================================= IPC FMT data =================================

D/RIL-IPC ( 1891): [0000]   02 02 04 32 30 36 30 31  23 DD 07                  ...20601 #..

D/RIL-IPC ( 1891): ================================================================================

D/RIL     ( 1891): 0 RIL request in the queue (0 pending, 0 handled, 0 unhandled)

D/RIL     ( 1891): 1 RIL request in the queue (1 pending, 0 handled, 0 unhandled)

D/RIL-IPC ( 1891): 

D/RIL-IPC ( 1891): xmm626_sec_modem_fmt_send: Sent FMT message

D/RIL-IPC ( 1891): xmm626_sec_modem_fmt_send: Message: mseq=0x67, command=IPC_NET_REGIST, type=IPC_TYPE_GET, size=2

D/RIL-IPC ( 1891): ================================= IPC FMT data =================================

D/RILJ    ( 2563): [0129]> VOICE_REGISTRATION_STATE

D/RIL-IPC ( 1891): [0000]   FF 03                                              ..

D/RIL-IPC ( 1891): ================================================================================

D/RILJ    ( 2563): [0126]< QUERY_NETWORK_SELECTION_MODE {0}

D/RIL-IPC ( 1891): 

D/RIL-IPC ( 1891): xmm626_sec_modem_fmt_recv: Received FMT message

D/RIL-IPC ( 1891): xmm626_sec_modem_fmt_recv: Message: aseq=0x67, command=IPC_NET_REGIST, type=IPC_TYPE_RESP, size=11

D/RIL-IPC ( 1891): ================================= IPC FMT data =================================

D/RIL-IPC ( 1891): [0000]   04 03 03 9B DD 07 FE 4E  EE 03 00                  .......N ...

D/RIL-IPC ( 1891): ================================================================================

D/RIL     ( 1891): 0 RIL request in the queue (0 pending, 0 handled, 0 unhandled)

D/RILJ    ( 2563): [0130]> QUERY_NETWORK_SELECTION_MODE

D/RIL     ( 1891): 1 RIL request in the queue (1 pending, 0 handled, 0 unhandled)

D/RIL-IPC ( 1891): 

D/RIL-IPC ( 1891): xmm626_sec_modem_fmt_send: Sent FMT message

D/RIL-IPC ( 1891): xmm626_sec_modem_fmt_send: Message: mseq=0x68, command=IPC_NET_REGIST, type=IPC_TYPE_GET, size=2

D/RIL-IPC ( 1891): ================================= IPC FMT data =================================

D/RIL-IPC ( 1891): [0000]   FF 02                                              ..

D/RIL-IPC ( 1891): ================================================================================

D/RILJ    ( 2563): [0131]> OPERATOR

D/RIL-IPC ( 1891): 

D/RIL-IPC ( 1891): xmm626_sec_modem_fmt_recv: Received FMT message

D/RIL-IPC ( 1891): xmm626_sec_modem_fmt_recv: Message: aseq=0x68, command=IPC_NET_REGIST, type=IPC_TYPE_RESP, size=11

D/RIL-IPC ( 1891): ================================= IPC FMT data =================================

D/RIL-IPC ( 1891): [0000]   04 02 02 9B DD 07 FE 4E  EE 03 00                  .......N ...

D/RIL-IPC ( 1891): ================================================================================

D/RIL     ( 1891): 0 RIL request in the queue (0 pending, 0 handled, 0 unhandled)

D/RIL     ( 1891): 1 RIL request in the queue (1 pending, 0 handled, 0 unhandled)

D/RILJ    ( 2563): [0127]< OPERATOR {Proximus, Proximus, 20601}

D/RIL-IPC ( 1891): 

D/RIL-IPC ( 1891): xmm626_sec_modem_fmt_send: Sent FMT message

D/RIL-IPC ( 1891): xmm626_sec_modem_fmt_send: Message: mseq=0x69, command=IPC_NET_PLMN_SEL, type=IPC_TYPE_GET, size=0

D/RILJ    ( 2563): [0128]< DATA_REGISTRATION_STATE {2, 7dd, 3ee4efe, 9, 3}

D/RILJ    ( 2563): [0129]< VOICE_REGISTRATION_STATE {1, 7dd, 3ee4efe, 9, null, null, null, null, null, null, null, null, null, null, null}

D/RILJ    ( 2563): [0132]> DATA_REGISTRATION_STATE

D/RIL-IPC ( 1891): 

D/RIL-IPC ( 1891): xmm626_sec_modem_fmt_recv: Received FMT message

D/RIL-IPC ( 1891): xmm626_sec_modem_fmt_recv: Message: aseq=0x69, command=IPC_NET_PLMN_SEL, type=IPC_TYPE_RESP, size=1

D/RIL-IPC ( 1891): ================================= IPC FMT data =================================

D/RIL-IPC ( 1891): [0000]   02                                                 .

D/RIL-IPC ( 1891): ================================================================================

D/RIL     ( 1891): 0 RIL request in the queue (0 pending, 0 handled, 0 unhandled)

D/RIL     ( 1891): 1 RIL request in the queue (1 pending, 0 handled, 0 unhandled)

D/RIL-IPC ( 1891): 

D/RIL-IPC ( 1891): xmm626_sec_modem_fmt_send: Sent FMT message

D/RIL-IPC ( 1891): xmm626_sec_modem_fmt_send: Message: mseq=0x6a, command=IPC_NET_SERVING_NETWORK, type=IPC_TYPE_GET, size=0

D/RILJ    ( 2563): [0130]< QUERY_NETWORK_SELECTION_MODE {0}

D/RILJ    ( 2563): [0133]> VOICE_REGISTRATION_STATE

D/RIL-IPC ( 1891): 

D/RIL-IPC ( 1891): xmm626_sec_modem_fmt_recv: Received FMT message

D/RIL-IPC ( 1891): xmm626_sec_modem_fmt_recv: Message: aseq=0x6a, command=IPC_NET_SERVING_NETWORK, type=IPC_TYPE_RESP, size=11

D/RIL-IPC ( 1891): ================================= IPC FMT data =================================

D/RIL-IPC ( 1891): [0000]   02 02 04 32 30 36 30 31  23 DD 07                  ...20601 #..

D/RIL-IPC ( 1891): ================================================================================

D/RIL     ( 1891): 0 RIL request in the queue (0 pending, 0 handled, 0 unhandled)

D/RIL     ( 1891): 1 RIL request in the queue (1 pending, 0 handled, 0 unhandled)

D/RIL-IPC ( 1891): 

D/RIL-IPC ( 1891): xmm626_sec_modem_fmt_send: Sent FMT message

D/RIL-IPC ( 1891): xmm626_sec_modem_fmt_send: Message: mseq=0x6b, command=IPC_NET_REGIST, type=IPC_TYPE_GET, size=2

D/RIL-IPC ( 1891): ================================= IPC FMT data =================================

D/RIL-IPC ( 1891): [0000]   FF 03                                              ..

D/RIL-IPC ( 1891): ================================================================================

D/RILJ    ( 2563): [0131]< OPERATOR {Proximus, Proximus, 20601}

D/RIL-IPC ( 1891): 

D/RIL-IPC ( 1891): xmm626_sec_modem_fmt_recv: Received FMT message

D/RIL-IPC ( 1891): xmm626_sec_modem_fmt_recv: Message: aseq=0x6b, command=IPC_NET_REGIST, type=IPC_TYPE_RESP, size=11

D/RILJ    ( 2563): [0134]> QUERY_NETWORK_SELECTION_MODE

D/RIL-IPC ( 1891): ================================= IPC FMT data =================================

D/RIL-IPC ( 1891): [0000]   04 03 03 9B DD 07 FE 4E  EE 03 00                  .......N ...

D/RIL-IPC ( 1891): ================================================================================

D/RIL     ( 1891): 0 RIL request in the queue (0 pending, 0 handled, 0 unhandled)

D/RILJ    ( 2563): [0132]< DATA_REGISTRATION_STATE {2, 7dd, 3ee4efe, 9, 3}

D/RIL     ( 1891): 1 RIL request in the queue (1 pending, 0 handled, 0 unhandled)

D/RIL-IPC ( 1891): 

D/RIL-IPC ( 1891): xmm626_sec_modem_fmt_send: Sent FMT message

D/RIL-IPC ( 1891): xmm626_sec_modem_fmt_send: Message: mseq=0x6c, command=IPC_NET_REGIST, type=IPC_TYPE_GET, size=2

D/RIL-IPC ( 1891): ================================= IPC FMT data =================================

D/RIL-IPC ( 1891): [0000]   FF 02                                              ..

D/RIL-IPC ( 1891): ================================================================================

D/RIL     ( 1891): 2 RIL requests in the queue (1 pending, 1 handled, 0 unhandled)

D/RIL-IPC ( 1891): 

D/RIL-IPC ( 1891): xmm626_sec_modem_fmt_send: Sent FMT message

D/RIL-IPC ( 1891): xmm626_sec_modem_fmt_send: Message: mseq=0x6d, command=IPC_NET_PLMN_SEL, type=IPC_TYPE_GET, size=0

D/RIL-IPC ( 1891): 

D/RIL-IPC ( 1891): xmm626_sec_modem_fmt_recv: Received FMT message

D/RIL-IPC ( 1891): xmm626_sec_modem_fmt_recv: Message: aseq=0x6c, command=IPC_NET_REGIST, type=IPC_TYPE_RESP, size=11

D/RIL-IPC ( 1891): ================================= IPC FMT data =================================

D/RIL-IPC ( 1891): [0000]   04 02 02 9B DD 07 FE 4E  EE 03 00                  .......N ...

D/RIL-IPC ( 1891): ================================================================================

D/RIL     ( 1891): 1 RIL request in the queue (0 pending, 1 handled, 0 unhandled)

D/RIL-IPC ( 1891): 

D/RIL-IPC ( 1891): xmm626_sec_modem_fmt_recv: Received FMT message

D/RIL-IPC ( 1891): xmm626_sec_modem_fmt_recv: Message: aseq=0x6d, command=IPC_NET_PLMN_SEL, type=IPC_TYPE_RESP, size=1

D/RIL-IPC ( 1891): ================================= IPC FMT data =================================

D/RIL-IPC ( 1891): [0000]   02                                                 .

D/RIL-IPC ( 1891): ================================================================================

D/RIL     ( 1891): 0 RIL request in the queue (0 pending, 0 handled, 0 unhandled)

D/RILJ    ( 2563): [0133]< VOICE_REGISTRATION_STATE {1, 7dd, 3ee4efe, 9, null, null, null, null, null, null, null, null, null, null, null}

D/RILJ    ( 2563): [0134]< QUERY_NETWORK_SELECTION_MODE {0}

D/GSM     ( 2563): [GsmSST] Poll ServiceState done:  oldSS=[0 home Proximus Proximus 20601  HSDPA CSS not supported -1 -1 RoamInd=-1 DefRoamInd=-1 EmergOnly=false] newSS=[0 home Proximus Proximus 20601  HSDPA CSS not supported -1 -1 RoamInd=-1 DefRoamInd=-1 EmergOnly=false] oldGprs=1 newData=1 oldMaxDataCalls=1 mNewMaxDataCalls=1 oldReasonDataDenied=-1 mNewReasonDataDenied=-1 oldType=HSDPA newType=HSDPA

D/RIL-IPC ( 1891): 

D/RIL-IPC ( 1891): xmm626_sec_modem_fmt_recv: Received FMT message

D/RIL-IPC ( 1891): xmm626_sec_modem_fmt_recv: Message: aseq=0xff, command=IPC_NET_REGIST, type=IPC_TYPE_NOTI, size=11

D/RIL-IPC ( 1891): ================================= IPC FMT data =================================

D/RIL-IPC ( 1891): [0000]   04 02 02 9B DD 07 FE 4E  EE 03 00                  .......N ...

D/RIL-IPC ( 1891): ================================================================================

D/RIL-IPC ( 1891): 

D/RIL-IPC ( 1891): xmm626_sec_modem_fmt_recv: Received FMT message

D/RIL-IPC ( 1891): xmm626_sec_modem_fmt_recv: Message: aseq=0xff, command=IPC_NET_REGIST, type=IPC_TYPE_NOTI, size=11

D/RIL-IPC ( 1891): ================================= IPC FMT data =================================

D/RIL-IPC ( 1891): [0000]   04 03 02 9B DD 07 FE 4E  EE 03 00                  .......N ...

D/RIL-IPC ( 1891): ================================================================================

D/RIL-IPC ( 1891): 

D/RILJ    ( 2563): [UNSL]< UNSOL_RESPONSE_VOICE_NETWORK_STATE_CHANGED

D/RIL-IPC ( 1891): xmm626_sec_modem_fmt_recv: Received FMT message

D/RIL-IPC ( 1891): xmm626_sec_modem_fmt_recv: Message: aseq=0x00, command=IPC_NET_SERVING_NETWORK, type=IPC_TYPE_NOTI, size=11

D/RIL-IPC ( 1891): ================================= IPC FMT data =================================

D/RIL-IPC ( 1891): [0000]   02 02 04 32 30 36 30 31  23 DD 07                  ...20601 #..

D/RIL-IPC ( 1891): ================================================================================

D/RILJ    ( 2563): [UNSL]< UNSOL_RESPONSE_VOICE_NETWORK_STATE_CHANGED

D/RILJ    ( 2563): [0135]> OPERATOR

D/RILJ    ( 2563): [UNSL]< UNSOL_RESPONSE_VOICE_NETWORK_STATE_CHANGED

D/RIL     ( 1891): 1 RIL request in the queue (1 pending, 0 handled, 0 unhandled)

D/RILJ    ( 2563): [0136]> DATA_REGISTRATION_STATE

D/RIL     ( 1891): 3 RIL requests data in the queue

D/RIL     ( 1891): 0 RIL request in the queue (0 pending, 0 handled, 0 unhandled)

D/RIL     ( 1891): 2 RIL requests data in the queue

D/RILJ    ( 2563): [0135]< OPERATOR {Proximus, Proximus, 20601}

D/RILJ    ( 2563): [0137]> VOICE_REGISTRATION_STATE

D/RIL     ( 1891): 1 RIL request in the queue (1 pending, 0 handled, 0 unhandled)

D/RIL     ( 1891): 2 RIL requests data in the queue

D/RIL     ( 1891): 0 RIL request in the queue (0 pending, 0 handled, 0 unhandled)

D/RIL     ( 1891): 1 RIL request data in the queue

D/RIL     ( 1891): 1 RIL request in the queue (1 pending, 0 handled, 0 unhandled)

D/RIL     ( 1891): 1 RIL request data in the queue

D/RIL     ( 1891): 0 RIL request in the queue (0 pending, 0 handled, 0 unhandled)

D/RILJ    ( 2563): [0138]> QUERY_NETWORK_SELECTION_MODE

D/RILJ    ( 2563): [0136]< DATA_REGISTRATION_STATE {1, 7dd, 3ee4efe, 9, 3}

D/RIL     ( 1891): 1 RIL request in the queue (1 pending, 0 handled, 0 unhandled)

D/RILJ    ( 2563): [0139]> OPERATOR

D/RIL-IPC ( 1891): 

D/RIL-IPC ( 1891): xmm626_sec_modem_fmt_recv: Received FMT message

D/RIL-IPC ( 1891): xmm626_sec_modem_fmt_recv: Message: aseq=0x00, command=IPC_DISP_RSSI_INFO, type=IPC_TYPE_NOTI, size=1

D/RIL-IPC ( 1891): ================================= IPC FMT data =================================

D/RIL-IPC ( 1891): [0000]   52                                                 R

D/RIL-IPC ( 1891): ================================================================================

D/RIL     ( 1891): Signal strength is 15

D/RIL-IPC ( 1891): 

D/RIL-IPC ( 1891): xmm626_sec_modem_fmt_send: Sent FMT message

D/RIL-IPC ( 1891): xmm626_sec_modem_fmt_send: Message: mseq=0x6e, command=IPC_NET_PLMN_SEL, type=IPC_TYPE_GET, size=0

D/RILJ    ( 2563): [0137]< VOICE_REGISTRATION_STATE {1, 7dd, 3ee4efe, 9, null, null, null, null, null, null, null, null, null, null, null}

D/RIL-IPC ( 1891): 

D/RIL-IPC ( 1891): xmm626_sec_modem_fmt_recv: Received FMT message

D/RIL-IPC ( 1891): xmm626_sec_modem_fmt_recv: Message: aseq=0x6e, command=IPC_NET_PLMN_SEL, type=IPC_TYPE_RESP, size=1

D/RIL-IPC ( 1891): ================================= IPC FMT data =================================

D/RIL-IPC ( 1891): [0000]   02                                                 .

D/RIL-IPC ( 1891): ================================================================================

D/RIL     ( 1891): 0 RIL request in the queue (0 pending, 0 handled, 0 unhandled)

D/RILJ    ( 2563): [0140]> DATA_REGISTRATION_STATE

D/RIL     ( 1891): 1 RIL request in the queue (1 pending, 0 handled, 0 unhandled)

D/RIL-IPC ( 1891): 

D/RIL-IPC ( 1891): xmm626_sec_modem_fmt_send: Sent FMT message

D/RIL-IPC ( 1891): xmm626_sec_modem_fmt_send: Message: mseq=0x6f, command=IPC_NET_SERVING_NETWORK, type=IPC_TYPE_GET, size=0

D/RILJ    ( 2563): [0138]< QUERY_NETWORK_SELECTION_MODE {0}

D/RIL-IPC ( 1891): 

D/RIL-IPC ( 1891): xmm626_sec_modem_fmt_recv: Received FMT message

D/RIL-IPC ( 1891): xmm626_sec_modem_fmt_recv: Message: aseq=0x6f, command=IPC_NET_SERVING_NETWORK, type=IPC_TYPE_RESP, size=11

D/RIL-IPC ( 1891): ================================= IPC FMT data =================================

D/RIL-IPC ( 1891): [0000]   02 02 04 32 30 36 30 31  23 DD 07                  ...20601 #..

D/RIL-IPC ( 1891): ================================================================================

D/RIL     ( 1891): 0 RIL request in the queue (0 pending, 0 handled, 0 unhandled)

D/RIL     ( 1891): 1 RIL request in the queue (1 pending, 0 handled, 0 unhandled)

D/RIL-IPC ( 1891): 

D/RIL-IPC ( 1891): xmm626_sec_modem_fmt_send: Sent FMT message

D/RIL-IPC ( 1891): xmm626_sec_modem_fmt_send: Message: mseq=0x70, command=IPC_NET_REGIST, type=IPC_TYPE_GET, size=2

D/RIL-IPC ( 1891): ================================= IPC FMT data =================================

D/RIL-IPC ( 1891): [0000]   FF 03                                              ..

D/RIL-IPC ( 1891): ================================================================================

D/RILJ    ( 2563): [0141]> VOICE_REGISTRATION_STATE

D/RILJ    ( 2563): [0139]< OPERATOR {Proximus, Proximus, 20601}

D/RIL-IPC ( 1891): 

D/RIL-IPC ( 1891): xmm626_sec_modem_fmt_recv: Received FMT message

D/RIL-IPC ( 1891): xmm626_sec_modem_fmt_recv: Message: aseq=0x70, command=IPC_NET_REGIST, type=IPC_TYPE_RESP, size=11

D/RIL-IPC ( 1891): ================================= IPC FMT data =================================

D/RIL-IPC ( 1891): [0000]   04 03 02 9B DD 07 FE 4E  EE 03 00                  .......N ...

D/RIL-IPC ( 1891): ================================================================================

D/RIL     ( 1891): 0 RIL request in the queue (0 pending, 0 handled, 0 unhandled)

D/RIL     ( 1891): 1 RIL request in the queue (1 pending, 0 handled, 0 unhandled)

D/RIL-IPC ( 1891): 

D/RILJ    ( 2563): [0140]< DATA_REGISTRATION_STATE {1, 7dd, 3ee4efe, 9, 3}

D/RILJ    ( 2563): [0142]> QUERY_NETWORK_SELECTION_MODE

D/RIL-IPC ( 1891): xmm626_sec_modem_fmt_send: Sent FMT message

D/RIL-IPC ( 1891): xmm626_sec_modem_fmt_send: Message: mseq=0x71, command=IPC_NET_REGIST, type=IPC_TYPE_GET, size=2

D/RIL-IPC ( 1891): ================================= IPC FMT data =================================

D/RIL-IPC ( 1891): [0000]   FF 02                                              ..

D/RIL-IPC ( 1891): ================================================================================

D/RIL-IPC ( 1891): 

D/RIL-IPC ( 1891): xmm626_sec_modem_fmt_recv: Received FMT message

D/RIL-IPC ( 1891): xmm626_sec_modem_fmt_recv: Message: aseq=0x71, command=IPC_NET_REGIST, type=IPC_TYPE_RESP, size=11

D/RIL-IPC ( 1891): ================================= IPC FMT data =================================

D/RIL-IPC ( 1891): [0000]   04 02 02 9B DD 07 FE 4E  EE 03 00                  .......N ...

D/RIL-IPC ( 1891): ================================================================================

D/RIL     ( 1891): 0 RIL request in the queue (0 pending, 0 handled, 0 unhandled)

D/RILJ    ( 2563): [0143]> OPERATOR

D/RIL     ( 1891): 1 RIL request in the queue (1 pending, 0 handled, 0 unhandled)

D/RIL-IPC ( 1891): 

D/RIL-IPC ( 1891): xmm626_sec_modem_fmt_send: Sent FMT message

D/RIL-IPC ( 1891): xmm626_sec_modem_fmt_send: Message: mseq=0x72, command=IPC_NET_PLMN_SEL, type=IPC_TYPE_GET, size=0

D/RILJ    ( 2563): [0144]> DATA_REGISTRATION_STATE

D/RIL-IPC ( 1891): 

D/RIL-IPC ( 1891): xmm626_sec_modem_fmt_recv: Received FMT message

D/RIL-IPC ( 1891): xmm626_sec_modem_fmt_recv: Message: aseq=0x72, command=IPC_NET_PLMN_SEL, type=IPC_TYPE_RESP, size=1

D/RIL-IPC ( 1891): ================================= IPC FMT data =================================

D/RIL-IPC ( 1891): [0000]   02                                                 .

D/RIL-IPC ( 1891): ================================================================================

D/RIL     ( 1891): 0 RIL request in the queue (0 pending, 0 handled, 0 unhandled)

D/RIL     ( 1891): 1 RIL request in the queue (1 pending, 0 handled, 0 unhandled)

D/RIL-IPC ( 1891): 

D/RIL-IPC ( 1891): xmm626_sec_modem_fmt_send: Sent FMT message

D/RIL-IPC ( 1891): xmm626_sec_modem_fmt_send: Message: mseq=0x73, command=IPC_NET_SERVING_NETWORK, type=IPC_TYPE_GET, size=0

D/RILJ    ( 2563): [0141]< VOICE_REGISTRATION_STATE {1, 7dd, 3ee4efe, 9, null, null, null, null, null, null, null, null, null, null, null}

D/RILJ    ( 2563): [0145]> VOICE_REGISTRATION_STATE

D/RIL     ( 1891): 2 RIL requests in the queue (1 pending, 1 handled, 0 unhandled)

D/RIL-IPC ( 1891): 

D/RIL-IPC ( 1891): xmm626_sec_modem_fmt_recv: Received FMT message

D/RIL-IPC ( 1891): xmm626_sec_modem_fmt_recv: Message: aseq=0x73, command=IPC_NET_SERVING_NETWORK, type=IPC_TYPE_RESP, size=11

D/RIL-IPC ( 1891): ================================= IPC FMT data =================================

D/RIL-IPC ( 1891): [0000]   02 02 04 32 30 36 30 31  23 DD 07                  ...20601 #..

D/RIL-IPC ( 1891): ================================================================================

D/RIL     ( 1891): 1 RIL request in the queue (1 pending, 0 handled, 0 unhandled)

D/RIL-IPC ( 1891): 

D/RIL-IPC ( 1891): xmm626_sec_modem_fmt_send: Sent FMT message

D/RIL-IPC ( 1891): xmm626_sec_modem_fmt_send: Message: mseq=0x74, command=IPC_NET_REGIST, type=IPC_TYPE_GET, size=2

D/RIL-IPC ( 1891): ================================= IPC FMT data =================================

D/RIL-IPC ( 1891): [0000]   FF 03                                              ..

D/RIL-IPC ( 1891): ================================================================================

D/RILJ    ( 2563): [0146]> QUERY_NETWORK_SELECTION_MODE

D/RIL-IPC ( 1891): 

D/RIL-IPC ( 1891): xmm626_sec_modem_fmt_recv: Received FMT message

D/RIL-IPC ( 1891): xmm626_sec_modem_fmt_recv: Message: aseq=0x74, command=IPC_NET_REGIST, type=IPC_TYPE_RESP, size=11

D/RIL-IPC ( 1891): ================================= IPC FMT data =================================

D/RIL-IPC ( 1891): [0000]   04 03 02 9B DD 07 FE 4E  EE 03 00                  .......N ...

D/RIL-IPC ( 1891): ================================================================================

D/RIL     ( 1891): 0 RIL request in the queue (0 pending, 0 handled, 0 unhandled)

D/RILJ    ( 2563): [0142]< QUERY_NETWORK_SELECTION_MODE {0}

D/RIL     ( 1891): 1 RIL request in the queue (1 pending, 0 handled, 0 unhandled)

D/RIL-IPC ( 1891): 

D/RIL-IPC ( 1891): xmm626_sec_modem_fmt_send: Sent FMT message

D/RIL-IPC ( 1891): xmm626_sec_modem_fmt_send: Message: mseq=0x75, command=IPC_NET_REGIST, type=IPC_TYPE_GET, size=2

D/RIL-IPC ( 1891): ================================= IPC FMT data =================================

D/RIL-IPC ( 1891): [0000]   FF 02                                              ..

D/RIL-IPC ( 1891): ================================================================================

D/RIL-IPC ( 1891): 

D/RIL-IPC ( 1891): xmm626_sec_modem_fmt_recv: Received FMT message

D/RIL-IPC ( 1891): xmm626_sec_modem_fmt_recv: Message: aseq=0x75, command=IPC_NET_REGIST, type=IPC_TYPE_RESP, size=11

D/RIL-IPC ( 1891): ================================= IPC FMT data =================================

D/RIL-IPC ( 1891): [0000]   04 02 02 9B DD 07 FE 4E  EE 03 00                  .......N ...

D/RIL-IPC ( 1891): ================================================================================

D/RIL     ( 1891): 0 RIL request in the queue (0 pending, 0 handled, 0 unhandled)

D/RILJ    ( 2563): [0143]< OPERATOR {Proximus, Proximus, 20601}

D/RIL     ( 1891): 1 RIL request in the queue (1 pending, 0 handled, 0 unhandled)

D/RIL-IPC ( 1891): 

D/RIL-IPC ( 1891): xmm626_sec_modem_fmt_send: Sent FMT message

D/RIL-IPC ( 1891): xmm626_sec_modem_fmt_send: Message: mseq=0x76, command=IPC_NET_PLMN_SEL, type=IPC_TYPE_GET, size=0

D/RILJ    ( 2563): [0144]< DATA_REGISTRATION_STATE {1, 7dd, 3ee4efe, 9, 3}

D/RIL-IPC ( 1891): 

D/RIL-IPC ( 1891): xmm626_sec_modem_fmt_recv: Received FMT message

D/RIL-IPC ( 1891): xmm626_sec_modem_fmt_recv: Message: aseq=0x76, command=IPC_NET_PLMN_SEL, type=IPC_TYPE_RESP, size=1

D/RIL-IPC ( 1891): ================================= IPC FMT data =================================

D/RIL-IPC ( 1891): [0000]   02                                                 .

D/RIL-IPC ( 1891): ================================================================================

D/RIL     ( 1891): 0 RIL request in the queue (0 pending, 0 handled, 0 unhandled)

D/RILJ    ( 2563): [0145]< VOICE_REGISTRATION_STATE {1, 7dd, 3ee4efe, 9, null, null, null, null, null, null, null, null, null, null, null}

D/RILJ    ( 2563): [0146]< QUERY_NETWORK_SELECTION_MODE {0}

D/GSM     ( 2563): [GsmSST] Poll ServiceState done:  oldSS=[0 home Proximus Proximus 20601  HSDPA CSS not supported -1 -1 RoamInd=-1 DefRoamInd=-1 EmergOnly=false] newSS=[0 home Proximus Proximus 20601  HSDPA CSS not supported -1 -1 RoamInd=-1 DefRoamInd=-1 EmergOnly=false] oldGprs=1 newData=0 oldMaxDataCalls=1 mNewMaxDataCalls=1 oldReasonDataDenied=-1 mNewReasonDataDenied=-1 oldType=HSDPA newType=HSDPA

D/GSM     ( 2563): [GsmDCT] handleMessage msg={ what=270352 when=0 obj=android.os.AsyncResult@41d1a868 }

D/GSM     ( 2563): [GsmDCT] onDataConnectionAttached

D/GSM     ( 2563): [GsmDCT] overall state is IDLE

D/GSM     ( 2563): [GsmDCT] notifyOffApnOfAvailability type:dun

D/GSM     ( 2563): [GsmDCT] isDataPossible(dun): possible=true isDataAllowed=true apnTypePossible=true apnContextisEnabled=false apnContextState()=IDLE

D/GSM     ( 2563): [GsmDCT] get active apn string for type:dun

D/GSM     ( 2563): [GsmDCT] notifyOffApnOfAvailability type:supl

D/GSM     ( 2563): [GsmDCT] isDataPossible(supl): possible=true isDataAllowed=true apnTypePossible=true apnContextisEnabled=false apnContextState()=IDLE

D/GSM     ( 2563): [GsmDCT] get active apn string for type:supl

D/GSM     ( 2563): [GsmDCT] notifyOffApnOfAvailability type:hipri

D/GSM     ( 2563): [GsmDCT] isDataPossible(hipri): possible=true isDataAllowed=true apnTypePossible=true apnContextisEnabled=false apnContextState()=IDLE

D/GSM     ( 2563): [GsmDCT] get active apn string for type:hipri

D/GSM     ( 2563): [GsmDCT] notifyOffApnsOfAvailability skipped apn due to isReady==false: {mApnType=default mState=IDLE mWaitingApns=null mWaitingApnsPermanentFailureCountDown=0 mApnSetting=null mDataConnectionAc=null mReason=simLoaded mRetryCount=0 mDataEnabled=true mDependencyMet=true}

D/GSM     ( 2563): [GsmDCT] notifyOffApnOfAvailability type:mms

D/GSM     ( 2563): [GsmDCT] isDataPossible(mms): possible=true isDataAllowed=true apnTypePossible=true apnContextisEnabled=false apnContextState()=IDLE

D/GSM     ( 2563): [GsmDCT] get active apn string for type:mms

D/GSM     ( 2563): [ApnContext:dun] setRetryCount: 0

D/GSM     ( 2563): [ApnContext:supl] setRetryCount: 0

D/GSM     ( 2563): [ApnContext:hipri] setRetryCount: 0

D/GSM     ( 2563): [ApnContext:default] setRetryCount: 0

D/GSM     ( 2563): [ApnContext:mms] setRetryCount: 0

D/GSM     ( 2563): [ApnContext:default] set reason as dataAttached,current state IDLE

D/GSM     ( 2563): [GsmDCT] trySetupData for type:default due to dataAttached

D/GSM     ( 2563): [GsmDCT] trySetupData with mIsPsRestricted=false

D/GSM     ( 2563): [GsmDCT] notifyOffApnOfAvailability type:dun

D/GSM     ( 2563): [GsmDCT] isDataPossible(dun): possible=true isDataAllowed=true apnTypePossible=true apnContextisEnabled=false apnContextState()=IDLE

D/GSM     ( 2563): [GsmDCT] get active apn string for type:dun

D/GSM     ( 2563): [GsmDCT] notifyOffApnOfAvailability type:supl

D/GSM     ( 2563): [GsmDCT] isDataPossible(supl): possible=true isDataAllowed=true apnTypePossible=true apnContextisEnabled=false apnContextState()=IDLE

D/GSM     ( 2563): [GsmDCT] get active apn string for type:supl

D/GSM     ( 2563): [GsmDCT] notifyOffApnOfAvailability type:hipri

D/GSM     ( 2563): [GsmDCT] isDataPossible(hipri): possible=true isDataAllowed=true apnTypePossible=true apnContextisEnabled=false apnContextState()=IDLE

D/GSM     ( 2563): [GsmDCT] get active apn string for type:hipri

D/GSM     ( 2563): [GsmDCT] notifyOffApnsOfAvailability skipped apn due to isReady==false: {mApnType=default mState=IDLE mWaitingApns=null mWaitingApnsPermanentFailureCountDown=0 mApnSetting=null mDataConnectionAc=null mReason=dataAttached mRetryCount=0 mDataEnabled=true mDependencyMet=true}

D/GSM     ( 2563): [GsmDCT] notifyOffApnOfAvailability type:mms

D/GSM     ( 2563): [GsmDCT] isDataPossible(mms): possible=true isDataAllowed=true apnTypePossible=true apnContextisEnabled=false apnContextState()=IDLE

D/GSM     ( 2563): [GsmDCT] get active apn string for type:mms

D/RIL-IPC ( 1891): 

D/RIL-IPC ( 1891): xmm626_sec_modem_fmt_recv: Received FMT message

D/RIL-IPC ( 1891): xmm626_sec_modem_fmt_recv: Message: aseq=0x76, command=IPC_PB_ACCESS, type=IPC_TYPE_NOTI, size=5

D/RIL-IPC ( 1891): ================================= IPC FMT data =================================

D/RIL-IPC ( 1891): [0000]   01 01 0C FF FF                                     .....

D/RIL-IPC ( 1891): ================================================================================

D/RIL-IPC ( 1891): Unhandled IPC FMT message: IPC_PB_ACCESS

D/RIL-IPC ( 1891): 

D/RIL-IPC ( 1891): xmm626_sec_modem_fmt_recv: Received FMT message

D/RIL-IPC ( 1891): xmm626_sec_modem_fmt_recv: Message: aseq=0x76, command=IPC_PB_3GPB_CAPA, type=IPC_TYPE_NOTI, size=86

D/RIL-IPC ( 1891): ================================= IPC FMT data =================================

D/RIL-IPC ( 1891): [0000]   00 0C 01 90 01 14 00 00  00 02 90 01 28 00 00 00   ........ ....(...

D/RIL-IPC ( 1891): [0010]   03 90 01 28 00 00 00 04  F4 01 23 00 00 00 05 00   ...(.... ..#.....

D/RIL-IPC ( 1891): [0020]   00 FF 00 00 00 06 0A 00  0A 00 0A 00 08 00 00 28   ........ .......(

D/RIL-IPC ( 1891): [0030]   00 00 00 09 00 00 28 00  00 00 0A 00 00 28 00 00   ......(. .....(..

D/RIL-IPC ( 1891): [0040]   00 0B 00 00 FE 00 00 00  0C 00 00 FF 00 00 00 0D   ........ ........

D/RIL-IPC ( 1891): [0050]   00 00 F5 00 00 00                                  ......

D/RIL-IPC ( 1891): ================================================================================

D/RIL-IPC ( 1891): Unhandled IPC FMT message: IPC_PB_3GPB_CAPA

D/RIL-IPC ( 1891): 

D/RIL-IPC ( 1891): xmm626_sec_modem_fmt_recv: Received FMT message

D/RIL-IPC ( 1891): xmm626_sec_modem_fmt_recv: Message: aseq=0x76, command=IPC_SEC_PIN_STATUS, type=IPC_TYPE_NOTI, size=2

D/RIL-IPC ( 1891): ================================= IPC FMT data =================================

D/RIL-IPC ( 1891): [0000]   83 00                                              ..

D/RIL-IPC ( 1891): ================================================================================

D/RIL     ( 1891): ipc2ril_sec_pin_status_response: Selecting status application 2 on 10

D/RILJ    ( 2563): [UNSL]< UNSOL_RESPONSE_SIM_STATUS_CHANGED

D/RIL_UiccController( 2563): Received EVENT_ICC_STATUS_CHANGED, calling getIccCardStatus

D/RILJ    ( 2563): [0147]> GET_SIM_STATUS

D/RIL     ( 1891): 1 RIL request in the queue (1 pending, 0 handled, 0 unhandled)

D/RIL     ( 1891): 1 RIL request data in the queue

D/RIL     ( 1891): 0 RIL request in the queue (0 pending, 0 handled, 0 unhandled)

D/RILJ    ( 2563): [0147]< GET_SIM_STATUS IccCardState {CARDSTATE_PRESENT,PINSTATE_UNKNOWN,num_apps=1,gsm_id=0{APPTYPE_SIM,APPSTATE_READY},cdma_id=-1,ims_id=-1}

D/RIL_UiccController( 2563): Received EVENT_GET_ICC_STATUS_DONE

D/RIL_UiccCard( 2563): 1 applications

D/RIL_UiccCardApplication( 2563): APPTYPE_SIM update. New {APPTYPE_SIM,APPSTATE_READY}

D/RIL_UiccCard( 2563): update: radioState=RADIO_ON mLastRadioState=RADIO_ON

D/RIL_UiccController( 2563): Notifying IccChangedRegistrants

D/GSM     ( 2563): [GsmDCT] handleMessage msg={ what=270369 when=-1ms obj=android.os.AsyncResult@41d259b0 }

